<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.86" y2="0" width="0.254" layer="20"/>
<wire x1="22.86" y1="0" x2="22.86" y2="26.67" width="0.254" layer="20"/>
<wire x1="22.86" y1="26.67" x2="0" y2="26.67" width="0.254" layer="20" curve="180"/>
<wire x1="0" y1="26.67" x2="0" y2="0" width="0.254" layer="20"/>
<text>+</text>
<text>DNP</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="EIA3216">
</package>
<package name="ANTENNA-CHIP5">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="FIDUCIAL-1X2">
</package>
<package name="QFN20">
</package>
<package name="PAD.03X.05">
</package>
</packages>
</library>
<library name="PES_DigitalIC">
<packages>
<package name="SOIC20W">
</package>
</packages>
</library>
<library name="PES_DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-123_MINI-SMA">
<description>&lt;b&gt;Molded plasitc,JEDEC SOD-123/Mini SMA&lt;/b&gt;&lt;p&gt;
Source: Comchip CGRM4001-G.pdf</description>
</package>
</packages>
</library>
<library name="PES_Passives">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="PES_Connectors">
<packages>
<package name="2X3">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="SparkFun" package="CRYSTAL-SMD-5X3" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun" package="C0402" value="3.9nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="C0402" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="C0402" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="C0402" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="C0402" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="C0402" value="33nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="SparkFun" package="C0402" value="2.7nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="C0402" value="2.2nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="C0402" value="4.7pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun" package="C0402" value="1.0pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun" package="C0402" value="1.5pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun" package="C0402" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun" package="C0402" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="SparkFun" package="C0402" value="8.2nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun" package="SOT23-5" value="3.3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$3" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U1" library="SparkFun" package="QFN20" value="NRF24L01SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun" package="ANTENNA-CHIP5" value="ANTENNA2SMD5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="SparkFun" package="PAD.03X.05" value=""/>
<element name="U$1" library="PES_DigitalIC" package="SOIC20W" value="ATTINY861"/>
<element name="D1" library="PES_DiscreteSemi" package="SOD-123_MINI-SMA" value=""/>
<element name="C11" library="PES_Passives" package="0603-CAP" value="0.1uF"/>
<element name="R3" library="PES_Passives" package="0603-RES" value="4.7k"/>
<element name="C12" library="PES_Passives" package="0603-CAP" value="0.1uF"/>
<element name="J1" library="PES_Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="JP1" library="PES_Connectors" package="1X02" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="C10" pad="C"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="0"/>
<contactref element="C11" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="C12" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="C10" pad="A"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="18"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="R3" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="U$1" pad="5"/>
<contactref element="C12" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="L1" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="L2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="N$5">
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="ANT">
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="Y1" pad="FEED"/>
</signal>
<signal name="N$3">
<contactref element="L3" pad="1"/>
<contactref element="L2" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$9">
<contactref element="C7" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="CE">
<contactref element="U1" pad="1"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="CSN">
<contactref element="U1" pad="2"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="3"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="4"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="5"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="IQR">
<contactref element="U1" pad="6"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="RAW">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="R3" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="U$1" pad="10"/>
<contactref element="C11" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="12"/>
</signal>
<signal name="SPI_MISO">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="SPI_SCK">
<contactref element="J1" pad="3"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
