(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 0)
    (area 83.594999 40.224999 236.575001 106.715001)
    (thickness 1.6)
    (drawings 15)
    (tracks 4048)
    (zones 0)
    (modules 200)
    (nets 247)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.0762)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 170.3 74.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDREF)
  (net 2 "Net-(C401-Pad1)")
  (net 3 /ADC/Vcm12)
  (net 4 /ADC/Vcm34)
  (net 5 +1V8)
  (net 6 "Net-(C406-Pad2)")
  (net 7 "Net-(C406-Pad1)")
  (net 8 GND)
  (net 9 "Net-(C601-Pad1)")
  (net 10 "Net-(C602-Pad2)")
  (net 11 "Net-(C801-Pad1)")
  (net 12 "Net-(C802-Pad2)")
  (net 13 "Net-(C1001-Pad1)")
  (net 14 "Net-(C1002-Pad2)")
  (net 15 "Net-(C1201-Pad1)")
  (net 16 "Net-(C1202-Pad2)")
  (net 17 /Power/Vin)
  (net 18 "Net-(C1304-Pad2)")
  (net 19 "Net-(C1304-Pad1)")
  (net 20 -5V)
  (net 21 "Net-(C1307-Pad2)")
  (net 22 "Net-(C1307-Pad1)")
  (net 23 +5V)
  (net 24 /ADC/Filter1/Vin)
  (net 25 /ADC/Filter2/Vin)
  (net 26 /ADC/Filter3/Vin)
  (net 27 /ADC/Filter4/Vin)
  (net 28 "Net-(J602-Pad1)")
  (net 29 "Net-(J603-Pad1)")
  (net 30 "Net-(J605-Pad1)")
  (net 31 "Net-(J607-Pad1)")
  (net 32 "Net-(J802-Pad1)")
  (net 33 "Net-(J803-Pad1)")
  (net 34 "Net-(J805-Pad1)")
  (net 35 "Net-(J807-Pad1)")
  (net 36 "Net-(J1002-Pad1)")
  (net 37 "Net-(J1003-Pad1)")
  (net 38 "Net-(J1005-Pad1)")
  (net 39 "Net-(J1007-Pad1)")
  (net 40 "Net-(J1202-Pad1)")
  (net 41 "Net-(J1203-Pad1)")
  (net 42 "Net-(J1205-Pad1)")
  (net 43 "Net-(J1207-Pad1)")
  (net 44 "Net-(R201-Pad2)")
  (net 45 "Net-(R402-Pad1)")
  (net 46 "/ADC/Diff Conv1/Vin")
  (net 47 "Net-(R601-Pad2)")
  (net 48 "Net-(R602-Pad2)")
  (net 49 "Net-(R603-Pad2)")
  (net 50 "Net-(R604-Pad1)")
  (net 51 "Net-(R606-Pad2)")
  (net 52 "Net-(R610-Pad2)")
  (net 53 "/ADC/Diff Conv2/Vin")
  (net 54 "Net-(R801-Pad2)")
  (net 55 "Net-(R802-Pad2)")
  (net 56 "Net-(R803-Pad2)")
  (net 57 "Net-(R804-Pad1)")
  (net 58 "Net-(R806-Pad2)")
  (net 59 "Net-(R810-Pad2)")
  (net 60 "/ADC/Diff Conv3/Vin")
  (net 61 "Net-(R1001-Pad2)")
  (net 62 "Net-(R1002-Pad2)")
  (net 63 "Net-(R1003-Pad2)")
  (net 64 "Net-(R1004-Pad1)")
  (net 65 "Net-(R1006-Pad2)")
  (net 66 "Net-(R1010-Pad2)")
  (net 67 "/ADC/Diff Conv4/Vin")
  (net 68 "Net-(R1201-Pad2)")
  (net 69 "Net-(R1202-Pad2)")
  (net 70 "Net-(R1203-Pad2)")
  (net 71 "Net-(R1204-Pad1)")
  (net 72 "Net-(R1206-Pad2)")
  (net 73 "Net-(R1210-Pad2)")
  (net 74 /vccio_en)
  (net 75 /v_good)
  (net 76 /data_clk-)
  (net 77 /data_clk+)
  (net 78 /fr_clk-)
  (net 79 /fr_clk+)
  (net 80 /out3a-)
  (net 81 /out3a+)
  (net 82 /out3b-)
  (net 83 /out4b+)
  (net 84 /out4a+)
  (net 85 /out4b-)
  (net 86 /out3b+)
  (net 87 /out4a-)
  (net 88 /out1a+)
  (net 89 /out1b-)
  (net 90 /out1b+)
  (net 91 /out2a+)
  (net 92 /out2b+)
  (net 93 /out2a-)
  (net 94 /out2b-)
  (net 95 /out1a-)
  (net 96 /ADC/v1+)
  (net 97 /ADC/v1-)
  (net 98 /ADC/v2+)
  (net 99 /ADC/v2-)
  (net 100 /ADC/v3+)
  (net 101 /ADC/v3-)
  (net 102 /ADC/v4+)
  (net 103 /ADC/v4-)
  (net 104 "/ADC/Diff Conv1/v+")
  (net 105 "/ADC/Diff Conv1/v-")
  (net 106 "/ADC/Diff Conv2/v+")
  (net 107 "/ADC/Diff Conv2/v-")
  (net 108 "/ADC/Diff Conv3/v+")
  (net 109 "/ADC/Diff Conv3/v-")
  (net 110 "/ADC/Diff Conv4/v+")
  (net 111 "/ADC/Diff Conv4/v-")
  (net 112 /MISO)
  (net 113 /SCK)
  (net 114 /MOSI)
  (net 115 /~CS)
  (net 116 "Net-(J1301-Pad3)")
  (net 117 "Net-(RV601-Pad3)")
  (net 118 "Net-(RV602-Pad3)")
  (net 119 "Net-(RV801-Pad3)")
  (net 120 "Net-(RV802-Pad3)")
  (net 121 "Net-(RV1001-Pad3)")
  (net 122 "Net-(RV1002-Pad3)")
  (net 123 "Net-(RV1201-Pad3)")
  (net 124 "Net-(RV1202-Pad3)")
  (net 125 /MicroZed-JX1/LVDS12-)
  (net 126 /MicroZed-JX1/LVDS12+)
  (net 127 "Net-(U201-Pad7)")
  (net 128 "Net-(U201-Pad3)")
  (net 129 "Net-(U201-Pad1)")
  (net 130 "Net-(U201-Pad89)")
  (net 131 "Net-(U201-Pad87)")
  (net 132 "Net-(U201-Pad93)")
  (net 133 "Net-(U201-Pad91)")
  (net 134 /MicroZed-JX1/LVDS20+)
  (net 135 "Net-(U201-Pad83)")
  (net 136 "Net-(U201-Pad81)")
  (net 137 /MicroZed-JX1/LVDS20-)
  (net 138 "Net-(U201-Pad92)")
  (net 139 "Net-(U201-Pad94)")
  (net 140 "Net-(U201-Pad84)")
  (net 141 "Net-(U201-Pad90)")
  (net 142 "Net-(U201-Pad82)")
  (net 143 "Net-(U201-Pad88)")
  (net 144 "Net-(U201-Pad68)")
  (net 145 "Net-(U201-Pad62)")
  (net 146 "Net-(U201-Pad64)")
  (net 147 "Net-(U201-Pad76)")
  (net 148 "Net-(U201-Pad70)")
  (net 149 "Net-(U201-Pad74)")
  (net 150 "Net-(U201-Pad50)")
  (net 151 "Net-(U201-Pad54)")
  (net 152 "Net-(U201-Pad56)")
  (net 153 "Net-(U201-Pad44)")
  (net 154 "Net-(U201-Pad48)")
  (net 155 "Net-(U201-Pad42)")
  (net 156 "Net-(U201-Pad38)")
  (net 157 "Net-(U201-Pad36)")
  (net 158 "Net-(U201-Pad32)")
  (net 159 "Net-(U201-Pad30)")
  (net 160 "Net-(U201-Pad26)")
  (net 161 "Net-(U201-Pad24)")
  (net 162 "Net-(U201-Pad20)")
  (net 163 "Net-(U201-Pad14)")
  (net 164 /MicroZed-JX1/SE1)
  (net 165 "Net-(U201-Pad18)")
  (net 166 "Net-(U201-Pad12)")
  (net 167 "Net-(U201-Pad6)")
  (net 168 "Net-(U201-Pad4)")
  (net 169 "Net-(U201-Pad2)")
  (net 170 "Net-(U201-Pad8)")
  (net 171 "Net-(U301-Pad49)")
  (net 172 "Net-(U301-Pad47)")
  (net 173 "Net-(U301-Pad43)")
  (net 174 "Net-(U301-Pad41)")
  (net 175 "Net-(U301-Pad37)")
  (net 176 "Net-(U301-Pad35)")
  (net 177 "Net-(U301-Pad31)")
  (net 178 "Net-(U301-Pad17)")
  (net 179 "Net-(U301-Pad23)")
  (net 180 "Net-(U301-Pad13)")
  (net 181 "Net-(U301-Pad19)")
  (net 182 "Net-(U301-Pad29)")
  (net 183 "Net-(U301-Pad25)")
  (net 184 "Net-(U301-Pad5)")
  (net 185 "Net-(U301-Pad7)")
  (net 186 "Net-(U301-Pad3)")
  (net 187 "Net-(U301-Pad1)")
  (net 188 "Net-(U301-Pad9)")
  (net 189 "Net-(U301-Pad89)")
  (net 190 "Net-(U301-Pad87)")
  (net 191 "Net-(U301-Pad93)")
  (net 192 "Net-(U301-Pad97)")
  (net 193 "Net-(U301-Pad99)")
  (net 194 "Net-(U301-Pad95)")
  (net 195 "Net-(U301-Pad73)")
  (net 196 "Net-(U301-Pad69)")
  (net 197 "Net-(U301-Pad67)")
  (net 198 "Net-(U301-Pad61)")
  (net 199 "Net-(U301-Pad53)")
  (net 200 "Net-(U301-Pad63)")
  (net 201 "Net-(U301-Pad55)")
  (net 202 "Net-(U301-Pad83)")
  (net 203 "Net-(U301-Pad81)")
  (net 204 "Net-(U301-Pad75)")
  (net 205 "Net-(U301-Pad100)")
  (net 206 "Net-(U301-Pad96)")
  (net 207 "Net-(U301-Pad98)")
  (net 208 "Net-(U301-Pad94)")
  (net 209 "Net-(U301-Pad84)")
  (net 210 "Net-(U301-Pad90)")
  (net 211 "Net-(U301-Pad82)")
  (net 212 "Net-(U301-Pad88)")
  (net 213 /MicroZed-JX2/LVDS19-)
  (net 214 /MicroZed-JX2/LVDS19+)
  (net 215 /MicroZed-JX2/LVDS11-)
  (net 216 /MicroZed-JX2/LVDS11+)
  (net 217 "Net-(U301-Pad14)")
  (net 218 "Net-(U301-Pad6)")
  (net 219 "Net-(U301-Pad4)")
  (net 220 "Net-(U301-Pad2)")
  (net 221 "Net-(U301-Pad8)")
  (net 222 "Net-(C601-Pad2)")
  (net 223 "Net-(C801-Pad2)")
  (net 224 "Net-(C1001-Pad2)")
  (net 225 "Net-(C1201-Pad2)")
  (net 226 "Net-(C1306-Pad1)")
  (net 227 "Net-(C1306-Pad2)")
  (net 228 /MicroZed-JX1/LVDS2+)
  (net 229 "Net-(U1303-Pad8)")
  (net 230 /ADC/1v8_analog)
  (net 231 /ADC/enc+)
  (net 232 /ADC/enc-)
  (net 233 /MicroZed-JX2/LVDS17+)
  (net 234 /MicroZed-JX2/LVDS17-)
  (net 235 /MicroZed-JX1/LVDS8-)
  (net 236 /MicroZed-JX1/LVDS8+)
  (net 237 /MicroZed-JX1/LVDS4+)
  (net 238 /MicroZed-JX1/LVDS4-)
  (net 239 /MicroZed-JX1/LVDS2-)
  (net 240 /MicroZed-JX1/SE0)
  (net 241 /enc+)
  (net 242 /enc-)
  (net 243 "Net-(D101-Pad1)")
  (net 244 "Net-(D1201-Pad1)")
  (net 245 "Net-(D1202-Pad1)")
  (net 246 "Net-(D1203-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +5V)
    (add_net -5V)
    (add_net /ADC/1v8_analog)
    (add_net "/ADC/Diff Conv1/Vin")
    (add_net "/ADC/Diff Conv1/v+")
    (add_net "/ADC/Diff Conv1/v-")
    (add_net "/ADC/Diff Conv2/Vin")
    (add_net "/ADC/Diff Conv2/v+")
    (add_net "/ADC/Diff Conv2/v-")
    (add_net "/ADC/Diff Conv3/Vin")
    (add_net "/ADC/Diff Conv3/v+")
    (add_net "/ADC/Diff Conv3/v-")
    (add_net "/ADC/Diff Conv4/Vin")
    (add_net "/ADC/Diff Conv4/v+")
    (add_net "/ADC/Diff Conv4/v-")
    (add_net /ADC/Filter1/Vin)
    (add_net /ADC/Filter2/Vin)
    (add_net /ADC/Filter3/Vin)
    (add_net /ADC/Filter4/Vin)
    (add_net /ADC/Vcm12)
    (add_net /ADC/Vcm34)
    (add_net /ADC/enc+)
    (add_net /ADC/enc-)
    (add_net /ADC/v1+)
    (add_net /ADC/v1-)
    (add_net /ADC/v2+)
    (add_net /ADC/v2-)
    (add_net /ADC/v3+)
    (add_net /ADC/v3-)
    (add_net /ADC/v4+)
    (add_net /ADC/v4-)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /MicroZed-JX1/LVDS12+)
    (add_net /MicroZed-JX1/LVDS12-)
    (add_net /MicroZed-JX1/LVDS2+)
    (add_net /MicroZed-JX1/LVDS2-)
    (add_net /MicroZed-JX1/LVDS20+)
    (add_net /MicroZed-JX1/LVDS20-)
    (add_net /MicroZed-JX1/LVDS4+)
    (add_net /MicroZed-JX1/LVDS4-)
    (add_net /MicroZed-JX1/LVDS8+)
    (add_net /MicroZed-JX1/LVDS8-)
    (add_net /MicroZed-JX1/SE0)
    (add_net /MicroZed-JX1/SE1)
    (add_net /MicroZed-JX2/LVDS11+)
    (add_net /MicroZed-JX2/LVDS11-)
    (add_net /MicroZed-JX2/LVDS17+)
    (add_net /MicroZed-JX2/LVDS17-)
    (add_net /MicroZed-JX2/LVDS19+)
    (add_net /MicroZed-JX2/LVDS19-)
    (add_net /Power/Vin)
    (add_net /SCK)
    (add_net /data_clk+)
    (add_net /data_clk-)
    (add_net /enc+)
    (add_net /enc-)
    (add_net /fr_clk+)
    (add_net /fr_clk-)
    (add_net /out1a+)
    (add_net /out1a-)
    (add_net /out1b+)
    (add_net /out1b-)
    (add_net /out2a+)
    (add_net /out2a-)
    (add_net /out2b+)
    (add_net /out2b-)
    (add_net /out3a+)
    (add_net /out3a-)
    (add_net /out3b+)
    (add_net /out3b-)
    (add_net /out4a+)
    (add_net /out4a-)
    (add_net /out4b+)
    (add_net /out4b-)
    (add_net /v_good)
    (add_net /vccio_en)
    (add_net /~CS)
    (add_net GND)
    (add_net GNDREF)
    (add_net "Net-(C1001-Pad1)")
    (add_net "Net-(C1001-Pad2)")
    (add_net "Net-(C1002-Pad2)")
    (add_net "Net-(C1201-Pad1)")
    (add_net "Net-(C1201-Pad2)")
    (add_net "Net-(C1202-Pad2)")
    (add_net "Net-(C1304-Pad1)")
    (add_net "Net-(C1304-Pad2)")
    (add_net "Net-(C1306-Pad1)")
    (add_net "Net-(C1306-Pad2)")
    (add_net "Net-(C1307-Pad1)")
    (add_net "Net-(C1307-Pad2)")
    (add_net "Net-(C401-Pad1)")
    (add_net "Net-(C406-Pad1)")
    (add_net "Net-(C406-Pad2)")
    (add_net "Net-(C601-Pad1)")
    (add_net "Net-(C601-Pad2)")
    (add_net "Net-(C602-Pad2)")
    (add_net "Net-(C801-Pad1)")
    (add_net "Net-(C801-Pad2)")
    (add_net "Net-(C802-Pad2)")
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D1201-Pad1)")
    (add_net "Net-(D1202-Pad1)")
    (add_net "Net-(D1203-Pad1)")
    (add_net "Net-(J1002-Pad1)")
    (add_net "Net-(J1003-Pad1)")
    (add_net "Net-(J1005-Pad1)")
    (add_net "Net-(J1007-Pad1)")
    (add_net "Net-(J1202-Pad1)")
    (add_net "Net-(J1203-Pad1)")
    (add_net "Net-(J1205-Pad1)")
    (add_net "Net-(J1207-Pad1)")
    (add_net "Net-(J1301-Pad3)")
    (add_net "Net-(J602-Pad1)")
    (add_net "Net-(J603-Pad1)")
    (add_net "Net-(J605-Pad1)")
    (add_net "Net-(J607-Pad1)")
    (add_net "Net-(J802-Pad1)")
    (add_net "Net-(J803-Pad1)")
    (add_net "Net-(J805-Pad1)")
    (add_net "Net-(J807-Pad1)")
    (add_net "Net-(R1001-Pad2)")
    (add_net "Net-(R1002-Pad2)")
    (add_net "Net-(R1003-Pad2)")
    (add_net "Net-(R1004-Pad1)")
    (add_net "Net-(R1006-Pad2)")
    (add_net "Net-(R1010-Pad2)")
    (add_net "Net-(R1201-Pad2)")
    (add_net "Net-(R1202-Pad2)")
    (add_net "Net-(R1203-Pad2)")
    (add_net "Net-(R1204-Pad1)")
    (add_net "Net-(R1206-Pad2)")
    (add_net "Net-(R1210-Pad2)")
    (add_net "Net-(R201-Pad2)")
    (add_net "Net-(R402-Pad1)")
    (add_net "Net-(R601-Pad2)")
    (add_net "Net-(R602-Pad2)")
    (add_net "Net-(R603-Pad2)")
    (add_net "Net-(R604-Pad1)")
    (add_net "Net-(R606-Pad2)")
    (add_net "Net-(R610-Pad2)")
    (add_net "Net-(R801-Pad2)")
    (add_net "Net-(R802-Pad2)")
    (add_net "Net-(R803-Pad2)")
    (add_net "Net-(R804-Pad1)")
    (add_net "Net-(R806-Pad2)")
    (add_net "Net-(R810-Pad2)")
    (add_net "Net-(RV1001-Pad3)")
    (add_net "Net-(RV1002-Pad3)")
    (add_net "Net-(RV1201-Pad3)")
    (add_net "Net-(RV1202-Pad3)")
    (add_net "Net-(RV601-Pad3)")
    (add_net "Net-(RV602-Pad3)")
    (add_net "Net-(RV801-Pad3)")
    (add_net "Net-(RV802-Pad3)")
    (add_net "Net-(U1303-Pad8)")
    (add_net "Net-(U201-Pad1)")
    (add_net "Net-(U201-Pad12)")
    (add_net "Net-(U201-Pad14)")
    (add_net "Net-(U201-Pad18)")
    (add_net "Net-(U201-Pad2)")
    (add_net "Net-(U201-Pad20)")
    (add_net "Net-(U201-Pad24)")
    (add_net "Net-(U201-Pad26)")
    (add_net "Net-(U201-Pad3)")
    (add_net "Net-(U201-Pad30)")
    (add_net "Net-(U201-Pad32)")
    (add_net "Net-(U201-Pad36)")
    (add_net "Net-(U201-Pad38)")
    (add_net "Net-(U201-Pad4)")
    (add_net "Net-(U201-Pad42)")
    (add_net "Net-(U201-Pad44)")
    (add_net "Net-(U201-Pad48)")
    (add_net "Net-(U201-Pad50)")
    (add_net "Net-(U201-Pad54)")
    (add_net "Net-(U201-Pad56)")
    (add_net "Net-(U201-Pad6)")
    (add_net "Net-(U201-Pad62)")
    (add_net "Net-(U201-Pad64)")
    (add_net "Net-(U201-Pad68)")
    (add_net "Net-(U201-Pad7)")
    (add_net "Net-(U201-Pad70)")
    (add_net "Net-(U201-Pad74)")
    (add_net "Net-(U201-Pad76)")
    (add_net "Net-(U201-Pad8)")
    (add_net "Net-(U201-Pad81)")
    (add_net "Net-(U201-Pad82)")
    (add_net "Net-(U201-Pad83)")
    (add_net "Net-(U201-Pad84)")
    (add_net "Net-(U201-Pad87)")
    (add_net "Net-(U201-Pad88)")
    (add_net "Net-(U201-Pad89)")
    (add_net "Net-(U201-Pad90)")
    (add_net "Net-(U201-Pad91)")
    (add_net "Net-(U201-Pad92)")
    (add_net "Net-(U201-Pad93)")
    (add_net "Net-(U201-Pad94)")
    (add_net "Net-(U301-Pad1)")
    (add_net "Net-(U301-Pad100)")
    (add_net "Net-(U301-Pad13)")
    (add_net "Net-(U301-Pad14)")
    (add_net "Net-(U301-Pad17)")
    (add_net "Net-(U301-Pad19)")
    (add_net "Net-(U301-Pad2)")
    (add_net "Net-(U301-Pad23)")
    (add_net "Net-(U301-Pad25)")
    (add_net "Net-(U301-Pad29)")
    (add_net "Net-(U301-Pad3)")
    (add_net "Net-(U301-Pad31)")
    (add_net "Net-(U301-Pad35)")
    (add_net "Net-(U301-Pad37)")
    (add_net "Net-(U301-Pad4)")
    (add_net "Net-(U301-Pad41)")
    (add_net "Net-(U301-Pad43)")
    (add_net "Net-(U301-Pad47)")
    (add_net "Net-(U301-Pad49)")
    (add_net "Net-(U301-Pad5)")
    (add_net "Net-(U301-Pad53)")
    (add_net "Net-(U301-Pad55)")
    (add_net "Net-(U301-Pad6)")
    (add_net "Net-(U301-Pad61)")
    (add_net "Net-(U301-Pad63)")
    (add_net "Net-(U301-Pad67)")
    (add_net "Net-(U301-Pad69)")
    (add_net "Net-(U301-Pad7)")
    (add_net "Net-(U301-Pad73)")
    (add_net "Net-(U301-Pad75)")
    (add_net "Net-(U301-Pad8)")
    (add_net "Net-(U301-Pad81)")
    (add_net "Net-(U301-Pad82)")
    (add_net "Net-(U301-Pad83)")
    (add_net "Net-(U301-Pad84)")
    (add_net "Net-(U301-Pad87)")
    (add_net "Net-(U301-Pad88)")
    (add_net "Net-(U301-Pad89)")
    (add_net "Net-(U301-Pad9)")
    (add_net "Net-(U301-Pad90)")
    (add_net "Net-(U301-Pad93)")
    (add_net "Net-(U301-Pad94)")
    (add_net "Net-(U301-Pad95)")
    (add_net "Net-(U301-Pad96)")
    (add_net "Net-(U301-Pad97)")
    (add_net "Net-(U301-Pad98)")
    (add_net "Net-(U301-Pad99)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 166.31 81.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1101 (at -3.05 -0.05 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 103 /ADC/v4-))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 171.12 70.07)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C401 (at 2.28 0.03) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C401-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 167.07 70.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at 2.23 0.05) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /ADC/Vcm12))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 168.69 77.76)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 2.41 -0.06) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 /ADC/Vcm34))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 167.24 80.67 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C404 (at 2.36 -0.21 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 230 /ADC/1v8_analog))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 168.86 80.67 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C405 (at -2.45 -0.07 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 231 /ADC/enc+))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 241 /enc+))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 166.37 73.83 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C406 (at -2.17 -0.01 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C406-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C406-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 174.35 73.86 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C407 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 169.44 74.1 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C408 (at 0 -1.3 270) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C406-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C406-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 168.74 76.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C409 (at -2.35 -0.05 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C406-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 168.69 72.15)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C410 (at 2.21 0.05) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C406-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 165.97486 69.43226 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C501 (at 1.93226 -0.17486 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 96 /ADC/v1+))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 97 /ADC/v1-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 131.572 47.244)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C601 (at 2.3495 -0.0508) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 222 "Net-(C601-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C601-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 131.064 51.054 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C602 (at -1.27 1.016 270) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C602-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 163.72 72.64 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C701 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 98 /ADC/v2+))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 99 /ADC/v2-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 132.588 63.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C801 (at 2.4511 0.0381) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 223 "Net-(C801-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C801-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 131.572 66.548)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C802 (at -2.54 0.0127) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C802-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 164.68 76.14 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C901 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 100 /ADC/v3+))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 101 /ADC/v3-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 132.842 79.756)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1001 (at -3.048 0) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 224 "Net-(C1001-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C1001-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 132.08 83.058)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1002 (at -2.54 0) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C1002-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 166.64 78.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1101 (at 2.44 0.2 180) (layer F.SilkS))
    (fp_text value 10n (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 102 /ADC/v4+))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 103 /ADC/v4-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 132.08 96.52)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1201 (at 2.63652 0.06604) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 225 "Net-(C1201-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C1201-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 133.35 101.092 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1202 (at -2.86004 0.01524 180) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C1202-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 222.25 76.708 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1301 (at 1.992 1.25 270) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /Power/Vin))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 219.958296 53.2559 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1302 (at -0.0254 -1.4859 90) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /Power/Vin))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 217.0516 98.9558 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1303 (at 0.0127 -1.1684 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 223.173 97.3429 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1304 (at -0.1524 1.3589 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C1304-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C1304-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 217.0516 97.0762 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1305 (at 1.4056 1.0642 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 223.730196 53.8147 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1307 (at -1.1147 -0.969804 270) (layer B.SilkS))
    (fp_text value 22n (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(C1307-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C1307-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 217.00471 50.246852 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1308 (at 2.6797 -0.0381 180) (layer F.SilkS))
    (fp_text value 22u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 217.00471 48.113252 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1309 (at 2.6797 0.0635 180) (layer F.SilkS))
    (fp_text value 22u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 166.24 69.05 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D501 (at -0.37 3.42 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 97 /ADC/v1-))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 162.64 69.05 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D502 (at -0.29 3.37 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 97 /ADC/v1-))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 166.24 66.95 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D503 (at -0.36 2.07 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 96 /ADC/v1+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 162.64 66.95 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D504 (at -0.21 2.05 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 96 /ADC/v1+))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 162.84 73.25 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D701 (at 6.45 0.56 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 99 /ADC/v2-))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 159.29 73.35 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D702 (at 2.9 -0.05 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 99 /ADC/v2-))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 162.84 71.2 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D703 (at 6.12 0.57 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 98 /ADC/v2+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 159.29 71.3 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D704 (at 2.65 0 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 98 /ADC/v2+))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 164.74 77.35 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D901 (at 5.93 -0.46 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 101 /ADC/v3-))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 161.24 77.35 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D902 (at 2.39 0.23 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 101 /ADC/v3-))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 164.74 75.3 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D903 (at 6.17 -0.68 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 100 /ADC/v3+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 161.29 75.3 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D904 (at 2.75 0 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 100 /ADC/v3+))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 162.61 81.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1102 (at 2.882 0.08 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 103 /ADC/v4-))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 166.24 79.51 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1103 (at -2.93 -0.46 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 102 /ADC/v4+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer B.Cu) (tedit 58641739)
    (at 162.66 79.57 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1104 (at 2.78 -0.02 180) (layer B.SilkS))
    (fp_text value D_Schottky (at 0.1 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 102 /ADC/v4+))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module robosub_footprints:BNC-Coax-TE (layer F.Cu) (tedit 59B58541)
    (at 96.5123 48.86434 90)
    (fp_text reference J401 (at 5.439024 1.048299 90) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 -0.5 90) (layer F.Fab))
    (pad ~ thru_hole circle (at -5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad ~ thru_hole circle (at 5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 /ADC/Filter1/Vin))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (model robosub.3dshapes/1-1634612-0.wrl
      (at (xyz 0 0.62 0.23))
      (scale (xyz 7 7 7))
      (rotate (xyz -90 0 180))
    )
  )
  (module robosub_footprints:BNC-Coax-TE (layer F.Cu) (tedit 59B58541)
    (at 96.4361 65.4099 90)
    (fp_text reference J402 (at 5.5499 0.9398 90) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 -0.5 90) (layer F.Fab))
    (pad ~ thru_hole circle (at -5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad ~ thru_hole circle (at 5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 /ADC/Filter2/Vin))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (model robosub.3dshapes/1-1634612-0.wrl
      (at (xyz 0 0.62 0.23))
      (scale (xyz 7 7 7))
      (rotate (xyz -90 0 180))
    )
  )
  (module robosub_footprints:BNC-Coax-TE (layer F.Cu) (tedit 59B58541)
    (at 96.7917 81.6151 90)
    (fp_text reference J403 (at 6.42366 0.63374 90) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 -0.5 90) (layer F.Fab))
    (pad ~ thru_hole circle (at -5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad ~ thru_hole circle (at 5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 /ADC/Filter3/Vin))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (model robosub.3dshapes/1-1634612-0.wrl
      (at (xyz 0 0.62 0.23))
      (scale (xyz 7 7 7))
      (rotate (xyz -90 0 180))
    )
  )
  (module robosub_footprints:BNC-Coax-TE (layer F.Cu) (tedit 59B58541)
    (at 96.4234 98.468 90)
    (fp_text reference J404 (at 5.770124 1.100999 90) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 -0.5 90) (layer F.Fab))
    (pad ~ thru_hole circle (at -5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad ~ thru_hole circle (at 5.08 -5.08 90) (size 2.5 2.5) (drill 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 /ADC/Filter4/Vin))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (model robosub.3dshapes/1-1634612-0.wrl
      (at (xyz 0 0.62 0.23))
      (scale (xyz 7 7 7))
      (rotate (xyz -90 0 180))
    )
  )
  (module robosub_footprints:BarrelJack-CUI (layer F.Cu) (tedit 59B57947)
    (at 233.15 52.99 270)
    (fp_text reference J1301 (at -1.524 5.08 270) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 2.7 270) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 116 "Net-(J1301-Pad3)"))
    (pad 1 thru_hole circle (at 2.5 0 270) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 17 /Power/Vin))
    (pad 2 thru_hole circle (at -2.5 0 270) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 8 GND))
    (model robosub.3dshapes/pj-031dh.wrl
      (at (xyz -0.13 0 0.1))
      (scale (xyz 2.5 2.5 2.5))
      (rotate (xyz -90 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 159.512 85.598 135)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L401 (at 0 1.45 135) (layer B.SilkS))
    (fp_text value Ferrite_Bead (at 0 -1.5 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 135) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 160.782 63.5 245)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L402 (at 0 -1.35 245) (layer B.SilkS))
    (fp_text value Ferrite_Bead (at 29.9212 -22.987 245) (layer B.Fab))
    (fp_text user %R (at 0 0 245) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 245) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 245) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module robosub_footprints:Inductor-3.6mm-Pitch-4.0mm-Length-1.5mm-Width (layer F.Cu) (tedit 59B573D1)
    (at 221.13221 48.976852)
    (fp_text reference L1301 (at 1.25419 -2.424252) (layer F.SilkS))
    (fp_text value 4.7u (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 1.8 0) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C1307-Pad1)"))
    (pad 2 smd rect (at -1.8 0) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (model robosub.3dshapes/nr5040-inductor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 158.97 90.68)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at 0.267229 -1.6317) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R201-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 170.43 67.59)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 2k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 114 /MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 169.0438 66.4179 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R402 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R402-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 +1V8))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 171.57 66.54 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R403 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R402-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 162.94 68.85)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R505 (at 0.0127 1.27) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 "/ADC/Diff Conv1/v-"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 /ADC/v1-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 162.89 66.95)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R506 (at 0 -1.2954) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 "/ADC/Diff Conv1/v+"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 /ADC/v1+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.82802 46.27608)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at -2.2479 -0.0254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R601-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 131.33982 54.61998)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 0 1.45) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 /ADC/Filter1/Vin))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R602-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.70102 50.80998)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at -2.4511 -0.0254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R603-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 129.48562 52.61338 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R604 (at 2.23162 0.03538 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R604-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(J603-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 134.98472 54.65808 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R605 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R604-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(R602-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 136.92782 52.65148 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R606 (at 0.1143 1.4859 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R604-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R606-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 131.572 45.466)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R607 (at -2.54 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C601-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 134.22272 50.53058 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R608 (at 0.52342 -1.15928 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 222 "Net-(C601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J605-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 136.57292 50.61948 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R609 (at -2.298 -0.0381 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(C601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R606-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 136.57222 48.87958 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R610 (at -2.2733 0.0254 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(C601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R610-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.842 52.07 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R611 (at 1.016 -1.27 270) (layer B.SilkS))
    (fp_text value 3.16k (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R604-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 136.68652 45.08228 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R612 (at -2.3876 0.0381 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "/ADC/Diff Conv1/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J607-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 136.63572 47.03808 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R613 (at -2.2225 0.0508 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "/ADC/Diff Conv1/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R610-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 159.69 73.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R705 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 107 "/ADC/Diff Conv2/v-"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 /ADC/v2-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 159.59 71.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R706 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 "/ADC/Diff Conv2/v+"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 /ADC/v2+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.8623 63.1493)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R801 (at -2.4765 -0.0508) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R801-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 133.3045 71.22396)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R802 (at -2.14376 0) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /ADC/Filter2/Vin))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R802-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.2908 67.9753)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R803 (at -2.4003 -0.0254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R803-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 130.0787 69.5501 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R804 (at 2.0787 -0.0499 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R804-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J803-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.20086 71.15792 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R805 (at -2.21996 -0.06604 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R804-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R802-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.23642 69.07512 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R806 (at -2.28092 0.01524 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R804-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R806-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.588 61.214)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R807 (at 2.286 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C801-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.5806 65.1432 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R808 (at 2.3876 -0.0889 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 223 "Net-(C801-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J805-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.26182 67.05836 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R809 (at -2.25552 0.03556 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(C801-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R806-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.27522 65.32608 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R810 (at -2.298 -0.01524 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(C801-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R810-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 133.35 68.834 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R811 (at 2.286 0 270) (layer B.SilkS))
    (fp_text value 3.16k (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C802-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R804-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.3304 61.7396 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R812 (at -2.2352 0.0762 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "/ADC/Diff Conv2/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J807-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.3304 63.5557 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R813 (at -2.2352 0 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "/ADC/Diff Conv2/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R810-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 161.54 77.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R905 (at -2.6 0) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 109 "/ADC/Diff Conv3/v-"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 /ADC/v3-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 161.59 75.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R906 (at -2.35 -0.1) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 108 "/ADC/Diff Conv3/v+"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 /ADC/v3+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.86738 79.17924)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1001 (at -2.75336 -0.01524) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R1001-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 133.68042 87.54854)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1002 (at 2.20958 0.84346) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /ADC/Filter3/Vin))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R1002-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.97914 84.11192)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1003 (at -2.5654 0.04064) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R1003-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 130.55622 85.78832 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1004 (at 2.80416 -0.04064 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(R1004-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J1003-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.53614 87.1015 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1005 (at -2.49936 0.04318 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R1004-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R1002-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.58694 85.1838 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1006 (at -2.57048 -0.0254 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R1004-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.842 77.724)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1007 (at -3.048 0.254) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C1001-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.88286 81.3992 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1008 (at 2.58572 0.02032 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 224 "Net-(C1001-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J1005-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.58694 83.29404 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1009 (at -2.47396 0.16764 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(C1001-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.58694 81.54652 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1010 (at -2.47396 -0.09652 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(C1001-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R1010-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 134.62 84.582)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1011 (at -2.57232 0.00508) (layer B.SilkS))
    (fp_text value 3.16k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C1002-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(R1004-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.63266 78.07688 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1012 (at -2.42824 0 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "/ADC/Diff Conv3/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1007-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.63266 79.80408 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1013 (at -2.47396 -0.04572 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "/ADC/Diff Conv3/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R1010-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 162.92 81.73)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1105 (at -2.74 0.03) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 "/ADC/Diff Conv4/v-"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 /ADC/v4-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 162.86 79.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1106 (at -2.67 -0.09) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 110 "/ADC/Diff Conv4/v+"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 /ADC/v4+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.64894 95.73496)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1201 (at -2.74828 -0.08128) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R1201-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 133.07914 104.41668)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1202 (at -2.38576 0.48532) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /ADC/Filter4/Vin))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R1202-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 125.14094 101.06388)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1203 (at -2.55524 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R1203-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 130.08886 102.29324 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1204 (at 2.62636 0.04572 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(R1204-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J1203-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.16022 103.77152 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1205 (at -2.39268 0.1016 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R1204-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R1202-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.16022 101.60744 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1206 (at -2.4892 0 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R1204-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R1206-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.08 94.234)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1207 (at -2.38 -0.034) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C1201-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 132.25294 97.92952 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1208 (at 2.75844 0 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 225 "Net-(C1201-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J1205-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.16022 99.83452 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1209 (at -2.52476 0 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(C1201-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R1206-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.16206 98.09716 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1210 (at -2.5534 0.09652 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(C1201-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R1210-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 131.62 99.54 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1211 (at -2.65176 -0.07112 180) (layer B.SilkS))
    (fp_text value 3.16k (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C1202-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(R1204-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.1653 94.61736 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1212 (at -2.57048 0.00508 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "/ADC/Diff Conv4/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1207-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 137.17038 96.3598 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1213 (at -2.67716 0.04572 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "/ADC/Diff Conv4/Vin"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R1210-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 224.923996 52.8241 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1301 (at -0.1524 1.2192 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 223.266 78.474 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1302 (at 0.326 -1.234 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 /vccio_en))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 222.0689 55.4807)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1303 (at 0.0381 1.2192) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 75 /v_good))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.65962 42.66928 270)
    (fp_text reference RV601 (at 0.00508 2.89052 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J602-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R601-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(RV601-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.73582 54.22628 270)
    (fp_text reference RV602 (at 0 3.81 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J603-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R603-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(RV602-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.7574 59.8727 270)
    (fp_text reference RV801 (at 0 3.81 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J802-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R801-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(RV801-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.9606 70.8963 270)
    (fp_text reference RV802 (at -0.10922 3.19786 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J803-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R803-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(RV802-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.82886 76.05504 270)
    (fp_text reference RV1001 (at -0.14224 3.22486 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J1002-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R1001-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(RV1001-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.72946 87.15484 270)
    (fp_text reference RV1002 (at 0 3.81 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J1003-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R1003-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(RV1002-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.82598 92.55488 270)
    (fp_text reference RV1201 (at 0.04064 3.23088 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1202-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R1201-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(RV1201-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:TC33X-2 (layer F.Cu) (tedit 58CCCA8D)
    (at 124.71422 103.9036 270)
    (fp_text reference RV1202 (at 0 3.81 270) (layer F.SilkS))
    (fp_text value POT (at -2.54 0 360) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.45 270) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J1203-Pad1)"))
    (pad 1 smd rect (at -1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R1203-Pad2)"))
    (pad 3 smd rect (at 1 1.8 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(RV1202-Pad3)"))
    (model robosub.3dshapes/tc-332x-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 400 400 400))
      (rotate (xyz -90 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-52-1EP_7x8mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 170.96758 73.83382)
    (descr "UKG Package; 52-Lead Plastic QFN (7mm x 8mm); (see Linear Technology QFN_52_05-08-1729.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U401 (at 2.62242 -4.72382) (layer F.SilkS))
    (fp_text value LTC2171-14 (at 0 5.25) (layer F.Fab))
    (pad 1 smd rect (at -3.4 -3.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 /ADC/v1+))
    (pad 2 smd rect (at -3.4 -2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 97 /ADC/v1-))
    (pad 3 smd rect (at -3.4 -2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /ADC/Vcm12))
    (pad 4 smd rect (at -3.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 98 /ADC/v2+))
    (pad 5 smd rect (at -3.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 99 /ADC/v2-))
    (pad 6 smd rect (at -3.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C406-Pad1)"))
    (pad 7 smd rect (at -3.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C406-Pad1)"))
    (pad 8 smd rect (at -3.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C406-Pad2)"))
    (pad 9 smd rect (at -3.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C406-Pad2)"))
    (pad 10 smd rect (at -3.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 100 /ADC/v3+))
    (pad 11 smd rect (at -3.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 101 /ADC/v3-))
    (pad 12 smd rect (at -3.4 2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /ADC/Vcm34))
    (pad 13 smd rect (at -3.4 2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 102 /ADC/v4+))
    (pad 14 smd rect (at -3.4 3.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 103 /ADC/v4-))
    (pad 15 smd rect (at -2.75 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 230 /ADC/1v8_analog))
    (pad 16 smd rect (at -2.25 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 230 /ADC/1v8_analog))
    (pad 17 smd rect (at -1.75 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 231 /ADC/enc+))
    (pad 18 smd rect (at -1.25 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 232 /ADC/enc-))
    (pad 19 smd rect (at -0.75 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 115 /~CS))
    (pad 20 smd rect (at -0.25 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 113 /SCK))
    (pad 21 smd rect (at 0.25 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 112 /MISO))
    (pad 22 smd rect (at 0.75 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 23 smd rect (at 1.25 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 85 /out4b-))
    (pad 24 smd rect (at 1.75 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 83 /out4b+))
    (pad 25 smd rect (at 2.25 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 87 /out4a-))
    (pad 26 smd rect (at 2.75 3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 84 /out4a+))
    (pad 27 smd rect (at 3.4 3.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 82 /out3b-))
    (pad 28 smd rect (at 3.4 2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 86 /out3b+))
    (pad 29 smd rect (at 3.4 2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 /out3a-))
    (pad 30 smd rect (at 3.4 1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 81 /out3a+))
    (pad 31 smd rect (at 3.4 1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 /fr_clk-))
    (pad 32 smd rect (at 3.4 0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 /fr_clk+))
    (pad 33 smd rect (at 3.4 0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 34 smd rect (at 3.4 -0.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 35 smd rect (at 3.4 -0.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 /data_clk-))
    (pad 36 smd rect (at 3.4 -1.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 /data_clk+))
    (pad 37 smd rect (at 3.4 -1.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 94 /out2b-))
    (pad 38 smd rect (at 3.4 -2.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 92 /out2b+))
    (pad 39 smd rect (at 3.4 -2.75) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 93 /out2a-))
    (pad 40 smd rect (at 3.4 -3.25) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 91 /out2a+))
    (pad 41 smd rect (at 2.75 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 89 /out1b-))
    (pad 42 smd rect (at 2.25 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 /out1b+))
    (pad 43 smd rect (at 1.75 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 95 /out1a-))
    (pad 44 smd rect (at 1.25 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 88 /out1a+))
    (pad 45 smd rect (at 0.75 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 46 smd rect (at 0.25 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 114 /MOSI))
    (pad 47 smd rect (at -0.25 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 48 smd rect (at -0.75 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C401-Pad1)"))
    (pad 49 smd rect (at -1.25 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 50 smd rect (at -1.75 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R402-Pad1)"))
    (pad 51 smd rect (at -2.25 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 230 /ADC/1v8_analog))
    (pad 52 smd rect (at -2.75 -3.9 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 230 /ADC/1v8_analog))
    (pad 53 smd rect (at 2.02875 2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at 2.02875 0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at 2.02875 -0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at 2.02875 -2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at 0.67625 2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at 0.67625 0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at 0.67625 -0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at 0.67625 -2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -0.67625 2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -0.67625 0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -0.67625 -0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -0.67625 -2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -2.02875 2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -2.02875 0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -2.02875 -0.80625) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 53 smd rect (at -2.02875 -2.41875) (size 1.3525 1.6125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-52-1EP_7x8mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 148.45434 62.64892)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U501 (at 0 -2.6) (layer F.SilkS))
    (fp_text value el5170 (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "/ADC/Diff Conv1/Vin"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 /ADC/Vcm12))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 105 "/ADC/Diff Conv1/v-"))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 104 "/ADC/Diff Conv1/v+"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 131.327821 48.89788)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U601 (at -1.025821 4.95012) (layer F.SilkS))
    (fp_text value LM324 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J602-Pad1)"))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R601-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /ADC/Filter1/Vin))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J602-Pad1)"))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R603-Pad2)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J603-Pad1)"))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J605-Pad1)"))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J605-Pad1)"))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C602-Pad2)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C601-Pad1)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J607-Pad1)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J607-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 148.52038 70.41878)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U701 (at 0 -2.6) (layer F.SilkS))
    (fp_text value el5170 (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 "/ADC/Diff Conv2/Vin"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 /ADC/Vcm12))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 107 "/ADC/Diff Conv2/v-"))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 106 "/ADC/Diff Conv2/v+"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 131.9888 65.6893)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U801 (at 0 -5.375) (layer F.SilkS))
    (fp_text value LM324 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J802-Pad1)"))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R801-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /ADC/Filter2/Vin))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J802-Pad1)"))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R803-Pad2)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J803-Pad1)"))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J805-Pad1)"))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J805-Pad1)"))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C802-Pad2)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C801-Pad1)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J807-Pad1)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J807-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 148.582 77.754)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U901 (at 0 -2.6) (layer F.SilkS))
    (fp_text value el5170 (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "/ADC/Diff Conv3/Vin"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /ADC/Vcm34))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 109 "/ADC/Diff Conv3/v-"))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 108 "/ADC/Diff Conv3/v+"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 132.37742 82.02404)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1001 (at -1.31342 5.09796) (layer F.SilkS))
    (fp_text value LM324 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J1002-Pad1)"))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R1001-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /ADC/Filter3/Vin))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J1002-Pad1)"))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R1003-Pad2)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J1003-Pad1)"))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J1005-Pad1)"))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J1005-Pad1)"))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1002-Pad2)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C1001-Pad1)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1007-Pad1)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1007-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 148.59438 88.03424)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1101 (at 0 -2.6) (layer F.SilkS))
    (fp_text value el5170 (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 67 "/ADC/Diff Conv4/Vin"))
    (pad 2 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 3 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 4 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /ADC/Vcm34))
    (pad 5 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 111 "/ADC/Diff Conv4/v-"))
    (pad 6 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 7 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 8 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 110 "/ADC/Diff Conv4/v+"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 131.78558 98.69152)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1201 (at -0.72158 4.94048) (layer F.SilkS))
    (fp_text value LM324 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1202-Pad1)"))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R1201-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /ADC/Filter4/Vin))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1202-Pad1)"))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R1203-Pad2)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J1203-Pad1)"))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J1205-Pad1)"))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J1205-Pad1)"))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C1202-Pad2)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C1201-Pad1)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1207-Pad1)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1207-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm_ThermalVias (layer F.Cu) (tedit 5974B455)
    (at 222.054496 53.9054)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1301 (at -0.404696 2.2992) (layer F.SilkS))
    (fp_text value TS30013 (at 0 2.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C1307-Pad1)"))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /v_good))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C1307-Pad2)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C1307-Pad1)"))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C1307-Pad1)"))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C1307-Pad1)"))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at 0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at -0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58CE4E7E)
    (at 220.379 97.9652)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1302 (at 0.093 2.3648) (layer F.SilkS))
    (fp_text value LM2776 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 -5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C1304-Pad2)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C1304-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881C7)
    (at 121.158 46.482)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J601 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /ADC/Filter1/Vin))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881CD)
    (at 128.524 43.18)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J602 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J602-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881C1)
    (at 127.254 56.388)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J603 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J603-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881C9)
    (at 131.064 43.18)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J604 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C602-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881C3)
    (at 129.794 56.388)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J605 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J605-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881C5)
    (at 133.604 43.18)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J606 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C601-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881CB)
    (at 136.144 43.18)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J607 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J607-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88071)
    (at 121.158 63.246)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J801 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /ADC/Filter2/Vin))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88073)
    (at 128.524 58.928)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(J802-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8806A)
    (at 128.016 72.644)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J803 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J803-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8806C)
    (at 130.81 72.644)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J804 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C802-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88061)
    (at 133.604 58.928)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J805 (at -2.794 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(J805-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8806F)
    (at 131.064 58.928)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J806 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C801-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B881A4)
    (at 136.144 58.928)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J807 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(J807-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B882B7)
    (at 121.158 79.248)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1001 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /ADC/Filter3/Vin))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B882AF)
    (at 129.032 75.692)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1002 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(J1002-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B882B4)
    (at 128.27 89.154)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1003 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J1003-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B882B9)
    (at 131.064 89.154)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1004 (at -0.083219 -1.34416) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C1002-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B882B5)
    (at 134.112 75.692)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1005 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J1005-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B882B2)
    (at 131.572 75.692)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1006 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C1001-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B882BB)
    (at 136.652 75.692)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1007 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J1007-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88349)
    (at 120.904 96.012)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /ADC/Filter4/Vin))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8834D)
    (at 128.27 92.202)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1202 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J1202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88355)
    (at 128.524 104.902)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1203 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J1203-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8834B)
    (at 142.748 102.108)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1204 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C1202-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88353)
    (at 133.35 92.202)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1205 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(J1205-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88350)
    (at 130.81 92.202)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1206 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C1201-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88357)
    (at 135.89 92.202)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1207 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(J1207-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59B8851A)
    (at 156.972 86.868 135)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L403 (at 0 1.45 135) (layer B.SilkS))
    (fp_text value Ferrite_Bead (at 0 -1.5 135) (layer B.Fab))
    (fp_text user %R (at 0 0 135) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 135) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 135) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59B8853F)
    (at 158.75 62.738 245)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L404 (at 0 1.45 245) (layer B.SilkS))
    (fp_text value Ferrite_Bead (at 0 -1.5 245) (layer B.Fab))
    (fp_text user %R (at 0 0 245) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 245) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 245) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8843A)
    (at 157.734 67.818)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J501 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /ADC/v1-))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88430)
    (at 156.718 66.294)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J502 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 /ADC/v1+))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88437)
    (at 155.194 75.946)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J701 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 /ADC/v2-))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88432)
    (at 154.432 74.168)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J702 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 /ADC/v2+))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8843F)
    (at 153.67 80.772)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J901 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /ADC/v3-))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8842D)
    (at 153.924 78.994)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J902 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 /ADC/v3+))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B8843C)
    (at 153.67 84.582)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1101 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /ADC/v4-))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 59B88434)
    (at 155.194 83.058)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1102 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 /ADC/v4+))
  )
  (module robosub_footprints:fci-61083-2x50 locked (layer F.Cu) (tedit 59B71047)
    (at 177.8 95.25)
    (fp_text reference U201 (at -21.3 4.05) (layer F.SilkS))
    (fp_text value micro-zed-jx1 (at 0 -5.08) (layer F.Fab))
    (pad 49 smd rect (at -0.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 125 /MicroZed-JX1/LVDS12-))
    (pad 47 smd rect (at -1.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 126 /MicroZed-JX1/LVDS12+))
    (pad 45 smd rect (at -2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 43 smd rect (at -2.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 87 /out4a-))
    (pad 41 smd rect (at -3.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 84 /out4a+))
    (pad 39 smd rect (at -4.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 37 smd rect (at -5.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 235 /MicroZed-JX1/LVDS8-))
    (pad 35 smd rect (at -6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 236 /MicroZed-JX1/LVDS8+))
    (pad 33 smd rect (at -6.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 31 smd rect (at -7.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 85 /out4b-))
    (pad 21 smd rect (at -11.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 17 smd rect (at -13.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 228 /MicroZed-JX1/LVDS2+))
    (pad 23 smd rect (at -10.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 237 /MicroZed-JX1/LVDS4+))
    (pad 15 smd rect (at -14 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 13 smd rect (at -14.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 242 /enc-))
    (pad 19 smd rect (at -12.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 239 /MicroZed-JX1/LVDS2-))
    (pad 11 smd rect (at -15.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 241 /enc+))
    (pad 29 smd rect (at -8.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 83 /out4b+))
    (pad 25 smd rect (at -10 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 238 /MicroZed-JX1/LVDS4-))
    (pad 27 smd rect (at -9.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -18 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R201-Pad2)"))
    (pad 7 smd rect (at -17.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U201-Pad7)"))
    (pad 3 smd rect (at -18.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U201-Pad3)"))
    (pad 1 smd rect (at -19.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U201-Pad1)"))
    (pad 9 smd rect (at -16.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 240 /MicroZed-JX1/SE0))
    (pad 89 smd rect (at 15.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(U201-Pad89)"))
    (pad 87 smd rect (at 14.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(U201-Pad87)"))
    (pad 93 smd rect (at 17.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(U201-Pad93)"))
    (pad 91 smd rect (at 16.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(U201-Pad91)"))
    (pad 85 smd rect (at 14 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 97 smd rect (at 18.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 99 smd rect (at 19.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 95 smd rect (at 18 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 73 smd rect (at 9.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 134 /MicroZed-JX1/LVDS20+))
    (pad 69 smd rect (at 7.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 78 /fr_clk-))
    (pad 71 smd rect (at 8.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 67 smd rect (at 6.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 79 /fr_clk+))
    (pad 61 smd rect (at 4.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 81 /out3a+))
    (pad 53 smd rect (at 1.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 86 /out3b+))
    (pad 63 smd rect (at 5.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 80 /out3a-))
    (pad 55 smd rect (at 2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 82 /out3b-))
    (pad 65 smd rect (at 6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 51 smd rect (at 0.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 59 smd rect (at 3.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 57 smd rect (at 2.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 83 smd rect (at 13.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(U201-Pad83)"))
    (pad 81 smd rect (at 12.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(U201-Pad81)"))
    (pad 75 smd rect (at 10 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 137 /MicroZed-JX1/LVDS20-))
    (pad 77 smd rect (at 10.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 79 smd rect (at 11.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 100 smd rect (at 19.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 96 smd rect (at 18 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 98 smd rect (at 18.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 92 smd rect (at 16.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(U201-Pad92)"))
    (pad 94 smd rect (at 17.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(U201-Pad94)"))
    (pad 86 smd rect (at 14 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 84 smd rect (at 13.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(U201-Pad84)"))
    (pad 90 smd rect (at 15.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(U201-Pad90)"))
    (pad 82 smd rect (at 12.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(U201-Pad82)"))
    (pad 88 smd rect (at 14.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(U201-Pad88)"))
    (pad 68 smd rect (at 6.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U201-Pad68)"))
    (pad 62 smd rect (at 4.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U201-Pad62)"))
    (pad 64 smd rect (at 5.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U201-Pad64)"))
    (pad 58 smd rect (at 2.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 60 smd rect (at 3.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 66 smd rect (at 6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 76 smd rect (at 10 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U201-Pad76)"))
    (pad 78 smd rect (at 10.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 70 smd rect (at 7.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U201-Pad70)"))
    (pad 74 smd rect (at 9.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U201-Pad74)"))
    (pad 80 smd rect (at 11.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 72 smd rect (at 8.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 50 smd rect (at -0.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U201-Pad50)"))
    (pad 54 smd rect (at 1.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(U201-Pad54)"))
    (pad 56 smd rect (at 2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(U201-Pad56)"))
    (pad 44 smd rect (at -2.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(U201-Pad44)"))
    (pad 46 smd rect (at -2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 52 smd rect (at 0.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 48 smd rect (at -1.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(U201-Pad48)"))
    (pad 42 smd rect (at -3.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(U201-Pad42)"))
    (pad 34 smd rect (at -6.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 38 smd rect (at -5.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(U201-Pad38)"))
    (pad 40 smd rect (at -4.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 36 smd rect (at -6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U201-Pad36)"))
    (pad 32 smd rect (at -7.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U201-Pad32)"))
    (pad 30 smd rect (at -8.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(U201-Pad30)"))
    (pad 26 smd rect (at -10 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(U201-Pad26)"))
    (pad 28 smd rect (at -9.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 24 smd rect (at -10.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U201-Pad24)"))
    (pad 20 smd rect (at -12.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U201-Pad20)"))
    (pad 22 smd rect (at -11.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 14 smd rect (at -14.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U201-Pad14)"))
    (pad 10 smd rect (at -16.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 164 /MicroZed-JX1/SE1))
    (pad 18 smd rect (at -13.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U201-Pad18)"))
    (pad 12 smd rect (at -15.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U201-Pad12)"))
    (pad 16 smd rect (at -14 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -18 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U201-Pad6)"))
    (pad 4 smd rect (at -18.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(U201-Pad4)"))
    (pad 2 smd rect (at -19.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(U201-Pad2)"))
    (pad 8 smd rect (at -17.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U201-Pad8)"))
    (pad ~ thru_hole circle (at -22.1 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask))
    (pad ~ thru_hole circle (at 22.1 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask))
    (model robosub.3dshapes/s61083-2x50-7.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (module robosub_footprints:fci-61083-2x50 (layer F.Cu) (tedit 59B71047)
    (at 177.8 50.8)
    (fp_text reference U301 (at -21 4.1) (layer F.SilkS))
    (fp_text value micro-zed-jx2 (at 0 -5.08) (layer F.Fab))
    (pad 49 smd rect (at -0.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U301-Pad49)"))
    (pad 47 smd rect (at -1.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U301-Pad47)"))
    (pad 45 smd rect (at -2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 43 smd rect (at -2.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U301-Pad43)"))
    (pad 41 smd rect (at -3.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U301-Pad41)"))
    (pad 39 smd rect (at -4.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 37 smd rect (at -5.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U301-Pad37)"))
    (pad 35 smd rect (at -6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U301-Pad35)"))
    (pad 33 smd rect (at -6.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 31 smd rect (at -7.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U301-Pad31)"))
    (pad 21 smd rect (at -11.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 17 smd rect (at -13.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U301-Pad17)"))
    (pad 23 smd rect (at -10.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U301-Pad23)"))
    (pad 15 smd rect (at -14 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 13 smd rect (at -14.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U301-Pad13)"))
    (pad 19 smd rect (at -12.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(U301-Pad19)"))
    (pad 11 smd rect (at -15.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 75 /v_good))
    (pad 29 smd rect (at -8.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(U301-Pad29)"))
    (pad 25 smd rect (at -10 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(U301-Pad25)"))
    (pad 27 smd rect (at -9.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd rect (at -18 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(U301-Pad5)"))
    (pad 7 smd rect (at -17.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(U301-Pad7)"))
    (pad 3 smd rect (at -18.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(U301-Pad3)"))
    (pad 1 smd rect (at -19.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(U301-Pad1)"))
    (pad 9 smd rect (at -16.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(U301-Pad9)"))
    (pad 89 smd rect (at 15.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(U301-Pad89)"))
    (pad 87 smd rect (at 14.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(U301-Pad87)"))
    (pad 93 smd rect (at 17.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(U301-Pad93)"))
    (pad 91 smd rect (at 16.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 85 smd rect (at 14 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 97 smd rect (at 18.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(U301-Pad97)"))
    (pad 99 smd rect (at 19.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(U301-Pad99)"))
    (pad 95 smd rect (at 18 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(U301-Pad95)"))
    (pad 73 smd rect (at 9.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(U301-Pad73)"))
    (pad 69 smd rect (at 7.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(U301-Pad69)"))
    (pad 71 smd rect (at 8.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 67 smd rect (at 6.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(U301-Pad67)"))
    (pad 61 smd rect (at 4.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(U301-Pad61)"))
    (pad 53 smd rect (at 1.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(U301-Pad53)"))
    (pad 63 smd rect (at 5.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(U301-Pad63)"))
    (pad 55 smd rect (at 2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(U301-Pad55)"))
    (pad 65 smd rect (at 6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 51 smd rect (at 0.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 59 smd rect (at 3.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 57 smd rect (at 2.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 83 smd rect (at 13.2 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(U301-Pad83)"))
    (pad 81 smd rect (at 12.4 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(U301-Pad81)"))
    (pad 75 smd rect (at 10 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(U301-Pad75)"))
    (pad 77 smd rect (at 10.8 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 79 smd rect (at 11.6 -2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 100 smd rect (at 19.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(U301-Pad100)"))
    (pad 96 smd rect (at 18 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(U301-Pad96)"))
    (pad 98 smd rect (at 18.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(U301-Pad98)"))
    (pad 92 smd rect (at 16.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 94 smd rect (at 17.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(U301-Pad94)"))
    (pad 86 smd rect (at 14 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 84 smd rect (at 13.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(U301-Pad84)"))
    (pad 90 smd rect (at 15.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(U301-Pad90)"))
    (pad 82 smd rect (at 12.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(U301-Pad82)"))
    (pad 88 smd rect (at 14.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(U301-Pad88)"))
    (pad 68 smd rect (at 6.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 233 /MicroZed-JX2/LVDS17+))
    (pad 62 smd rect (at 4.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 77 /data_clk+))
    (pad 64 smd rect (at 5.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 76 /data_clk-))
    (pad 58 smd rect (at 2.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 60 smd rect (at 3.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 66 smd rect (at 6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 76 smd rect (at 10 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 213 /MicroZed-JX2/LVDS19-))
    (pad 78 smd rect (at 10.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 70 smd rect (at 7.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 234 /MicroZed-JX2/LVDS17-))
    (pad 74 smd rect (at 9.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 214 /MicroZed-JX2/LVDS19+))
    (pad 80 smd rect (at 11.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 72 smd rect (at 8.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 50 smd rect (at -0.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 215 /MicroZed-JX2/LVDS11-))
    (pad 54 smd rect (at 1.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 92 /out2b+))
    (pad 56 smd rect (at 2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 94 /out2b-))
    (pad 44 smd rect (at -2.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 93 /out2a-))
    (pad 46 smd rect (at -2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 52 smd rect (at 0.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 48 smd rect (at -1.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 216 /MicroZed-JX2/LVDS11+))
    (pad 42 smd rect (at -3.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 91 /out2a+))
    (pad 34 smd rect (at -6.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 38 smd rect (at -5.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 112 /MISO))
    (pad 40 smd rect (at -4.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 36 smd rect (at -6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 114 /MOSI))
    (pad 32 smd rect (at -7.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 89 /out1b-))
    (pad 30 smd rect (at -8.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 90 /out1b+))
    (pad 26 smd rect (at -10 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 113 /SCK))
    (pad 28 smd rect (at -9.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 24 smd rect (at -10.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 115 /~CS))
    (pad 20 smd rect (at -12.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 95 /out1a-))
    (pad 22 smd rect (at -11.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 14 smd rect (at -14.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(U301-Pad14)"))
    (pad 10 smd rect (at -16.4 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 74 /vccio_en))
    (pad 18 smd rect (at -13.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 88 /out1a+))
    (pad 12 smd rect (at -15.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 16 smd rect (at -14 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 6 smd rect (at -18 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(U301-Pad6)"))
    (pad 4 smd rect (at -18.8 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(U301-Pad4)"))
    (pad 2 smd rect (at -19.6 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(U301-Pad2)"))
    (pad 8 smd rect (at -17.2 2.2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(U301-Pad8)"))
    (pad ~ thru_hole circle (at -22.1 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask))
    (pad ~ thru_hole circle (at 22.1 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask))
    (model robosub.3dshapes/s61083-2x50-7.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59C2DFDD)
    (at 170.2 80.67 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C411 (at -2.27 0.04 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 232 /ADC/enc-))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 242 /enc-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59CC16EE)
    (at 168.05 67.94 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C412 (at 2.44 -0.05 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 230 /ADC/1v8_analog))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59C2E3AE)
    (at 215.38 71.374 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1310 (at 3.48 -0.026 180) (layer F.SilkS))
    (fp_text value 22u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59C2E3A2)
    (at 215.392 69.342 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1311 (at 3.492 0.042 180) (layer F.SilkS))
    (fp_text value 22u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module robosub_footprints:Inductor-3.6mm-Pitch-4.0mm-Length-1.5mm-Width (layer F.Cu) (tedit 59C2E353)
    (at 219.71 70.612)
    (fp_text reference L1302 (at 1.29 -2.54) (layer F.SilkS))
    (fp_text value 4.7u (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 1.8 0) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(C1306-Pad1)"))
    (pad 2 smd rect (at -1.8 0) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (model robosub.3dshapes/nr5040-inductor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59C2E3C6)
    (at 220.218 74.168)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1306 (at -0.254 -1.27) (layer B.SilkS))
    (fp_text value 22n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 227 "Net-(C1306-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 226 "Net-(C1306-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm_ThermalVias (layer F.Cu) (tedit 59C2E34C)
    (at 220.521 76.466)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1303 (at 0.779 -2.266) (layer F.SilkS))
    (fp_text value TS30042 (at 0 2.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(C1306-Pad1)"))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(U1303-Pad8)"))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /vccio_en))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(C1306-Pad2)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(C1306-Pad1)"))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(C1306-Pad1)"))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(C1306-Pad1)"))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at 0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (pad 17 thru_hole circle (at -0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59C3281C)
    (at 183.83 71.53)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L405 (at -0.33 -1.33) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 230 /ADC/1v8_analog))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_KiCAD-Logo_CopperAndSilkScreenTop (layer F.Cu) (tedit 0)
    (at 107.8 102.7)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbols:Symbol_Barrel_Polarity (layer F.Cu) (tedit 5765E9A7)
    (at 229.6 61.2 90)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (fp_text reference REF** (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value Symbol_Barrel_Polarity (at 0 2 90) (layer F.Fab))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 115.2 44.8)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 59C3398B)
    (at 234.2 81 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D101 (at -0.1 1.1 90) (layer F.SilkS))
    (fp_text value ORG (at 0 1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 240 /MicroZed-JX1/SE0))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(D101-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59C338DD)
    (at 234.1 60 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1201 (at -0.2 1.2 90) (layer F.SilkS))
    (fp_text value YLW (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 /Power/Vin))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(D1201-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59C33990)
    (at 213.7 42.6)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1202 (at -0.5 -1.2) (layer F.SilkS))
    (fp_text value RED (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 +5V))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(D1202-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59C33979)
    (at 234.1 69.8 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1203 (at -0.2 1.2 90) (layer F.SilkS))
    (fp_text value GRN (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(D1203-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59C33985)
    (at 234.2 83.7 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 0 -1.2 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 243 "Net-(D101-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59C338E1)
    (at 234.1 63.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1214 (at 0 -1.1 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 244 "Net-(D1201-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59C33994)
    (at 210.2 42.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1215 (at 0 1.1 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 245 "Net-(D1202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59C3397F)
    (at 234.1 73 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1216 (at 0 -1.1 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 246 "Net-(D1203-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module robosub_footprints:robosub_logo-large (layer F.Cu) (tedit 0)
    (at 107.8 93.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text Debug (at 232 82.3 90) (layer F.SilkS))
  (gr_text 5V (at 213.5 44.4 180) (layer F.SilkS))
  (gr_text 1.8V (at 232 69.9 90) (layer F.SilkS))
  (gr_text Vin (at 232 59.9 90) (layer F.SilkS))
  (gr_text "Hydropone ADC\nRyan Summers\nRev A" (at 232.46 87.11) (layer B.SilkS))
  (gr_text - (at 229.7 64.08) (layer F.SilkS))
  (gr_text + (at 229.68 58.08) (layer F.SilkS))
  (gr_line (start 83.67 106.64) (end 83.67 40.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 236.5 106.64) (end 83.67 106.64) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 236.5 40.3) (end 236.5 106.64) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.67 40.3) (end 236.5 40.3) (layer Edge.Cuts) (width 0.15))
  (zone (net 8) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.686 40.64) (xy 154.686 60.452) (xy 167.64 65.786) (xy 170.688 65.786) (xy 170.688 77.47)
        (xy 168.91 77.47) (xy 168.91 81.28) (xy 155.194 88.646) (xy 155.194 106.426) (xy 236.16 106.38)
        (xy 236.03 40.49)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.924 40.64) (xy 153.924 60.96) (xy 167.64 66.548) (xy 169.926 66.548) (xy 169.926 76.708)
        (xy 168.148 76.708) (xy 168.148 80.772) (xy 154.178 87.884) (xy 154.178 106.426) (xy 83.68 106.64)
        (xy 83.67 40.33)
      )
    )
  )
  (zone (net 5) (net_name +1V8) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 235.966 93.472) (xy 155.194 93.472) (xy 155.194 88.646) (xy 168.91 81.28) (xy 168.916 67.59)
        (xy 154.686 61.722) (xy 154.686 52.832) (xy 235.966 52.832)
      )
    )
  )
  (zone (net 23) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 236.22 40.64) (xy 120.396 41.148) (xy 120.142 106.172) (xy 132.08 106.172) (xy 132.08 48.768)
        (xy 149.606 48.768) (xy 149.606 93.472) (xy 153.924 93.472) (xy 153.924 52.07) (xy 235.966 52.07)
      )
    )
  )
  (zone (net 20) (net_name -5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 236.22 94.234) (xy 148.844 94.234) (xy 148.824 49.512) (xy 132.842 49.53) (xy 132.842 106.172)
        (xy 236.22 106.172)
      )
    )
  )
  (zone (net 20) (net_name -5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 217.17 97.536) (xy 220.472 97.536) (xy 220.472 94.488) (xy 217.17 94.488)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 216.662 96.52) (xy 216.662 100.076) (xy 212.344 100.076) (xy 212.344 96.52)
      )
    )
  )
  (zone (net 23) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 216.916 43.942) (xy 216.916 51.054) (xy 221.488 51.054) (xy 221.488 43.942)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 235.458 50.546) (xy 229.362 50.546) (xy 229.362 46.228) (xy 235.458 46.228)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.2 101.6) (xy 124.772 101.6) (xy 124.714 99.06) (xy 120.142 99.06)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.9 68.4) (xy 124.726 68.4) (xy 124.714 66.294) (xy 119.888 66.294)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.9 51.286) (xy 125.222 51.308) (xy 125.222 49.022) (xy 119.9 49)
      )
    )
  )
  (zone (net 5) (net_name +1V8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.214 53.848) (xy 192.278 53.848) (xy 192.278 57.15) (xy 188.214 57.15)
      )
    )
  )
  (zone (net 23) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.308 44.704) (xy 182.372 44.704) (xy 182.372 47.752) (xy 178.308 47.752)
      )
    )
  )
  (zone (net 5) (net_name +1V8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.182 89.408) (xy 190.246 89.408) (xy 190.246 91.948) (xy 186.182 91.948)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.888 84.328) (xy 125.476 84.328) (xy 125.476 82.042) (xy 119.888 82.042)
      )
    )
  )
  (zone (net 226) (net_name "Net-(C1306-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.266 70.104) (xy 220.218 70.104) (xy 220.218 73.406) (xy 218.44 73.406) (xy 218.44 75.946)
        (xy 223.266 75.946)
      )
    )
  )
  (zone (net 5) (net_name +1V8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219.71 72.644) (xy 219.71 65.532) (xy 215.138 65.532) (xy 215.138 72.644)
      )
    )
  )
  (zone (net 5) (net_name +1V8) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.2 69.4) (xy 186.8 69.4) (xy 186.8 73.2) (xy 184.3 73.2)
      )
    )
  )
  (zone (net 230) (net_name /ADC/1v8_analog) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.8 70.5) (xy 183.4 70.5) (xy 183.4 73.2) (xy 180.9 73.2)
      )
    )
  )
)
