<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="-0.635" x2="103.175" y2="-0.635" width="0" layer="20"/>
<wire x1="103.175" y1="-0.635" x2="103.175" y2="43.805" width="0" layer="20"/>
<wire x1="103.175" y1="43.805" x2="5.08" y2="43.805" width="0" layer="20"/>
<wire x1="5.08" y1="43.805" x2="5.08" y2="-0.635" width="0" layer="20"/>
<text>www.gelberhund.com/relaypi</text>
<text>V2.0</text>
<text>Raspberry Pi Relay Board</text>
<text>DANGER</text>
<text>HIGH</text>
<text>VOLTAGE</text>
<text>DANGER</text>
<text>HIGH</text>
<text>VOLTAGE</text>
<text>6 5 4 3 2 1</text>
<text>HOT</text>
</plain>
<libraries>
<library name="dz">
<packages>
<package name="HDR3">
</package>
<package name="RASPBERRY_PI_HEADER">
</package>
<package name="HDR2">
</package>
<package name="OAC5">
</package>
<package name="HDR2_5V_PWR">
</package>
<package name="LED0603">
</package>
<package name="R0603">
</package>
<package name="HDR10">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOP-14">
<description>&lt;h3&gt;14-pin SOP-14 package&lt;/h3&gt;
Used on WS2801 RGB controller</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TEMP" library="dz" package="HDR3" value="3X1"/>
<element name="RPI_HDR" library="dz" package="RASPBERRY_PI_HEADER" value="RASPBERRY_PI_HEADERRASPI_HDR"/>
<element name="RELAY7" library="dz" package="HDR2" value="2X1+-"/>
<element name="RELAY8" library="dz" package="HDR2" value="2X1+-"/>
<element name="K2" library="dz" package="OAC5" value="SRLY-19"/>
<element name="K3" library="dz" package="OAC5" value="SRLY-19"/>
<element name="K4" library="dz" package="OAC5" value="SRLY-19"/>
<element name="K5" library="dz" package="OAC5" value="SRLY-19"/>
<element name="K6" library="dz" package="OAC5" value="SRLY-19"/>
<element name="RELAY1" library="dz" package="HDR2" value="2X1+-"/>
<element name="RELAY2" library="dz" package="HDR2" value="2X1+-"/>
<element name="RELAY3" library="dz" package="HDR2" value="2X1+-"/>
<element name="RELAY4" library="dz" package="HDR2" value="2X1+-"/>
<element name="RELAY5" library="dz" package="HDR2" value="2X1+-"/>
<element name="RELAY6" library="dz" package="HDR2" value="2X1+-"/>
<element name="K1" library="dz" package="OAC5" value="SRLY-19"/>
<element name="RLY_PWR" library="dz" package="HDR2_5V_PWR" value="2X15V_PWR"/>
<element name="LED1" library="dz" package="LED0603" value="LED"/>
<element name="R1" library="dz" package="R0603" value="330"/>
<element name="LED2" library="dz" package="LED0603" value="LED"/>
<element name="R2" library="dz" package="R0603" value="330"/>
<element name="R3" library="dz" package="R0603" value="330"/>
<element name="R4" library="dz" package="R0603" value="330"/>
<element name="R5" library="dz" package="R0603" value="330"/>
<element name="R6" library="dz" package="R0603" value="330"/>
<element name="LED3" library="dz" package="LED0603" value="LED"/>
<element name="LED4" library="dz" package="LED0603" value="LED"/>
<element name="LED5" library="dz" package="LED0603" value="LED"/>
<element name="LED6" library="dz" package="LED0603" value="LED"/>
<element name="U1" library="SparkFun-DigitalIC" package="SOP-14" value="WS2801"/>
<element name="U2" library="SparkFun-DigitalIC" package="SOP-14" value="WS2801"/>
<element name="LED7" library="dz" package="LED0603" value="LED"/>
<element name="LED8" library="dz" package="LED0603" value="LED"/>
<element name="R7" library="dz" package="R0603" value="330"/>
<element name="R8" library="dz" package="R0603" value="330"/>
<element name="U3" library="SparkFun-DigitalIC" package="SOP-14" value="WS2801"/>
<element name="." library="dz" package="HDR10" value=""/>
<element name="RELAY9" library="dz" package="HDR2" value="2X1+-"/>
<element name="LED9" library="dz" package="LED0603" value="LED"/>
<element name="R9" library="dz" package="R0603" value="330"/>
<element name="R10" library="dz" package="R0603" value="330"/>
</elements>
<signals>
<signal name="GPIO17">
<contactref element="RPI_HDR" pad="11"/>
</signal>
<signal name="GPIO18">
<contactref element="RPI_HDR" pad="12"/>
</signal>
<signal name="GPIO22">
<contactref element="RPI_HDR" pad="15"/>
</signal>
<signal name="GPIO23">
<contactref element="RPI_HDR" pad="16"/>
</signal>
<signal name="GPIO24">
<contactref element="RPI_HDR" pad="18"/>
</signal>
<signal name="GPIO25">
<contactref element="RPI_HDR" pad="22"/>
</signal>
<signal name="GPIO4">
<contactref element="RPI_HDR" pad="7"/>
<contactref element="TEMP" pad="D"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="5.0V">
<contactref element="RPI_HDR" pad="2"/>
<contactref element="TEMP" pad="+"/>
<contactref element="RLY_PWR" pad="+"/>
<contactref element="U1" pad="14"/>
<contactref element="U2" pad="14"/>
<contactref element="U3" pad="14"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="GND">
<contactref element="RPI_HDR" pad="6"/>
<contactref element="TEMP" pad="-"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="5"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="5"/>
<contactref element="U1" pad="7"/>
<contactref element="U2" pad="7"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="SPI_CE1">
<contactref element="RPI_HDR" pad="26"/>
</signal>
<signal name="O1">
<contactref element="K1" pad="4"/>
<contactref element="RELAY1" pad="-"/>
<contactref element="LED1" pad="C"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="O2">
<contactref element="K2" pad="4"/>
<contactref element="RELAY2" pad="-"/>
<contactref element="LED2" pad="C"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="O3">
<contactref element="K3" pad="4"/>
<contactref element="RELAY3" pad="-"/>
<contactref element="LED3" pad="C"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="O4">
<contactref element="K4" pad="4"/>
<contactref element="RELAY4" pad="-"/>
<contactref element="LED4" pad="C"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="O5">
<contactref element="K5" pad="4"/>
<contactref element="RELAY5" pad="-"/>
<contactref element="LED5" pad="C"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="O6">
<contactref element="K6" pad="4"/>
<contactref element="RELAY6" pad="-"/>
<contactref element="LED6" pad="C"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="O8">
<contactref element="RELAY8" pad="-"/>
<contactref element="LED8" pad="C"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="O7">
<contactref element="RELAY7" pad="-"/>
<contactref element="LED7" pad="C"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="HOT">
<contactref element="K2" pad="1"/>
<contactref element="K3" pad="1"/>
<contactref element="K4" pad="1"/>
<contactref element="K5" pad="1"/>
<contactref element="K6" pad="1"/>
<contactref element="K1" pad="1"/>
<contactref element="." pad="1"/>
<contactref element="." pad="2"/>
</signal>
<signal name="N$7">
<contactref element="K2" pad="2"/>
<contactref element="." pad="4"/>
</signal>
<signal name="N$8">
<contactref element="K3" pad="2"/>
<contactref element="." pad="5"/>
</signal>
<signal name="N$9">
<contactref element="K4" pad="2"/>
<contactref element="." pad="6"/>
</signal>
<signal name="N$10">
<contactref element="K5" pad="2"/>
<contactref element="." pad="7"/>
</signal>
<signal name="N$11">
<contactref element="K6" pad="2"/>
<contactref element="." pad="8"/>
</signal>
<signal name="N$12">
<contactref element="K1" pad="2"/>
<contactref element="." pad="3"/>
</signal>
<signal name="RXD">
<contactref element="RPI_HDR" pad="10"/>
</signal>
<signal name="TXD">
<contactref element="RPI_HDR" pad="8"/>
</signal>
<signal name="SPI_CE0">
<contactref element="RPI_HDR" pad="24"/>
</signal>
<signal name="R_PWR">
<contactref element="K1" pad="3"/>
<contactref element="K2" pad="3"/>
<contactref element="K3" pad="3"/>
<contactref element="K4" pad="3"/>
<contactref element="K5" pad="3"/>
<contactref element="K6" pad="3"/>
<contactref element="RELAY1" pad="+"/>
<contactref element="RELAY2" pad="+"/>
<contactref element="RELAY3" pad="+"/>
<contactref element="RELAY4" pad="+"/>
<contactref element="RELAY5" pad="+"/>
<contactref element="RELAY6" pad="+"/>
<contactref element="RELAY7" pad="+"/>
<contactref element="RELAY8" pad="+"/>
<contactref element="RLY_PWR" pad="-"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="RELAY9" pad="+"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="LED6" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="LED5" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="RPI_HDR" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R7" pad="1"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="R8" pad="1"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="13"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="12"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="1"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="O9">
<contactref element="U3" pad="8"/>
<contactref element="RELAY9" pad="-"/>
<contactref element="LED9" pad="C"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="RPI_HDR" pad="19"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="SPI_MISO">
<contactref element="RPI_HDR" pad="21"/>
</signal>
<signal name="SPI_CLK">
<contactref element="RPI_HDR" pad="23"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R9" pad="1"/>
<contactref element="LED9" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
