(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 28)
    (zones 0)
    (modules 8)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (user_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 1.8)
    (pad_drill 1.066)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 125.89764 116.08816)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module .pretty:Kemet1800pF_100v (layer B.Cu) (tedit 62CEF5AE)
    (at 134.37616 110.47382)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference CL (at 0 0) (layer B.SilkS))
    (fp_text value C (at -0.10828 0.67564 180) (layer B.SilkS) hide)
    (pad 2 thru_hole roundrect (at 2.5 0) (size 1.7 1.6) (drill 0.64) (layers *.Cu *.Mask B.SilkS) (roundrect_rratio 0.25))
    (pad 1 thru_hole roundrect (at -2.5 0) (size 1.7 1.6) (drill 0.64) (layers *.Cu *.Mask B.SilkS) (roundrect_rratio 0.25))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:22Ga_pad_1_066mm_rect2 (layer F.Cu) (tedit 63B7414B)
    (at 134.14514 114.51634 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference M3 (at 1.90766 0) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 -1.13 180) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.032 1.8) (drill 1.066) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25))
  )
  (module .pretty:22Ga_pad_1_066mm_rect2 (layer F.Cu) (tedit 600D9B6C)
    (at 136.62406 114.51634 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference OUT (at 0.0254 -0.03296) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.0254 -0.1752 180) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0 180) (size 2.032 1.8) (drill 1.066) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25))
  )
  (module .pretty:22Ga_pad_1_066mm_rect2 (layer F.Cu) (tedit 600D9B6C)
    (at 134.31794 93.0662)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference OUT (at 0.0254 -0.03296) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.0254 -0.1752 180) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 1.8) (drill 1.066) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25))
  )
  (module .pretty:Tayda_DPDT_Switch (layer B.Cu) (tedit 62069E70)
    (at 132.23316 101.01224)
    (fp_text reference On-On-On (at -2.415 4.46) (layer B.SilkS) hide)
    (fp_text value Tayda_DPDT_Switch (at -0.075 -0.05) (layer B.Fab))
    (pad 6 thru_hole roundrect (at 2.285 -4.7) (size 3.12 2) (drill oval 2.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 5 thru_hole roundrect (at -2.415 -4.7) (size 3.12 2) (drill oval 2.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 4 thru_hole roundrect (at 2.415 0) (size 3.12 2) (drill oval 2.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 3 thru_hole roundrect (at -2.415 0) (size 3.12 2) (drill oval 2.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 2 thru_hole roundrect (at 2.415 4.7) (size 3.12 2) (drill oval 2.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 1 thru_hole roundrect (at -2.415 4.7) (size 3.12 2) (drill oval 2.5 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
  )
  (module .pretty:PassinwindElectronics_100_10mm (layer F.Cu) (tedit 60A0AF65)
    (at 132.23316 103.3084)
    (fp_text reference PWE (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module .pretty:22Ga_pad_1_066mm_rect2 (layer F.Cu) (tedit 600D9B6C)
    (at 136.79686 93.0662)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference M1 (at -4.46032 0.0121) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 -1.13 180) (layer F.SilkS) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 2.032 1.8) (drill 1.066) (layers *.Cu *.Mask F.SilkS) (roundrect_rratio 0.25))
  )
  (module .pretty:Kemet1800pF_100v (layer B.Cu) (tedit 63B72829)
    (at 128.33528 112.01634 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference CM (at 0 0 90) (layer B.SilkS))
    (fp_text value C (at 0.01956 0.67564 270) (layer B.SilkS) hide)
    (pad 1 thru_hole roundrect (at -2.5 0 90) (size 1.7 1.6) (drill 0.64) (layers *.Cu *.Mask B.SilkS) (roundrect_rratio 0.25))
    (pad 2 thru_hole roundrect (at 2.5 0 90) (size 1.7 1.6) (drill 0.64) (layers *.Cu *.Mask B.SilkS) (roundrect_rratio 0.25))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 127.02794 114.95258) (end 125.89764 114.95258) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.00762 92.70638) (end 127.00762 91.57608) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.50798 92.70892) (end 138.63828 92.70892) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 137.43686 114.95512) (end 137.43686 116.08542) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "By CE 2023" (at 132.23316 98.6348) (layer B.SilkS))
  (gr_line (start 125.89764 114.95024) (end 125.87478 92.71508) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.44956 116.0905) (end 127.02794 116.08288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 138.63574 92.70492) (end 138.56716 114.95278) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.98984 91.57862) (end 137.5156 91.58116) (layer Edge.Cuts) (width 0.05))
)
