(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 7)
    (no_connects 1)
    (area 137.084999 111.684999 172.795001 132.155001)
    (thickness 1.6)
    (drawings 12)
    (tracks 15)
    (zones 0)
    (modules 6)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(F1-Pad1)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(F1-Pad2)")
  (net 8 "Net-(J3-Pad3)")
  (net 9 "Net-(J3-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5D2E49CA)
    (at 154.94 127 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 180) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Microfit3_Header_02x01_Angled_43045-020x (layer F.Cu) (tedit 5D2E4998)
    (at 162.56 125.73 90)
    (descr "Microfit3 02x01 header angled 43045-0200")
    (tags "connector Microfit 02x01 angled 3mm pitch")
    (fp_text reference J1 (at 1.27 7.62 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -6.604 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -3 90) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad "" np_thru_hole circle (at 0 4.32 90) (size 3.1 3.1) (drill 3.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_Microfit3_Header_02x01_Angled_43045-020x.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_NanoFit_1x02x2.50mm_Angled (layer F.Cu) (tedit 5D2E499A)
    (at 161.29 115.57 270)
    (descr "Molex Nano Fit, single row, side entry, through hole, Datasheet:http://www.molex.com/pdm_docs/sd/1053131208_sd.pdf")
    (tags "connector molex nano-fit 105313-xx04")
    (fp_text reference J2 (at 1.27 -3.81 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.25 3.5 270) (layer F.Fab))
    (fp_text user %R (at 1.25 -4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad "" np_thru_hole circle (at 0 -7.18 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.5 -7.18 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_NanoFit_1x02x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5D2E49B6)
    (at 156.21 123.19 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.31 90) (layer F.SilkS) hide)
    (fp_text value 330 (at 3.81 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_B (layer F.Cu) (tedit 5D2E4995)
    (at 147.32 123.19 180)
    (descr "USB B connector")
    (tags "USB_B USB_DEV")
    (fp_text reference J3 (at 7.62 1.27 270) (layer F.SilkS))
    (fp_text value USB_B (at 4.7 1.27 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 7 "Net-(F1-Pad2)"))
    (pad 4 thru_hole circle (at 2 0 90) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 2 2.54 90) (size 1.52 1.52) (drill 0.81) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad3)"))
    (pad 5 thru_hole circle (at 4.7 7.27 90) (size 2.7 2.7) (drill 2.3) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad5)"))
    (pad 5 thru_hole circle (at 4.7 -4.73 90) (size 2.7 2.7) (drill 2.3) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad5)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_B.wrl
      (at (xyz 0.18 -0.05 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_TE5_Littlefuse-395Series (layer F.Cu) (tedit 5D2E49A7)
    (at 152.4 115.57 270)
    (descr "Fuse, TE5, Littlefuse/Wickmann, No. 460, No560,")
    (tags "Fuse TE5 Littlefuse/Wickmann No. 460 No560 ")
    (fp_text reference F1 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value Polyfuse (at 2.35 3.1 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0.01 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(F1-Pad2)"))
  )
  (gr_text "Rev 0.0\nJuly 2019" (at 162.56 128.905) (layer B.SilkS))
  (gr_text "B003-5002 Cable Tester" (at 155.575 130.81) (layer F.SilkS))
  (dimension 35.56 (width 0.3) (layer Dwgs.User)
    (gr_text "35.560 mm" (at 154.94 135.97) (layer Dwgs.User))
    (feature1 (pts (xy 172.72 132.08) (xy 172.72 137.32)))
    (feature2 (pts (xy 137.16 132.08) (xy 137.16 137.32)))
    (crossbar (pts (xy 137.16 134.62) (xy 172.72 134.62)))
    (arrow1a (pts (xy 172.72 134.62) (xy 171.593496 135.206421)))
    (arrow1b (pts (xy 172.72 134.62) (xy 171.593496 134.033579)))
    (arrow2a (pts (xy 137.16 134.62) (xy 138.286504 135.206421)))
    (arrow2b (pts (xy 137.16 134.62) (xy 138.286504 134.033579)))
  )
  (dimension 20.32 (width 0.3) (layer Dwgs.User)
    (gr_text "20.320 mm" (at 179.15 121.92 270) (layer Dwgs.User))
    (feature1 (pts (xy 172.72 132.08) (xy 180.5 132.08)))
    (feature2 (pts (xy 172.72 111.76) (xy 180.5 111.76)))
    (crossbar (pts (xy 177.8 111.76) (xy 177.8 132.08)))
    (arrow1a (pts (xy 177.8 132.08) (xy 177.213579 130.953496)))
    (arrow1b (pts (xy 177.8 132.08) (xy 178.386421 130.953496)))
    (arrow2a (pts (xy 177.8 111.76) (xy 177.213579 112.886504)))
    (arrow2b (pts (xy 177.8 111.76) (xy 178.386421 112.886504)))
  )
  (gr_line (start 139.7 111.76) (end 170.18 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 132.08) (end 170.18 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 129.54) (end 172.72 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 114.3) (end 137.16 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.18 114.3) (end 170.18 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.18 129.54) (end 172.72 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.7 129.54) (end 139.7 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.7 114.3) (end 137.16 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
)
