(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 18)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(M1-Pad-)")
  (net 4 "Net-(M3-Pad-)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(M1-Pad-)")
    (add_net "Net-(M3-Pad-)")
  )
  (module alexglow-footprints:hlogoTiny (layer F.Cu) (tedit 600E2129)
    (at 104.75 90.5 90)
    (fp_text reference " " (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value " " (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module alexglow-footprints:bee-vibe-cu (layer F.Cu) (tedit 614CD706)
    (at 125.22231 106.291567)
    (fp_text reference M4 (at 0 6.223) (layer F.SilkS) hide)
    (fp_text value MOTOR10MM (at 0.75 0) (layer F.SilkS) hide)
    (fp_text user + (at -2.8575 -5.334) (layer F.SilkS))
    (fp_text user - (at 2.8575 -5.334) (layer F.SilkS))
    (pad + thru_hole circle (at -1.143 -6.096) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(M3-Pad-)"))
    (pad - thru_hole circle (at 1.143 -6.1595) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
  )
  (module alexglow-footprints:bee-vibe-cu (layer F.Cu) (tedit 614CD6D9)
    (at 105.22231 106.291567)
    (fp_text reference M2 (at 0 6.223) (layer F.SilkS) hide)
    (fp_text value MOTOR10MM (at 0.75 0) (layer F.SilkS) hide)
    (fp_text user - (at 2.8575 -5.334) (layer F.SilkS))
    (fp_text user + (at -2.8575 -5.334) (layer F.SilkS))
    (pad - thru_hole circle (at 1.143 -6.1595) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad + thru_hole circle (at -1.143 -6.096) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(M1-Pad-)"))
  )
  (module alexglow-footprints:bee-vibe-cu (layer F.Cu) (tedit 614CD6C0)
    (at 125.22231 76.291567)
    (fp_text reference M3 (at 0 6.223) (layer F.SilkS) hide)
    (fp_text value MOTOR10MM (at 0.75 0) (layer F.SilkS) hide)
    (fp_text user + (at -2.8575 -5.334) (layer F.SilkS))
    (fp_text user - (at 2.8575 -5.334) (layer F.SilkS))
    (pad + thru_hole circle (at -1.143 -6.096) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad - thru_hole circle (at 1.143 -6.1595) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(M3-Pad-)"))
  )
  (module alexglow-footprints:bee-vibe-cu (layer F.Cu) (tedit 614CD6A8)
    (at 105.22231 76.131567)
    (fp_text reference M1 (at 0 6.223) (layer F.SilkS) hide)
    (fp_text value MOTOR10MM (at 0.75 0) (layer F.SilkS) hide)
    (fp_text user - (at 2.8575 -5.334) (layer F.SilkS))
    (fp_text user + (at -2.8575 -5.334) (layer F.SilkS))
    (pad - thru_hole circle (at 1.143 -6.1595) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(M1-Pad-)"))
    (pad + thru_hole circle (at -1.143 -6.096) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (module alexglow-footprints:2-pin-power (layer F.Cu) (tedit 614915E7)
    (at 115.4 66.96 270)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value powerJump (at 1.25 -2.1 90) (layer F.SilkS))
    (fp_text user + (at 0 1.75 90) (layer F.SilkS))
    (fp_text user - (at 2.54 1.75 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 -0.1 270) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 270) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)") (solder_mask_margin 0.1016))
  )
  (gr_text "Purr Module" (at 115.25 104 90) (layer F.Cu))
  (gr_text "v1 • alex glow • @glowascii" (at 115.5 84.75 90) (layer F.Cu))
  (gr_line (start 112 65) (end 111 65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114 64) (end 112 65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117 64) (end 114 64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119 65) (end 117 64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.5 69) (end 105 65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.5 72.5) (end 97.5 69) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.5 69) (end 125 65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.5 72.5) (end 132.5 69) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.5 110) (end 132.5 72.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 115) (end 132.5 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105 115) (end 125 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.5 110) (end 105 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.5 72.5) (end 97.5 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111 65) (end 105 65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119 65) (end 125 65) (layer Edge.Cuts) (width 0.05))
)
