(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 217)
    (zones 0)
    (modules 15)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 34 168)
    (grid_origin 34 168)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "ledAsoex2019/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(U3-Pad7)")
  (net 4 "Net-(U3-Pad8)")
  (net 5 "Net-(U3-Pad5)")
  (net 6 "Net-(U3-Pad6)")
  (net 7 "Net-(U3-Pad3)")
  (net 8 "Net-(U3-Pad4)")
  (net 9 "Net-(U3-Pad1)")
  (net 10 "Net-(U3-Pad2)")
  (net 11 "Net-(U4-Pad18)")
  (net 12 "Net-(U4-Pad19)")
  (net 13 "Net-(U4-Pad16)")
  (net 14 "Net-(U4-Pad15)")
  (net 15 "Net-(U2-Pad17)")
  (net 16 "Net-(U4-Pad22)")
  (net 17 "Net-(U4-Pad23)")
  (net 18 "Net-(U2-Pad13)")
  (net 19 "Net-(U2-Pad12)")
  (net 20 "Net-(U4-Pad32)")
  (net 21 +5V)
  (net 22 "Net-(U4-Pad11)")
  (net 23 "Net-(U2-Pad15)")
  (net 24 "Net-(U2-Pad16)")
  (net 25 "Net-(U2-Pad14)")
  (net 26 "Net-(U2-Pad11)")
  (net 27 "Net-(U4-Pad6)")
  (net 28 "Net-(U4-Pad5)")
  (net 29 "Net-(U2-Pad18)")
  (net 30 "Net-(R1-Pad2)")
  (net 31 "Net-(J1-Pad1)")
  (net 32 "Net-(J1-Pad2)")
  (net 33 "Net-(R2-Pad2)")
  (net 34 "Net-(R3-Pad2)")
  (net 35 "Net-(J1-Pad3)")
  (net 36 "Net-(J1-Pad4)")
  (net 37 "Net-(R4-Pad2)")
  (net 38 "Net-(R5-Pad2)")
  (net 39 "Net-(J1-Pad5)")
  (net 40 "Net-(J1-Pad6)")
  (net 41 "Net-(R6-Pad2)")
  (net 42 "Net-(R7-Pad2)")
  (net 43 "Net-(J1-Pad7)")
  (net 44 "Net-(J1-Pad8)")
  (net 45 "Net-(R8-Pad2)")
  (net 46 "Net-(U4-Pad24)")
  (net 47 "Net-(U4-Pad25)")
  (net 48 "Net-(U4-Pad26)")
  (net 49 "Net-(U4-Pad29)")
  (net 50 "Net-(U4-Pad30)")
  (net 51 "Net-(U4-Pad3)")
  (net 52 "Net-(U4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad19)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad23)")
    (add_net "Net-(U4-Pad24)")
    (add_net "Net-(U4-Pad25)")
    (add_net "Net-(U4-Pad26)")
    (add_net "Net-(U4-Pad29)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad30)")
    (add_net "Net-(U4-Pad32)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
  )
  (net_class power ""
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module ludique:ENC28J60_MOD (layer F.Cu) (tedit 5D70875A)
    (at 106 131)
    (fp_text reference U3 (at 0 10.5) (layer F.SilkS))
    (fp_text value ENC28J60 (at 0 -8.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at -22.25 13.75) (size 4.2 4.2) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -22.25 -13.75) (size 4.2 4.2) (drill 2.75) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -23.46 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(U3-Pad2)"))
    (pad 1 thru_hole rect (at -26 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(U3-Pad1)"))
    (pad 4 thru_hole circle (at -23.46 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(U3-Pad4)"))
    (pad 3 thru_hole circle (at -26 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(U3-Pad3)"))
    (pad 6 thru_hole circle (at -23.46 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(U3-Pad6)"))
    (pad 5 thru_hole circle (at -26 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(U3-Pad5)"))
    (pad 8 thru_hole circle (at -23.46 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(U3-Pad8)"))
    (pad 7 thru_hole circle (at -26 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(U3-Pad7)"))
    (pad 10 thru_hole circle (at -23.46 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at -26 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 +3V3))
  )
  (module Teensy:Teensy32_mainpins (layer F.Cu) (tedit 5D6FFE1E)
    (at 102.75 112 270)
    (fp_text reference U4 (at 0 -10.16 270) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 10.16 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U4-Pad2)"))
    (pad 3 thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U4-Pad3)"))
    (pad 4 thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U2-Pad18)"))
    (pad 5 thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U4-Pad5)"))
    (pad 6 thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U4-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U2-Pad11)"))
    (pad 8 thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U2-Pad14)"))
    (pad 9 thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U2-Pad16)"))
    (pad 10 thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U2-Pad15)"))
    (pad 11 thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U4-Pad11)"))
    (pad 12 thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(U3-Pad7)"))
    (pad 13 thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U3-Pad5)"))
    (pad 33 thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 +5V))
    (pad 32 thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U4-Pad32)"))
    (pad 31 thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 30 thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U4-Pad30)"))
    (pad 29 thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U4-Pad29)"))
    (pad 28 thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U2-Pad12)"))
    (pad 27 thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U2-Pad13)"))
    (pad 26 thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U4-Pad26)"))
    (pad 25 thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U4-Pad25)"))
    (pad 24 thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U4-Pad24)"))
    (pad 23 thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U4-Pad23)"))
    (pad 22 thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U4-Pad22)"))
    (pad 21 thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U2-Pad17)"))
    (pad 14 thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U3-Pad4)"))
    (pad 15 thru_hole circle (at 16.51 5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U4-Pad15)"))
    (pad 16 thru_hole circle (at 16.51 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U4-Pad16)"))
    (pad 20 thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U3-Pad6)"))
    (pad 19 thru_hole circle (at 16.51 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U4-Pad19)"))
    (pad 18 thru_hole circle (at 16.51 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U4-Pad18)"))
    (pad 17 thru_hole circle (at 16.51 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 91.5 97 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 270) (layer F.SilkS))
    (fp_text value C (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 81.25 112 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value C (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 0)
    (at 107.25 143.25)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J2 (at 1.27 -4.50088) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x02 (at 1.27 4.50088) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 21 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer F.Cu) (tedit 0)
    (at 67 124.5 270)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 8.89 -4.50088 270) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x08 (at 8.89 4.50088 270) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 43 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 12.7 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 81.75 102)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -7.5) (layer F.SilkS))
    (fp_text value 74HC245 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad18)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad17)"))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad16)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad15)"))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad14)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad13)"))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad12)"))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R8-Pad2)"))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R7-Pad2)"))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R6-Pad2)"))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R4-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 74 143)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad8)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 73 137 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 72 129.5 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 72 120.5 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 69.5 113.75 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 69.25 105.75 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 65 117.25 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58AADA36)
    (at 65 107.25 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 71.25 (width 0.3) (layer F.SilkS)
    (gr_text "71,250 mm" (at 98.375 157.85) (layer F.SilkS))
    (feature1 (pts (xy 134 148.25) (xy 134 156.336421)))
    (feature2 (pts (xy 62.75 148.25) (xy 62.75 156.336421)))
    (crossbar (pts (xy 62.75 155.75) (xy 134 155.75)))
    (arrow1a (pts (xy 134 155.75) (xy 132.873496 156.336421)))
    (arrow1b (pts (xy 134 155.75) (xy 132.873496 155.163579)))
    (arrow2a (pts (xy 62.75 155.75) (xy 63.876504 156.336421)))
    (arrow2b (pts (xy 62.75 155.75) (xy 63.876504 155.163579)))
  )
  (dimension 51.25 (width 0.3) (layer F.SilkS)
    (gr_text "51,250 mm" (at 88.375 87.15) (layer F.SilkS))
    (feature1 (pts (xy 114 93) (xy 114 88.663579)))
    (feature2 (pts (xy 62.75 93) (xy 62.75 88.663579)))
    (crossbar (pts (xy 62.75 89.25) (xy 114 89.25)))
    (arrow1a (pts (xy 114 89.25) (xy 112.873496 89.836421)))
    (arrow1b (pts (xy 114 89.25) (xy 112.873496 88.663579)))
    (arrow2a (pts (xy 62.75 89.25) (xy 63.876504 89.836421)))
    (arrow2b (pts (xy 62.75 89.25) (xy 63.876504 88.663579)))
  )
  (dimension 55.25 (width 0.3) (layer F.SilkS)
    (gr_text "55,250 mm" (at 54.15 120.625 90) (layer F.SilkS))
    (feature1 (pts (xy 62.75 93) (xy 55.663579 93)))
    (feature2 (pts (xy 62.75 148.25) (xy 55.663579 148.25)))
    (crossbar (pts (xy 56.25 148.25) (xy 56.25 93)))
    (arrow1a (pts (xy 56.25 93) (xy 56.836421 94.126504)))
    (arrow1b (pts (xy 56.25 93) (xy 55.663579 94.126504)))
    (arrow2a (pts (xy 56.25 148.25) (xy 56.836421 147.123496)))
    (arrow2b (pts (xy 56.25 148.25) (xy 55.663579 147.123496)))
  )
  (gr_line (start 62.75 93) (end 62.75 148.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 93) (end 62.75 93) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 148.25) (end 114 93) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 62.75 148.25) (end 114 148.25) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 112.5 144 90) (layer F.SilkS))
  (gr_text +5VDC (at 103.75 143.75 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114 93.5) (xy 114 148.25) (xy 62.774121 148.25) (xy 62.75 93.5)
      )
    )
  )
  (zone (net 21) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.75 93.5) (xy 114 93.5) (xy 114 148.25) (xy 62.75 148.25)
      )
    )
  )
)
