(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 17)
    (no_connects 0)
    (area 118.014287 46.4 158.825001 106.755001)
    (thickness 1.6)
    (drawings 10)
    (tracks 110)
    (zones 0)
    (modules 12)
    (nets 9)
  )
  (page A4)
  (title_block
    (title Arduino_Nano_Shield_Layout)
    (date 2018-03-26)
    (rev 0)
    (company "Author: Thong Huynh")
    (comment 1 "Naura - WSU")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 107.95 52.578)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D2-Pad2)")
  (net 3 /SIGNAL)
  (net 4 VCC)
  (net 5 +5V)
  (net 6 PROBE)
  (net 7 "Net-(Q1-Pad2)")
  (net 8 "Net-(Q1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /SIGNAL)
    (add_net GND)
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net PROBE)
    (add_net VCC)
  )
  (module custom_nano_footprint:Arduino_Nano_Socket (layer F.Cu) (tedit 5ABCA3E0)
    (at 148.59 104.14)
    (descr https://store.arduino.cc/arduino-nano)
    (zone_connect 2)
    (fp_text reference U1 (at 9.16 0.96) (layer F.SilkS))
    (fp_text value Arduino_Nano_Socket (at 0 -21.082 90) (layer F.Fab))
    (fp_text user 3.3V (at 6.35 -6.35 90) (layer F.SilkS))
    (pad VIN thru_hole circle (at 7.62 -39.37) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 VCC) (zone_connect 2))
    (pad GND2 thru_hole circle (at 7.62 -36.83) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad RST2 thru_hole circle (at 7.62 -34.29) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 5V thru_hole circle (at 7.62 -31.75) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +5V) (zone_connect 2))
    (pad A7 thru_hole circle (at 7.62 -29.21) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad A6 thru_hole circle (at 7.62 -26.67) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad A5 thru_hole circle (at 7.62 -24.13) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad A4 thru_hole circle (at 7.62 -21.59) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad A3 thru_hole circle (at 7.62 -19.05) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad A2 thru_hole circle (at 7.62 -16.51) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad A1 thru_hole circle (at 7.62 -13.97) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad A0 thru_hole circle (at 7.62 -11.43) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /SIGNAL) (zone_connect 2))
    (pad AREF thru_hole circle (at 7.62 -8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 3V3 thru_hole circle (at 7.62 -6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D13 thru_hole circle (at 7.62 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D12 thru_hole circle (at -7.62 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D11 thru_hole circle (at -7.62 -6.35) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D10 thru_hole circle (at -7.62 -8.89) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D9 thru_hole circle (at -7.62 -11.43) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D8 thru_hole circle (at -7.62 -13.97) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D7 thru_hole circle (at -7.62 -16.51) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D6 thru_hole circle (at -7.62 -19.05) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D5 thru_hole circle (at -7.62 -21.59) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D4 thru_hole circle (at -7.62 -24.13) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D3 thru_hole circle (at -7.62 -26.67) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D2 thru_hole circle (at -7.62 -29.21) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad GND1 thru_hole circle (at -7.62 -31.75) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad RST1 thru_hole circle (at -7.62 -34.29) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D0 thru_hole circle (at -7.62 -36.83) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad D1 thru_hole rect (at -7.62 -39.37) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -7.62 -41.91) (size 1.85 1.85) (drill 1.85) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 7.62 -41.91) (size 1.85 1.85) (drill 1.85) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at -7.62 -1.27) (size 1.85 1.85) (drill 1.85) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad "" np_thru_hole circle (at 7.62 -1.27) (size 1.85 1.85) (drill 1.85) (layers *.Cu *.Mask)
      (zone_connect 2))
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 5ABC9DE6)
    (at 144.78 95.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at -0.43 -2.2) (layer F.SilkS))
    (fp_text value LED (at -0.93 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /SIGNAL))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 5ABC9DA5)
    (at 149.86 71.12 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at 3.71 -0.08 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_GH_SM02B-GHS-TB_02x1.25mm_Angled (layer F.Cu) (tedit 5ABC9DEF)
    (at 148.59 100.33)
    (descr "JST GH series connector, SM02B-GHS-TB, side entry type")
    (tags "connector jst GH SMT side horizontal entry 1.25mm pitch")
    (attr smd)
    (fp_text reference P1 (at 1.96 -3.98) (layer F.SilkS))
    (fp_text value Probe_Port (at 0 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0.45) (layer F.Fab))
    (pad 1 smd rect (at -0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.625 -1.6) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 PROBE))
    (pad "" smd rect (at 2.35 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.35 1.6) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_JST:JST_GH_SM02B-GHS-TB_02x1.25mm_Angled (layer F.Cu) (tedit 5ABC9DB8)
    (at 148.59 64.77 180)
    (descr "JST GH series connector, SM02B-GHS-TB, side entry type")
    (tags "connector jst GH SMT side horizontal entry 1.25mm pitch")
    (attr smd)
    (fp_text reference P2 (at 2.04 -3.78 180) (layer F.SilkS))
    (fp_text value Probe_Port (at 0 4.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.625 -1.6 180) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.625 -1.6 180) (size 0.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 PROBE))
    (pad "" smd rect (at 2.35 1.6 180) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.35 1.6 180) (size 1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow placed (layer F.Cu) (tedit 5ABC9DDA)
    (at 147.32 90.17)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.18 2.73) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABCA2C1)
    (at 144.78 85.09)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.07 -1.79) (layer F.SilkS))
    (fp_text value 1K (at -0.28 1.76) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 152.4 85.09)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 220 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /SIGNAL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABCA2C4)
    (at 152.4 80.01 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0.05 1.76 180) (layer F.SilkS))
    (fp_text value 27K (at -0.05 -1.84 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 144.78 80.01)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 PROBE))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5ABC9DAE)
    (at 149.86 74.93 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 220 (at 0.26 1.68 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_nano_footprint:robosub_logo-medium (layer B.Cu) (tedit 5ABD2400)
    (at 148 100.45)
    (fp_text reference "" (at 0 0) (layer B.SilkS) hide)
    (fp_text value "" (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text "Team Naura-WSU\nThong Huynh\nNicholas Heitman\nHenderson Reaves\nLuke Riske" (at 148.2 68.3) (layer B.SilkS))
  (gr_text V1.0 (at 153.6 62.2) (layer F.SilkS))
  (gr_text "Nano Socket with Leak Sensor" (at 147.65 105) (layer F.SilkS))
  (dimension 47.15 (width 0.3) (layer F.SilkS)
    (gr_text "1.8563 in" (at 123.55 83.4 270) (layer F.SilkS))
    (feature1 (pts (xy 126.25 106.7) (xy 126.25 106.7)))
    (feature2 (pts (xy 126.25 59.55) (xy 126.25 59.55)))
    (crossbar (pts (xy 126.25 59.55) (xy 126.25 106.7)))
    (arrow1a (pts (xy 126.25 106.7) (xy 125.663579 105.573496)))
    (arrow1b (pts (xy 126.25 106.7) (xy 126.836421 105.573496)))
    (arrow2a (pts (xy 126.25 59.55) (xy 125.663579 60.676504)))
    (arrow2b (pts (xy 126.25 59.55) (xy 126.836421 60.676504)))
  )
  (dimension 18.353338 (width 0.3) (layer F.SilkS)
    (gr_text "0.7226 in" (at 148.55 53.65 1.092702536) (layer F.SilkS))
    (feature1 (pts (xy 157.7 55.3) (xy 157.7 55.3)))
    (feature2 (pts (xy 139.35 55.65) (xy 139.35 55.65)))
    (crossbar (pts (xy 139.35 55.65) (xy 157.7 55.3)))
    (arrow1a (pts (xy 157.7 55.3) (xy 156.584884 55.907797)))
    (arrow1b (pts (xy 157.7 55.3) (xy 156.562518 54.735168)))
    (arrow2a (pts (xy 139.35 55.65) (xy 140.487482 56.214832)))
    (arrow2b (pts (xy 139.35 55.65) (xy 140.465116 55.042203)))
  )
  (dimension 20.300062 (width 0.3) (layer F.SilkS)
    (gr_text "0.7992 in" (at 148.45 47.6 0.1411223243) (layer F.SilkS))
    (feature1 (pts (xy 138.45 49.5) (xy 138.45 49.5)))
    (feature2 (pts (xy 158.75 49.45) (xy 158.75 49.45)))
    (crossbar (pts (xy 158.75 49.45) (xy 138.45 49.5)))
    (arrow1a (pts (xy 138.45 49.5) (xy 139.575056 48.910806)))
    (arrow1b (pts (xy 138.45 49.5) (xy 139.577945 50.083644)))
    (arrow2a (pts (xy 158.75 49.45) (xy 157.622055 48.866356)))
    (arrow2b (pts (xy 158.75 49.45) (xy 157.624944 50.039194)))
  )
  (gr_line (start 158.75 59.69) (end 138.43 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 106.68) (end 158.75 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 106.68) (end 158.75 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 59.69) (end 138.43 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
)
