(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "MounT_K85_Teensy")
    (date "2022-10-25")
    (rev "005")
    (company "Brian K. White - b.kenyon.w@gmail.com")
    (comment 1 "CC-BY-SA")
    (comment 2 "github.com/bkw777/MounT")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (grid_origin 147.32 96.52)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_${TITLE}_${REVISION}")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 "+3V3")
  (net 9 "/DTR_TTL")
  (net 10 "/DSR_TTL")
  (net 11 "/TX_TTL")
  (net 12 "/RX_TTL")
  (net 13 "/DTR_232")
  (net 14 "unconnected-(J1-Pad17)")
  (net 15 "unconnected-(J1-Pad18)")
  (net 16 "/CTS_232")
  (net 17 "/RTS_232")
  (net 18 "/RX_232")
  (net 19 "/TX_232")
  (net 20 "unconnected-(J1-Pad19)")
  (net 21 "unconnected-(J1-Pad20)")
  (net 22 "unconnected-(J1-Pad16)")
  (net 23 "unconnected-(J1-Pad14)")
  (net 24 "unconnected-(J1-Pad21)")
  (net 25 "unconnected-(J1-Pad22)")
  (net 26 "unconnected-(J1-Pad23)")
  (net 27 "unconnected-(J1-Pad24)")
  (net 28 "unconnected-(J1-Pad30)")
  (net 29 "unconnected-(J1-Pad31)")
  (net 30 "unconnected-(J1-Pad32)")
  (net 31 "unconnected-(J1-Pad33)")
  (net 32 "unconnected-(J1-Pad35)")
  (net 33 "unconnected-(J1-Pad36)")
  (net 34 "unconnected-(J1-Pad37)")
  (net 35 "unconnected-(J1-Pad13)")
  (net 36 "unconnected-(J1-Pad12)")
  (net 37 "unconnected-(J1-Pad11)")
  (net 38 "unconnected-(J1-Pad10)")
  (net 39 "unconnected-(J1-Pad9)")
  (net 40 "unconnected-(J1-Pad6)")
  (net 41 "unconnected-(J1-Pad5)")
  (net 42 "unconnected-(J1-Pad4)")
  (net 43 "unconnected-(J1-Pad38)")
  (net 44 "unconnected-(J1-Pad40)")
  (net 45 "unconnected-(J1-Pad41)")
  (net 46 "unconnected-(J1-Pad42)")
  (net 47 "unconnected-(J1-Pad43)")
  (net 48 "unconnected-(J1-Pad44)")
  (net 49 "unconnected-(J1-Pad45)")
  (net 50 "unconnected-(J1-Pad47)")
  (net 51 "unconnected-(J1-Pad48)")
  (net 52 "unconnected-(J2-Pad25)")
  (net 53 "unconnected-(J2-Pad24)")
  (net 54 "unconnected-(J2-Pad23)")
  (net 55 "/RI_232")
  (net 56 "unconnected-(J2-Pad21)")
  (net 57 "unconnected-(J2-Pad19)")
  (net 58 "unconnected-(J2-Pad18)")
  (net 59 "unconnected-(J2-Pad17)")
  (net 60 "unconnected-(J2-Pad16)")
  (net 61 "unconnected-(J2-Pad15)")
  (net 62 "unconnected-(J2-Pad14)")
  (net 63 "unconnected-(J2-Pad13)")
  (net 64 "unconnected-(J2-Pad12)")
  (net 65 "unconnected-(J2-Pad11)")
  (net 66 "unconnected-(J2-Pad10)")
  (net 67 "unconnected-(J2-Pad9)")
  (net 68 "/DSR_DCD_232")
  (net 69 "unconnected-(J1-Pad25)")
  (net 70 "unconnected-(J1-Pad26)")
  (net 71 "unconnected-(J1-Pad27)")
  (net 72 "unconnected-(J1-Pad28)")
  (net 73 "unconnected-(J1-Pad29)")
  (net 74 "unconnected-(J1-Pad39)")
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 175.7426 100.7364 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -0.0254 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 171.45 98.806 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -0.0254 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 171.45 100.7364)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -0.0254 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 176.3776 94.361 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -0.0254 0) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:C_0805" (layer "F.Cu")
    (tedit 5F4898F2)
    (at 175.7426 98.806 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -0.0254 -0.0254 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "0_LOCAL:Teensy_3.5_3.6_4.1_DIP_friction" (layer "F.Cu")
    (tedit 5F63C04C)
    (at 147.32 96.52 180)
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -10.16) (layer "F.SilkS") hide)
    (fp_text value "Teensy_3.5_3.6_4.1" (at 0 10.16) (layer "F.Fab"))
    (fp_text user "MK64FX512VMD12" (at 1.27 1.143) (layer "F.SilkS") hide)
    (fp_text user "MK66FX1MBVMD18/" (at 1.27 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole roundrect (at -29.21 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -26.67 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 "/RX_TTL") (pinfunction "0_RX1_MOSI1_Touch") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -24.13 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 "/TX_TTL") (pinfunction "1_TX1_MISO1_Touch") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -21.59 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 42 "unconnected-(J1-Pad4)") (pinfunction "2_PWM") (pintype "bidirectional+no_connect"))
    (pad "5" thru_hole circle (at -19.05 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 41 "unconnected-(J1-Pad5)") (pinfunction "3_PWM_CAN0TX_SCL2") (pintype "bidirectional+no_connect"))
    (pad "6" thru_hole circle (at -16.51 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 40 "unconnected-(J1-Pad6)") (pinfunction "4_PWM_CAN0RX_SDA2") (pintype "bidirectional+no_connect"))
    (pad "7" thru_hole circle (at -13.97 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 "/DTR_TTL") (pinfunction "5_PWM_TX1_MISO1") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at -11.43 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 "/DSR_TTL") (pinfunction "6_PWM") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at -8.89 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 39 "unconnected-(J1-Pad9)") (pinfunction "7_RX3_MOSI0_SCL0") (pintype "bidirectional+no_connect"))
    (pad "10" thru_hole circle (at -6.35 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J1-Pad10)") (pinfunction "8_TX3_MISO0_SDA0") (pintype "bidirectional+no_connect"))
    (pad "11" thru_hole circle (at -3.81 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 37 "unconnected-(J1-Pad11)") (pinfunction "9_PWM_RX2_CS0") (pintype "bidirectional+no_connect"))
    (pad "12" thru_hole circle (at -1.27 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J1-Pad12)") (pinfunction "10_PWM_TX2_CS0") (pintype "bidirectional+no_connect"))
    (pad "13" thru_hole circle (at 1.2446 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 35 "unconnected-(J1-Pad13)") (pinfunction "11_MOSI0") (pintype "bidirectional+no_connect"))
    (pad "14" thru_hole circle (at 3.81 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad14)") (pinfunction "12_MISO0") (pintype "bidirectional+no_connect"))
    (pad "15" thru_hole circle (at 6.35 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 "+3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "16" thru_hole circle (at 8.89 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J1-Pad16)") (pinfunction "24") (pintype "bidirectional+no_connect"))
    (pad "17" thru_hole circle (at 11.43 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J1-Pad17)") (pinfunction "25") (pintype "bidirectional+no_connect"))
    (pad "18" thru_hole circle (at 13.97 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J1-Pad18)") (pinfunction "26_TX1_SCL2") (pintype "bidirectional+no_connect"))
    (pad "19" thru_hole circle (at 16.51 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J1-Pad19)") (pinfunction "27_RX1_SCK0") (pintype "bidirectional+no_connect"))
    (pad "20" thru_hole circle (at 19.05 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J1-Pad20)") (pinfunction "28_MOSI0") (pintype "bidirectional+no_connect"))
    (pad "21" thru_hole circle (at 21.59 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J1-Pad21)") (pinfunction "29_PWM_CAN0TX_Touch") (pintype "bidirectional+no_connect"))
    (pad "22" thru_hole circle (at 24.13 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J1-Pad22)") (pinfunction "30_PWM_CAN0RX_Touch") (pintype "bidirectional+no_connect"))
    (pad "23" thru_hole circle (at 26.67 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J1-Pad23)") (pinfunction "31_A12_RX4_CS1") (pintype "bidirectional+no_connect"))
    (pad "24" thru_hole circle (at 29.21 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 27 "unconnected-(J1-Pad24)") (pinfunction "32_A13_TX4_SCK1") (pintype "bidirectional+no_connect"))
    (pad "25" thru_hole circle (at 29.21 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 69 "unconnected-(J1-Pad25)") (pinfunction "33_A14_TX5_CAN1TX_SCL0") (pintype "bidirectional+no_connect"))
    (pad "26" thru_hole circle (at 26.67 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 70 "unconnected-(J1-Pad26)") (pinfunction "34_A15_RX5_CAN1RX_SDA0") (pintype "bidirectional+no_connect"))
    (pad "27" thru_hole circle (at 24.13 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 71 "unconnected-(J1-Pad27)") (pinfunction "35_A16_PWM") (pintype "bidirectional+no_connect"))
    (pad "28" thru_hole circle (at 21.59 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 72 "unconnected-(J1-Pad28)") (pinfunction "36_A17_PWM") (pintype "bidirectional+no_connect"))
    (pad "29" thru_hole circle (at 19.05 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 73 "unconnected-(J1-Pad29)") (pinfunction "37_A18_PWM_SCL1") (pintype "bidirectional+no_connect"))
    (pad "30" thru_hole circle (at 16.51 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J1-Pad30)") (pinfunction "38_A19_PWM_SDA1") (pintype "bidirectional+no_connect"))
    (pad "31" thru_hole circle (at 13.97 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J1-Pad31)") (pinfunction "39_A20") (pintype "bidirectional+no_connect"))
    (pad "32" thru_hole circle (at 11.43 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 30 "unconnected-(J1-Pad32)") (pinfunction "A21_DAC0") (pintype "bidirectional+no_connect"))
    (pad "33" thru_hole circle (at 8.89 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 31 "unconnected-(J1-Pad33)") (pinfunction "A22_DAC1") (pintype "bidirectional+no_connect"))
    (pad "34" thru_hole circle (at 6.35 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole circle (at 3.81 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 32 "unconnected-(J1-Pad35)") (pinfunction "13_SCK0_LED") (pintype "bidirectional+no_connect"))
    (pad "36" thru_hole circle (at 1.27 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 33 "unconnected-(J1-Pad36)") (pinfunction "14_A0_PWM_SCK0") (pintype "bidirectional+no_connect"))
    (pad "37" thru_hole circle (at -1.27 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J1-Pad37)") (pinfunction "15_A1_CS0_Touch") (pintype "bidirectional+no_connect"))
    (pad "38" thru_hole circle (at -3.81 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J1-Pad38)") (pinfunction "16_A2_SCL0_Touch") (pintype "bidirectional+no_connect"))
    (pad "39" thru_hole circle (at -6.35 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 74 "unconnected-(J1-Pad39)") (pinfunction "17_A3_SDA0_Touch") (pintype "bidirectional+no_connect"))
    (pad "40" thru_hole circle (at -8.89 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 44 "unconnected-(J1-Pad40)") (pinfunction "18_A4_SDA0_Touch") (pintype "bidirectional+no_connect"))
    (pad "41" thru_hole circle (at -11.43 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J1-Pad41)") (pinfunction "19_A5_SCL0_Touch") (pintype "bidirectional+no_connect"))
    (pad "42" thru_hole circle (at -13.97 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 46 "unconnected-(J1-Pad42)") (pinfunction "20_A6_PWM_CS0_SCK1") (pintype "bidirectional+no_connect"))
    (pad "43" thru_hole circle (at -16.51 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J1-Pad43)") (pinfunction "21_A7_PWM_CS0_MOSI1") (pintype "bidirectional+no_connect"))
    (pad "44" thru_hole circle (at -19.05 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J1-Pad44)") (pinfunction "22_A8_PWM_Touch") (pintype "bidirectional+no_connect"))
    (pad "45" thru_hole circle (at -21.59 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 49 "unconnected-(J1-Pad45)") (pinfunction "23_A9_PWM_Touch") (pintype "bidirectional+no_connect"))
    (pad "46" thru_hole circle (at -24.13 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 "+3V3") (pinfunction "3V3") (pintype "power_out"))
    (pad "47" thru_hole circle (at -26.67 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 50 "unconnected-(J1-Pad47)") (pinfunction "AGND") (pintype "power_out+no_connect"))
    (pad "48" thru_hole circle (at -29.21 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 51 "unconnected-(J1-Pad48)") (pinfunction "Vin") (pintype "power_in+no_connect"))
  )
  (footprint "0_LOCAL:SOIC-16_W3.90mm" (layer "B.Cu")
    (tedit 6157DC02)
    (at 172.212 98.044 180)
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 0.762) (layer "B.SilkS") hide)
    (fp_text value "MAX3232" (at 0 0) (layer "B.SilkS"))
    (fp_text user "REF**" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -4.445 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)") (pinfunction "C1+") (pintype "passive"))
    (pad "2" smd roundrect locked (at -3.175 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)") (pinfunction "VS+") (pintype "power_out"))
    (pad "3" smd roundrect locked (at -1.905 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C1-Pad2)") (pinfunction "C1-") (pintype "passive"))
    (pad "4" smd roundrect locked (at -0.635 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)") (pinfunction "C2+") (pintype "passive"))
    (pad "5" smd roundrect locked (at 0.635 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C2-Pad2)") (pinfunction "C2-") (pintype "passive"))
    (pad "6" smd roundrect locked (at 1.905 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C5-Pad1)") (pinfunction "VS-") (pintype "power_out"))
    (pad "7" smd roundrect locked (at 3.175 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 68 "/DSR_DCD_232") (pinfunction "T2OUT") (pintype "output"))
    (pad "8" smd roundrect locked (at 4.445 -2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/DTR_232") (pinfunction "R2IN") (pintype "input"))
    (pad "9" smd roundrect locked (at 4.445 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/DSR_TTL") (pinfunction "R2OUT") (pintype "output"))
    (pad "10" smd roundrect locked (at 3.175 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/DTR_TTL") (pinfunction "T2IN") (pintype "input"))
    (pad "11" smd roundrect locked (at 1.905 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "/TX_TTL") (pinfunction "T1IN") (pintype "input"))
    (pad "12" smd roundrect locked (at 0.635 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "/RX_TTL") (pinfunction "R1OUT") (pintype "output"))
    (pad "13" smd roundrect locked (at -0.635 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/TX_232") (pinfunction "R1IN") (pintype "input"))
    (pad "14" smd roundrect locked (at -1.905 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "/RX_232") (pinfunction "T1OUT") (pintype "output"))
    (pad "15" smd roundrect locked (at -3.175 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "16" smd roundrect locked (at -4.445 2.7 180) (size 0.6 1.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "0_LOCAL:PinHeader_1x02_P2.54mm_Horizontal" (layer "B.Cu")
    (tedit 6157B0B5)
    (at 121.92 101.6 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at 4.385 2.27 90) (layer "B.SilkS") hide)
    (fp_text value "Jumper_2_Bridged" (at 4.385 -4.81 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -1.27 180) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 17 "/RTS_232") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -2.54 90) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 "/CTS_232") (pinfunction "B") (pintype "passive"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/Jumper.stp"
      (offset (xyz 4.1 -3.77 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 90))
    )
  )
  (footprint "0_LOCAL:DSUB-25_Male_Vertical_P2.77x2.84mm" (layer "B.Cu")
    (tedit 5F4932F5)
    (at 163.94 95.0976 180)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (property "Sheetfile" "File: MounT_K85_Teensy.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.4605 -1.2827 180) (layer "B.SilkS") hide)
    (fp_text value "DB25_Male" (at 16.62 -8.73 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 16.62 -1.42 180) (layer "B.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.77 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 19 "/TX_232") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.54 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 18 "/RX_232") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 8.31 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 17 "/RTS_232") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 11.08 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 16 "/CTS_232") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 13.85 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 68 "/DSR_DCD_232") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 16.62 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 19.39 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 68 "/DSR_DCD_232") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 22.16 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 67 "unconnected-(J2-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" thru_hole circle locked (at 24.93 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 66 "unconnected-(J2-Pad10)") (pinfunction "10") (pintype "passive+no_connect"))
    (pad "11" thru_hole circle locked (at 27.7 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 65 "unconnected-(J2-Pad11)") (pinfunction "11") (pintype "passive+no_connect"))
    (pad "12" thru_hole circle locked (at 30.47 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 64 "unconnected-(J2-Pad12)") (pinfunction "12") (pintype "passive+no_connect"))
    (pad "13" thru_hole circle locked (at 33.24 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 63 "unconnected-(J2-Pad13)") (pinfunction "13") (pintype "passive+no_connect"))
    (pad "14" thru_hole circle locked (at 1.385 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 62 "unconnected-(J2-Pad14)") (pinfunction "P14") (pintype "passive+no_connect"))
    (pad "15" thru_hole circle locked (at 4.155 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 61 "unconnected-(J2-Pad15)") (pinfunction "P15") (pintype "passive+no_connect"))
    (pad "16" thru_hole circle locked (at 6.925 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 60 "unconnected-(J2-Pad16)") (pinfunction "P16") (pintype "passive+no_connect"))
    (pad "17" thru_hole circle locked (at 9.695 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 59 "unconnected-(J2-Pad17)") (pinfunction "P17") (pintype "passive+no_connect"))
    (pad "18" thru_hole circle locked (at 12.465 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 58 "unconnected-(J2-Pad18)") (pinfunction "P18") (pintype "passive+no_connect"))
    (pad "19" thru_hole circle locked (at 15.235 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 57 "unconnected-(J2-Pad19)") (pinfunction "P19") (pintype "passive+no_connect"))
    (pad "20" thru_hole circle locked (at 18.005 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 13 "/DTR_232") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle locked (at 20.775 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 56 "unconnected-(J2-Pad21)") (pinfunction "P21") (pintype "passive+no_connect"))
    (pad "22" thru_hole circle locked (at 23.545 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 55 "/RI_232") (pinfunction "P22") (pintype "passive+no_connect"))
    (pad "23" thru_hole circle locked (at 26.315 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 54 "unconnected-(J2-Pad23)") (pinfunction "P23") (pintype "passive+no_connect"))
    (pad "24" thru_hole circle locked (at 29.085 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 53 "unconnected-(J2-Pad24)") (pinfunction "P24") (pintype "passive+no_connect"))
    (pad "25" thru_hole circle locked (at 31.855 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 52 "unconnected-(J2-Pad25)") (pinfunction "P25") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/0_LOCAL.3dshapes/A_DS_25_PP_Z_cut.step"
      (offset (xyz 16.625 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 177.9016 105.5116) (end 177.9016 87.5284) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 116.7384 105.5116) (end 177.9016 105.5116) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 177.9016 87.5284) (end 116.7384 87.5284) (layer "Edge.Cuts") (width 0.0254))
  (gr_line (start 116.7384 87.5284) (end 116.7384 105.5116) (layer "Edge.Cuts") (width 0.0254))
  (gr_text "Teensy MounT" (at 147.32 90.932) (layer "B.SilkS"))
  (gr_text "CTS" (at 119.38 90.5764) (layer "B.SilkS"))
  (gr_text "DB25M this side" (at 147.32 93.345) (layer "B.SilkS"))
  (gr_text "${COMMENT2} ${TITLE} ${REVISION}" (at 147.32 102.235) (layer "B.SilkS"))
  (gr_text "RTS" (at 121.92 90.5764) (layer "B.SilkS"))
  (gr_text "USB" (at 174.1932 95.885 -90) (layer "F.SilkS"))
  (gr_text "3V3" (at 171.45 102.235) (layer "F.SilkS"))
  (gr_text "DCD" (at 144.5006 95.9358 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 163.9062 95.9358 -90) (layer "F.SilkS"))
  (gr_text "SD CARD" (at 124.46 96.52) (layer "F.SilkS"))
  (gr_text "TX_TTL" (at 171.45 90.17 270) (layer "F.SilkS"))
  (gr_text "CTS" (at 152.8318 95.9358 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 176.53 90.17 -90) (layer "F.SilkS"))
  (gr_text "RX_TTL" (at 173.99 90.17 270) (layer "F.SilkS"))
  (gr_text "GND" (at 140.97 102.743 -90) (layer "F.SilkS"))
  (gr_text "RTS" (at 155.575 95.9358 -90) (layer "F.SilkS"))
  (gr_text "DSR" (at 150.0378 95.9358 -90) (layer "F.SilkS"))
  (gr_text "TX" (at 161.1122 95.9358 -90) (layer "F.SilkS"))
  (gr_text "RI" (at 140.335 97.1042 -90) (layer "F.SilkS"))
  (gr_text "Teensy this side" (at 160.655 100.965) (layer "F.SilkS"))
  (gr_text "DSR_TTL" (at 158.75 90.17 270) (layer "F.SilkS"))
  (gr_text "GND" (at 147.2692 95.9358 -90) (layer "F.SilkS"))
  (gr_text "DTR" (at 145.8976 97.1042 -90) (layer "F.SilkS"))
  (gr_text "RX" (at 158.3436 95.9358 -90) (layer "F.SilkS"))
  (gr_text "DTR_TTL" (at 161.29 90.17 270) (layer "F.SilkS"))
  (gr_text "3V3" (at 140.97 90.424 -90) (layer "F.SilkS"))
  (gr_text "C1-C5\n${00000000-0000-0000-0000-00005f3a1bdb:VALUE}" (at 170.18 96.52) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 177.9016 105.5116)
        (xy 116.7384 105.5116)
        (xy 116.7384 87.5284)
        (xy 177.9016 87.5284)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 177.9016 105.5116)
        (xy 116.7384 105.5116)
        (xy 116.7384 87.5284)
        (xy 177.9016 87.5284)
      )
    )
  )
)
