(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 26)
    (zones 0)
    (modules 4)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 171.486 106.418)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "PMT_FT_PCBoard:Harwin H2175" (layer F.Cu) (tedit 6180367D)
    (at 171.486 113.648)
    (fp_text reference SIG (at 0 2) (layer F.SilkS))
    (fp_text value "Harwin H2175" (at 0 -1.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module "PMT_FT_PCBoard:Harwin H2175" (layer F.Cu) (tedit 61803A28)
    (at 175.486 97.518)
    (fp_text reference GND (at 3.112 0.01) (layer F.SilkS))
    (fp_text value "Harwin H2175" (at 0 -1.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module "PMT_FT_PCBoard:Harwin H2175" (layer F.Cu) (tedit 6180367D)
    (at 168.486 97.518)
    (fp_text reference HV (at -2.588 0.01) (layer F.SilkS))
    (fp_text value "Harwin H2175" (at 0 -1.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  )
  (module PMT_FT_PCBoard:8pin_Cermatec_FT (layer F.Cu) (tedit 6180354C)
    (at 171.486 106.418)
    (fp_text reference "CeramTec 9294-01-W" (at 0 3.302) (layer F.SilkS))
    (fp_text value 8pin_Cermatec_FT (at 0.4 7.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -5.969) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 4.674 -3.734) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.817 1.321) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.591 5.385) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -2.591 5.385) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -5.817 1.321) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -4.674 -3.734) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  )
  (gr_text "Pin HARWiN H2175-05\nPinSkt MillMax 0300-1-15" (at 159.548 117.086) (layer F.SilkS))
  (gr_line (start 184.186 93.718) (end 184.186 119.118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.786 119.118) (end 184.186 119.118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.786 93.718) (end 158.786 119.118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.786 93.718) (end 184.186 93.718) (layer Edge.Cuts) (width 0.05))
)
