(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 138)
    (no_connects 0)
    (area 86.309999 83.769999 167.690001 127.050001)
    (thickness 1.6)
    (drawings 14)
    (tracks 402)
    (zones 0)
    (modules 46)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFE7B3F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(C3-Pad1)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(R7-Pad1)")
  (net 9 "Net-(R8-Pad1)")
  (net 10 "Net-(R9-Pad2)")
  (net 11 "Net-(R10-Pad2)")
  (net 12 "Net-(R11-Pad2)")
  (net 13 "Net-(R12-Pad2)")
  (net 14 /SCL0)
  (net 15 /SDA0)
  (net 16 /SDA1)
  (net 17 /SCL1)
  (net 18 "Net-(R13-Pad1)")
  (net 19 "Net-(R14-Pad1)")
  (net 20 "Net-(R15-Pad1)")
  (net 21 "Net-(R16-Pad2)")
  (net 22 3V3)
  (net 23 "Net-(R18-Pad2)")
  (net 24 "Net-(R19-Pad1)")
  (net 25 "Net-(R20-Pad1)")
  (net 26 "Net-(C9-Pad1)")
  (net 27 "Net-(C10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net +5V)
    (add_net /SCL0)
    (add_net /SCL1)
    (add_net /SDA0)
    (add_net /SDA1)
    (add_net 3V3)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad2)")
  )
  (module opt3001:SON65P200X240X70-6N (layer B.Cu) (tedit 5BC0BE0C)
    (at 140.5 111.35)
    (attr smd)
    (fp_text reference U4 (at -0.281659 1.81031) (layer B.SilkS))
    (fp_text value OPT3001 (at 0.024053 -2.05958) (layer Cmts.User) hide)
    (pad 1 smd rect (at -1 0.65) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -1 0) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1 -0.65) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1 0.65) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 21 "Net-(R16-Pad2)"))
    (pad 4 smd rect (at 1 -0.65) (size 0.5 0.4) (layers B.Cu B.Mask)
      (net 17 /SCL1))
    (pad 5 smd rect (at 1 0) (size 0.5 0.4) (layers B.Cu B.Mask))
    (pad 3 smd rect (at 0 0) (size 0.64 1.35) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module 54602-908LF:AMPHENOL_54602-908LF (layer F.Cu) (tedit 5C953B65)
    (at 109.22 105.41 270)
    (fp_text reference J1 (at -8.91 -8.83 270) (layer F.SilkS))
    (fp_text value 54602-908LF (at -4.34797 8.79026 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -4.445 -6.35 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at -3.175 -8.89 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -1.905 -6.35 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -0.635 -8.89 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 0.635 -6.35 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 1.905 -8.89 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 3.175 -6.35 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 8 thru_hole circle (at 4.445 -8.89 90) (size 1.268 1.268) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad Hole np_thru_hole circle (at -5.715 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 5.715 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module PI4MSD5V9540BUEX:SOP65P490X110-8N (layer F.Cu) (tedit 5C9553B6)
    (at 126.6 105.95)
    (attr smd)
    (fp_text reference U1 (at -0.4 -2.55) (layer F.SilkS))
    (fp_text value PI4MSD5V9540BUEX (at -1.46772 5.99918) (layer Cmts.User) hide)
    (pad 2 smd rect (at -2.11 -0.325) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 7 smd rect (at 2.11 -0.325) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 16 /SDA1))
    (pad 1 smd rect (at -2.11 -0.975) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 3 smd rect (at -2.11 0.325) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -2.11 0.975) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 15 /SDA0))
    (pad 8 smd rect (at 2.11 -0.975) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 17 /SCL1))
    (pad 6 smd rect (at 2.11 0.325) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.11 0.975) (size 1.25 0.46) (layers F.Cu F.Mask)
      (net 14 /SCL0))
  )
  (module opt3001:SON65P200X240X70-6N (layer F.Cu) (tedit 5BC0BE0C)
    (at 141.05 106)
    (attr smd)
    (fp_text reference U2 (at -0.281659 -1.81031) (layer F.SilkS))
    (fp_text value OPT3001 (at 0.024053 2.05958) (layer Cmts.User) hide)
    (pad 1 smd rect (at -1 -0.65) (size 0.5 0.4) (layers F.Cu F.Mask)
      (net 22 3V3))
    (pad 2 smd rect (at -1 0) (size 0.5 0.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1 0.65) (size 0.5 0.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1 -0.65) (size 0.5 0.4) (layers F.Cu F.Mask)
      (net 19 "Net-(R14-Pad1)"))
    (pad 4 smd rect (at 1 0.65) (size 0.5 0.4) (layers F.Cu F.Mask)
      (net 14 /SCL0))
    (pad 5 smd rect (at 1 0) (size 0.5 0.4) (layers F.Cu F.Mask))
    (pad 3 smd rect (at 0 0) (size 0.64 1.35) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C95583F)
    (at 147.8 98.65 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.35 0.05 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C990B9E)
    (at 149.4 119.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.65 -0.1 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C95583A)
    (at 145.9 98.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at -2.35 -0.05 270) (layer F.SilkS))
    (fp_text value 600 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 22 3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 147.2 118.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at 0 1.45) (layer B.SilkS))
    (fp_text value 600 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C955831)
    (at 149.7 98.7 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.3 0.15 90) (layer F.SilkS))
    (fp_text value 3.3M (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 8 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C990B97)
    (at 151.2 119.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.7 -0.2 270) (layer B.SilkS))
    (fp_text value 3.3M (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 9 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 156.4 101.35 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 680 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 10 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C9BF90D)
    (at 150.45 100.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -0.1 1.65 270) (layer B.SilkS))
    (fp_text value 680 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 27 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 11 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C9BF906)
    (at 152.15 100.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0.15 -1.75 270) (layer B.SilkS))
    (fp_text value 680 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 27 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 12 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 159 101.35 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 680 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 13 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_4x4mm_Pitch0.65mm (layer B.Cu) (tedit 5C990699)
    (at 148.95 112.7)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.65")
    (attr smd)
    (fp_text reference U7 (at 0 3.55) (layer B.SilkS))
    (fp_text value AS73211 (at 0 -3.4) (layer B.Fab))
    (pad 1 smd rect (at -2 0.975) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2 0.325) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2 -0.325) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2 -0.975) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 17 /SCL1))
    (pad 5 smd rect (at -0.975 -2 270) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 16 /SDA1))
    (pad 6 smd rect (at -0.325 -2 270) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.325 -2 270) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (pad 8 smd rect (at 0.975 -2 270) (size 0.8 0.35) (layers B.Cu B.Mask))
    (pad 9 smd rect (at 2 -0.975) (size 0.8 0.35) (layers B.Cu B.Mask))
    (pad 10 smd rect (at 2 -0.325) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2 0.325) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2 0.975) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 0.975 2 270) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 9 "Net-(R8-Pad1)"))
    (pad 14 smd rect (at 0.325 2 270) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 15 smd rect (at -0.325 2 270) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.975 2 270) (size 0.8 0.35) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers B.Cu B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers B.Cu B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers B.Cu B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers B.Cu B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:VSSOP-8_2.4x2.1mm_Pitch0.5mm (layer F.Cu) (tedit 58934277)
    (at 151.55 110.8)
    (descr http://www.ti.com/lit/ml/mpds050d/mpds050d.pdf)
    (tags "VSSOP DCU R-PDSO-G8 Pitch0.5mm")
    (attr smd)
    (fp_text reference U8 (at 0 -2.54) (layer F.SilkS))
    (fp_text value PCA9306 (at 0 2.413) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.75) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.55 -0.25) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -1.55 0.25) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 14 /SCL0))
    (pad 4 smd rect (at -1.55 0.75) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 15 /SDA0))
    (pad 5 smd rect (at 1.55 0.75) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 13 "Net-(R12-Pad2)"))
    (pad 6 smd rect (at 1.55 0.25) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 10 "Net-(R9-Pad2)"))
    (pad 7 smd rect (at 1.55 -0.25) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 23 "Net-(R18-Pad2)"))
    (pad 8 smd rect (at 1.55 -0.75) (size 0.75 0.25) (layers F.Cu F.Mask)
      (net 23 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/VSSOP-8_2.4x2.1mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:VSSOP-8_2.4x2.1mm_Pitch0.5mm (layer B.Cu) (tedit 5C990650)
    (at 149.75 105.25)
    (descr http://www.ti.com/lit/ml/mpds050d/mpds050d.pdf)
    (tags "VSSOP DCU R-PDSO-G8 Pitch0.5mm")
    (attr smd)
    (fp_text reference U9 (at 0 2.25) (layer B.SilkS))
    (fp_text value PCA9306 (at 0 -2.413) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.55 0.75) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 24 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at -1.55 0.25) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -1.55 -0.25) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 20 "Net-(R15-Pad1)"))
    (pad 4 smd rect (at -1.55 -0.75) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 16 /SDA1))
    (pad 5 smd rect (at 1.55 -0.75) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 12 "Net-(R11-Pad2)"))
    (pad 6 smd rect (at 1.55 -0.25) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 11 "Net-(R10-Pad2)"))
    (pad 7 smd rect (at 1.55 0.25) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 27 "Net-(C10-Pad1)"))
    (pad 8 smd rect (at 1.55 0.75) (size 0.75 0.25) (layers B.Cu B.Mask)
      (net 27 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/VSSOP-8_2.4x2.1mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module opt3001:TCS34007 (layer F.Cu) (tedit 5C92B40A)
    (at 156.4 105.05)
    (attr smd)
    (fp_text reference U10 (at -0.281659 -1.81031) (layer F.SilkS))
    (fp_text value TCS34007 (at 0.024053 2.05958) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.8 -0.96) (size 1 0.3) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -0.8 -0.32) (size 1 0.3) (layers F.Cu F.Mask)
      (net 10 "Net-(R9-Pad2)"))
    (pad 3 smd rect (at -0.8 0.32) (size 1 0.3) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.8 0.32) (size 1 0.3) (layers F.Cu F.Mask)
      (net 13 "Net-(R12-Pad2)"))
    (pad 4 smd rect (at -0.8 0.96) (size 1 0.3) (layers F.Cu F.Mask))
    (pad 5 smd rect (at 0.8 0.96) (size 1 0.3) (layers F.Cu F.Mask))
    (pad 7 smd rect (at 0.8 -0.32) (size 1 0.3) (layers F.Cu F.Mask))
    (pad 8 smd rect (at 0.8 -0.96) (size 1 0.3) (layers F.Cu F.Mask))
  )
  (module opt3001:TCS34007 (layer B.Cu) (tedit 5C92B40A)
    (at 156.45 111.65)
    (attr smd)
    (fp_text reference U11 (at -0.281659 1.81031) (layer B.SilkS))
    (fp_text value TCS34007 (at 0.024053 -2.05958) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.8 0.96) (size 1 0.3) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -0.8 0.32) (size 1 0.3) (layers B.Cu B.Mask)
      (net 11 "Net-(R10-Pad2)"))
    (pad 3 smd rect (at -0.8 -0.32) (size 1 0.3) (layers B.Cu B.Mask)
      (net 25 "Net-(R20-Pad1)"))
    (pad 6 smd rect (at 0.8 -0.32) (size 1 0.3) (layers B.Cu B.Mask)
      (net 12 "Net-(R11-Pad2)"))
    (pad 4 smd rect (at -0.8 -0.96) (size 1 0.3) (layers B.Cu B.Mask))
    (pad 5 smd rect (at 0.8 -0.96) (size 1 0.3) (layers B.Cu B.Mask))
    (pad 7 smd rect (at 0.8 0.32) (size 1 0.3) (layers B.Cu B.Mask))
    (pad 8 smd rect (at 0.8 0.96) (size 1 0.3) (layers B.Cu B.Mask))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C9930FB)
    (at 122.75 110.35 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.5 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C954A5F)
    (at 151.6 115.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.4 0.15 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 14 /SCL0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C954A64)
    (at 150 115.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.45 0.1 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 15 /SDA0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C9BF7A1)
    (at 142.7 114.7 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.35 -0.15 270) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 21 "Net-(R16-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C9BF7A9)
    (at 144.4 114.7 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.35 -0.2 270) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 17 /SCL1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5C955394)
    (at 126.6 111.5 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -0.8 -3.45 540) (layer F.SilkS))
    (fp_text value 24LC08 (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 14 /SCL0))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 15 /SDA0))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5C95569E)
    (at 129.7 100.7 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at -0.2 3.05 180) (layer F.SilkS))
    (fp_text value 24LC08 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 17 /SCL1))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 16 /SDA1))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 22 3V3))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C993129)
    (at 121.05 110.35 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.5 -0.05 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C953B56)
    (at 124.5 100.9 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.3 -0.1 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C953B5A)
    (at 126.25 100.9 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.35 0 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_4x4mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 148.7 104.9)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.65")
    (attr smd)
    (fp_text reference U6 (at 0 -3.4) (layer F.SilkS))
    (fp_text value AS73211 (at 0 3.4) (layer F.Fab))
    (pad 1 smd rect (at -2 -0.975) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2 -0.325) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2 0.325) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2 0.975) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 14 /SCL0))
    (pad 5 smd rect (at -0.975 2 90) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 18 "Net-(R13-Pad1)"))
    (pad 6 smd rect (at -0.325 2 90) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.325 2 90) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 8 smd rect (at 0.975 2 90) (size 0.8 0.35) (layers F.Cu F.Mask))
    (pad 9 smd rect (at 2 0.975) (size 0.8 0.35) (layers F.Cu F.Mask))
    (pad 10 smd rect (at 2 0.325) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2 -0.325) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 2 -0.975) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 0.975 -2 90) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 8 "Net-(R7-Pad1)"))
    (pad 14 smd rect (at 0.325 -2 90) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (pad 15 smd rect (at -0.325 -2 90) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.975 -2 90) (size 0.8 0.35) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.65 109.95 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 18 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 15 /SDA0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 144.05 108.7 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 19 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 15 /SDA0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 146.6 108 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 20 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 17 /SCL1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 143.4 108.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 16 /SDA1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 21 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C9929F7)
    (at 132.7 111 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -3 0.05 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 22 3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 155.55 96.35 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U12 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value MCP1700T-1802E/TT (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 5C9BF86B)
    (at 145.55 97.85 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U13 (at -3 0 360) (layer B.SilkS))
    (fp_text value MCP1700T-1802E/TT (at 0 -2.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 27 "Net-(C10-Pad1)"))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 156.55 109.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 23 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 149.35 107.8)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 1.45) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 24 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 154.2 109 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 25 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C9BF400)
    (at 148.1 113.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.25 -1.3 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C9BF510)
    (at 143.95 98.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.4 -0.1 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 22 3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C9BF795)
    (at 143.6 117.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C7 (at 2.65 -0.05 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C9BF870)
    (at 142 99.85 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C8 (at 2.65 0 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C9BF40A)
    (at 159.05 95.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 1.6 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 26 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C9BF901)
    (at 151.2 96.85)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C10 (at 0.15 -1.65) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 27 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 86.36 127) (end 86.36 126.746) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.64 127) (end 86.36 127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.64 83.82) (end 86.614 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.64 83.82) (end 167.64 127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.487 127) (end 89.154 127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.487 116.84) (end 86.487 127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.408 116.84) (end 86.487 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.487 93.98) (end 90.043 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.487 83.82) (end 86.487 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.9 83.82) (end 86.487 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "MALT Sensor Board v4\nCopyright© 2019 Microsoft Corporation" (at 118.872 88.519) (layer F.SilkS))
  (gr_line (start 104.14 93.98) (end 88.9 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.14 116.84) (end 104.14 93.98) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.9 116.84) (end 104.14 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.2 78.05) (xy 176.8 77.9) (xy 176.8 133.5) (xy 83.2 133.55) (xy 83.15 78.05)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.9 81.1) (xy 171 81.1) (xy 171.2 129.75) (xy 84.95 129.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.25 81.65) (xy 171.2 81.55) (xy 171.1 129.25) (xy 84.5 128.9) (xy 85.25 81.9)
      )
    )
  )
)
