(kicad_pcb (version 20171130) (host pcbnew 5.0.1-1.fc29)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 14)
    (zones 0)
    (modules 9)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(F1-Pad1)")
  (net 2 "Net-(F1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C0D8107)
    (at 172 82)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C0D8107)
    (at 172 104)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C0D8107)
    (at 114 104)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Fuse:Fuseholder_TR5_Littelfuse_No560_No460 (layer F.Cu) (tedit 5C0D920B)
    (at 128 102 180)
    (descr "Fuse, Fuseholder, TR5, Littelfuse/Wickmann, No. 460, No560,")
    (tags "Fuse Fuseholder TR5 Littelfuse/Wickmann No. 460 No560 ")
    (fp_text reference F1 (at -4 -2.5 180) (layer F.SilkS))
    (fp_text value 200mA/250V (at -8 -4 180) (layer F.SilkS))
    (fp_text user %R (at 2.75 -2.75 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0.01 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuseholder_TR5_Littelfuse_No560_No460.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_RND:TerminalBlock_RND_205-00012_1x02_P5.00mm_Horizontal (layer F.Cu) (tedit 5B294F52)
    (at 115 90 270)
    (descr "terminal block RND 205-00012, 2 pins, pitch 5mm, size 10x7.6mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00012_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00012 pitch 5mm size 10x7.6mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J1 (at -3.64 0) (layer F.SilkS))
    (fp_text value Mains (at -4 0) (layer F.Fab))
    (fp_text user %R (at 2.5 -5.16 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00012_1x02_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 171 94 90)
    (descr "JST XH series connector, B02B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J2 (at 6.116 0 180) (layer F.SilkS))
    (fp_text value Out (at 6 0) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Elevendroids_Converter_ACDC:Elevendroids_Converter_ACDC_HLK-PMxx (layer F.Cu) (tedit 5C0D7A76)
    (at 135 90)
    (descr http://www.hlktech.net/product_detail.php?ProId=54)
    (tags "ACDC-Converter 3W THT")
    (fp_text reference PS1 (at -0.032 -8.75) (layer F.SilkS))
    (fp_text value HLK-PM01 (at 14.7 13.75) (layer F.Fab))
    (fp_text user %R (at 14.954 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 0 5) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(F1-Pad1)"))
    (pad 3 thru_hole circle (at 29.4 -5.2) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 4 thru_hole circle (at 29.4 10.2) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
  )
  (module Varistor:RV_Disc_D7mm_W4.2mm_P5mm (layer F.Cu) (tedit 5C0D921F)
    (at 128 95 90)
    (descr "Varistor, diameter 7mm, width 4.2mm, pitch 5mm")
    (tags "varistor SIOV")
    (fp_text reference RV1 (at 7 1 180) (layer F.SilkS))
    (fp_text value 275VAC (at 2.5 -2.2 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5 1.8 90) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Varistor.3dshapes/RV_Disc_D7mm_W4.2mm_P5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C0D8107)
    (at 114 82)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "HLK-PMxx PSU\n(c) Michal Potrzebicz\n2018-12-09" (at 124.46 81.788) (layer F.SilkS))
  (gr_text AC (at 114.808 99.568) (layer F.SilkS))
  (gr_text DC+ (at 171.704 98.552) (layer F.SilkS))
  (gr_arc (start 172 104) (end 172 108) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172 82) (end 176 82) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 114 104) (end 110 104) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 114 82) (end 114 78) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172 78) (end 114 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176 104) (end 176 82) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 108) (end 172 108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110 82) (end 110 104) (layer Edge.Cuts) (width 0.15))
)
