(kicad_pcb (version 20170123) (host pcbnew "(2017-08-02 revision 9760937)-master")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 186)
    (zones 0)
    (modules 17)
    (nets 56)
  )
  (page A4)
  (title_block
    (title "GPS Mezzanine")
    (date 2017-09-04)
    (rev A)
    (company "QWERTY Embedded Design, LLC")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (trace_clearance 0)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100 100)
    (visible_elements FFFFFF7B)
    (pcbplotparams
      (layerselection 0x010ef_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 +1V8)
  (net 2 GND)
  (net 3 +5V)
  (net 4 I2C0_SCL)
  (net 5 I2C0_SDA)
  (net 6 I2C1_SCL)
  (net 7 I2C1_SDA)
  (net 8 PWR_BTN_N)
  (net 9 RST_BTN_N)
  (net 10 SYS_DCIN)
  (net 11 GPIO_B)
  (net 12 GPIO_A)
  (net 13 SPIO_SCL)
  (net 14 SPIO_DIN)
  (net 15 SPIO_CS)
  (net 16 SPIO_DOUT)
  (net 17 PCM_FS)
  (net 18 PCM_CLK)
  (net 19 PCM_DO)
  (net 20 PCM_DI)
  (net 21 GPIO_D)
  (net 22 GPIO_F)
  (net 23 GPIO_H)
  (net 24 GPIO_J)
  (net 25 GPIO_L)
  (net 26 UART1_TX)
  (net 27 UART1_RX)
  (net 28 GPIO_C)
  (net 29 GPIO_E)
  (net 30 GPIO_G)
  (net 31 GPIO_I)
  (net 32 GPIO_K)
  (net 33 UART0_CTS)
  (net 34 UART0_TX)
  (net 35 UART0_RX)
  (net 36 UART0_RTS)
  (net 37 GPS_TX)
  (net 38 GPS_RX)
  (net 39 +3V3)
  (net 40 "Net-(LD1-Pad2)")
  (net 41 FIX)
  (net 42 "Net-(U2-Pad2)")
  (net 43 "Net-(U2-Pad6)")
  (net 44 "Net-(U2-Pad7)")
  (net 45 "Net-(U2-Pad14)")
  (net 46 "Net-(U2-Pad15)")
  (net 47 "Net-(U2-Pad16)")
  (net 48 "Net-(U2-Pad17)")
  (net 49 "Net-(U2-Pad18)")
  (net 50 "Net-(U2-Pad20)")
  (net 51 +BATT)
  (net 52 "Net-(U3-Pad6)")
  (net 53 "Net-(U3-Pad9)")
  (net 54 GPS_1PPS)
  (net 55 "Net-(JK1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +BATT)
    (add_net FIX)
    (add_net GPIO_A)
    (add_net GPIO_B)
    (add_net GPIO_C)
    (add_net GPIO_D)
    (add_net GPIO_E)
    (add_net GPIO_F)
    (add_net GPIO_G)
    (add_net GPIO_H)
    (add_net GPIO_I)
    (add_net GPIO_J)
    (add_net GPIO_K)
    (add_net GPIO_L)
    (add_net GPS_1PPS)
    (add_net GPS_RX)
    (add_net GPS_TX)
    (add_net I2C0_SCL)
    (add_net I2C0_SDA)
    (add_net I2C1_SCL)
    (add_net I2C1_SDA)
    (add_net "Net-(JK1-Pad1)")
    (add_net "Net-(LD1-Pad2)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad9)")
    (add_net PCM_CLK)
    (add_net PCM_DI)
    (add_net PCM_DO)
    (add_net PCM_FS)
    (add_net PWR_BTN_N)
    (add_net RST_BTN_N)
    (add_net SPIO_CS)
    (add_net SPIO_DIN)
    (add_net SPIO_DOUT)
    (add_net SPIO_SCL)
    (add_net SYS_DCIN)
    (add_net UART0_CTS)
    (add_net UART0_RTS)
    (add_net UART0_RX)
    (add_net UART0_TX)
    (add_net UART1_RX)
    (add_net UART1_TX)
  )
  (net_class Power ""
    (clearance 0.1778)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +5V)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A21B256)
    (at 153.1 112.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0 -3.08) (layer F.SilkS))
    (fp_text value CONN_01X04 (at -0.7 -3.08) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +1V8))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 UART1_TX))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 UART1_RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 96boards:U.FL-R-SMT-1 (layer F.Cu) (tedit 5A1B9D46)
    (at 102.54 112.25 90)
    (fp_text reference JK1 (at 3 0.5) (layer F.SilkS))
    (fp_text value uFL (at 0.05 -2.15 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 1.525 90) (size 1 1.05) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(JK1-Pad1)"))
    (pad 2 smd rect (at -1.475 0 90) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.475 0 90) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5A1B9C9F)
    (at 104 104)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference MH1 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value M2.5 (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5A21B2BA)
    (at 104 135.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference MH2 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value M2.5 (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Housings_SSOP:SSOP-14_5.3x6.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 132.09 114.28 270)
    (descr "SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot337-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -5.28 -2.41) (layer F.SilkS))
    (fp_text value TXS0104E (at 0 4.2 270) (layer F.Fab))
    (pad 1 smd rect (at -3.45 -1.95 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +1V8))
    (pad 2 smd rect (at -3.45 -1.3 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 UART0_RX))
    (pad 3 smd rect (at -3.45 -0.65 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 UART0_TX))
    (pad 4 smd rect (at -3.45 0 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO_A))
    (pad 5 smd rect (at -3.45 0.65 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO_B))
    (pad 6 smd rect (at -3.45 1.3 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -3.45 1.95 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 3.45 1.95 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 GPIO_C))
    (pad 9 smd rect (at 3.45 1.3 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at 3.45 0.65 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 FIX))
    (pad 11 smd rect (at 3.45 0 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 GPS_1PPS))
    (pad 12 smd rect (at 3.45 -0.65 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 GPS_RX))
    (pad 13 smd rect (at 3.45 -1.3 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 GPS_TX))
    (pad 14 smd rect (at 3.45 -1.95 270) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
    (model Housings_SSOP.3dshapes/SSOP-14_5.3x6.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 137.22 117.73)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.35) (layer F.SilkS))
    (fp_text value .1uF (at 0 -1.42) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 137.21 110.83)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.04 1.52) (layer F.SilkS))
    (fp_text value .1uF (at -0.09 1.52) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +1V8))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 96boards:BAT-HLD-001 (layer F.Cu) (tedit 5A1B2522)
    (at 120.5 142.5)
    (fp_text reference BT1 (at -13.5 4.5) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0.1 -9.9) (layer F.Fab))
    (pad 2 smd circle (at 0 0) (size 17.8 17.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 11.45 0.05) (size 2.5 5.1) (layers F.Cu F.Paste F.Mask)
      (net 51 +BATT))
    (pad 1 smd rect (at -11.45 0) (size 2.5 5.1) (layers F.Cu F.Paste F.Mask)
      (net 51 +BATT))
  )
  (module 96boards:FGPMMOPA6H (layer F.Cu) (tedit 59ACB960)
    (at 115 119 180)
    (fp_text reference U2 (at 0 -8.89 180) (layer F.SilkS))
    (fp_text value FGPMMOPA6H (at 0 -6.985 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -8 -6.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
    (pad 2 smd rect (at -8 -5.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -8 -3.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -8 -2.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 51 +BATT))
    (pad 5 smd rect (at -8 -0.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 41 FIX))
    (pad 6 smd rect (at -8 0.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -8 2.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -8 3.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -8 5.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 37 GPS_TX))
    (pad 10 smd rect (at -8 6.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 38 GPS_RX))
    (pad 11 smd rect (at 8 6.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(JK1-Pad1)"))
    (pad 12 smd rect (at 8 5.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 8 3.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GPS_1PPS))
    (pad 14 smd rect (at 8 2.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 8 0.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U2-Pad15)"))
    (pad 16 smd rect (at 8 -0.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 8 -2.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 8 -3.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U2-Pad18)"))
    (pad 19 smd rect (at 8 -5.25 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 8 -6.75 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U2-Pad20)"))
    (pad "" np_thru_hole circle (at 0.2 -0.8 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59ACB90E)
    (at 128.067 126.48 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.489 0 270) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59ACB92C)
    (at 130.0353 129.1971 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.305005 0.051215 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59ACB912)
    (at 126.162 126.48 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.489 0 270) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 59ACB97B)
    (at 130.5877 122.257 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference LD1 (at -0.1523 1.257 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(LD1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59ACB977)
    (at 127.527 122.257 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.013 1.367 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(LD1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 FIX))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59ACB96D)
    (at 137.23 119.59 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.01 -1.48 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 GPIO_C))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 59ACC265)
    (at 130.790995 126.785215 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U1 (at -0.178215 -2.686005) (layer F.SilkS))
    (fp_text value MCP1700T-3302E/TT (at 0 2.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0.214785 -0.209005) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 39 +3V3))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 96boards:Pin_Header_SMD_2x20_Pitch2mm locked (layer B.Cu) (tedit 598D2D18)
    (at 110 105 270)
    (descr "Double row SMD 2mm pin header, 2x20 contacts")
    (attr smd)
    (fp_text reference P1 (at -1 2 270) (layer B.SilkS))
    (fp_text value CONN_02X20 (at -1 4 270) (layer B.Fab))
    (pad 39 smd rect (at 1.25 -38) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 1.25 -36) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (pad 35 smd rect (at 1.25 -34) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 1 +1V8))
    (pad 33 smd rect (at 1.25 -32) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 32 GPIO_K))
    (pad 31 smd rect (at 1.25 -30) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 31 GPIO_I))
    (pad 29 smd rect (at 1.25 -28) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 30 GPIO_G))
    (pad 27 smd rect (at 1.25 -26) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 29 GPIO_E))
    (pad 25 smd rect (at 1.25 -24) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 28 GPIO_C))
    (pad 23 smd rect (at 1.25 -22) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 12 GPIO_A))
    (pad 21 smd rect (at 1.25 -20) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 7 I2C1_SDA))
    (pad 19 smd rect (at 1.25 -18) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 6 I2C1_SCL))
    (pad 17 smd rect (at 1.25 -16) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 5 I2C0_SDA))
    (pad 15 smd rect (at 1.25 -14) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 4 I2C0_SCL))
    (pad 13 smd rect (at 1.25 -12) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 27 UART1_RX))
    (pad 11 smd rect (at 1.25 -10) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 26 UART1_TX))
    (pad 9 smd rect (at 1.25 -8) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 36 UART0_RTS))
    (pad 7 smd rect (at 1.25 -6) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 35 UART0_RX))
    (pad 5 smd rect (at 1.25 -4) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 34 UART0_TX))
    (pad 3 smd rect (at 1.25 -2) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 33 UART0_CTS))
    (pad 40 smd rect (at -3.25 -38) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 38 smd rect (at -3.25 -36) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 10 SYS_DCIN))
    (pad 36 smd rect (at -3.25 -34) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 10 SYS_DCIN))
    (pad 34 smd rect (at -3.25 -32) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 25 GPIO_L))
    (pad 32 smd rect (at -3.25 -30) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 24 GPIO_J))
    (pad 30 smd rect (at -3.25 -28) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 23 GPIO_H))
    (pad 28 smd rect (at -3.25 -26) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 22 GPIO_F))
    (pad 26 smd rect (at -3.25 -24) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 21 GPIO_D))
    (pad 24 smd rect (at -3.25 -22) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 11 GPIO_B))
    (pad 22 smd rect (at -3.25 -20) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 20 PCM_DI))
    (pad 20 smd rect (at -3.25 -18) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 19 PCM_DO))
    (pad 18 smd rect (at -3.25 -16) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 18 PCM_CLK))
    (pad 16 smd rect (at -3.25 -14) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 17 PCM_FS))
    (pad 14 smd rect (at -3.25 -12) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 16 SPIO_DOUT))
    (pad 12 smd rect (at -3.25 -10) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 15 SPIO_CS))
    (pad 10 smd rect (at -3.25 -8) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 14 SPIO_DIN))
    (pad 8 smd rect (at -3.25 -6) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 13 SPIO_SCL))
    (pad 6 smd rect (at -3.25 -4) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 9 RST_BTN_N))
    (pad 4 smd rect (at -3.25 -2) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 8 PWR_BTN_N))
    (pad "" np_thru_hole circle (at -1 -1) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 2 smd rect (at -3.25 0) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.25 0) (size 0.89 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -1 -37) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz -0.0394 -0.749 0.01576))
      (scale (xyz 0.787 0.787 0.5))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text UART1 (at 144.145 116.205 90) (layer F.SilkS))
  (gr_text GND (at 148.7 120.1) (layer F.SilkS))
  (gr_text RX (at 148.8 117.4) (layer F.SilkS))
  (gr_text TX (at 148.71 114.95) (layer F.SilkS))
  (gr_text 1.8V (at 148.3 112.3) (layer F.SilkS))
  (gr_text m_w (at 144 149) (layer F.SilkS))
  (gr_text "96BOARDS\nGPS MEZZANINE" (at 143.89 141.59) (layer F.SilkS))
  (dimension 31.5 (width 0.3) (layer F.Fab)
    (gr_text "31.500 mm" (at 96.15 119.75 90) (layer F.Fab))
    (feature1 (pts (xy 104 104) (xy 94.8 104)))
    (feature2 (pts (xy 104 135.5) (xy 94.8 135.5)))
    (crossbar (pts (xy 97.5 135.5) (xy 97.5 104)))
    (arrow1a (pts (xy 97.5 104) (xy 98.086421 105.126504)))
    (arrow1b (pts (xy 97.5 104) (xy 96.913579 105.126504)))
    (arrow2a (pts (xy 97.5 135.5) (xy 98.086421 134.373496)))
    (arrow2b (pts (xy 97.5 135.5) (xy 96.913579 134.373496)))
  )
  (gr_text "R0 - 2017" (at 144 147) (layer F.SilkS))
  (gr_text FIX (at 134.2 122.28) (layer F.SilkS))
  (dimension 4 (width 0.3) (layer F.Fab)
    (gr_text 4mm (at 95 107 90) (layer F.Fab))
    (feature1 (pts (xy 104 100) (xy 92.3 100)))
    (feature2 (pts (xy 104 104) (xy 92.3 104)))
    (crossbar (pts (xy 95 104) (xy 95 100)))
    (arrow1a (pts (xy 95 100) (xy 95.586421 101.126504)))
    (arrow1b (pts (xy 95 100) (xy 94.413579 101.126504)))
    (arrow2a (pts (xy 95 104) (xy 95.586421 102.873496)))
    (arrow2b (pts (xy 95 104) (xy 94.413579 102.873496)))
  )
  (dimension 6 (width 0.3) (layer F.Fab)
    (gr_text 6mm (at 113 95) (layer F.Fab))
    (feature1 (pts (xy 110 104) (xy 110 92.3)))
    (feature2 (pts (xy 104 104) (xy 104 92.3)))
    (crossbar (pts (xy 104 95) (xy 110 95)))
    (arrow1a (pts (xy 110 95) (xy 108.873496 95.586421)))
    (arrow1b (pts (xy 110 95) (xy 108.873496 94.413579)))
    (arrow2a (pts (xy 104 95) (xy 105.126504 95.586421)))
    (arrow2b (pts (xy 104 95) (xy 105.126504 94.413579)))
  )
  (dimension 4 (width 0.3) (layer F.Fab)
    (gr_text 4mm (at 97 95) (layer F.Fab))
    (feature1 (pts (xy 104 104) (xy 104 92.3)))
    (feature2 (pts (xy 100 104) (xy 100 92.3)))
    (crossbar (pts (xy 100 95) (xy 104 95)))
    (arrow1a (pts (xy 104 95) (xy 102.873496 95.586421)))
    (arrow1b (pts (xy 104 95) (xy 102.873496 94.413579)))
    (arrow2a (pts (xy 100 95) (xy 101.126504 95.586421)))
    (arrow2b (pts (xy 100 95) (xy 101.126504 94.413579)))
  )
  (dimension 55 (width 0.3) (layer F.Fab)
    (gr_text "55.000 mm" (at 127.5 88.65) (layer F.Fab))
    (feature1 (pts (xy 155 100) (xy 155 87.3)))
    (feature2 (pts (xy 100 100) (xy 100 87.3)))
    (crossbar (pts (xy 100 90) (xy 155 90)))
    (arrow1a (pts (xy 155 90) (xy 153.873496 90.586421)))
    (arrow1b (pts (xy 155 90) (xy 153.873496 89.413579)))
    (arrow2a (pts (xy 100 90) (xy 101.126504 90.586421)))
    (arrow2b (pts (xy 100 90) (xy 101.126504 89.413579)))
  )
  (dimension 54 (width 0.3) (layer F.Fab)
    (gr_text "54.000 mm" (at 88.65 127 90) (layer F.Fab))
    (feature1 (pts (xy 100 100) (xy 87.3 100)))
    (feature2 (pts (xy 100 154) (xy 87.3 154)))
    (crossbar (pts (xy 90 154) (xy 90 100)))
    (arrow1a (pts (xy 90 100) (xy 90.586421 101.126504)))
    (arrow1b (pts (xy 90 100) (xy 89.413579 101.126504)))
    (arrow2a (pts (xy 90 154) (xy 90.586421 152.873496)))
    (arrow2b (pts (xy 90 154) (xy 89.413579 152.873496)))
  )
  (gr_line (start 100 154) (end 155 154) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155 100) (end 155 154) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 154) (end 100 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 100) (end 155 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 100) (xy 155 100) (xy 155 154) (xy 100 154)
      )
    )
  )
)
