(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 13)
    (no_connects 0)
    (area 147.244999 72.949999 179.653001 126.440001)
    (thickness 1.6)
    (drawings 54)
    (tracks 45)
    (zones 0)
    (modules 10)
    (nets 24)
  )
  (page A4)
  (title_block
    (date "lun. 30 mars 2015")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 135.89 126.873)
    (grid_origin 135.89 126.873)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Vin)
  (net 4 /A0)
  (net 5 /A1)
  (net 6 /A2)
  (net 7 /A3)
  (net 8 "/A4(SDA)")
  (net 9 "/A5(SCL)")
  (net 10 /7)
  (net 11 "/6(**)")
  (net 12 "/5(**)")
  (net 13 /4)
  (net 14 "/3(**)")
  (net 15 /2)
  (net 16 "/1(Tx)")
  (net 17 "/0(Rx)")
  (net 18 "Net-(P9-Pad6)")
  (net 19 "Net-(P10-Pad6)")
  (net 20 "Net-(P9-Pad2)")
  (net 21 "Net-(P9-Pad1)")
  (net 22 "Net-(P10-Pad2)")
  (net 23 "Net-(P10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "/0(Rx)")
    (add_net "/1(Tx)")
    (add_net /2)
    (add_net "/3(**)")
    (add_net /4)
    (add_net "/5(**)")
    (add_net "/6(**)")
    (add_net /7)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net "/A4(SDA)")
    (add_net "/A5(SCL)")
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P10-Pad6)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad6)")
  )
  (module BrewPi:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 590F1B75)
    (at 162.56 99.695 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.2 0.05 270) (layer F.SilkS) hide)
    (fp_text value 4.7kΩ (at 5.2 -2.2 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/A4(SDA)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module BrewPi:BrewPi (layer F.Cu) (tedit 0)
    (at 164.084 83.439)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module BrewPi:Socket_Strip_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 590F235E)
    (at 156.718 75.565 90)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference P4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Digital (at 0 20.11 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /7))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/6(**)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/5(**)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/3(**)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/1(Tx)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/0(Rx)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module BrewPi:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 590F23D7)
    (at 161.798 123.825 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Analog (at 0 15.03 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/A4(SDA)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/A5(SCL)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module BrewPi:Socket_Strip_Straight_1x04_Pitch2.54mm_F (layer F.Cu) (tedit 590F250C)
    (at 176.53 107.061 180)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/6(**)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/5(**)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module BrewPi:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 590F23A5)
    (at 149.098 123.825 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Vin))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module BrewPi:Pulse_RJ12_E5566-QOLK22-L (layer F.Cu) (tedit 59230494)
    (at 149.606 92.329 270)
    (fp_text reference P9 (at 5.98 4 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 6.07 1.53 270) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 6.51 -4.84 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "/A4(SDA)"))
    (pad 5 thru_hole circle (at 4.47 -4.84 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at 8.55 -4.84 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(P9-Pad1)"))
    (pad 6 thru_hole circle (at 3.45 -2.3 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(P9-Pad6)"))
    (pad 4 thru_hole circle (at 5.49 -2.3 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7.53 -2.3 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(P9-Pad2)"))
    (pad "" np_thru_hole circle (at 12 0 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
  )
  (module BrewPi:Pulse_RJ12_E5566-QOLK22-L (layer F.Cu) (tedit 59230494)
    (at 149.606 107.823 270)
    (fp_text reference P10 (at 5.98 4 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 6.07 1.53 270) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 6.51 -4.84 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "/A4(SDA)"))
    (pad 5 thru_hole circle (at 4.47 -4.84 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at 8.55 -4.84 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(P10-Pad1)"))
    (pad 6 thru_hole circle (at 3.45 -2.3 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(P10-Pad6)"))
    (pad 4 thru_hole circle (at 5.49 -2.3 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7.53 -2.3 270) (size 1.52 1.52) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(P10-Pad2)"))
    (pad "" np_thru_hole circle (at 12 0 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
  )
  (module BrewPi:Mandelbrot (layer F.Cu) (tedit 0)
    (at 173.228 91.313)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module BrewPi:Installation_Arduino (layer F.Cu) (tedit 592448B8)
    (at 171.196 115.697)
    (fp_text reference G*** (at 0.06 -7.1) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.25 7.82) (layer F.SilkS) hide)
  )
  (gr_text GND (at 149.606 113.157 315) (layer F.SilkS))
  (gr_text +5V (at 156.464 111.633 45) (layer F.SilkS))
  (gr_text Data (at 156.972 113.919 45) (layer F.SilkS))
  (gr_text GND (at 149.606 97.409 315) (layer F.SilkS))
  (gr_text +5V (at 156.464 95.631 45) (layer F.SilkS))
  (gr_text Data (at 156.718 97.917 45) (layer F.SilkS))
  (gr_text 6 (at 173.99 117.221) (layer B.SilkS))
  (gr_text 5 (at 172.974 117.221) (layer B.SilkS))
  (gr_text 4 (at 171.958 117.221) (layer B.SilkS))
  (gr_text 3 (at 170.942 117.221) (layer B.SilkS))
  (gr_text 2 (at 169.926 117.221) (layer B.SilkS))
  (gr_text 1 (at 168.91 117.221) (layer B.SilkS))
  (gr_line (start 153.416 89.789) (end 154.94 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 89.789) (end 153.416 89.789) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 91.059) (end 148.59 89.789) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 94.869) (end 147.32 91.059) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "RJ12 Wiring\n1: Unused\n2: Unused\n3: Data\n4: GND\n5: +5V\n6: Unused" (at 172.974 87.757) (layer B.SilkS))
  (gr_text RELAY2 (at 170.434 101.981 180) (layer F.SilkS))
  (gr_text RELAY1 (at 170.434 104.521 180) (layer F.SilkS))
  (gr_text GND (at 172.212 107.061 180) (layer F.SilkS))
  (gr_text +5V (at 172.212 99.441 180) (layer F.SilkS))
  (gr_line (start 147.32 94.869) (end 147.32 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 77.851) (end 154.94 88.265) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 73.025) (end 154.94 77.851) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 73.025) (end 154.94 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Unofficial\nArduino Shield\nRev. 2" (at 164.084 94.615) (layer F.SilkS))
  (gr_text RJ12 (at 154.178 118.745) (layer F.SilkS))
  (gr_text RJ12 (at 154.178 102.997) (layer F.SilkS))
  (gr_line (start 147.32 126.365) (end 177.038 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 126.365) (end 177.038 126.111) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 74.549) (end 175.514 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 85.979) (end 177.038 74.549) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 88.519) (end 177.038 85.979) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 121.285) (end 179.578 88.519) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 123.825) (end 179.578 121.285) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 126.365) (end 177.038 123.825) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.038 85.979) (xy 177.038 74.549) (xy 175.514 73.025) (xy 154.94 73.025) (xy 154.94 88.265)
        (xy 153.416 89.789) (xy 148.59 89.789) (xy 147.32 91.059) (xy 147.32 126.365) (xy 177.038 126.365)
        (xy 177.038 123.825) (xy 179.578 121.285) (xy 179.578 88.519)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.038 85.979) (xy 177.038 74.549) (xy 175.514 73.025) (xy 154.94 73.025) (xy 154.94 88.265)
        (xy 153.416 89.789) (xy 148.59 89.789) (xy 147.32 91.059) (xy 147.32 126.365) (xy 177.038 126.365)
        (xy 177.038 123.825) (xy 179.578 121.285) (xy 179.578 88.519)
      )
    )
  )
)
