(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 51)
    (no_connects 0)
    (area 136.449999 88.824999 178.510001 118.185001)
    (thickness 1.6)
    (drawings 7)
    (tracks 16)
    (zones 0)
    (modules 38)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.9878 7.0104)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 +BATT)
  (net 3 GND)
  (net 4 +5V)
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D3-Pad1)")
  (net 7 "Net-(R1-Pad2)")
  (net 8 "Net-(U1-Pad2)")
  (net 9 "Net-(U1-Pad3)")
  (net 10 "Net-(U1-Pad5)")
  (net 11 /PH)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /PH)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
  )
  (net_class PWR ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net +BATT)
    (add_net GND)
  )
  (module footprints:SRR1208-220ML (layer F.Cu) (tedit 59BD93F2)
    (at 143.51 97.79 270)
    (fp_text reference L1 (at 5.715 -7.62 270) (layer F.SilkS))
    (fp_text value 22uH (at 0 0 270) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User) hide)
    (pad 1 smd rect (at -4.9911 0 270) (size 3.9878 7.0104) (layers F.Cu F.Paste F.Mask)
      (net 11 /PH) (zone_connect 2))
    (pad 2 smd rect (at 4.9911 0 270) (size 3.9878 7.0104) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59BCBAFA)
    (at 153.035 95.25 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.155 0 180) (layer F.SilkS))
    (fp_text value 10nF (at 1.25 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /PH) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59BCB9B6)
    (at 171.45 99.06 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -4.445 0 360) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 -2.54 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT) (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59BCB9B1)
    (at 168.91 99.06 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -4.445 0 360) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT) (zone_connect 2))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59BCBAC0)
    (at 154.94 114.3)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -3.81 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (zone_connect 2))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_5x5.3 (layer F.Cu) (tedit 59BCBAD8)
    (at 154.94 109.855)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C5 (at -5.08 -1.905) (layer F.SilkS))
    (fp_text value 220uF (at 0 -3.92) (layer F.Fab))
    (fp_text user + (at -1.37 -0.08) (layer F.Fab))
    (fp_text user + (at -3.38 2.34) (layer F.SilkS))
    (fp_text user %R (at 0 3.92) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (zone_connect 2))
    (pad 2 smd rect (at 2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/CP_Elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 59BCB98C)
    (at 161.29 92.71 180)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value STPS5L60U (at 0 2.6 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 180) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 11 /PH) (zone_connect 2))
    (pad 2 smd rect (at 2.5 0 180) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 59BCBEDA)
    (at 170.18 92.71 180)
    (descr "Diode SMD 1206, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference VBAT (at 0 1.905 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.8 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 59BCBEF6)
    (at 142.01 116.205 180)
    (descr "Diode SMD 1206, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference +5V (at 0.278 1.905 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.8 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 59BD8B92)
    (at 174.95 114.3 180)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference -VBAT+ (at 1.75 5.969 180) (layer F.SilkS))
    (fp_text value -VBAT+ (at 1.75 6 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 +BATT) (zone_connect 2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 59BD8BA2)
    (at 139.7 111.45 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference +5V- (at 1.75 6.096 90) (layer F.SilkS))
    (fp_text value -5V+ (at 1.75 6 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 +5V) (zone_connect 2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59BCBB7F)
    (at 158.67 105.41)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.35 1.905) (layer F.SilkS))
    (fp_text value 30.9K±0.1% (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (zone_connect 2))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59BCBC09)
    (at 163.75 105.41)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 1.35 1.905) (layer F.SilkS))
    (fp_text value 10K±0.1% (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59BCB834)
    (at 175.18 92.71)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59BCBAC6)
    (at 148.05 116.205)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:TI_SO-PowerPAD-8 (layer F.Cu) (tedit 59BCC8AB)
    (at 158.75 99.06)
    (descr "8-Lead Plastic PSOP, Exposed Die Pad (TI DDA0008B, see http://www.ti.com/lit/ds/symlink/lm3404.pdf)")
    (tags "SSOP 0.50 exposed pad")
    (attr smd)
    (fp_text reference U1 (at 0 -3.3) (layer F.SilkS))
    (fp_text value TPS5430 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.78 -1.905) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.78 -0.635) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.78 0.635) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.78 1.905) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at 2.78 1.905) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.78 0.635) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 2.78 -0.635) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 8 smd rect (at 2.78 -1.905) (size 1.91 0.61) (layers F.Cu F.Paste F.Mask)
      (net 11 /PH) (zone_connect 2))
    (pad 9 smd rect (at 0.6025 0.775) (size 1.205 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 9 smd rect (at 0.6025 -0.775) (size 1.205 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 9 smd rect (at -0.6025 0.775) (size 1.205 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (pad 9 smd rect (at -0.6025 -0.775) (size 1.205 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_paste_margin_ratio -0.2) (zone_connect 2))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/TI_SO-PowerPAD-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB773)
    (at 158.75 115.57)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB768)
    (at 158.75 114.3)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB756)
    (at 158.75 113.03)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB74D)
    (at 160.02 111.76)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB744)
    (at 160.02 110.49)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB73A)
    (at 160.02 109.22)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB6F2)
    (at 168.275 103.505)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB6FD)
    (at 169.545 103.505)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB704)
    (at 170.815 103.505)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB714)
    (at 172.085 103.505)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB72C)
    (at 172.085 104.775)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB725)
    (at 170.815 104.775)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB720)
    (at 169.545 104.775)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB71B)
    (at 168.275 104.775)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB73F)
    (at 161.29 109.22)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB749)
    (at 161.29 110.49)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB751)
    (at 161.29 111.76)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB764)
    (at 160.02 113.03)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB76F)
    (at 160.02 114.3)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module footprints:via-0.7mm (layer F.Cu) (tedit 59BCB778)
    (at 160.02 115.57)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.7mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.7 0.7) (drill 0.3302) (layers *.Cu)
      (net 3 GND) (zone_connect 2))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 163.83 114.3)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 156.845 111.76 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text "Buck Converter\nIn: 8-36V\nOut: 5V/3A\n\nBryan Orabutt" (at 157.48 101.6) (layer B.SilkS))
  (dimension 30.48 (width 0.3) (layer Eco1.User)
    (gr_text "30.480 mm" (at 185.5 104.14 270) (layer Eco1.User))
    (feature1 (pts (xy 179.07 119.38) (xy 186.85 119.38)))
    (feature2 (pts (xy 179.07 88.9) (xy 186.85 88.9)))
    (crossbar (pts (xy 184.15 88.9) (xy 184.15 119.38)))
    (arrow1a (pts (xy 184.15 119.38) (xy 183.563579 118.253496)))
    (arrow1b (pts (xy 184.15 119.38) (xy 184.736421 118.253496)))
    (arrow2a (pts (xy 184.15 88.9) (xy 183.563579 90.026504)))
    (arrow2b (pts (xy 184.15 88.9) (xy 184.736421 90.026504)))
  )
  (dimension 41.91 (width 0.3) (layer Eco1.User)
    (gr_text "41.910 mm" (at 157.48 84.375) (layer Eco1.User))
    (feature1 (pts (xy 178.435 88.9) (xy 178.435 83.025)))
    (feature2 (pts (xy 136.525 88.9) (xy 136.525 83.025)))
    (crossbar (pts (xy 136.525 85.725) (xy 178.435 85.725)))
    (arrow1a (pts (xy 178.435 85.725) (xy 177.308496 86.311421)))
    (arrow1b (pts (xy 178.435 85.725) (xy 177.308496 85.138579)))
    (arrow2a (pts (xy 136.525 85.725) (xy 137.651504 86.311421)))
    (arrow2b (pts (xy 136.525 85.725) (xy 137.651504 85.138579)))
  )
  (gr_line (start 178.435 118.11) (end 136.525 118.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.435 88.9) (end 178.435 118.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.525 88.9) (end 178.435 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.525 118.11) (end 136.525 88.9) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 87.63) (xy 180.34 87.63) (xy 180.34 121.92) (xy 133.35 121.92)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.94 120.65) (xy 147.955 120.65) (xy 147.955 115.57) (xy 154.94 115.57) (xy 154.94 107.315)
        (xy 158.75 107.315) (xy 158.75 104.775) (xy 158.75 101.6) (xy 157.48 101.6) (xy 157.48 91.44)
        (xy 160.02 91.44) (xy 160.02 99.06) (xy 172.72 99.06) (xy 172.72 120.65)
      )
    )
  )
  (zone (net 2) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.355 120.65) (xy 173.355 98.425) (xy 163.195 98.425) (xy 163.195 95.885) (xy 166.37 95.885)
        (xy 166.37 89.535) (xy 178.435 89.535) (xy 179.07 90.805) (xy 179.07 120.65)
      )
    )
  )
  (zone (net 11) (net_name /PH) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.655 97.79) (xy 162.56 97.79) (xy 162.56 95.25) (xy 165.735 95.25) (xy 165.735 90.805)
        (xy 165.735 88.9) (xy 135.255 88.9) (xy 135.255 99.695) (xy 151.765 99.695) (xy 151.765 95.25)
        (xy 156.21 95.25) (xy 156.21 90.805) (xy 161.29 90.805) (xy 161.29 94.615) (xy 160.655 94.615)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.255 120.015) (xy 147.32 120.015) (xy 147.32 114.935) (xy 154.305 114.935) (xy 154.305 106.68)
        (xy 158.115 106.68) (xy 158.115 104.775) (xy 154.305 104.775) (xy 154.305 100.33) (xy 135.255 100.33)
      )
    )
  )
)
