<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="6.0325" y1="0" x2="37.4525" y2="0" width="0" layer="20"/>
<wire x1="37.4525" y1="0" x2="37.4525" y2="6.35" width="0" layer="20"/>
<wire x1="37.4525" y1="6.35" x2="43.4975" y2="6.35" width="0" layer="20"/>
<wire x1="43.4975" y1="6.35" x2="43.4975" y2="22.85" width="0" layer="20"/>
<wire x1="43.4975" y1="22.85" x2="0" y2="22.85" width="0" layer="20"/>
<wire x1="0" y1="22.85" x2="0" y2="6.35" width="0" layer="20"/>
<wire x1="0" y1="6.35" x2="6.0325" y2="6.35" width="0" layer="20"/>
<wire x1="6.0325" y1="6.35" x2="6.0325" y2="0" width="0" layer="20"/>
<hole x="21.2725" y="7.62" drill="2.2"/>
<hole x="21.2725" y="17.78" drill="2.2"/>
<hole x="1.27" y="21.59" drill="2"/>
<hole x="42.2275" y="21.59" drill="2"/>
<text>The Real Phoenix ©2017</text>
<text>Control Board for Nano GameBoy</text>
</plain>
<libraries>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JOYSTICK_MINI">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TACT_PANA-EVQ">
</package>
</packages>
</library>
<library name="TRP_Custom">
<packages>
<package name="SMD_SOIC_BOTTOM">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
<package name="LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="SparkFun-Electromechanical" package="JOYSTICK_MINI" value="">
<attribute name="PROD_ID" value="SWCH-09905"/>
</element>
<element name="START_SW" library="adafruit" package="TACT_PANA-EVQ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SELECT_SW" library="adafruit" package="TACT_PANA-EVQ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y_SW" library="adafruit" package="TACT_PANA-EVQ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B_SW" library="adafruit" package="TACT_PANA-EVQ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A_SW" library="adafruit" package="TACT_PANA-EVQ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X_SW" library="adafruit" package="TACT_PANA-EVQ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="UP" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="DOWN" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RIGHT" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="LEFT" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="A" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="START" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SELECT" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Y" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="B" library="TRP_Custom" package="SMD_SOIC_BOTTOM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U$2" library="TRP_Custom" package="LOGO" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="B_SW" pad="P$2"/>
<contactref element="Y_SW" pad="P$2"/>
<contactref element="SELECT_SW" pad="P$2"/>
<contactref element="START_SW" pad="P$2"/>
<contactref element="A_SW" pad="P$2"/>
<contactref element="X_SW" pad="P$2"/>
<contactref element="S1" pad="GND"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="B_SW" pad="P$1"/>
<contactref element="B" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="Y_SW" pad="P$1"/>
<contactref element="Y" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="SELECT_SW" pad="P$1"/>
<contactref element="SELECT" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="START_SW" pad="P$1"/>
<contactref element="START" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="A_SW" pad="P$1"/>
<contactref element="A" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="X_SW" pad="P$1"/>
<contactref element="X" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="S1" pad="C"/>
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="S1" pad="B"/>
<contactref element="RIGHT" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="S1" pad="D"/>
<contactref element="DOWN" pad="1"/>
</signal>
<signal name="UP">
<contactref element="S1" pad="A"/>
<contactref element="UP" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
