(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 507)
    (zones 0)
    (modules 30)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.254)
    (zone_clearance 0.3556)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.6096 0.6096)
    (mod_text_width 0.1524)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 139.065 111.125)
    (visible_elements 7FFCDF3F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "#RST")
  (net 3 D7)
  (net 4 D6)
  (net 5 D5)
  (net 6 D4)
  (net 7 D3)
  (net 8 D2)
  (net 9 D1)
  (net 10 D0)
  (net 11 A15)
  (net 12 A9)
  (net 13 A8)
  (net 14 A7)
  (net 15 A6)
  (net 16 A5)
  (net 17 A4)
  (net 18 A3)
  (net 19 A2)
  (net 20 A1)
  (net 21 A0)
  (net 22 "#RD")
  (net 23 +3V3)
  (net 24 "Net-(C6-Pad1)")
  (net 25 "Net-(C7-Pad1)")
  (net 26 PGEC)
  (net 27 PGED)
  (net 28 MCLR)
  (net 29 "Net-(C8-Pad1)")
  (net 30 +5V)
  (net 31 "Net-(J3-PadR)")
  (net 32 MIDI)
  (net 33 "Net-(Q1-Pad3)")
  (net 34 "Net-(J3-PadT)")
  (net 35 "Net-(R3-Pad1)")
  (net 36 "Net-(C9-Pad1)")
  (net 37 "Net-(D1-Pad1)")
  (net 38 "Net-(D1-Pad2)")
  (net 39 "Net-(D1-Pad3)")
  (net 40 R)
  (net 41 G)
  (net 42 B)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "#RD")
    (add_net "#RST")
    (add_net +3V3)
    (add_net +5V)
    (add_net A0)
    (add_net A1)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net B)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net G)
    (add_net GND)
    (add_net MCLR)
    (add_net MIDI)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(J3-PadR)")
    (add_net "Net-(J3-PadT)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R3-Pad1)")
    (add_net PGEC)
    (add_net PGED)
    (add_net R)
  )
  (module PJS-icons:metroid (layer F.Cu) (tedit 5A0106A6)
    (at 128.905 60.96)
    (fp_text reference icon1 (at 0 2.54) (layer F.Fab) hide)
    (fp_text value Metroid (at 0 -2.54) (layer F.SilkS) hide)
    (pad "" smd circle (at -0.635 0) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0.635 0) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0 -0.635) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
  )
  (module Gameboy:GameBoy_Cartridge_1x32_P1.50mm_Edge locked (layer F.Cu) (tedit 5B835044)
    (at 152.3111 115.1636)
    (descr "Game Boy cartridge edge connector")
    (tags "gameboy cartridge")
    (attr virtual)
    (fp_text reference J1 (at -22.2631 -4.1656) (layer F.SilkS))
    (fp_text value Gameboy (at 0 5) (layer F.Fab) hide)
    (fp_text user %R (at 0 3) (layer F.Fab))
    (fp_text user 32 (at 23.4569 -5.1816) (layer F.SilkS))
    (fp_text user 1 (at -23.7 -4.5) (layer F.SilkS))
    (fp_text user "Gameboy connector modified from:" (at 0 8.5) (layer Cmts.User))
    (fp_text user https://github.com/Gekkio/gb-hardware/tree/master/GB-BRK-CART (at 0 10.5) (layer Cmts.User))
    (fp_text user "Which was licensed under Creative Commons Attribution 4.0 International." (at 0 12.5) (layer Cmts.User))
    (fp_text user "Recommended thickness 0.8mm" (at 0 18) (layer Cmts.User))
    (pad 32 connect rect (at 23.4 0 90) (size 6 1.3) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 31 connect rect (at 21.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 30 connect rect (at 20.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 2 "#RST"))
    (pad 29 connect rect (at 18.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 3 D7))
    (pad 28 connect rect (at 17.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 4 D6))
    (pad 27 connect rect (at 15.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 5 D5))
    (pad 26 connect rect (at 14.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 6 D4))
    (pad 25 connect rect (at 12.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 7 D3))
    (pad 24 connect rect (at 11.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 8 D2))
    (pad 23 connect rect (at 9.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 9 D1))
    (pad 22 connect rect (at 8.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 10 D0))
    (pad 21 connect rect (at 6.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 11 A15))
    (pad 20 connect rect (at 5.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 19 connect rect (at 3.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 18 connect rect (at 2.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 17 connect rect (at 0.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 16 connect rect (at -0.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 15 connect rect (at -2.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 12 A9))
    (pad 14 connect rect (at -3.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 13 A8))
    (pad 13 connect rect (at -5.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 14 A7))
    (pad 12 connect rect (at -6.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 15 A6))
    (pad 11 connect rect (at -8.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 16 A5))
    (pad 10 connect rect (at -9.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 17 A4))
    (pad 9 connect rect (at -11.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 18 A3))
    (pad 8 connect rect (at -12.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 19 A2))
    (pad 7 connect rect (at -14.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 20 A1))
    (pad 6 connect rect (at -15.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 21 A0))
    (pad 5 connect rect (at -17.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 4 connect rect (at -18.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask)
      (net 22 "#RD"))
    (pad 3 connect rect (at -20.25 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad 1 connect rect (at -23.4 0 90) (size 6 1.3) (layers F.Cu F.Mask)
      (net 30 +5V))
    (pad 2 connect rect (at -21.75 -0.25 90) (size 5.5 1) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at 0 -11.35) (size 7.2 7.2) (drill 7.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -36.35) (size 2.3 2.3) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module Housings_QFP:TQFP-64_10x10mm_Pitch0.5mm (layer F.Cu) (tedit 58CC9A48)
    (at 163.195 85.979 180)
    (descr "64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at -5.969 -4.826 180) (layer F.SilkS))
    (fp_text value PIC32MX3xxFxxH_TQFP (at 0 7.45 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 64 smd rect (at -3.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 63 smd rect (at -3.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 A9))
    (pad 62 smd rect (at -2.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 61 smd rect (at -2.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 A8))
    (pad 60 smd rect (at -1.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 A7))
    (pad 59 smd rect (at -1.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 A1))
    (pad 58 smd rect (at -0.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 A0))
    (pad 57 smd rect (at -0.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 56 smd rect (at 0.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C7-Pad1)"))
    (pad 55 smd rect (at 0.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 D3))
    (pad 54 smd rect (at 1.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 D2))
    (pad 53 smd rect (at 1.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 D1))
    (pad 52 smd rect (at 2.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 D0))
    (pad 51 smd rect (at 2.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 50 smd rect (at 3.25 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 49 smd rect (at 3.75 -5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 48 smd rect (at 5.7 -3.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 47 smd rect (at 5.7 -3.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 46 smd rect (at 5.7 -2.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 A15))
    (pad 45 smd rect (at 5.7 -2.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 D7))
    (pad 44 smd rect (at 5.7 -1.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 D6))
    (pad 43 smd rect (at 5.7 -1.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 D5))
    (pad 42 smd rect (at 5.7 -0.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 D4))
    (pad 41 smd rect (at 5.7 -0.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 5.7 0.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 5.7 0.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 5.7 1.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 37 smd rect (at 5.7 1.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "#RST"))
    (pad 36 smd rect (at 5.7 2.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "#RD"))
    (pad 35 smd rect (at 5.7 2.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 A6))
    (pad 34 smd rect (at 5.7 3.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 A2))
    (pad 33 smd rect (at 5.7 3.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 A3))
    (pad 32 smd rect (at 3.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 A5))
    (pad 31 smd rect (at 3.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 A4))
    (pad 30 smd rect (at 2.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 R))
    (pad 29 smd rect (at 2.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 G))
    (pad 28 smd rect (at 1.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 B))
    (pad 27 smd rect (at 1.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 0.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 25 smd rect (at 0.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -0.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at -0.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 MIDI))
    (pad 22 smd rect (at -1.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at -1.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -2.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -2.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 18 smd rect (at -3.25 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -3.75 5.7 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -5.7 3.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 PGED))
    (pad 15 smd rect (at -5.7 3.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 PGEC))
    (pad 14 smd rect (at -5.7 2.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -5.7 2.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -5.7 1.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -5.7 1.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -5.7 0.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 9 smd rect (at -5.7 0.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -5.7 -0.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -5.7 -0.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 MCLR))
    (pad 6 smd rect (at -5.7 -1.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -5.7 -1.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -5.7 -2.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.7 -2.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -5.7 -3.25 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -5.7 -3.75 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 154.432 85.864 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.397 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 165.354 96.52 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 165.862 76.188 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 173.482 85.09)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 162.56 75.946 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 175.006 92.202 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 163.576 96.52 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 175.514 63.5)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at -1.016 12.192) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 PGEC))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 PGED))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 +3V3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 MCLR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 172.732 89.662)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 172.72 87.884 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.905 0 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 MCLR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 160.02 71.12 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 2.2nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C8-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 161.544 65.786 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 2.2nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS_smt_parts:35RASMT2BHNTRX (layer F.Cu) (tedit 5B8758AC)
    (at 136.906 58.166 270)
    (fp_text reference J3 (at 15.494 2.921) (layer F.SilkS))
    (fp_text value 35RASMT2BHNTRX (at 7 6 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 3.5 0 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.5 0 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad S smd rect (at 2.4 3.675 270) (size 2.4 2.55) (layers F.Cu F.Paste F.Mask))
    (pad R smd rect (at 4.3 -3.675 270) (size 2.4 2.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J3-PadR)"))
    (pad T smd rect (at 11.7 3.575 270) (size 2.9 2.75) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J3-PadT)"))
  )
  (module PJS_smt_parts:35RASMT2BHNTRX (layer F.Cu) (tedit 5B8758AC)
    (at 167.894 58.166 270)
    (fp_text reference J4 (at 15.24 2.54) (layer F.SilkS))
    (fp_text value 35RASMT2BHNTRX (at 7 6 270) (layer F.Fab))
    (pad T smd rect (at 11.7 3.575 270) (size 2.9 2.75) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C8-Pad1)"))
    (pad R smd rect (at 4.3 -3.675 270) (size 2.4 2.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C9-Pad1)"))
    (pad S smd rect (at 2.4 3.675 270) (size 2.4 2.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 10.5 0 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.5 0 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  )
  (module Rohm:SOT-416FL (layer F.Cu) (tedit 5B8755A3)
    (at 156.845 69.215 270)
    (fp_text reference Q1 (at 1.651 0.1) (layer F.SilkS))
    (fp_text value RE1C002UN (at 0.9 1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.5 0.525 270) (size 0.46 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 MIDI))
    (pad 2 smd rect (at 0.5 0.525 270) (size 0.46 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.525 270) (size 0.46 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q1-Pad3)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 141.605 66.675 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J3-PadR)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 153.67 68.58)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.27) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 MIDI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 160.02 69.215 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.143 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q1-Pad3)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 161.544 64.008)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SOP-4_4.4x2.8mm_Pitch1.27mm (layer F.Cu) (tedit 58A079E7)
    (at 144.78 71.12)
    (descr "4-Lead Plastic Small Outline http://www.vishay.com/docs/49633/sg2098.pdf")
    (tags "SOP 1.27")
    (attr smd)
    (fp_text reference U2 (at -2.032 -2.286) (layer F.SilkS))
    (fp_text value TLP290 (at 1 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 3.15 -0.64) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 MIDI))
    (pad 3 smd rect (at 3.15 0.64) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.15 0.64) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J3-PadT)"))
    (pad 1 smd rect (at -3.15 -0.64) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/SOP-4_4.4x2.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS_smt_parts:RGB_LED_PLCC6_3.5x3.4 (layer F.Cu) (tedit 5B8DB680)
    (at 152.041 64.262 180)
    (fp_text reference D1 (at -0.105 2.54 180) (layer F.SilkS))
    (fp_text value CLX6E-FKC-CH1M1D1BB7C3D3 (at 0.25 2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.375 -1 180) (size 0.9 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.375 0 180) (size 0.9 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at -1.375 1 180) (size 0.9 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at 1.375 1 180) (size 0.9 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 R))
    (pad 5 smd rect (at 1.375 0 180) (size 0.9 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 G))
    (pad 6 smd rect (at 1.375 -1 180) (size 0.9 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 B))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 156.21 62.484 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 261 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D1-Pad3)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 156.21 64.262 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -1.778 0 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 156.21 66.04 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 60.4 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 131.572 75.962 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 133.858 89.932 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-223 (layer F.Cu) (tedit 59D24B44)
    (at 133.858 83.058 180)
    (zone_connect 2)
    (fp_text reference U3 (at 0 -6.1 180) (layer F.SilkS))
    (fp_text value AP2114H-3_3TRG1 (at 0.15 5.65 180) (layer F.Fab))
    (fp_text user %R (at -0.05 0.025 180) (layer F.Fab))
    (pad 3 smd rect (at 2.3 3.1 180) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 30 +5V) (zone_connect 2))
    (pad 2 smd rect (at 0 3.1 180) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3) (zone_connect 2))
    (pad 1 smd rect (at -2.3 3.1 180) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 smd rect (at 0 -3.1 180) (size 3.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 23 +3V3) (zone_connect 2))
  )
  (gr_text U3 (at 137.922 79.248 90) (layer F.SilkS))
  (gr_text "Gameboy\nMIDI\nV0" (at 171.45 102.87) (layer F.SilkS))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT.\n\n\n\n" (at 14.605 186.055) (layer B.SilkS))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT.\n\n\n\n" (at 14.605 186.055) (layer F.SilkS))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT.\n\n\n\n" (at 14.605 186.055) (layer B.Cu))
  (gr_text "Copyright (c) 2018 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT.\n\n\n\n" (at 14.605 186.055) (layer F.Cu))
  (gr_text "Gameboy MIDI adapter\nV0 PJS 3Sep2018\nMIT license " (at 131.445 84.455 90) (layer B.SilkS))
  (gr_line (start 176.911 110.5636) (end 176.911 119.1636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.011 110.5636) (end 176.911 110.5636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.011 60.7636) (end 178.011 110.5636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.011 58.1636) (end 174.011 60.7636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.011 60.7636) (end 178.011 60.7636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.611 58.1636) (end 174.011 58.1636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.611 110.5636) (end 126.611 58.1636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.711 110.5636) (end 126.611 110.5636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.711 119.1636) (end 127.711 110.5636) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.711 119.1636) (end 176.911 119.1636) (layer Edge.Cuts) (width 0.05))
  (gr_text OUT (at 160.528 59.436) (layer F.SilkS))
  (gr_text IN (at 141.478 59.436) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.968 57.15) (xy 179.578 57.15) (xy 179.578 119.126) (xy 179.578 120.396) (xy 124.968 120.396)
      )
    )
  )
  (zone (net 23) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 80.518) (xy 134.112 75.946) (xy 138.176 75.946) (xy 138.176 104.394) (xy 129.032 104.394)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.968 57.15) (xy 179.578 57.15) (xy 179.578 111.76) (xy 124.968 111.76)
      )
    )
  )
)
