(kicad_pcb (version 20171130) (host pcbnew 5.0.0+dfsg1-2)
  (general
    (thickness 1.6)
    (drawings 27)
    (tracks 81)
    (zones 0)
    (modules 11)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.00508)
    (aux_axis_origin 0 0)
    (grid_origin 132.390001 82.804)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /5V_DET)
  (net 3 GND)
  (net 4 "Net-(R3-Pad1)")
  (net 5 /OE)
  (net 6 /TX0*_5V)
  (net 7 +3V3)
  (net 8 /TX0*)
  (net 9 /RX0*)
  (net 10 /RX0*_5V)
  (net 11 "Net-(A1-Pad1)")
  (net 12 "Net-(A1-Pad20)")
  (net 13 "Net-(A1-Pad2)")
  (net 14 "Net-(A1-Pad19)")
  (net 15 "Net-(A1-Pad3)")
  (net 16 "Net-(A1-Pad4)")
  (net 17 "Net-(A1-Pad5)")
  (net 18 "Net-(A1-Pad16)")
  (net 19 /CLEAR)
  (net 20 /TX1)
  (net 21 "Net-(A1-Pad8)")
  (net 22 "Net-(A1-Pad12)")
  (net 23 "Net-(U1-Pad4)")
  (net 24 "Net-(U1-Pad5)")
  (net 25 "Net-(U1-Pad6)")
  (net 26 "Net-(U1-Pad9)")
  (net 27 "Net-(U1-Pad10)")
  (net 28 "Net-(U1-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /5V_DET)
    (add_net /CLEAR)
    (add_net /OE)
    (add_net /RX0*)
    (add_net /RX0*_5V)
    (add_net /TX0*)
    (add_net /TX0*_5V)
    (add_net /TX1)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad9)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 142.576001 109.22 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -5.375 270) (layer F.SilkS))
    (fp_text value TXB0104DR (at 0 5.375 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /TX0*))
    (pad 3 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /RX0*))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /OE))
    (pad 9 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /RX0*_5V))
    (pad 13 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /TX0*_5V))
    (pad 14 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mitsu-huzzah-interface-footprints:Adafruit_HUZZAH_ESP8266_breakout_revA_WithMountingHoles (layer F.Cu) (tedit 5C15C8A3)
    (at 132.390001 82.804)
    (descr "32-bit microcontroller module with WiFi, https://www.adafruit.com/product/2471")
    (tags "ESP8266 WiFi microcontroller")
    (fp_text reference A1 (at 10.16 -7.35) (layer F.SilkS))
    (fp_text value HUZZAH (at 10.16 35.29) (layer F.Fab))
    (fp_text user %R (at 10.16 -5.588) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad1)"))
    (pad 18 thru_hole oval (at 20.32 5.08) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 /OE))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad2)"))
    (pad 17 thru_hole oval (at 20.32 7.62) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 /5V_DET))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad3)"))
    (pad 16 thru_hole oval (at 20.32 10.16) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad16)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad4)"))
    (pad 15 thru_hole oval (at 20.32 12.7) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 /TX1))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad5)"))
    (pad 14 thru_hole oval (at 20.32 15.24) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 /TX0*))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 /CLEAR))
    (pad "" thru_hole oval (at 20.32 17.78) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 /RX0*))
    (pad 13 thru_hole oval (at 20.32 20.32) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad "" thru_hole oval (at 0 17.78) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 20.32 22.86) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad12)"))
    (pad 8 thru_hole oval (at 0 20.32) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad8)"))
    (pad 11 thru_hole oval (at 20.32 25.4) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 9 thru_hole oval (at 0 22.86) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad "" np_thru_hole circle (at 0 -3.81) (size 2.9 2.9) (drill 2.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 20.32 -3.81) (size 2.9 2.9) (drill 2.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 31.75) (size 2.9 2.9) (drill 2.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 20.32 31.75) (size 2.9 2.9) (drill 2.9) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 25.4) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 20 thru_hole oval (at 20.32 0) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad20)"))
    (pad 19 thru_hole oval (at 20.32 2.54) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad19)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Adafruit_HUZZAH_ESP8266_breakout_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_KMR2 (layer F.Cu) (tedit 5A02FC95)
    (at 133.914001 119.38 180)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.45 180) (layer F.SilkS))
    (fp_text value KMR2 (at 0 2.55 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.45 180) (layer F.Fab))
    (pad 1 smd rect (at -2.05 -0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at -2.05 0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /CLEAR))
    (pad 1 smd rect (at 2.05 -0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 2.05 0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /CLEAR))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_KMR2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 145.485001 112.014 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 145.485001 106.426 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 +3V3))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal (layer F.Cu) (tedit 5A0EDEC2)
    (at 139.542 119.634)
    (descr "JST PH series connector, S4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J1 (at 9.358001 4.318) (layer F.SilkS))
    (fp_text value AIRCON (at 3 7.45) (layer F.Fab))
    (fp_text user %R (at 3 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /RX0*_5V))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /TX0*_5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 152.710001 119.38 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 2.54 1.016) (layer F.SilkS))
    (fp_text value DEBUG (at 2.54 1.27) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /TX1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5C15D956)
    (at 141.280001 91.299 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.907 0 270) (layer F.SilkS))
    (fp_text value 1K (at 4.459 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /OE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 133.900001 123.317 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value 1K (at 2.78 -0.127 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R3-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 145.852001 91.299 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.907 0 270) (layer F.SilkS))
    (fp_text value 6K8 (at 3.951 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /5V_DET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 143.566001 91.299 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.907 0 90) (layer F.SilkS))
    (fp_text value 3K9 (at -3.951 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /5V_DET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 152.710001 117.602) (layer F.SilkS))
  (gr_text DEBUG (at 150.170001 117.602) (layer F.SilkS))
  (gr_text "DEBUG TX" (at 150.932001 95.504) (layer F.SilkS))
  (gr_text GND (at 150.932001 108.204) (layer F.SilkS))
  (gr_text +3V3 (at 150.932001 103.124) (layer F.SilkS))
  (gr_text TX (at 150.932001 98.044) (layer F.SilkS))
  (gr_text 5V_DETECT (at 150.932001 90.424) (layer F.SilkS))
  (gr_text OE (at 150.932001 87.884) (layer F.SilkS))
  (gr_text CLR (at 133.914001 95.504) (layer F.SilkS))
  (gr_text RX (at 133.914001 98.044) (layer F.SilkS))
  (gr_text GND (at 133.914001 108.204) (layer F.SilkS))
  (gr_text +5V (at 133.914001 105.664) (layer F.SilkS))
  (gr_text TX (at 145.598001 117.856) (layer F.SilkS))
  (gr_text RX (at 143.566001 117.856) (layer F.SilkS))
  (gr_text +5V (at 141.534001 117.856) (layer F.SilkS))
  (gr_text GND (at 139.502001 117.856) (layer F.SilkS))
  (gr_text @dgoodlad (at 150.932001 123.698) (layer B.SilkS))
  (gr_text v02 (at 132.390001 123.698) (layer B.Cu))
  (gr_text "Mitsubishi AC\nX\nHUZZAH.revA" (at 142.550001 80.772) (layer F.SilkS))
  (gr_arc (start 132.390001 123.19) (end 129.596001 123.19) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.710001 123.19) (end 152.710001 125.984) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.710001 78.994) (end 155.504001 78.994) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.390001 78.994) (end 132.390001 76.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.710001 76.2) (end 132.390001 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.504001 123.19) (end 155.504001 78.994) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.390001 125.984) (end 152.710001 125.984) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.596001 78.994) (end 129.596001 123.19) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.596001 76.2) (xy 155.504001 76.2) (xy 155.504001 125.984) (xy 129.596001 125.984)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.504001 125.984) (xy 129.596001 125.984) (xy 129.596001 76.2) (xy 155.504001 76.2)
      )
    )
  )
)
