(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" power)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3.3V")
  (net 2 "GND")
  (net 3 "SCL")
  (net 4 "SDA")
  (net 5 "unconnected-(ADC1-ADDR-Pad5)")
  (net 6 "unconnected-(ADC1-ALRT-Pad6)")
  (net 7 "unconnected-(ADC1-A--Pad7)")
  (net 8 "Temp_in")
  (net 9 "Temp_out")
  (net 10 "Net-(ADC1-A2)")
  (net 11 "unconnected-(ADC1-A3-Pad11)")
  (net 12 "unconnected-(ADC1-A+-Pad12)")
  (net 13 "Net-(Board1-Pin_2)")
  (net 14 "Net-(Board1-Pin_3)")
  (net 15 "unconnected-(Board1-Pin_4-Pad4)")
  (net 16 "unconnected-(Board1-Pin_5-Pad5)")
  (net 17 "+5V")
  (net 18 "unconnected-(ESP32-S2-PA02_A0_D0-Pad1)")
  (net 19 "Net-(Top1-Pin_2)")
  (net 20 "Net-(Top1-Pin_3)")
  (net 21 "unconnected-(Top1-Pin_4-Pad4)")
  (net 22 "unconnected-(Top1-Pin_5-Pad5)")
  (net 23 "Net-(ESP32-S2-PB08_A6_D6_TX)")
  (net 24 "Net-(ESP32-S2-PB09_A7_D7_RX)")
  (net 25 "unconnected-(ESP32-S2-PA7_A8_D8_SCK-Pad9)")
  (net 26 "Net-(ESP32-S2-PA5_A9_D9_MISO)")
  (net 27 "Net-(ESP32-S2-PA6_A10_D10_MOSI)")
  (net 28 "Net-(ESP32-S2-5V)")
  (net 29 "unconnected-(Debug1-Pin_4-Pad4)")
  (net 30 "unconnected-(Debug1-Pin_5-Pad5)")
  (footprint "seedft2:XIO_th" (layer "F.Cu")
    (at 60.2315 54.3383 -90)
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ESP32-S2" (at -1.239757 0.107799) (layer "F.SilkS"))
    (fp_text value "ESP32-S2" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -7.62 7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(ESP32-S2-PA02_A0_D0-Pad1)") (pinfunction "PA02_A0_D0") (pintype "bidirectional+no_connect") (thermal_bridge_angle 45))
    (pad "2" thru_hole oval (at -5.08 7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 9 "Temp_out") (pinfunction "PA4_A1_D1") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -2.54 7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 8 "Temp_in") (pinfunction "PA10_A2_D2") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 0 7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(ADC1-A2)") (pinfunction "PA11_A3_D3") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 2.54 7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 4 "SDA") (pinfunction "PA8_A4_D4_SDA") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "6" thru_hole oval (at 5.08 7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 3 "SCL") (pinfunction "PA9_A5_D5_SCL") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "7" thru_hole oval (at 7.62 7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(ESP32-S2-PB08_A6_D6_TX)") (pinfunction "PB08_A6_D6_TX") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 7.62 -7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(ESP32-S2-PB09_A7_D7_RX)") (pinfunction "PB09_A7_D7_RX") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 5.08 -7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(ESP32-S2-PA7_A8_D8_SCK-Pad9)") (pinfunction "PA7_A8_D8_SCK") (pintype "bidirectional+no_connect") (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at 2.54 -7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(ESP32-S2-PA5_A9_D9_MISO)") (pinfunction "PA5_A9_D9_MISO") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "11" thru_hole oval (at 0 -7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(ESP32-S2-PA6_A10_D10_MOSI)") (pinfunction "PA6_A10_D10_MOSI") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -2.54 -7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "3V3") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "13" thru_hole oval (at -5.08 -7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "14" thru_hole oval (at -7.62 -7.625 270) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(ESP32-S2-5V)") (pinfunction "5V") (pintype "bidirectional") (thermal_bridge_angle 45))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (at 57.6662 73.66 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Top1" (at 2.52175 -1.052695) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Socket" (at -2.54 -7.62 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Top1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(Top1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(Top1-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(Top1-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+5V") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" locked (layer "F.Cu")
    (at 104.6562 74.6344 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference locked "Temp Out" (at 0.069592 -5.912883 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at -5.08 10.16 90) (layer "F.Fab") hide)
    (fp_text user locked "Temp Out" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Temp_out") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "softub:DIP-12_500_ELL" (layer "F.Cu")
    (at 83.82 53.34)
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ADC1" (at -10.16 0 90) (layer "F.Fab"))
    (fp_text value "~" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "Vin") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "2" thru_hole oval (at -3.81 6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "SCL") (pinfunction "SCL") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "SDA") (pinfunction "SDA") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "unconnected-(ADC1-ADDR-Pad5)") (pinfunction "ADDR") (pintype "bidirectional+no_connect") (thermal_bridge_angle 45))
    (pad "6" thru_hole oval (at 6.35 6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "unconnected-(ADC1-ALRT-Pad6)") (pinfunction "ALRT") (pintype "power_in+no_connect") (thermal_bridge_angle 45))
    (pad "7" thru_hole oval (at 6.35 -6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(ADC1-A--Pad7)") (pinfunction "A-") (pintype "power_in+no_connect") (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Temp_in") (pinfunction "A0") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Temp_out") (pinfunction "A1") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(ADC1-A2)") (pinfunction "A2") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "11" thru_hole oval (at -3.81 -6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(ADC1-A3-Pad11)") (pinfunction "A3") (pintype "bidirectional+no_connect") (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -6.35) (size 1.2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(ADC1-A+-Pad12)") (pinfunction "A+") (pintype "power_in+no_connect") (thermal_bridge_angle 45))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (at 99.06 45.72)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x08, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Debug1" (at -2.056772 0.799642) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x08_Pin" (at 0 20.11) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.54 12.7 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Temp_out") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Temp_in") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(ADC1-A2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(Debug1-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(Debug1-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+5V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "softub:DIP-12_400_ELL" (layer "F.Cu")
    (at 83.82 71.12)
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -0.848372 0 90) (layer "F.Fab"))
    (fp_text value "~" (at 12.7 0) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 1 "+3.3V") (pinfunction "LV") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "2" thru_hole oval (at -3.81 5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(ESP32-S2-PB08_A6_D6_TX)") (pinfunction "A1") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(ESP32-S2-PB09_A7_D7_RX)") (pinfunction "A2") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(ESP32-S2-PA6_A10_D10_MOSI)") (pinfunction "A3") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(ESP32-S2-PA5_A9_D9_MISO)") (pinfunction "A4") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "6" thru_hole oval (at 6.35 5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND1") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "7" thru_hole oval (at 6.35 -5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND2") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Board1-Pin_3)") (pinfunction "B4") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Board1-Pin_2)") (pinfunction "B3") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Top1-Pin_2)") (pinfunction "B2") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "11" thru_hole oval (at -3.81 -5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(Top1-Pin_3)") (pinfunction "B1") (pintype "bidirectional") (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -5.08) (size 1.2 2) (drill 0.99) (layers "*.Cu" "*.Mask")
      (net 17 "+5V") (pinfunction "HV") (pintype "power_in") (thermal_bridge_angle 45))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" locked (layer "F.Cu")
    (at 57.6662 68.0304 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference locked "Board1" (at 1.9904 0.7538) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Socket" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Board1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Board1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(Board1-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(Board1-Pin_5-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+5V") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 52.115088 71.276737)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr through_hole)
    (fp_text reference "JP1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Remove for USB" (at -2.647671 -1.737682 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(ESP32-S2-5V)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+5V") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 104.6562 70.2456 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "SofTub.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Temp_In1" (at 3.129642 -0.273228 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03_Socket" (at 5.08 4.87 90) (layer "F.Fab") hide)
    (fp_text user "Temp In" (at -0.074252 -5.543779) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Temp_in") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 111.76 66.04) (end 111.76 79.700287)
    (layer "Edge.Cuts"))
  (gr_line (start 101.55 43.18) (end 48.31 43.18)
    (layer "Edge.Cuts"))
  (gr_line (start 101.6 66.04) (end 111.76 66.04)
    (layer "Edge.Cuts"))
  (gr_line (start 111.81 79.700287) (end 48.31 79.700287)
    (layer "Edge.Cuts"))
  (gr_line (start 101.6 43.18) (end 101.6 66.04)
    (layer "Edge.Cuts"))
  (gr_line (start 48.31 43.18) (end 48.31 79.700287)
    (layer "Edge.Cuts"))
  (gr_text "Softub WiFi Controller\nhttps://github.com/steve1066d/softub-wifi" (at 91.056 64.111209) (layer "B.SilkS"))
  (gr_text "BSS138" (at 80.713031 72.646731) (layer "F.SilkS"))
  (gr_text "3.3" (at 96.050585 58.931667) (layer "F.SilkS"))
  (gr_text "Adafruit 1085" (at 79.675275 51.264134) (layer "F.SilkS"))
  (gr_text "Adafruit 757" (at 79.795944 70.088542) (layer "F.SilkS"))
  (gr_text "5v" (at 69.264919 71.589137) (layer "F.SilkS"))
  (gr_text "A2" (at 95.954086 50.8) (layer "F.SilkS"))
  (gr_text "ADS1115" (at 80.73483 53.84666) (layer "F.SilkS"))
  (gr_text "Softub WiFi Controller\nhttps://github.com/steve1066d/softub-wifi" (at 49.187719 79.340938) (layer "F.SilkS"))
  (gr_text "Tout" (at 96.029704 46.208404) (layer "F.SilkS"))
  (gr_text "RX" (at 61.471005 71.589137) (layer "F.SilkS"))
  (gr_text "Tin" (at 96.047031 48.738113) (layer "F.SilkS"))
  (gr_text "5v" (at 96.050585 61.341892) (layer "F.SilkS"))
  (gr_text "Adafruit 5325" (at 55.251812 49.23689) (layer "F.SilkS"))
  (gr_text "TX" (at 59.152155 71.589137) (layer "F.SilkS"))
  (gr_text "Gnd" (at 95.624581 63.829891) (layer "F.SilkS"))
  (gr_text "v1.1" (at 107.556678 78.883386) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 101.6 55.88)
        (xy 111.76 55.88)
        (xy 111.76 66.04)
        (xy 101.6 66.04)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 43.18 40.64)
        (xy 114.3 40.64)
        (xy 114.3 81.28)
        (xy 43.18 81.28)
      )
    )
  )
)
