(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 27)
    (no_connects 0)
    (area 122.368057 84.5184 197.590343 153.360001)
    (thickness 1.6002)
    (drawings 2)
    (tracks 140)
    (zones 0)
    (modules 13)
    (nets 23)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 159.9792 119.2974)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 /HV6)
  (net 6 /HV5)
  (net 7 /HV10)
  (net 8 /HV4)
  (net 9 /HV9)
  (net 10 /HV3)
  (net 11 /HV8)
  (net 12 /HV2)
  (net 13 /HV7)
  (net 14 /HV1)
  (net 15 /HV12)
  (net 16 /HV11)
  (net 17 "Net-(J1-Pad15)")
  (net 18 "Net-(NX1-Pad6)")
  (net 19 "Net-(NX1-Pad11)")
  (net 20 "Net-(NX1-Pad16)")
  (net 21 "Net-(LED1-Pad1-DO)")
  (net 22 "Net-(LED2-Pad1-DO)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV11)
    (add_net /HV12)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(LED1-Pad1-DO)")
    (add_net "Net-(LED2-Pad1-DO)")
    (add_net "Net-(NX1-Pad11)")
    (add_net "Net-(NX1-Pad16)")
    (add_net "Net-(NX1-Pad6)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 163.2292 144.0474 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AA1E063)
    (at 176.4792 116.0474 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.4 0.05 270) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AA1E05B)
    (at 143.9292 116.0474 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 5AA1E084)
    (at 159.9792 89.2974)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 5AA1E076)
    (at 135.9792 137.2974)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 5AA1E06E)
    (at 183.9792 137.2974)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 170.1392 99.2174 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 270) (layer F.SilkS))
    (fp_text value Nixie (at 1.27 22.65 270) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV12))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /HV11))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV1))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mynixies:mynixies-B17A-8331 (layer F.Cu) (tedit 5B2C5C93)
    (at 160.16262 119.16482)
    (attr virtual)
    (fp_text reference NX1 (at 0 -19.05) (layer F.SilkS) hide)
    (fp_text value GR10N (at -0.18342 -12.86742) (layer F.SilkS))
    (fp_text user 8 (at -7.62 8.89) (layer Dwgs.User))
    (fp_text user 7 (at 0 11.684) (layer Dwgs.User))
    (fp_text user 5 (at 7.747 8.76046) (layer Dwgs.User))
    (fp_text user RD (at 10.922 5.969) (layer Dwgs.User))
    (fp_text user 4 (at 11.43 2.159) (layer Dwgs.User))
    (fp_text user 3 (at 10.287 -5.842) (layer Dwgs.User))
    (fp_text user 2 (at 8.001 -8.76046) (layer Dwgs.User))
    (fp_text user A (at 4.572 -11.049) (layer Dwgs.User))
    (fp_text user 1 (at 0 -11.811) (layer Dwgs.User))
    (fp_text user 6 (at -4.191 -11.049) (layer Dwgs.User))
    (fp_text user 0 (at -10.16 -5.842) (layer Dwgs.User))
    (fp_text user LD (at -11.938 -2.54) (layer Dwgs.User))
    (fp_text user 9 (at -11.303 2.286) (layer Dwgs.User))
    (pad 1 thru_hole circle (at -5.85978 6.985) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 11 /HV8))
    (pad 3 thru_hole circle (at 0 9.1186) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 13 /HV7))
    (pad 5 thru_hole circle (at 5.85978 6.985) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 6 /HV5))
    (pad 6 thru_hole circle (at 7.89686 4.5593) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 18 "Net-(NX1-Pad6)"))
    (pad 7 thru_hole circle (at 8.9789 1.58242) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 8 /HV4))
    (pad 9 thru_hole circle (at 7.89686 -4.5593) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 10 /HV3))
    (pad 10 thru_hole circle (at 5.85978 -6.985) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 12 /HV2))
    (pad 11 thru_hole circle (at 3.11658 -8.56742) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 19 "Net-(NX1-Pad11)"))
    (pad 12 thru_hole circle (at 0 -9.1186) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 14 /HV1))
    (pad 13 thru_hole circle (at -3.11658 -8.56742) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 5 /HV6))
    (pad 15 thru_hole circle (at -7.89686 -4.5593) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 7 /HV10))
    (pad 16 thru_hole circle (at -8.9789 -1.58242) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(NX1-Pad16)"))
    (pad 17 thru_hole circle (at -8.9789 1.58242) (size 2.7432 2.7432) (drill 1.8288) (layers *.Cu *.Paste *.Mask)
      (net 9 /HV9))
    (pad "" np_thru_hole circle (at -3.11658 8.56742) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.11658 8.56742) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 8.9789 -1.58242) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.85978 -6.985) (size 1.8288 1.8288) (drill 1.8288) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 10.16 10.16) (drill 10.16) (layers *.Cu *.Mask))
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5B2C5A1D)
    (at 143.7292 119.42364)
    (attr smd)
    (fp_text reference LED1 (at 3.175 -0.254 90) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED1-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3-DI smd rect (at -1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 /Din))
    (pad 4-VD smd rect (at -1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5B2C5A11)
    (at 176.47672 119.42364)
    (attr smd)
    (fp_text reference LED2 (at 3.175 -0.254 90) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(LED2-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3-DI smd rect (at -1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LED1-Pad1-DO)"))
    (pad 4-VD smd rect (at -1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 152.2292 93.7974)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R1 (at 7.62 3.31) (layer B.SilkS))
    (fp_text value 10K (at 7.62 -3.31) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(NX1-Pad11)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 141.9792 112.2974 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 2.31 90) (layer B.SilkS))
    (fp_text value 40K (at 5.08 -2.31 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(NX1-Pad16)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /HV11))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 171.2292 127.0474)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 2.31) (layer B.SilkS))
    (fp_text value 40K (at 5.08 -2.31) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(NX1-Pad6)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /HV12))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 160.02 119.38) (end 192.52 119.38) (layer Edge.Cuts) (width 0.127))
  (gr_text "nixies.us\nGR10N" (at 162.17 144.33) (layer B.Mask))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 193.04 86.36) (xy 127 85.4) (xy 127 152.4) (xy 193.04 153.36)
      )
    )
  )
)
