(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 312)
    (zones 0)
    (modules 55)
    (nets 31)
  )
  (page A4)
  (title_block
    (title "Smart Mac Lamp OnOff Feedback")
    (date 2019-09-01)
    (rev 2)
    (comment 1 1006026)
    (comment 2 62006024LP)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2.6)
    (user_trace_width 5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.3 4.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fe_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad2)")
  (net 3 +5V)
  (net 4 GNDD)
  (net 5 "Net-(IC1-Pad10)")
  (net 6 "Net-(IC1-Pad11)")
  (net 7 "Net-(IC1-Pad13)")
  (net 8 "Net-(IC1-Pad14)")
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(F1-Pad2)")
  (net 11 "Net-(D2-Pad1)")
  (net 12 "Net-(C2-Pad2)")
  (net 13 +24V)
  (net 14 "Net-(C1-Pad1)")
  (net 15 "Net-(PL14-Pad1)")
  (net 16 Earth)
  (net 17 "Net-(D4-Pad2)")
  (net 18 "Net-(C10-Pad1)")
  (net 19 "Net-(R5-Pad2)")
  (net 20 "Net-(C1-Pad2)")
  (net 21 "Net-(Q1-Pad3)")
  (net 22 "Net-(R6-Pad1)")
  (net 23 "Net-(C4-Pad1)")
  (net 24 "Net-(R4-Pad1)")
  (net 25 "Net-(R1-Pad2)")
  (net 26 "Net-(D3-Pad3)")
  (net 27 "Net-(C11-Pad1)")
  (net 28 "Net-(D4-Pad1)")
  (net 29 "Net-(RL1-Pad7)")
  (net 30 "Net-(RL1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +5V)
    (add_net Earth)
    (add_net GNDD)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad3)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(PL14-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(RL1-Pad2)")
    (add_net "Net-(RL1-Pad7)")
  )
  (net_class "AC IN" ""
    (clearance 0.2)
    (trace_width 3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class "AC neutral" ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "Relay Omron G2R:Relay OMRON G2R-1A-E" (layer F.Cu) (tedit 5D6C596B)
    (at 79.28864 102.3874)
    (fp_text reference RL1 (at 0 0.5) (layer F.SilkS))
    (fp_text value "G2R-1A-E-TV8-ASI 24VDC" (at 0 -0.5) (layer F.Fab))
    (fp_text user RL1 (at 19 -3.75) (layer F.SilkS))
    (pad 7 thru_hole circle (at 15.4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(RL1-Pad7)"))
    (pad 2 thru_hole circle (at 15.2 7.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(RL1-Pad2)"))
    (pad 8 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 +24V))
    (pad 6 thru_hole circle (at 20 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(PL14-Pad1)"))
    (pad 5 thru_hole circle (at 25 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(C2-Pad2)"))
    (pad 4 thru_hole circle (at 25 7.5) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(C2-Pad2)"))
    (pad 3 thru_hole circle (at 20 7.5) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 "Net-(PL14-Pad1)"))
    (pad 1 thru_hole rect (at 0 7.5) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad1)"))
  )
  (module "Relay Omron G2R:87437-0443" (layer F.Cu) (tedit 5D6C5624)
    (at 161.38398 81.06156)
    (descr 87437-0443)
    (tags Connector)
    (attr smd)
    (fp_text reference PL3 (at -2.072 -1.642) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at -2.072 -1.642) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -2.25 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 2 smd rect (at 0 -0.75 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 3 smd rect (at 0 0.75 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 4 smd rect (at 0 2.25 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 5 smd rect (at -3.9 -2.25 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 6 smd rect (at -3.9 -0.75 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 7 smd rect (at -3.9 0.75 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 8 smd rect (at -3.9 2.25 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
  )
  (module "Relay Omron G2R:87437-0443" (layer F.Cu) (tedit 5D6C5624)
    (at 161.78276 109.02188)
    (descr 87437-0443)
    (tags Connector)
    (attr smd)
    (fp_text reference PL2 (at -2.072 -1.642) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at -2.072 -1.642) (layer F.SilkS) hide)
    (pad 8 smd rect (at -3.9 2.25 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 7 smd rect (at -3.9 0.75 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 6 smd rect (at -3.9 -0.75 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 5 smd rect (at -3.9 -2.25 90) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 4 smd rect (at 0 2.25 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 3 smd rect (at 0 0.75 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0 -0.75 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 1 smd rect (at 0 -2.25 90) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
  )
  (module "Relay Omron G2R:SHDR2W165P0X508_1X2_908X1140X1425P" (layer F.Cu) (tedit 5D6C5596)
    (at 80.33512 81.34604 90)
    (descr 10-32-1021)
    (tags Connector)
    (fp_text reference PL6 (at 0 0 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(F1-Pad2)"))
  )
  (module "Relay Omron G2R:87437-0443" (layer F.Cu) (tedit 5D6C548E)
    (at 75.74534 88.7222 180)
    (descr 87437-0443)
    (tags Connector)
    (attr smd)
    (fp_text reference PL10 (at -7.48792 3.65252 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at -2.072 -1.642 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -2.25 270) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 2 smd rect (at 0 -0.75 270) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 3 smd rect (at 0 0.75 270) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad13)"))
    (pad 4 smd rect (at 0 2.25 270) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at -3.9 -2.25 270) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD))
    (pad 6 smd rect (at -3.9 -0.75 270) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 7 smd rect (at -3.9 0.75 270) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad13)"))
    (pad 8 smd rect (at -3.9 2.25 270) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
  )
  (module "Relay Omron G2R:874370273" (layer F.Cu) (tedit 5D6C5417)
    (at 78.04658 95.93072 180)
    (descr 87437-0273)
    (tags Connector)
    (attr smd)
    (fp_text reference PL1 (at 2.34188 -2.32156 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at -0.5 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.675 -0.75 270) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad A1 smd rect (at -2.225 -0.75 270) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.675 0.75 270) (size 0.85 2.65) (layers F.Cu F.Paste F.Mask)
      (net 13 +24V))
    (pad A2 smd rect (at -2.225 0.75 270) (size 0.85 3.55) (layers F.Cu F.Paste F.Mask)
      (net 13 +24V))
  )
  (module Capacitor_SMD:CP_Elec_4x4.5 (layer F.Cu) (tedit 5BCA39CF)
    (at 132.48386 79.41396 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 4.0x4.5mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C4 (at 3.85318 -1.88722 90) (layer F.SilkS))
    (fp_text value "10uF 16V" (at 0 3.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 23 "Net-(C4-Pad1)"))
    (pad 2 smd roundrect (at 1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 4 GNDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 110.8456 84.24394 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -2.79376 0.09652 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GNDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.03682 104.23652 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 GNDD))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.65794 78.73792 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0.0157 1.9177 90) (layer F.SilkS))
    (fp_text value 470n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(C10-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.33452 106.0039 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 3.24912 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.28 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.41022 105.9785 270)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 3.051 0.0508) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.28 270) (layer F.Fab))
    (fp_text user %R (at 0.20112 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 150.2918 94.3102)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C11 (at 10.92454 -8.09244) (layer F.SilkS))
    (fp_text value 2200u (at 3.75 10.25) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GNDD))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 147.88134 74.1934 180)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C7 (at 10.50544 9.9441 180) (layer F.SilkS))
    (fp_text value 2200u (at 3.75 10.25 180) (layer F.Fab))
    (fp_text user %R (at 3.84302 -0.28194 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GNDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 147.52066 110.4011 180)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C6 (at 3.75 -10.25 180) (layer F.SilkS))
    (fp_text value 2200u (at 3.75 10.25 180) (layer F.Fab))
    (fp_text user %R (at 3.75 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GNDD))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D18.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 139.2682 92.46362 180)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=18mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 18mm Electrolytic Capacitor")
    (fp_text reference C9 (at 3.75 -10.25 180) (layer F.SilkS))
    (fp_text value 2200u (at 3.75 10.25 180) (layer F.Fab))
    (fp_text user %R (at 3.75 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GNDD))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D18.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L26.5mm_W5.0mm_P22.50mm_MKS4 (layer F.Cu) (tedit 5AE50EF0)
    (at 111.99622 120.46204 90)
    (descr "C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 22.50mm  length 26.5mm width 5mm Capacitor")
    (fp_text reference C1 (at 11.25 -3.75 90) (layer F.SilkS))
    (fp_text value "220n 275V" (at 11.25 3.75 90) (layer F.Fab))
    (fp_text user %R (at 13.83538 26.01468 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L26.5mm_W5.0mm_P22.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x02_P5.08mm_Drill1.5mm (layer F.Cu) (tedit 5D6BEEE9)
    (at 92.66174 119.65686 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference PL14 (at 0.66802 -3.30454 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 2.54 3.81 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 15 "Net-(PL14-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 15 "Net-(PL14-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x02_P5.08mm_Drill1.5mm (layer F.Cu) (tedit 5D6BF056)
    (at 129.72034 119.4943 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference PL12 (at 5.4864 -3.68046 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 2.54 3.81 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x02_P5.08mm_Drill1.5mm (layer F.Cu) (tedit 5D6BF045)
    (at 120.37568 119.65686 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference PL11 (at 5.64896 -3.4925 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 2.54 3.81 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 14 "Net-(C1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x02_P5.08mm_Drill1.5mm (layer F.Cu) (tedit 5D6BEEF9)
    (at 104.26446 119.4943 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference PL13 (at 0.50546 -3.6449 90) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 2.54 3.81 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 12 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3.50012 3.50012) (drill 1.50114) (layers *.Cu *.Mask)
      (net 12 "Net-(C2-Pad2)"))
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 92.44792 73.86828 180)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D5 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 30V (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(D3-Pad3)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 99.7555 73.86828)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at -2.97642 2.14376) (layer F.SilkS))
    (fp_text value 30V (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.81262 95.26778 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value BAS32L (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_2114_3652Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.79758 105.80116 270)
    (descr "Diode SMD 2114 (3652 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 4.1021 0.1905) (layer F.SilkS))
    (fp_text value 10V (at 0 2.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -2.1875 0 270) (size 1.675 3.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.149254)
      (net 20 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at 2.1875 0 270) (size 1.675 3.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.149254)
      (net 12 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_2114_3652Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:Diode_Bridge_Vishay_KBU (layer F.Cu) (tedit 5A4F7739)
    (at 130.44932 67.4624 180)
    (descr "Vishay KBU rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88656/kbu4.pdf")
    (tags "Vishay KBU rectifier diode bridge")
    (fp_text reference D3 (at 0.2032 -3.86842 180) (layer F.SilkS))
    (fp_text value KBU6D (at 7.5 6.2 180) (layer F.Fab))
    (fp_text user %R (at 5.14604 3.1115 180) (layer F.Fab))
    (pad 4 thru_hole circle (at 15.24 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 GNDD))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 26 "Net-(D3-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/Diode_Bridge_Vishay_KBU.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open (layer F.Cu) (tedit 5D6C57E0)
    (at 107.66298 67.58686 180)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F1 (at 24.3205 -3.78714 180) (layer F.SilkS))
    (fp_text value "4A 250V" (at 2.0828 -5.98678 180) (layer F.SilkS))
    (fp_text user %R (at 11.25 4 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 26 "Net-(D3-Pad3)"))
    (pad 2 thru_hole circle (at 22.5 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(F1-Pad2)"))
    (pad "" np_thru_hole circle (at 11.25 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MFSOP6-5_4.4x3.6mm_P1.27mm (layer F.Cu) (tedit 5A02F25C)
    (at 122.41276 94.65564 90)
    (descr https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.5pin%20MFSOP6.html)
    (tags "MFSOP 4 pin SMD")
    (attr smd)
    (fp_text reference U1 (at -0.0889 -2.88544 180) (layer F.SilkS))
    (fp_text value TLP131 (at 0 2.921 90) (layer F.Fab))
    (fp_text user %R (at 0.38608 -0.08382 90) (layer F.Fab))
    (pad 6 smd rect (at 3.15 -1.27 90) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R4-Pad1)"))
    (pad 3 smd rect (at -3.15 1.27 90) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C2-Pad2)"))
    (pad 4 smd rect (at 3.15 1.27 90) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at -3.15 -1.27 90) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at 3.15 0 90) (size 1.2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MFSOP6-5_4.4x3.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-2 (layer F.Cu) (tedit 5A70FB7B)
    (at 99.42576 82.85734)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference Q1 (at 0.08128 7.04596) (layer F.SilkS))
    (fp_text value T1235-600G (at 0 6.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 3 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 26 "Net-(D3-Pad3)"))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 115.32846 78.65618)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(IC1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 127.28702 82.78138 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.75614 0 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 125.1077 82.7913 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.66446 -0.02032 90) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(IC1-Pad11)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 117.6378 91.694 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 270k (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GNDD))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 121.2342 85.65134 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.23266 -1.37922) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R6-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(IC1-Pad10)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 125.57736 85.6234 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R6-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 121.22404 88.02624 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0.13716 -1.3843 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R6-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GNDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 120.5611 82.75574 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -2.66954 0.0127 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(IC1-Pad11)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(IC1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 122.70994 82.76844 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 3.11658 0.06096 270) (layer F.SilkS))
    (fp_text value 1.5k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(IC1-Pad11)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GNDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 86.34222 95.26016 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 GNDD))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 87.99368 85.37702)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -2.7843 2.02184) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at -0.14778 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(C10-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 117.4526 97.99828)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 330 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.6714 82.66176 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -1.1176 1.59766 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(D4-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5D6BF6D4)
    (at 161.07918 63.35776 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 5.08 -2.37 270) (layer F.SilkS))
    (fp_text value 100 (at 5.08 2.37 270) (layer F.Fab))
    (fp_text user %R (at 5.35686 -0.12446 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 Earth))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDD))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5D6BEEA7)
    (at 88.99144 114.23904)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 15 "Net-(PL14-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 125.07214 119.73052)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 14 "Net-(C1-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 118.60784 78.36916)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 1.1811 -1.2573) (layer F.SilkS))
    (fp_text value TestPoint (at 1.2954 -1.11506) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 7 "Net-(IC1-Pad13)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 75.29322 102.3239)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 13 +24V))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5D6BEEC2)
    (at 107.8865 114.45748)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 12 "Net-(C2-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 75.5904 109.78388)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 11 "Net-(D2-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 81.75244 67.4624)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 10 "Net-(F1-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 107.51566 75.27798)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 9 "Net-(C10-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 154.22118 106.77398)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 4 GNDD))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 125.19914 77.8891)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.648) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 3 +5V))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 158.88462 75.69962)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at -3.38328 -0.57404) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 4 GNDD))
  )
  (module digikey-footprints:SOIC-14_W3.9mm (layer F.Cu) (tedit 5995D3F3)
    (at 115.61572 84.4423 270)
    (fp_text reference IC1 (at 5.45592 2.27076) (layer F.SilkS))
    (fp_text value LM339 (at 0 5.29 270) (layer F.Fab))
    (fp_text user REF** (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IC1-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.54 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.27 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V) (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.27 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 2.54 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 3.81 2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 3.81 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 2.54 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 1.27 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad10)") (solder_mask_margin 0.07))
    (pad 11 smd rect (at 0 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad11)") (solder_mask_margin 0.07))
    (pad 12 smd rect (at -1.27 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GNDD) (solder_mask_margin 0.07))
    (pad 13 smd rect (at -2.54 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad13)") (solder_mask_margin 0.07))
    (pad 14 smd rect (at -3.81 -2.7 270) (size 0.55 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad14)") (solder_mask_margin 0.07))
  )
  (gr_text "62006024LP Rev 2" (at 103.225 92.825) (layer F.SilkS))
  (gr_text 01006026.2 (at 101.1 96.425) (layer F.Cu))
  (gr_line (start 157.65 64.925) (end 157.65 67.925) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.85 67.925) (end 153.85 64.925) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.7504 64.925) (end 157.65 64.925) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155.7504 67.925) (end 153.85 67.925) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.825 116.6) (end 157.825 119.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.025 119.6) (end 154.025 116.6) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 155.9254 116.6) (end 157.825 116.6) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155.9254 119.6) (end 154.025 119.6) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.675 116.375) (end 79.675 119.375) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.875 119.375) (end 75.875 116.375) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 77.7754 116.375) (end 79.675 116.375) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 77.7754 119.375) (end 75.875 119.375) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 77.7509 67.86584) (end 75.8505 67.86584) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 77.7509 64.86584) (end 79.6505 64.86584) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.8505 67.86584) (end 75.8505 64.86584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79.6505 64.86584) (end 79.6505 67.86584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.8505 122.46584) (end 73.8505 61.96584) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.8505 122.46584) (end 73.8505 122.46584) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.8505 61.96584) (end 164.8505 122.46584) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.8505 61.96584) (end 164.8505 61.96584) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.36002 73.69302) (xy 82.36966 73.9902) (xy 83.75142 63.53048) (xy 148.92528 63.3095) (xy 148.92528 71.3613)
        (xy 154.44724 75.96124) (xy 162.88258 75.96124) (xy 163.03498 112.89792) (xy 148.72462 113.12652) (xy 148.72462 121.59234)
        (xy 137.40892 121.5009) (xy 137.50036 113.12652) (xy 119.09806 94.63278) (xy 107.50296 94.54134) (xy 92.96654 94.4499)
        (xy 88.7349 99.32416) (xy 76.45654 99.34448)
      )
    )
  )
  (zone (net 4) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.86988 75.97394) (xy 162.84194 73.72096) (xy 162.1282 72.51192) (xy 161.10966 72.04456) (xy 160.09366 72.51192)
        (xy 157.56636 75.97394)
      )
    )
  )
  (zone (net 16) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.825 63.675) (xy 152.775 69.1) (xy 154.225 70.725) (xy 157.075 70.725) (xy 158.4 69.425)
        (xy 158.45 63.75)
      )
    )
  )
)
