(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 110)
    (zones 0)
    (modules 0)
    (nets 2)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 5)
    (user_trace_width 10)
    (user_trace_width 20)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.5 0.5)
    (user_via 2 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (gr_circle (center 207.6 32.8) (end 209.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 167.6 32.8) (end 169.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 127.6 32.8) (end 129.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 87.6 32.8) (end 89.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 247.6 32.8) (end 246.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 257.6 32.8) (end 259.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 47.6 32.8) (end 49.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 37.6 32.8) (end 36.1 32.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 27.6 37.8) (end 27.6 27.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 266.6 37.8) (end 27.6 37.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 266.6 27.8) (end 266.6 37.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 27.6 27.8) (end 266.6 27.8) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 266.1 36.8) (xy 261.1 36.8) (xy 261.1 35.8) (xy 266.1 35.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 266.1 35.8) (xy 261.1 35.8) (xy 261.1 36.8) (xy 266.1 36.8)
      )
    )
  )
)
