<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="387.35" y1="0" x2="387.35" y2="43.18" width="0" layer="20"/>
<wire x1="387.35" y1="43.18" x2="0" y2="43.18" width="0" layer="20"/>
<wire x1="0" y1="43.18" x2="0" y2="0" width="0" layer="20"/>
<text>DIO0
DIO1</text>
<text>DIO2
DIO3</text>
<text>AI0
AI1</text>
<text>AI2
AI3</text>
<text>AO0
AO1</text>
<text>AO2
AO3</text>
<text>AO4
AO5</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>G</text>
<text>G</text>
<text>G</text>
<text>G</text>
<text>SPARES</text>
<text>DUAL DB25</text>
<text>J007634A  FPGA BREAKOUT</text>
<text>20180817</text>
<text>S</text>
<text>S</text>
<text>DIO4
DIO5</text>
<text>DIO6
DIO7</text>
<text>DIO8
DIO9</text>
<text>DIO10
DIO11</text>
<text>DIO12
DIO13</text>
<text>DIO14
DIO15</text>
<text>GND  +24</text>
<text>GPIOs
TOP</text>
<text>AIN
BOT</text>
<text>DIO
TOP</text>
<text>AO6
BOT</text>
<text>AC INLET</text>
<text>AOTF</text>
<text>AOM</text>
<wire x1="387.35" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>AIGND</text>
<text>AOGND</text>
<text>DGND
</text>
<text>AIGND</text>
<text>N.C.</text>
<text>N.O.</text>
</plain>
<libraries>
<library name="STEVES_BU">
<packages>
<package name="DUAL-BNC">
</package>
<package name="DUAL-DB25F">
</package>
<package name="DUAL-HDMI">
<description>Dual HDMI
TE 1888811-1</description>
</package>
<package name="LOGO_BMP_OP">
</package>
</packages>
</library>
<library name="con-3m">
<description>&lt;b&gt;3M Connectors&lt;/b&gt;&lt;p&gt;
PCMCIA-CompactFlash Connectors&lt;p&gt;
Zero Insertion Force Socked&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PAK100/2500-34">
<description>&lt;b&gt;3M (TM) Pak 100 4-Wall Header&lt;/b&gt; Straight&lt;p&gt;
Source: 3M</description>
</package>
<package name="PAK100/2500-50">
<description>&lt;b&gt;3M (TM) Pak 100 4-Wall Header&lt;/b&gt; Straight&lt;p&gt;
Source: 3M</description>
</package>
</packages>
</library>
<library name="45xx">
<description>&lt;b&gt;CMOS Logic Devices, 4500 Series &lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;li&gt;http://www.ee.washington.edu
&lt;li&gt;http://www.onsemi.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_LOCK">
</package>
<package name="2X5-SHROUDED">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="KK-156-4">
<description>&lt;b&gt;KK 156 HEADER&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com/pdm_docs/sd/026604100_sd.pdf</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J11" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J13" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J14" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J15" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON1" library="con-3m" package="PAK100/2500-34" value="2534-">
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON2" library="con-3m" package="PAK100/2500-34" value="2534-">
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J16" library="STEVES_BU" package="DUAL-DB25F" value="DUAL-DB25">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="STEVES_BU" package="DUAL-HDMI" value="DUAL-HDMI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON0" library="con-3m" package="PAK100/2500-50" value="2550-">
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="capacitor-wima" package="C2.5-2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="45xx" package="DIL16" value="4504N">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun" package="1X08_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-molex" package="KK-156-4" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="STEVES_BU" package="LOGO_BMP_OP" value="JFRC-LOGOLOGO_OP"/>
<element name="JP2" library="SparkFun" package="2X5-SHROUDED" value="M05X2SHD">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun" package="2X5-SHROUDED" value="M05X2SHD">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="J11" pad="P$4"/>
<contactref element="CON0" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J11" pad="P$3"/>
<contactref element="CON0" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="J12" pad="P$4"/>
<contactref element="CON0" pad="10"/>
</signal>
<signal name="N$8">
<contactref element="J12" pad="P$3"/>
<contactref element="CON0" pad="14"/>
</signal>
<signal name="AI4+">
<contactref element="J2" pad="1B"/>
<contactref element="CON0" pad="17"/>
</signal>
<signal name="AI7-">
<contactref element="CON0" pad="30"/>
<contactref element="J2" pad="12B"/>
</signal>
<signal name="AI5+">
<contactref element="J2" pad="4B"/>
<contactref element="CON0" pad="21"/>
</signal>
<signal name="AI6+">
<contactref element="J2" pad="7B"/>
<contactref element="CON0" pad="25"/>
</signal>
<signal name="AI7+">
<contactref element="J2" pad="10B"/>
<contactref element="CON0" pad="29"/>
</signal>
<signal name="AO0">
<contactref element="J13" pad="P$2"/>
<contactref element="CON0" pad="34"/>
</signal>
<signal name="AI0">
<contactref element="CON0" pad="1"/>
<contactref element="J11" pad="P$2"/>
</signal>
<signal name="AI1">
<contactref element="CON0" pad="5"/>
<contactref element="J11" pad="P$1"/>
</signal>
<signal name="AI2">
<contactref element="J12" pad="P$2"/>
<contactref element="CON0" pad="9"/>
</signal>
<signal name="AI3">
<contactref element="J12" pad="P$1"/>
<contactref element="CON0" pad="13"/>
</signal>
<signal name="AO1">
<contactref element="J13" pad="P$1"/>
<contactref element="CON0" pad="36"/>
</signal>
<signal name="AO2">
<contactref element="J14" pad="P$2"/>
<contactref element="CON0" pad="38"/>
</signal>
<signal name="AO3">
<contactref element="J14" pad="P$1"/>
<contactref element="CON0" pad="40"/>
</signal>
<signal name="AO4">
<contactref element="J15" pad="P$2"/>
<contactref element="CON0" pad="42"/>
</signal>
<signal name="AO5">
<contactref element="J15" pad="P$1"/>
<contactref element="CON0" pad="44"/>
</signal>
<signal name="AO6">
<contactref element="J16" pad="12B"/>
<contactref element="CON0" pad="46"/>
</signal>
<signal name="BLANKING">
<contactref element="J16" pad="13T"/>
<contactref element="CON0" pad="48"/>
</signal>
<signal name="DIOGND">
<contactref element="J16" pad="14T"/>
<contactref element="J16" pad="15T"/>
<contactref element="J16" pad="16T"/>
<contactref element="J16" pad="17T"/>
<contactref element="J16" pad="14B"/>
<contactref element="J16" pad="15B"/>
<contactref element="J16" pad="16B"/>
<contactref element="J16" pad="17B"/>
<contactref element="CON2" pad="16"/>
<contactref element="CON2" pad="14"/>
<contactref element="CON2" pad="12"/>
<contactref element="CON2" pad="10"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="CON1" pad="33"/>
<contactref element="CON1" pad="34"/>
<contactref element="CON1" pad="2"/>
<contactref element="J3" pad="P$4"/>
<contactref element="J3" pad="P$3"/>
<contactref element="CON1" pad="4"/>
<contactref element="J4" pad="P$4"/>
<contactref element="CON1" pad="6"/>
<contactref element="J4" pad="P$3"/>
<contactref element="CON1" pad="8"/>
<contactref element="J5" pad="P$4"/>
<contactref element="CON1" pad="10"/>
<contactref element="J5" pad="P$3"/>
<contactref element="CON1" pad="12"/>
<contactref element="J6" pad="P$4"/>
<contactref element="CON1" pad="14"/>
<contactref element="J6" pad="P$3"/>
<contactref element="CON1" pad="16"/>
<contactref element="J7" pad="P$4"/>
<contactref element="CON1" pad="18"/>
<contactref element="J7" pad="P$3"/>
<contactref element="CON1" pad="20"/>
<contactref element="J8" pad="P$4"/>
<contactref element="CON1" pad="22"/>
<contactref element="J8" pad="P$3"/>
<contactref element="CON1" pad="24"/>
<contactref element="J9" pad="P$4"/>
<contactref element="CON1" pad="26"/>
<contactref element="J9" pad="P$3"/>
<contactref element="CON1" pad="28"/>
<contactref element="J10" pad="P$4"/>
<contactref element="CON1" pad="30"/>
<contactref element="J10" pad="P$3"/>
<contactref element="CON1" pad="32"/>
<contactref element="CON2" pad="2"/>
<contactref element="CON2" pad="4"/>
<contactref element="CON2" pad="6"/>
<contactref element="CON2" pad="8"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="8"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="JP2" pad="9"/>
<contactref element="JP3" pad="9"/>
<contactref element="CON2" pad="18"/>
<contactref element="CON2" pad="20"/>
<contactref element="CON2" pad="22"/>
<contactref element="CON2" pad="24"/>
<contactref element="CON2" pad="26"/>
<contactref element="CON2" pad="28"/>
<contactref element="CON2" pad="30"/>
<contactref element="CON2" pad="32"/>
<contactref element="CON2" pad="33"/>
<contactref element="CON2" pad="34"/>
<contactref element="J2" pad="2T"/>
<contactref element="J2" pad="5T"/>
<contactref element="J2" pad="8T"/>
<contactref element="J2" pad="11T"/>
<contactref element="J2" pad="17T"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="DIO1">
<contactref element="J3" pad="P$1"/>
<contactref element="CON1" pad="3"/>
</signal>
<signal name="DIO2IN">
<contactref element="CON1" pad="5"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="DIO3">
<contactref element="CON1" pad="7"/>
<contactref element="J4" pad="P$1"/>
</signal>
<signal name="DIO4">
<contactref element="J5" pad="P$2"/>
<contactref element="CON1" pad="9"/>
</signal>
<signal name="DIO5">
<contactref element="J5" pad="P$1"/>
<contactref element="CON1" pad="11"/>
</signal>
<signal name="DIO6">
<contactref element="J6" pad="P$2"/>
<contactref element="CON1" pad="13"/>
</signal>
<signal name="DIO7">
<contactref element="J6" pad="P$1"/>
<contactref element="CON1" pad="15"/>
</signal>
<signal name="DIO8">
<contactref element="J7" pad="P$2"/>
<contactref element="CON1" pad="17"/>
</signal>
<signal name="DIO9">
<contactref element="J7" pad="P$1"/>
<contactref element="CON1" pad="19"/>
</signal>
<signal name="DIO10">
<contactref element="J8" pad="P$2"/>
<contactref element="CON1" pad="21"/>
</signal>
<signal name="DIO11">
<contactref element="J8" pad="P$1"/>
<contactref element="CON1" pad="23"/>
</signal>
<signal name="DIO12">
<contactref element="J9" pad="P$2"/>
<contactref element="CON1" pad="25"/>
</signal>
<signal name="DIO13">
<contactref element="J9" pad="P$1"/>
<contactref element="CON1" pad="27"/>
</signal>
<signal name="DIO14">
<contactref element="J10" pad="P$2"/>
<contactref element="CON1" pad="29"/>
</signal>
<signal name="DIO15">
<contactref element="J10" pad="P$1"/>
<contactref element="CON1" pad="31"/>
</signal>
<signal name="DIO7-2">
<contactref element="J16" pad="9T"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="DIO6-2">
<contactref element="J16" pad="10T"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="GPIO0">
<contactref element="J2" pad="1T"/>
<contactref element="CON2" pad="17"/>
</signal>
<signal name="GPIO1">
<contactref element="J2" pad="3T"/>
<contactref element="CON2" pad="19"/>
</signal>
<signal name="GPIO2">
<contactref element="J2" pad="4T"/>
<contactref element="CON2" pad="21"/>
</signal>
<signal name="GPIO3">
<contactref element="J2" pad="6T"/>
<contactref element="CON2" pad="23"/>
</signal>
<signal name="GPIO4">
<contactref element="J2" pad="7T"/>
<contactref element="CON2" pad="25"/>
</signal>
<signal name="GPIO5">
<contactref element="J2" pad="9T"/>
<contactref element="CON2" pad="27"/>
</signal>
<signal name="GPIO6">
<contactref element="J2" pad="10T"/>
<contactref element="CON2" pad="29"/>
</signal>
<signal name="GPIO7">
<contactref element="J2" pad="12T"/>
<contactref element="CON2" pad="31"/>
</signal>
<signal name="AI4-">
<contactref element="J2" pad="3B"/>
<contactref element="CON0" pad="18"/>
</signal>
<signal name="AI5-">
<contactref element="J2" pad="6B"/>
<contactref element="CON0" pad="22"/>
</signal>
<signal name="AI6-">
<contactref element="J2" pad="9N"/>
<contactref element="CON0" pad="26"/>
</signal>
<signal name="DIO5-2">
<contactref element="J16" pad="11T"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="DIO4-2">
<contactref element="J16" pad="12T"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="24VDC">
<contactref element="J16" pad="23T"/>
<contactref element="J16" pad="24T"/>
<contactref element="J16" pad="25T"/>
<contactref element="J16" pad="25B"/>
<contactref element="J16" pad="24B"/>
<contactref element="J16" pad="23B"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="AIGND">
<contactref element="J2" pad="2B"/>
<contactref element="J2" pad="5B"/>
<contactref element="J2" pad="8B"/>
<contactref element="J2" pad="11B"/>
<contactref element="J2" pad="17B"/>
<contactref element="CON0" pad="19"/>
<contactref element="CON0" pad="20"/>
<contactref element="CON0" pad="23"/>
<contactref element="CON0" pad="24"/>
<contactref element="CON0" pad="27"/>
<contactref element="CON0" pad="28"/>
<contactref element="CON0" pad="31"/>
<contactref element="CON0" pad="32"/>
<contactref element="CON0" pad="3"/>
<contactref element="CON0" pad="4"/>
<contactref element="CON0" pad="7"/>
<contactref element="CON0" pad="8"/>
<contactref element="CON0" pad="11"/>
<contactref element="CON0" pad="12"/>
<contactref element="CON0" pad="15"/>
<contactref element="CON0" pad="16"/>
<contactref element="SJ1" pad="2"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="+5VD">
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="C1" pad="1"/>
<contactref element="CON0" pad="49"/>
<contactref element="CON0" pad="50"/>
</signal>
<signal name="AOGND">
<contactref element="J13" pad="P$4"/>
<contactref element="J13" pad="P$3"/>
<contactref element="J14" pad="P$4"/>
<contactref element="J14" pad="P$3"/>
<contactref element="J15" pad="P$4"/>
<contactref element="J15" pad="P$3"/>
<contactref element="CON0" pad="33"/>
<contactref element="CON0" pad="35"/>
<contactref element="CON0" pad="43"/>
<contactref element="CON0" pad="41"/>
<contactref element="CON0" pad="39"/>
<contactref element="CON0" pad="37"/>
<contactref element="CON0" pad="45"/>
<contactref element="CON0" pad="47"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="CON2" pad="11"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="CON2" pad="9"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="DIO0IN">
<contactref element="CON1" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="DIO0">
<contactref element="J3" pad="P$2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="DIO2">
<contactref element="J4" pad="P$2"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="SPARE1">
<contactref element="CON2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SPARE2">
<contactref element="CON2" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SPARE3">
<contactref element="CON2" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="SPARE4">
<contactref element="CON2" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="TXOT">
<contactref element="J16" pad="1T"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RXIT">
<contactref element="J16" pad="2T"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="TXOB">
<contactref element="J16" pad="1B"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="RX1B">
<contactref element="J16" pad="2B"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="7"/>
<contactref element="CON2" pad="15"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="5"/>
<contactref element="CON2" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
