(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "RST-PB3")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "SCK-PB1")
  (net 6 "MisoPB0")
  (net 7 "PB0")
  (net 8 "PB1")
  (net 9 "PB2")
  (net 10 "Net-(R5-Pad1)")
  (net 11 "Net-(U1-PB2)")
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 175.5875 106.15 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "Untitled Field" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 180) (layer "F.SilkS"))
    (fp_text value "C_Small" (at 0 1.85 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 177.4 103.7)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -0.4 -2.825) (layer "F.SilkS"))
    (fp_text value "100k" (at -0.15 -1.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "RST-PB3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 166.6 114.8 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "180" (at -0.825 1.775) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "MisoPB0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 7 "PB0") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 173.45 114.55 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -4.175 0.05 180) (layer "F.SilkS"))
    (fp_text value "180" (at -3.1 0.025 -180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "SCK-PB1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "PB1") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 177.2 116.5 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -4.05 0.075 -180) (layer "F.SilkS"))
    (fp_text value "180" (at -2.975 0 -180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 11 "Net-(U1-PB2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 9 "PB2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 169.3 119.1 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.82) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 171.6 106.8 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 3.925 -0.15 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 2.95 -0.125 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "MisoPB0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "Net-(J1-Pad4)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:Button_4mm-4pad" (layer "F.Cu")
    (at 181.5 111.7 180)
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr smd)
    (fp_text reference "SW1" (at -0.025 0.125) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0.5 4.25) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "RST-PB3") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 2 -5 180) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R5-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd roundrect (at -2 -5 180) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "4" smd roundrect (at 2 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (at 181.55 107.5)
    (descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, ADC, SOT-23-6")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "ATtiny10-TS" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "MisoPB0") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "SCK-PB1") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1-PB2)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "5" smd roundrect (at 1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "RST-PB3") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:PROBE_PAD_0603" (layer "F.Cu")
    (at 162.9 114.7)
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr smd)
    (fp_text reference "H1" (at -0.25 1.475) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "PB0") (pinfunction "1") (pintype "input"))
  )
  (footprint "digikey-footprints:PROBE_PAD_0603" (layer "F.Cu")
    (at 177.25 119.8)
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr smd)
    (fp_text reference "H3" (at 0 1.325) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "PB2") (pinfunction "1") (pintype "input"))
  )
  (footprint "digikey-footprints:PROBE_PAD_0603" (layer "F.Cu")
    (at 173.4 118)
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr smd)
    (fp_text reference "H2" (at 0.025 1.35) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "PB1") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 165.45 105.1 -30)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33 150) (layer "F.SilkS"))
    (fp_text value "CONN-2x3" (at 1.27 7.41 150) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 60) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 330) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "MisoPB0") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 330) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 330) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "SCK-PB1") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 330) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 330) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "RST-PB3") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 330) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "++Sherms-Custom-Libs:CR2032-Battery-20mm-2pin-Dip" (layer "B.Cu")
    (at 173.3 122.4 180)
    (property "Sheetfile" "Attiny10-micro-Christmas-Tree-with-Sleep.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single-cell battery")
    (property "ki_keywords" "battery cell")
    (attr through_hole)
    (fp_text reference "BT1" (at 0.15 -1.925) (layer "F.Cu"))
    (fp_text value "Battery_Cell" (at -0.25 -3.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 21.25 180) (size 2.25 2.25) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 1.25 180) (size 2.25 2.25) (drill 1.25) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
  )
  (gr_circle (center 173.129492 112.3) (end 185.3 116.275)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Attiny10 Christmas Tree\nSherm Stebbins\n11-23-23 v4.2" (at 172.325 114.75) (layer "B.SilkS"))
  (gr_text "+" (at 170 101.05) (layer "F.SilkS"))
  (gr_text "-" (at 179 107.4) (layer "F.SilkS"))
  (gr_text "+" (at 183.95 107.4) (layer "F.SilkS"))
  (gr_text "NC" (at 178.55 110.2) (layer "F.SilkS"))
  (gr_text "+" (at 174.35 118.3) (layer "F.SilkS"))
  (gr_text "*" (at 174.3 120.53) (layer "F.SilkS"))
  (gr_text "-" (at 163.7 112.55) (layer "F.SilkS"))
  (gr_text "GND" (at 173.45 123.05) (layer "F.SilkS"))
  (gr_text "Rst" (at 161.525 111.425) (layer "F.SilkS"))
  (gr_text "." (at 178.69 106.48) (layer "F.SilkS"))
  (gr_text "*" (at 178.51 121.13) (layer "F.SilkS"))
  (gr_text "NC" (at 183.1 118.45) (layer "F.SilkS"))
  (gr_text "Miso" (at 166.975 102.45) (layer "F.SilkS"))
  (gr_text "+" (at 168.9 104.3) (layer "F.SilkS"))
  (gr_text "+" (at 171.65 101) (layer "Dwgs.User"))
  (gr_text "Tree1" (at 162.65 113.15) (layer "Dwgs.User"))
  (gr_text "Tree2" (at 173.15 122.75) (layer "Dwgs.User"))
  (gr_text "-" (at 171.75 121.05) (layer "Dwgs.User"))
  (gr_text "Tree3" (at 178 121.1) (layer "Dwgs.User"))
)
