(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 81)
    (zones 0)
    (modules 12)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.27 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.56 0.65)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V0)
  (net 2 "Net-(J6-Pad3)")
  (net 3 "Net-(J6-Pad2)")
  (net 4 "Net-(J6-Pad1)")
  (net 5 "Net-(C1-Pad2)")
  (net 6 "Net-(C1-Pad1)")
  (net 7 "Net-(J3-Pad3)")
  (net 8 "Net-(J3-Pad2)")
  (net 9 "Net-(J3-Pad1)")
  (net 10 "Net-(J4-Pad3)")
  (net 11 "Net-(J4-Pad2)")
  (net 12 "Net-(J4-Pad1)")
  (net 13 "Net-(J5-Pad3)")
  (net 14 "Net-(J5-Pad2)")
  (net 15 "Net-(J5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net +3V0)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
  )
  (net_class Minimum ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class Power ""
    (clearance 0.635)
    (trace_width 0.635)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.635)
    (diff_pair_gap 0.635)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 158.496 86.36 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 90) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 145.796 86.36 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TSOT-23-6_HandSoldering (layer F.Cu) (tedit 5A02FF57)
    (at 152.146 111.76 90)
    (descr "6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf")
    (tags "TSOT-23-6 MK06A TSOT-6 Hand-soldering")
    (attr smd)
    (fp_text reference Q2 (at -3.81 0.635 180) (layer F.SilkS))
    (fp_text value DMN2215UDM (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1.71 -0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (pad 5 smd rect (at 1.71 0 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J5-Pad3)"))
    (pad 4 smd rect (at 1.71 0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J6-Pad1)"))
    (pad 3 smd rect (at -1.71 0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J6-Pad2)"))
    (pad 2 smd rect (at -1.71 0 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J6-Pad3)"))
    (pad 1 smd rect (at -1.71 -0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 145.796 109.22 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 145.796 99.06 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TSOT-23-6_HandSoldering (layer F.Cu) (tedit 5A02FF57)
    (at 152.4 101.6 90)
    (descr "6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf")
    (tags "TSOT-23-6 MK06A TSOT-6 Hand-soldering")
    (attr smd)
    (fp_text reference Q1 (at -3.81 0.381 180) (layer F.SilkS))
    (fp_text value FDC6506P (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 1.71 -0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 5 smd rect (at 1.71 0 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (pad 4 smd rect (at 1.71 0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J4-Pad3)"))
    (pad 3 smd rect (at -1.71 0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at -1.71 0 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J4-Pad1)"))
    (pad 1 smd rect (at -1.71 -0.95 90) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 158.496 109.22 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 90) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 158.496 99.06 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x03_Female (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 152.654 83.439 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +3V0))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.654 91.694 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 152.654 94.234 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5E9FA901)
    (at 152.654 87.884 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at 0 -2.9 90) (layer F.SilkS))
    (fp_text value TPS709 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V0))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "TPS709 FDC6506P DMN2215UDM \nCriterion MS\n2020 04 21 A" (at 152.4 101.6 90) (layer B.SilkS))
  (gr_text S (at 148.336 114.3) (layer F.SilkS))
  (gr_text S (at 155.956 114.3) (layer F.SilkS))
  (gr_text G (at 155.956 111.76) (layer F.SilkS))
  (gr_text D (at 155.956 109.22) (layer F.SilkS))
  (gr_text G (at 148.336 111.76) (layer F.SilkS))
  (gr_text D (at 148.336 109.22) (layer F.SilkS))
  (gr_text S (at 155.956 104.14) (layer F.SilkS))
  (gr_text G (at 155.956 101.6) (layer F.SilkS))
  (gr_text D (at 155.956 99.06) (layer F.SilkS))
  (gr_text S (at 148.336 104.14) (layer F.SilkS))
  (gr_text G (at 148.336 101.6) (layer F.SilkS))
  (gr_text D (at 148.336 99.06) (layer F.SilkS))
  (gr_text GND (at 158.496 83.82) (layer F.SilkS))
  (gr_text 18V (at 145.796 82.55) (layer F.SilkS))
  (gr_text GND (at 145.796 83.82) (layer F.SilkS))
  (gr_text 3V0 (at 158.496 82.55) (layer F.SilkS))
  (gr_text NMOS (at 152.146 107.95) (layer F.SilkS))
  (gr_text PMOS (at 152.146 97.79) (layer F.SilkS))
  (gr_line (start 143.256 80.01) (end 143.256 116.84) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 161.036 80.01) (end 161.036 116.84) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 161.036 116.84) (end 143.256 116.84) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 143.256 80.01) (end 161.036 80.01) (layer Edge.Cuts) (width 0.254))
  (zone (net 6) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.781 96.52) (xy 152.781 81.28) (xy 153.416 80.645) (xy 155.321 80.645) (xy 155.956 81.28)
        (xy 155.956 95.885) (xy 155.321 96.52) (xy 153.416 96.52) (xy 152.781 95.885)
      )
    )
  )
)
