(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 69.5 65)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(H2-Pad1)")
	(net 2 "/S")
	(net 3 "/2")
	(net 4 "/1")
	(net 5 "/5")
	(net 6 "/4")
	(net 7 "/3")
	(footprint "TPW-Connectors:DIN-5-SHIELD"
		(locked yes)
		(layer "F.Cu")
		(at 50.112501 65 90)
		(property "Reference" "J1"
			(at 0 15.999999 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DIN 5"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 -0.799999 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5-pin DIN connector (5-pin DIN-5 stereo)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Kycon"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "KCDX-5S-S2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "5212044-1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "https://www.mouser.com/ProductDetail/Kycon/KCDX-5S-S2?qs=Hyo%2FOIDW0pNotQHJom5wpw%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "InCart" "Y"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIN*")
		(sheetname "/")
		(sheetfile "DIN-5-180_Breakout.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -7.5 12.5 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 12.5 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 7.5 12.5 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -5 15 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 5 15 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/5")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at -5 2.5 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/S")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at -2.5 2.5 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/S")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at 2.5 2.5 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/S")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at 5 2.5 90)
			(size 2.4 2.4)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD_USER_3DMODEL_DIR}/TE_Connectivity.3dshapes/c-5212044-1-1-3d.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 180)
			)
		)
	)
	(footprint "TerminalBlock_RND:TerminalBlock_RND_205-00236_1x06_P5.08mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 77.542501 77.7 90)
		(descr "terminal block RND 205-00236, 6 pins, pitch 5.08mm, size 30.5x8.45mm, drill diameter 1.1mm, pad diameter 2.1mm, http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00232_DB_EN.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_RND")
		(tags "THT terminal block RND 205-00236 pitch 5.08mm size 30.5x8.45mm drill 1.1mm pad 2.1mm")
		(property "Reference" "J3"
			(at 12.700001 -5.52 90)
			(layer "F.SilkS")
		)
		(property "Value" "PTH_1x06_5.08mm"
			(at 12.7 5.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "DIN-5-180_Breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 12.700001 -5.52 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.119048)
			(net 4 "/1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.079999 0 90)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.16 0 90)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.24 0 90)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/4")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.32 0 90)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/5")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25.4 0 90)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/S")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00236_1x06_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 69.5 71.35 180)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "PTH_1x06_2.54mm"
			(at 0 15.08 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "DIN-5-180_Breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 4 "/1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.079999 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/4")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/5")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/S")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 69.5 52.5 90)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "H1"
			(at 0 -3.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "DIN-5-180_Breakout.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/S")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 69.5 77.5 90)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "H2"
			(at 0 -3.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "DIN-5-180_Breakout.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(H2-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TPW-Decorative:sig-wlx"
		(layer "B.Cu")
		(at 64.7 53.5 -90)
		(property "Reference" "G1"
			(at 0 1.3 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "WLX"
			(at 0 -2.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TPW-Decorative:sig-wlx")
		(sheetname "/")
		(sheetfile "DIN-5-180_Breakout.kicad_sch")
		(attr exclude_from_pos_files)
		(embedded_fonts no)
	)
	(footprint "TPW-Decorative:webster-face"
		(layer "B.Cu")
		(at 59.8 53.6 -90)
		(property "Reference" "G2"
			(at 0 3.7 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "WebsterFace"
			(at 0 -4.7 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "DIN-5-180_Breakout.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
	)
	(gr_line
		(start 50 51)
		(end 50 79)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 50 51)
		(mid 50.585786 49.585786)
		(end 52 49)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 81 49)
		(mid 81.707107 49.292893)
		(end 82 50)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 52 81)
		(end 81 81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82 80)
		(end 82 50)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 52 81)
		(mid 50.585786 80.414214)
		(end 50 79)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 52 49)
		(end 81 49)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82 80)
		(mid 81.707107 80.707107)
		(end 81 81)
		(layer "Edge.Cuts")
	)
	(gr_text "6/S"
		(at 59.975 51.9825 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3"
		(at 75.9 66.9 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 95 70 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 75.9 76.6 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 99.5 72 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 75.9 71.9 0)
		(layer "F.SilkS")
	)
	(gr_text "FRONT"
		(at 99.5 75.5 0)
		(layer "F.SilkS")
	)
	(gr_text "S"
		(at 107 56.5 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 106.5 66 0)
		(layer "F.SilkS")
	)
	(gr_text "Pin"
		(at 59.34 78.335 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 104 70 0)
		(layer "F.SilkS")
	)
	(gr_text "Pin"
		(at 56.165 52.3 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 75.9 61.9 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 75.9 56.6 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 92.5 66 0)
		(layer "F.SilkS")
	)
	(gr_text "S"
		(at 75.9 51.8 0)
		(layer "F.SilkS")
	)
	(gr_text "SOCKET"
		(at 99.5 54.75 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 61.5625 78.0175 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "1"
		(at 72.675 71.35 90)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 80.93 67.54 90)
		(layer "B.SilkS")
	)
	(gr_text "2025"
		(at 65.6 74 90)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 61 60.999999 90)
		(layer "B.SilkS")
	)
	(gr_text "SOCKET"
		(at 56.5 56 90)
		(layer "B.SilkS")
	)
	(gr_text "4"
		(at 80.93 62.46 90)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 63.7 62.4 90)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 80.93 77.7 90)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 61 69.000001 90)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 80.93 57.38 90)
		(layer "B.SilkS")
	)
	(gr_text "S"
		(at 72.675 58.65 90)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 72.675 66.27 90)
		(layer "B.SilkS")
	)
	(gr_text "4"
		(at 72.675 63.73 90)
		(layer "B.SilkS")
	)
	(gr_text "FRONT"
		(at 54 73.5 90)
		(layer "B.SilkS")
	)
	(gr_text "2"
		(at 72.675 68.81 90)
		(layer "B.SilkS")
	)
	(gr_text "4"
		(at 63.5 67.7 90)
		(layer "B.SilkS")
	)
	(gr_text "2"
		(at 64.7 65 90)
		(layer "B.SilkS")
	)
	(gr_text "TPW-CGDDINS-BOB05"
		(at 76 65 90)
		(layer "B.SilkS")
	)
	(gr_text "2"
		(at 80.93 72.62 90)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 72.675 61.19 90)
		(layer "B.SilkS")
	)
	(gr_text "S"
		(at 55.6 65 90)
		(layer "B.SilkS")
	)
	(gr_text "S"
		(at 80.93 52.3 90)
		(layer "B.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 50 47) (xy 82 47)
		)
		(height -2)
		(orientation 0)
		(format
			(prefix "")
			(suffix "mm")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "32mm"
			(at 66 43.85 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 48 49) (xy 48 81)
		)
		(height -2)
		(orientation 1)
		(format
			(prefix "")
			(suffix "mm")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "32mm"
			(at 44.85 65 90)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 2)
		(net_name "/S")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 49 48) (xy 83 48) (xy 83 82) (xy 49 82)
			)
		)
	)
	(embedded_fonts no)
)
