<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="69.85" x2="25.38" y2="69.85" width="0" layer="20"/>
<wire x1="25.38" y1="69.85" x2="25.38" y2="100" width="0" layer="20"/>
<wire x1="25.38" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="69.85" width="0" layer="20"/>
<text>3v3</text>
<text>GND</text>
<text>PA16</text>
<text>PA17</text>
<text>PA18</text>
<text>PA19</text>
<text>PA07</text>
<text>PA15</text>
<text>PA14</text>
<text>ATSAMR21B18</text>
<text>v0.1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-PTH-1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 2x5 ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;tDoc (51) layer border represents maximum dimensions of plastic housing.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://portal.fciconnect.com/Comergent//fci/drawing/20021111.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="rtotte">
<packages>
<package name="ATSAMR21B18">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="1X09" value=""/>
<element name="U$1" library="rtotte" package="ATSAMR21B18" value="ATSAMR21B18"/>
<element name="J1" library="SparkFun-Connectors" package="2X5-PTH-1.27MM" value="CORTEX_DEBUG_PTH"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="VCC"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="PA30"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="PA31"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="PA16"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="4"/>
<contactref element="U$1" pad="PA17"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="PA18"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="PA19"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="PA07"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="RESETN"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="PA15"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="PA14"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
