(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 49)
    (no_connects 0)
    (area 93.142999 52.629999 194.893001 141.807001)
    (thickness 1.6)
    (drawings 7)
    (tracks 115)
    (zones 0)
    (modules 38)
    (nets 12)
  )
  (page USLetter)
  (title_block
    (title "Dyna MKIII Capboard")
    (rev 1.0)
    (company "SDS Labs")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 2.54)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 1.905)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C11-Pad2)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C7-Pad2)")
  (net 8 "Net-(C10-Pad1)")
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(D1-Pad2)")
  (net 11 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA203CF)
    (at 110.49 110.363 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C1 (at -5.715 -10.795 180) (layer F.SilkS))
    (fp_text value "68uF 450V" (at -0.254 -4.191 180) (layer F.SilkS))
    (fp_text user %R (at -5.461 10.795 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA20570)
    (at 100.457 70.104)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C2 (at 15.875 -10.795) (layer F.SilkS))
    (fp_text value "68uF 450V" (at 0 4.572) (layer F.SilkS))
    (fp_text user %R (at 14.224 -10.795) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L18_W5_P15 (layer F.Cu) (tedit 5AA204E3)
    (at 116.078 90.297 180)
    (descr "Film Capacitor Length 18mm x Width 5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.667 0.127 180) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 9.144 0 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA203D4)
    (at 136.271 110.363 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C4 (at 15.748 -11.049 180) (layer F.SilkS))
    (fp_text value "68uF 450V" (at -0.254 -3.937 180) (layer F.SilkS))
    (fp_text user %R (at 14.859 10.922 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA20576)
    (at 126.238 70.104)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C5 (at -5.842 -10.795) (layer F.SilkS))
    (fp_text value "68uF 450V" (at -0.127 4.318) (layer F.SilkS))
    (fp_text user %R (at -5.334 -10.795) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L18_W5_P15 (layer F.Cu) (tedit 5AA204F1)
    (at 142.24 90.17 180)
    (descr "Film Capacitor Length 18mm x Width 5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 2.921 0 180) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 9.398 0 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA203D9)
    (at 161.925 110.363 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C7 (at -6.223 -11.049 180) (layer F.SilkS))
    (fp_text value "68uF 450V" (at -0.254 -4.191 180) (layer F.SilkS))
    (fp_text user %R (at -5.207 10.668 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA2057B)
    (at 152.019 70.104)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C8 (at 15.748 -10.668) (layer F.SilkS))
    (fp_text value "68uF 450V" (at 0 4.191) (layer F.SilkS))
    (fp_text user %R (at 15.494 -10.287) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L18_W5_P15 (layer F.Cu) (tedit 5AA20501)
    (at 167.259 90.297 180)
    (descr "Film Capacitor Length 18mm x Width 5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 2.667 -0.127 180) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 9.144 0 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA203DE)
    (at 187.579 110.363 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C10 (at 14.859 -11.176 180) (layer F.SilkS))
    (fp_text value "68uF 450V" (at -0.508 -4.318 180) (layer F.SilkS))
    (fp_text user %R (at 15.113 10.668 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D25.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5AA20580)
    (at 177.8 70.104)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=25mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 25mm Electrolytic Capacitor")
    (fp_text reference C11 (at -5.715 -10.668) (layer F.SilkS))
    (fp_text value "68uF 450V" (at -0.508 4.191) (layer F.SilkS))
    (fp_text user %R (at -4.953 -10.287) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D25.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L18_W5_P15 (layer F.Cu) (tedit 5AA20514)
    (at 192.786 90.424 180)
    (descr "Film Capacitor Length 18mm x Width 5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C12 (at 2.921 0.127 180) (layer F.SilkS))
    (fp_text value "0.1uF 630V" (at 9.525 0 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 15 0 180) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5AA2037D)
    (at 117.729 133.731 180)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D1 (at 7.493 -0.254 180) (layer F.SilkS))
    (fp_text value D (at 7.62 3.66 180) (layer F.Fab) hide)
    (fp_text user %R (at 7.62 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 180) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5AA20381)
    (at 117.729 127.381 180)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.747 0 180) (layer F.SilkS))
    (fp_text value D (at 7.62 3.66 180) (layer F.Fab) hide)
    (fp_text user %R (at 7.874 0.889 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 180) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA2049D)
    (at 111.379 95.504 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 4.191 0.127 180) (layer F.SilkS))
    (fp_text value 330K (at 8.509 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA2054D)
    (at 98.806 84.963)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 9.017 0) (layer F.SilkS))
    (fp_text value 330K (at 4.318 0.127) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5AA203E9)
    (at 141.986 127.254 180)
    (descr "Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0516 series Axial Horizontal pin pitch 20.32mm 2W length 15.5mm diameter 5mm")
    (fp_text reference R3 (at 10.16 -3.56 180) (layer F.SilkS) hide)
    (fp_text value Choke (at 9.906 0.254 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA204AB)
    (at 137.668 95.504 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R4 (at 3.937 0 180) (layer F.SilkS))
    (fp_text value 330K (at 8.128 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA20540)
    (at 125.095 84.963)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R5 (at 9.017 0.127) (layer F.SilkS))
    (fp_text value 330K (at 4.699 0.127) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5AA203ED)
    (at 167.005 127.254 180)
    (descr "Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0516 series Axial Horizontal pin pitch 20.32mm 2W length 15.5mm diameter 5mm")
    (fp_text reference R6 (at 10.16 -3.56 180) (layer F.SilkS) hide)
    (fp_text value "6800 2W" (at 9.906 0.127 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA204C0)
    (at 163.195 95.504 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R7 (at 3.937 -0.127 180) (layer F.SilkS))
    (fp_text value 330K (at 8.255 -0.127 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA20532)
    (at 150.622 84.963)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R8 (at 9.017 0.127) (layer F.SilkS))
    (fp_text value 330K (at 4.191 0.127) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5AA203F6)
    (at 192.786 127.254 180)
    (descr "Resistor, Axial_DIN0516 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=15.5*5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0516 series Axial Horizontal pin pitch 20.32mm 2W length 15.5mm diameter 5mm")
    (fp_text reference R9 (at 9.906 -1.016 180) (layer F.SilkS) hide)
    (fp_text value R (at 10.033 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0516_L15.5mm_D5.0mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA204CD)
    (at 188.976 95.504 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R10 (at 3.683 0 180) (layer F.SilkS))
    (fp_text value 330K (at 8.128 -0.127 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5AA20521)
    (at 176.53 84.963)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R11 (at 8.89 0) (layer F.SilkS))
    (fp_text value 330K (at 4.445 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA203C2)
    (at 98.044 133.604)
    (fp_text reference J1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Trans. B+ (RED)" (at 3.81 5.207) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA20388)
    (at 98.044 127.508)
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Trans. B+ (RED)" (at -3.429 3.302 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA20363)
    (at 123.317 133.731)
    (fp_text reference J3 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Rect Cathode (2 or 8)" (at 2.921 5.461) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA2035F)
    (at 128.27 133.731)
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Choke 1" (at -2.667 3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA2035B)
    (at 155.829 133.858)
    (fp_text reference J5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Choke 2" (at 2.286 3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA20356)
    (at 160.655 133.858)
    (fp_text reference J6 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Output Center Tap (Red)" (at -1.397 5.207) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA20651)
    (at 172.466 133.604)
    (fp_text reference J7 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "To Pin 5" (at 2.667 4.064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA20653)
    (at 191.643 133.477)
    (fp_text reference J8 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "To Pin 6" (at -2.667 4.064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 8 "Net-(C10-Pad1)"))
  )
  (module sdsLogos:sdsLabs-large-fSilk (layer F.Cu) (tedit 5A94A1E6)
    (at 145.542 89.027 90)
    (fp_text reference G*** (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -5.08 90) (layer F.SilkS) hide)
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA206C2)
    (at 96.774 56.642)
    (fp_text reference J9 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value GND (at 5.207 -0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 5AA2058B)
    (at 191.262 56.261)
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value GND (at -4.953 -0.381) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 3 "Net-(C11-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_5mm_Pad (layer F.Cu) (tedit 5AA20603)
    (at 143.764 137.922)
    (descr "Mounting Hole 5mm")
    (tags "mounting hole 5mm")
    (fp_text reference REF** (at 0 -6) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm_Pad (at 0 6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_5mm_Pad (layer F.Cu) (tedit 5AA20608)
    (at 144.018 56.642)
    (descr "Mounting Hole 5mm")
    (tags "mounting hole 5mm")
    (fp_text reference REF** (at 0 -6) (layer F.SilkS) hide)
    (fp_text value MountingHole_5mm_Pad (at 0 6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 5) (layers *.Cu *.Mask))
  )
  (gr_text "Dyna MKIII Capboard" (at 120.777 55.245) (layer F.SilkS))
  (gr_circle (center 144.018 56.642) (end 146.05 56.642) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 144.018 137.795) (end 146.05 137.795) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.472 52.832) (end 93.472 141.478) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.818 52.832) (end 93.472 52.832) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.818 141.478) (end 194.818 52.832) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.472 141.478) (end 194.818 141.478) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name "Net-(C11-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.818 65.786) (xy 93.218 65.786) (xy 93.218 52.959) (xy 194.818 52.959)
      )
    )
  )
)
