(kicad_pcb (version 20170123) (host pcbnew "(2017-08-02 revision 9760937)-master")
  (general
    (thickness 1.6)
    (drawings 951)
    (tracks 1468)
    (zones 0)
    (modules 50)
    (nets 188)
  )
  (page A4)
  (title_block
    (title "PocketBeagle KiCAD")
    (date 2017-08-14)
    (comment 1 "Prototyped by: GHI Electronics, LLC")
    (comment 2 "Converted to KiCAD: QWERTY Embedded Design, LLC")
  )
  (layers
    (0 Top signal)
    (1 VDD signal)
    (2 DigitalGND signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.27 1.27)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x0103c_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory plots))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VDD_3V3A)
  (net 3 VDD_1V8)
  (net 4 VDD_RTC)
  (net 5 USB_DC)
  (net 6 VDD_5V)
  (net 7 VDD_3V3B)
  (net 8 VDD_3V3AUX)
  (net 9 SYS_5V)
  (net 10 CGND)
  (net 11 VIN.BAT)
  (net 12 VBUS.RAW)
  (net 13 "/(U1.P12)PWM1A")
  (net 14 "/(U1.T16)")
  (net 15 "/(U1.P5)GPIO-0.23")
  (net 16 "/(U1.R15)")
  (net 17 "/(U1.P15)UART4.RX")
  (net 18 "/(U1.T15)")
  (net 19 "/(U1.R16)UART4.TX")
  (net 20 "/(U1.N14)")
  (net 21 "/(U1.B11)I2C1.SCL")
  (net 22 "/(U1.R13)")
  (net 23 "/(U1.A11)I2C1.SDA")
  (net 24 "/(U1.T11)PWR.BTN")
  (net 25 /BAT.TEMP)
  (net 26 "/(U1.T7)")
  (net 27 "/(U1.P7)PRU-0.15")
  (net 28 "/(U1.T5)")
  (net 29 "/(U1.R7)")
  (net 30 "/(U1.T6)PRU-0.14")
  (net 31 "/(U1.P6)")
  (net 32 "/(U1.C13)SPI1.MOSI")
  (net 33 "/(U1.R11)RESET#")
  (net 34 "/(U1.C12)SPI1.MISO")
  (net 35 "/(U1.C3)PRU-0.6")
  (net 36 "/(U1.C5)SPI1.CLK")
  (net 37 "/(U1.B1)PRU-0.3")
  (net 38 "/(U1.A4)SPI1.CS")
  (net 39 "/(U1.B2)PRU-0.2")
  (net 40 "/(U1.R6)")
  (net 41 "/(U1.B3)PRU-0.5")
  (net 42 "/(U1.F3)AIN5~3.3V")
  (net 43 "/(U1.N13)AIN7~1.8V")
  (net 44 "/(U1.A1)PWM0A")
  (net 45 "/(U1.F1)")
  (net 46 "/(U1.R5)GPIO-0.26")
  (net 47 "/(U1.A2)PRU-0.1")
  (net 48 "/(U1.A12)UART0.RX")
  (net 49 "/(U1.A3)PRU-0.4")
  (net 50 "/(U1.B12)UART0.TX")
  (net 51 "/(U1.C4)PRU-0.7")
  (net 52 "/(U1.A10)I2C2.SCL")
  (net 53 "/(U1.C7)AIN4~1.8V")
  (net 54 "/(U1.B10)I2C2.SDA")
  (net 55 "/(U1.C6)AIN3~1.8V")
  (net 56 "/(U1.B6)AIN2~1.8V")
  (net 57 "/(U1.B8)AIN1~1.8V")
  (net 58 "/(U1.B4)PRU-0.16")
  (net 59 "/(U1.A8)AIN0~1.8V")
  (net 60 "/(U1.B7)VREF+")
  (net 61 "/(U1.B9)VREF-")
  (net 62 "/(U1.L14)USB1.ID")
  (net 63 "/(U1.B14)SPI0.MOSI")
  (net 64 "/(U1.L15)USB1.D+")
  (net 65 "/(U1.B13)SPI0.MISO")
  (net 66 "/(U1.L16)USB1.D-")
  (net 67 "/(U1.A13)SPI0.CLK")
  (net 68 "/(U1.A14)SPI0.CS")
  (net 69 "/(U1.M15)USB1.VBUS")
  (net 70 "/(U1.E1)")
  (net 71 "/(U1.M14)USB1.DRVVBUS")
  (net 72 "/(U1.F2)AIN6~3.3V")
  (net 73 "Net-(U3-Pad5)")
  (net 74 "/(U1.K14)USBC.ID")
  (net 75 "/(U1.K16)USBC.D-")
  (net 76 "/(U1.K15)USBC.D+")
  (net 77 /PMIC_PGOOD)
  (net 78 "/(U1.K3)LCD.D9.G6")
  (net 79 "/(U1.K2)LCD.D10.G7")
  (net 80 "/(U1.J1)LCD.D8.G5")
  (net 81 "/(U1.K1)LCD.D11.R3")
  (net 82 /N$1)
  (net 83 /N$5)
  (net 84 /N$2)
  (net 85 /N$6)
  (net 86 "/(U1.C9)AIN6~1.8V")
  (net 87 "/(U1.C8)AIN5~1.8V")
  (net 88 "/(U1.L2)LCD.D13.R5")
  (net 89 "/(U1.L1)LCD.D14.R6")
  (net 90 "/(U1.L3)LCD.D12.R4")
  (net 91 "/(U1.M3)LCD.D15.R7")
  (net 92 "/(U1.H1)LCD.D5.G2")
  (net 93 "/(U1.J3)LCD.D6.G3")
  (net 94 "/(U1.H2)LCD.D4.B7")
  (net 95 "/(U1.J2)LCD.D7.G4")
  (net 96 "/(U1.G2)LCD.D1.B4")
  (net 97 "/(U1.G1)LCD.D2.B5")
  (net 98 "/(U1.G3)LCD.D0.B3")
  (net 99 "/(U1.H3)LCD.D3.B6")
  (net 100 "/(U1.B16)MMC0.CMD")
  (net 101 "/(U1.C15)MMC0.D3")
  (net 102 "/(U1.B15)MMC0.CLK")
  (net 103 "/(U1.C16)MMC0.D2")
  (net 104 "/(U1.C14)MMC0.CD")
  (net 105 "/(U1.A15)MMC0.D1")
  (net 106 "Net-(R11-Pad8)")
  (net 107 "/(U1.A16)MMC0.D0")
  (net 108 "Net-(R11-Pad1)")
  (net 109 "/(U1.T14)USR1")
  (net 110 "Net-(U1-PadT13)")
  (net 111 "Net-(U1-PadT12)")
  (net 112 "Net-(U1-PadT4)")
  (net 113 "Net-(U1-PadT3)")
  (net 114 "Net-(U1-PadT2)")
  (net 115 "Net-(U1-PadT1)")
  (net 116 "/(U1.R14)USR2")
  (net 117 "Net-(U1-PadR12)")
  (net 118 "Net-(U1-PadR4)")
  (net 119 "Net-(U1-PadR3)")
  (net 120 "Net-(U1-PadR2)")
  (net 121 "Net-(U1-PadR1)")
  (net 122 /OSC.IN)
  (net 123 "/(U1.P14)USR3")
  (net 124 "/(U1.P13)USR0")
  (net 125 "Net-(U1-PadP4)")
  (net 126 "Net-(U1-PadP3)")
  (net 127 "Net-(U1-PadP2)")
  (net 128 "Net-(U1-PadP1)")
  (net 129 /OSC.OUT)
  (net 130 /OSC.GND)
  (net 131 /N$27)
  (net 132 /N$24)
  (net 133 "/(U1.M2)EEPROM.WP")
  (net 134 "Net-(U1-PadN2)")
  (net 135 "Net-(U1-PadN1)")
  (net 136 /N$22)
  (net 137 "Net-(U1-PadM13)")
  (net 138 /N$25)
  (net 139 "Net-(U1-PadM1)")
  (net 140 "Net-(U1-PadL13)")
  (net 141 "Net-(U1-PadK13)")
  (net 142 "Net-(U1-PadK4)")
  (net 143 "Net-(U1-PadJ15)")
  (net 144 "Net-(U1-PadJ14)")
  (net 145 "Net-(U1-PadJ6)")
  (net 146 "Net-(U1-PadH16)")
  (net 147 "Net-(U1-PadH15)")
  (net 148 "Net-(U1-PadH14)")
  (net 149 "Net-(U1-PadH6)")
  (net 150 "Net-(U1-PadG16)")
  (net 151 "Net-(U1-PadG15)")
  (net 152 "Net-(U1-PadG14)")
  (net 153 /N$11)
  (net 154 /N$9)
  (net 155 "Net-(U1-PadF16)")
  (net 156 "Net-(U1-PadF15)")
  (net 157 "Net-(U1-PadF14)")
  (net 158 /N$10)
  (net 159 /N$7)
  (net 160 "Net-(U1-PadE16)")
  (net 161 "Net-(U1-PadE15)")
  (net 162 "Net-(U1-PadE14)")
  (net 163 "Net-(U1-PadE13)")
  (net 164 /N$26)
  (net 165 /JTAG_EMU1)
  (net 166 /JTAG_EMU0)
  (net 167 "Net-(U1-PadD16)")
  (net 168 "Net-(U1-PadD15)")
  (net 169 "Net-(U1-PadD14)")
  (net 170 "Net-(U1-PadD13)")
  (net 171 "Net-(U1-PadD12)")
  (net 172 /N$31)
  (net 173 /N$32)
  (net 174 /N$12)
  (net 175 "Net-(U1-PadD5)")
  (net 176 /JTAG_TRST#)
  (net 177 /JTAG_TMS)
  (net 178 /JTAG_TCK)
  (net 179 /JTAG_TDO)
  (net 180 /JTAG_TDI)
  (net 181 "Net-(U1-PadB5)")
  (net 182 "Net-(U1-PadA6)")
  (net 183 "Net-(U1-PadA5)")
  (net 184 "Net-(FUD3-PadP$1)")
  (net 185 "Net-(FUD2-PadP$1)")
  (net 186 "Net-(FUD1-PadP$1)")
  (net 187 /N$4)
  (net_class Default "This is the default net class."
    (clearance 0)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/(U1.A1)PWM0A")
    (add_net "/(U1.A10)I2C2.SCL")
    (add_net "/(U1.A11)I2C1.SDA")
    (add_net "/(U1.A12)UART0.RX")
    (add_net "/(U1.A13)SPI0.CLK")
    (add_net "/(U1.A14)SPI0.CS")
    (add_net "/(U1.A15)MMC0.D1")
    (add_net "/(U1.A16)MMC0.D0")
    (add_net "/(U1.A2)PRU-0.1")
    (add_net "/(U1.A3)PRU-0.4")
    (add_net "/(U1.A4)SPI1.CS")
    (add_net "/(U1.A8)AIN0~1.8V")
    (add_net "/(U1.B1)PRU-0.3")
    (add_net "/(U1.B10)I2C2.SDA")
    (add_net "/(U1.B11)I2C1.SCL")
    (add_net "/(U1.B12)UART0.TX")
    (add_net "/(U1.B13)SPI0.MISO")
    (add_net "/(U1.B14)SPI0.MOSI")
    (add_net "/(U1.B15)MMC0.CLK")
    (add_net "/(U1.B16)MMC0.CMD")
    (add_net "/(U1.B2)PRU-0.2")
    (add_net "/(U1.B3)PRU-0.5")
    (add_net "/(U1.B4)PRU-0.16")
    (add_net "/(U1.B6)AIN2~1.8V")
    (add_net "/(U1.B7)VREF+")
    (add_net "/(U1.B8)AIN1~1.8V")
    (add_net "/(U1.B9)VREF-")
    (add_net "/(U1.C12)SPI1.MISO")
    (add_net "/(U1.C13)SPI1.MOSI")
    (add_net "/(U1.C14)MMC0.CD")
    (add_net "/(U1.C15)MMC0.D3")
    (add_net "/(U1.C16)MMC0.D2")
    (add_net "/(U1.C3)PRU-0.6")
    (add_net "/(U1.C4)PRU-0.7")
    (add_net "/(U1.C5)SPI1.CLK")
    (add_net "/(U1.C6)AIN3~1.8V")
    (add_net "/(U1.C7)AIN4~1.8V")
    (add_net "/(U1.C8)AIN5~1.8V")
    (add_net "/(U1.C9)AIN6~1.8V")
    (add_net "/(U1.E1)")
    (add_net "/(U1.F1)")
    (add_net "/(U1.F2)AIN6~3.3V")
    (add_net "/(U1.F3)AIN5~3.3V")
    (add_net "/(U1.G1)LCD.D2.B5")
    (add_net "/(U1.G2)LCD.D1.B4")
    (add_net "/(U1.G3)LCD.D0.B3")
    (add_net "/(U1.H1)LCD.D5.G2")
    (add_net "/(U1.H2)LCD.D4.B7")
    (add_net "/(U1.H3)LCD.D3.B6")
    (add_net "/(U1.J1)LCD.D8.G5")
    (add_net "/(U1.J2)LCD.D7.G4")
    (add_net "/(U1.J3)LCD.D6.G3")
    (add_net "/(U1.K1)LCD.D11.R3")
    (add_net "/(U1.K14)USBC.ID")
    (add_net "/(U1.K15)USBC.D+")
    (add_net "/(U1.K16)USBC.D-")
    (add_net "/(U1.K2)LCD.D10.G7")
    (add_net "/(U1.K3)LCD.D9.G6")
    (add_net "/(U1.L1)LCD.D14.R6")
    (add_net "/(U1.L14)USB1.ID")
    (add_net "/(U1.L15)USB1.D+")
    (add_net "/(U1.L16)USB1.D-")
    (add_net "/(U1.L2)LCD.D13.R5")
    (add_net "/(U1.L3)LCD.D12.R4")
    (add_net "/(U1.M14)USB1.DRVVBUS")
    (add_net "/(U1.M15)USB1.VBUS")
    (add_net "/(U1.M2)EEPROM.WP")
    (add_net "/(U1.M3)LCD.D15.R7")
    (add_net "/(U1.N13)AIN7~1.8V")
    (add_net "/(U1.N14)")
    (add_net "/(U1.P12)PWM1A")
    (add_net "/(U1.P13)USR0")
    (add_net "/(U1.P14)USR3")
    (add_net "/(U1.P15)UART4.RX")
    (add_net "/(U1.P5)GPIO-0.23")
    (add_net "/(U1.P6)")
    (add_net "/(U1.P7)PRU-0.15")
    (add_net "/(U1.R11)RESET#")
    (add_net "/(U1.R13)")
    (add_net "/(U1.R14)USR2")
    (add_net "/(U1.R15)")
    (add_net "/(U1.R16)UART4.TX")
    (add_net "/(U1.R5)GPIO-0.26")
    (add_net "/(U1.R6)")
    (add_net "/(U1.R7)")
    (add_net "/(U1.T11)PWR.BTN")
    (add_net "/(U1.T14)USR1")
    (add_net "/(U1.T15)")
    (add_net "/(U1.T16)")
    (add_net "/(U1.T5)")
    (add_net "/(U1.T6)PRU-0.14")
    (add_net "/(U1.T7)")
    (add_net /BAT.TEMP)
    (add_net /JTAG_EMU0)
    (add_net /JTAG_EMU1)
    (add_net /JTAG_TCK)
    (add_net /JTAG_TDI)
    (add_net /JTAG_TDO)
    (add_net /JTAG_TMS)
    (add_net /JTAG_TRST#)
    (add_net /N$1)
    (add_net /N$10)
    (add_net /N$11)
    (add_net /N$12)
    (add_net /N$2)
    (add_net /N$22)
    (add_net /N$24)
    (add_net /N$25)
    (add_net /N$26)
    (add_net /N$27)
    (add_net /N$31)
    (add_net /N$32)
    (add_net /N$4)
    (add_net /N$5)
    (add_net /N$6)
    (add_net /N$7)
    (add_net /N$9)
    (add_net /OSC.GND)
    (add_net /OSC.IN)
    (add_net /OSC.OUT)
    (add_net /PMIC_PGOOD)
    (add_net CGND)
    (add_net GND)
    (add_net "Net-(FUD1-PadP$1)")
    (add_net "Net-(FUD2-PadP$1)")
    (add_net "Net-(FUD3-PadP$1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R11-Pad8)")
    (add_net "Net-(U1-PadA5)")
    (add_net "Net-(U1-PadA6)")
    (add_net "Net-(U1-PadB5)")
    (add_net "Net-(U1-PadD12)")
    (add_net "Net-(U1-PadD13)")
    (add_net "Net-(U1-PadD14)")
    (add_net "Net-(U1-PadD15)")
    (add_net "Net-(U1-PadD16)")
    (add_net "Net-(U1-PadD5)")
    (add_net "Net-(U1-PadE13)")
    (add_net "Net-(U1-PadE14)")
    (add_net "Net-(U1-PadE15)")
    (add_net "Net-(U1-PadE16)")
    (add_net "Net-(U1-PadF14)")
    (add_net "Net-(U1-PadF15)")
    (add_net "Net-(U1-PadF16)")
    (add_net "Net-(U1-PadG14)")
    (add_net "Net-(U1-PadG15)")
    (add_net "Net-(U1-PadG16)")
    (add_net "Net-(U1-PadH14)")
    (add_net "Net-(U1-PadH15)")
    (add_net "Net-(U1-PadH16)")
    (add_net "Net-(U1-PadH6)")
    (add_net "Net-(U1-PadJ14)")
    (add_net "Net-(U1-PadJ15)")
    (add_net "Net-(U1-PadJ6)")
    (add_net "Net-(U1-PadK13)")
    (add_net "Net-(U1-PadK4)")
    (add_net "Net-(U1-PadL13)")
    (add_net "Net-(U1-PadM1)")
    (add_net "Net-(U1-PadM13)")
    (add_net "Net-(U1-PadN1)")
    (add_net "Net-(U1-PadN2)")
    (add_net "Net-(U1-PadP1)")
    (add_net "Net-(U1-PadP2)")
    (add_net "Net-(U1-PadP3)")
    (add_net "Net-(U1-PadP4)")
    (add_net "Net-(U1-PadR1)")
    (add_net "Net-(U1-PadR12)")
    (add_net "Net-(U1-PadR2)")
    (add_net "Net-(U1-PadR3)")
    (add_net "Net-(U1-PadR4)")
    (add_net "Net-(U1-PadT1)")
    (add_net "Net-(U1-PadT12)")
    (add_net "Net-(U1-PadT13)")
    (add_net "Net-(U1-PadT2)")
    (add_net "Net-(U1-PadT3)")
    (add_net "Net-(U1-PadT4)")
    (add_net "Net-(U3-Pad5)")
    (add_net SYS_5V)
    (add_net USB_DC)
    (add_net VBUS.RAW)
    (add_net VDD_1V8)
    (add_net VDD_3V3A)
    (add_net VDD_3V3AUX)
    (add_net VDD_3V3B)
    (add_net VDD_5V)
    (add_net VDD_RTC)
    (add_net VIN.BAT)
  )
  (module PocketBeagle.pretty:0603-LED (layer Top) (tedit 200000)
    (at 124.6841 95.0716 90)
    (attr smd)
    (fp_text reference LED1 (at -1.2706 -1.5195 90) (layer F.SilkS) hide)
    (fp_text value PWR (at 1.64786 -2.48216 90) (layer F.SilkS))
    (pad K smd rect (at 0 0.7493 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 187 /N$4))
    (pad A smd rect (at 0 -0.7493 90) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 8 VDD_3V3AUX))
  )
  (module PocketBeagle.pretty:0603-LED (layer Top) (tedit 200000)
    (at 123.6681 112.5976)
    (attr smd)
    (fp_text reference USR3 (at -0.7 1.7 90) (layer F.SilkS))
    (fp_text value LTST-C191TBKT (at 1.65 2.3 90) (layer F.SilkS) hide)
    (pad K smd rect (at 0 0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 84 /N$2))
    (pad A smd rect (at 0 -0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 123 "/(U1.P14)USR3"))
  )
  (module PocketBeagle.pretty:0603-LED (layer Top) (tedit 200000)
    (at 125.9541 112.5976)
    (attr smd)
    (fp_text reference USR2 (at -0.7 1.7 90) (layer F.SilkS))
    (fp_text value LTST-C191TBKT (at 1.65 2.3 90) (layer F.SilkS) hide)
    (pad K smd rect (at 0 0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 82 /N$1))
    (pad A smd rect (at 0 -0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 116 "/(U1.R14)USR2"))
  )
  (module PocketBeagle.pretty:0603-LED (layer Top) (tedit 200000)
    (at 128.2401 112.5976)
    (attr smd)
    (fp_text reference USR1 (at -0.7 1.7 90) (layer F.SilkS))
    (fp_text value LTST-C191TBKT (at 1.65 2.3 90) (layer F.SilkS) hide)
    (pad K smd rect (at 0 0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 83 /N$5))
    (pad A smd rect (at 0 -0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 109 "/(U1.T14)USR1"))
  )
  (module PocketBeagle.pretty:0603-LED (layer Top) (tedit 200000)
    (at 130.5261 112.5976)
    (attr smd)
    (fp_text reference USR0 (at -0.7 1.7 90) (layer F.SilkS))
    (fp_text value LTST-C191TBKT (at 1.65 2.3 90) (layer F.SilkS) hide)
    (pad K smd rect (at 0 0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 85 /N$6))
    (pad A smd rect (at 0 -0.7493) (size 0.79756 0.79756) (layers Top F.Paste F.Mask)
      (net 124 "/(U1.P13)USR0"))
  )
  (module PocketBeagle.pretty:MINI_PUSHBUTTON (layer Top) (tedit 200000)
    (at 129.2561 108.2796)
    (attr smd)
    (fp_text reference SW1 (at 1.8841 1.5754) (layer F.SilkS) hide)
    (fp_text value POWER (at -1.964 2.6803) (layer F.SilkS))
    (pad 4 smd rect (at 1.99898 0.7493) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 24 "/(U1.T11)PWR.BTN"))
    (pad 3 smd rect (at -1.99898 0.7493) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 24 "/(U1.T11)PWR.BTN"))
    (pad 2 smd rect (at 1.99898 -0.7493) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.99898 -0.7493) (size 1.19888 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module PocketBeagle.pretty:MICROSD (layer Top) (tedit 200000)
    (at 158.4647 107.2876)
    (attr smd)
    (fp_text reference X2 (at 15.44148 -8.81688) (layer F.SilkS))
    (fp_text value MICROSD (at 2.54 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 10.49782 -5.24764) (size 0.99822 0.99822) (drill 0.99822) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.49782 2.74828) (size 0.99822 0.99822) (drill 0.99822) (layers *.Cu *.Mask))
    (pad G4 smd rect (at 0.49784 -9.04748) (size 1.39954 1.59766) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad G3 smd rect (at 10.09904 -9.94918) (size 2.19964 1.19888) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad G2 smd rect (at 10.09904 5.5499) (size 2.19964 1.19888) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad G1 smd rect (at 0.59944 5.56006) (size 1.59766 1.19888) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad 9 smd rect (at 0 4.39928) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 104 "/(U1.C14)MMC0.CD"))
    (pad 8 smd rect (at 0 3.29946) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 105 "/(U1.A15)MMC0.D1"))
    (pad 7 smd rect (at 0 2.19964) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 107 "/(U1.A16)MMC0.D0"))
    (pad 6 smd rect (at 0 1.09982) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 0) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 102 "/(U1.B15)MMC0.CLK"))
    (pad 4 smd rect (at 0 -1.09982) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 3 smd rect (at 0 -2.19964) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 100 "/(U1.B16)MMC0.CMD"))
    (pad 2 smd rect (at 0 -3.29946) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 101 "/(U1.C15)MMC0.D3"))
    (pad 1 smd rect (at 0 -4.39928) (size 1.59766 0.6985) (layers Top F.Paste F.Mask)
      (net 103 "/(U1.C16)MMC0.D2"))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 155.1387 97.3576 270)
    (attr smd)
    (fp_text reference R5 (at -0.00702 -1.65296 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 42 "/(U1.F3)AIN5~3.3V"))
    (pad 6 smd rect (at 0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 72 "/(U1.F2)AIN6~3.3V"))
    (pad 5 smd rect (at 0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 86 "/(U1.C9)AIN6~1.8V"))
    (pad 3 smd rect (at 0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 86 "/(U1.C9)AIN6~1.8V"))
    (pad 2 smd rect (at -0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 87 "/(U1.C8)AIN5~1.8V"))
    (pad 1 smd rect (at -0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 87 "/(U1.C8)AIN5~1.8V"))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 124.0491 116.0266 180)
    (attr smd)
    (fp_text reference R4 (at -0.20008 -1.66684 180) (layer F.SilkS))
    (fp_text value 1k (at 0 0 180) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 84 /N$2))
    (pad 3 smd rect (at 0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 82 /N$1))
    (pad 2 smd rect (at -0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 83 /N$5))
    (pad 1 smd rect (at -0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 85 /N$6))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 155.1387 105.8158 270)
    (attr smd)
    (fp_text reference R8 (at 1.8342 -1.9613 90) (layer F.SilkS))
    (fp_text value 100k (at 0 0 270) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 4 smd rect (at 0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 94 "/(U1.H2)LCD.D4.B7"))
    (pad 3 smd rect (at 0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 92 "/(U1.H1)LCD.D5.G2"))
    (pad 2 smd rect (at -0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 93 "/(U1.J3)LCD.D6.G3"))
    (pad 1 smd rect (at -0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 95 "/(U1.J2)LCD.D7.G4"))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 155.1387 103.3774 270)
    (attr smd)
    (fp_text reference R7 (at -0.8774 -2.0613 90) (layer F.SilkS))
    (fp_text value 100k (at 0 0 270) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 80 "/(U1.J1)LCD.D8.G5"))
    (pad 3 smd rect (at 0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 78 "/(U1.K3)LCD.D9.G6"))
    (pad 2 smd rect (at -0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 79 "/(U1.K2)LCD.D10.G7"))
    (pad 1 smd rect (at -0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 81 "/(U1.K1)LCD.D11.R3"))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 155.1387 100.939 270)
    (attr smd)
    (fp_text reference R6 (at -0.289 -2.0113 270) (layer F.SilkS))
    (fp_text value 100k (at 0 0 270) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 6 smd rect (at 0.24892 -0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.8001 -0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 90 "/(U1.L3)LCD.D12.R4"))
    (pad 3 smd rect (at 0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 88 "/(U1.L2)LCD.D13.R5"))
    (pad 2 smd rect (at -0.24892 0.49784 270) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 89 "/(U1.L1)LCD.D14.R6"))
    (pad 1 smd rect (at -0.8001 0.49784 270) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 91 "/(U1.M3)LCD.D15.R7"))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 161.0823 95.8336)
    (attr smd)
    (fp_text reference R10 (at -1.57538 1.169 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 7 smd rect (at -0.24892 -0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 6 smd rect (at 0.24892 -0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 5 smd rect (at 0.8001 -0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 4 smd rect (at 0.8001 0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 102 "/(U1.B15)MMC0.CLK"))
    (pad 3 smd rect (at 0.24892 0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 100 "/(U1.B16)MMC0.CMD"))
    (pad 2 smd rect (at -0.24892 0.49784) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 101 "/(U1.C15)MMC0.D3"))
    (pad 1 smd rect (at -0.8001 0.49784) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 103 "/(U1.C16)MMC0.D2"))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 163.9779 95.8336 180)
    (attr smd)
    (fp_text reference R11 (at -1.44976 1.22622 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 106 "Net-(R11-Pad8)"))
    (pad 7 smd rect (at -0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 104 "/(U1.C14)MMC0.CD"))
    (pad 6 smd rect (at 0.24892 -0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 105 "/(U1.A15)MMC0.D1"))
    (pad 5 smd rect (at 0.8001 -0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 107 "/(U1.A16)MMC0.D0"))
    (pad 4 smd rect (at 0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 3 smd rect (at 0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 2 smd rect (at -0.24892 0.49784 180) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 1 smd rect (at -0.8001 0.49784 180) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 108 "Net-(R11-Pad1)"))
  )
  (module PocketBeagle.pretty:RN0804 (layer Top) (tedit 200000)
    (at 155.1387 108.2542 90)
    (attr smd)
    (fp_text reference R9 (at 0.5042 1.2113 90) (layer F.SilkS))
    (fp_text value 100k (at 0 0 90) (layer F.SilkS) hide)
    (pad 8 smd rect (at -0.8001 -0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 98 "/(U1.G3)LCD.D0.B3"))
    (pad 7 smd rect (at -0.24892 -0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 96 "/(U1.G2)LCD.D1.B4"))
    (pad 6 smd rect (at 0.24892 -0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 97 "/(U1.G1)LCD.D2.B5"))
    (pad 5 smd rect (at 0.8001 -0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 99 "/(U1.H3)LCD.D3.B6"))
    (pad 4 smd rect (at 0.8001 0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad 3 smd rect (at 0.24892 0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.24892 0.49784 90) (size 0.29972 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.8001 0.49784 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 170.5011 102.7536 270)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP9 (at 0.091 3.4961) (layer B.SilkS) hide)
    (fp_text value EMU0 (at 0.54058 2.49788) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 270) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 270) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 166 /JTAG_EMU0))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 172.0011 101.6286 270)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP11 (at 0.0984 -3.4367) (layer B.SilkS) hide)
    (fp_text value EMU1 (at 0.02474 -2.2937) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 270) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 270) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 165 /JTAG_EMU1))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 172.0011 106.1286 270)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP10 (at 0.0942 -3.9701) (layer B.SilkS) hide)
    (fp_text value TRST (at 0.0561 -2.16416) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 270) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 270) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 176 /JTAG_TRST#))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 170.5011 105.0036 270)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP5 (at 0.01524 3.46562) (layer B.SilkS) hide)
    (fp_text value TMS (at 0.00508 2.11688) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 270) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 270) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 177 /JTAG_TMS))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 172.0011 108.3786 270)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP7 (at 0.0286 -3.6145) (layer B.SilkS) hide)
    (fp_text value TDO (at 0.00066 -1.9889) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 270) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 270) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 179 /JTAG_TDO))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 170.5011 107.2536 270)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP6 (at 0.0106 3.5723) (layer B.SilkS) hide)
    (fp_text value TDI (at -0.00718 1.96194) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 270) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 270) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 180 /JTAG_TDI))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 172.0011 103.8786 270)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP8 (at 0.2868 -3.6145) (layer B.SilkS) hide)
    (fp_text value TCK (at 0.03534 -1.9254) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 270) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 270) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 178 /JTAG_TCK))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 145.6391 109.4226 180)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP2 (at 2.54 1.651 180) (layer B.SilkS) hide)
    (fp_text value VDD_CORE (at -6.13098 1.05858 180) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 180) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 180) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 154 /N$9))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 137.8921 109.4226 180)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP4 (at 2.54 1.651 180) (layer B.SilkS) hide)
    (fp_text value VDDS_PLL (at 5.6724 1.20336 180) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 180) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 180) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 153 /N$11))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 135.6061 109.4226 180)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP3 (at 2.54 1.651 180) (layer B.SilkS) hide)
    (fp_text value VDD_MPU (at 3.33052 -0.05394 180) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 180) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 180) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 158 /N$10))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 148.1791 109.4226 180)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP1 (at 2.54 1.651 180) (layer B.SilkS) hide)
    (fp_text value VDDS_DDR (at -3.63162 -0.05902 180) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 180) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 180) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 159 /N$7))
  )
  (module PocketBeagle.pretty:B1_27 (layer Bottom) (tedit 59927130)
    (at 150.7191 101.1676 180)
    (descr "TEST PAD")
    (tags "TEST PAD")
    (attr smd)
    (fp_text reference TP12 (at 2.54 1.651 180) (layer B.SilkS) hide)
    (fp_text value WP (at -1.65804 -0.00314 180) (layer B.SilkS))
    (fp_text user >TP_SIGNAL_NAME (at 6.86308 -1.40462 180) (layer B.SilkS) hide)
    (pad TP smd circle (at 0 0 180) (size 1.27 1.27) (layers Bottom B.Mask)
      (net 133 "/(U1.M2)EEPROM.WP"))
  )
  (module PocketBeagle.pretty:FIDUCIAL_40MIL (layer Top) (tedit 59925435)
    (at 171.7001 96.0788)
    (attr smd)
    (fp_text reference FUD1 (at 0.3 2.1) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL (at -0.1 -2.2) (layer F.SilkS) hide)
    (pad P$1 smd circle (at 0 0) (size 1.016 1.016) (layers Top F.Mask)
      (net 186 "Net-(FUD1-PadP$1)") (solder_mask_margin 0.35) (clearance 0.35))
  )
  (module PocketBeagle.pretty:FIDUCIAL_40MIL (layer Top) (tedit 59925435)
    (at 170.9553 110.9357)
    (attr smd)
    (fp_text reference FUD3 (at 0.3 2.1) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL (at -0.1 -2.2) (layer F.SilkS) hide)
    (pad P$1 smd circle (at 0 0) (size 1.016 1.016) (layers Top F.Mask)
      (net 184 "Net-(FUD3-PadP$1)") (solder_mask_margin 0.35) (clearance 0.35))
  )
  (module PocketBeagle.pretty:FIDUCIAL_40MIL (layer Top) (tedit 59925435)
    (at 130.6912 114.9217 270)
    (attr smd)
    (fp_text reference FUD2 (at 0.3 2.1 270) (layer F.SilkS) hide)
    (fp_text value FIDUCIAL (at -0.1 -2.2 270) (layer F.SilkS) hide)
    (pad P$1 smd circle (at 0 0 270) (size 1.016 1.016) (layers Top F.Mask)
      (net 185 "Net-(FUD2-PadP$1)") (solder_mask_margin 0.35) (clearance 0.35))
  )
  (module "PocketBeagle.pretty:TH-2X18-(35MIL-DIA)-W_O-SILK" (layer Top) (tedit 59924F19)
    (at 148.5011 117.7036)
    (attr virtual)
    (fp_text reference P1 (at -18.68678 3.34518) (layer F.SilkS))
    (fp_text value ~ (at 0 0) (layer F.SilkS))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 44 "/(U1.A1)PWM0A"))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 45 "/(U1.F1)"))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 46 "/(U1.R5)GPIO-0.26"))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 47 "/(U1.A2)PRU-0.1"))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 "/(U1.A12)UART0.RX"))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 49 "/(U1.A3)PRU-0.4"))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 50 "/(U1.B12)UART0.TX"))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 51 "/(U1.C4)PRU-0.7"))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 52 "/(U1.A10)I2C2.SCL"))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 53 "/(U1.C7)AIN4~1.8V"))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 54 "/(U1.B10)I2C2.SDA"))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 55 "/(U1.C6)AIN3~1.8V"))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 SYS_5V))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 "/(U1.B6)AIN2~1.8V"))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 "/(U1.B8)AIN1~1.8V"))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 "/(U1.B4)PRU-0.16"))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 "/(U1.A8)AIN0~1.8V"))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 60 "/(U1.B7)VREF+"))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 61 "/(U1.B9)VREF-"))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 VDD_3V3B))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 62 "/(U1.L14)USB1.ID"))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 63 "/(U1.B14)SPI0.MOSI"))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 64 "/(U1.L15)USB1.D+"))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 65 "/(U1.B13)SPI0.MISO"))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 66 "/(U1.L16)USB1.D-"))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 67 "/(U1.A13)SPI0.CLK"))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 USB_DC))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 68 "/(U1.A14)SPI0.CS"))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 69 "/(U1.M15)USB1.VBUS"))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 70 "/(U1.E1)"))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 71 "/(U1.M14)USB1.DRVVBUS"))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 72 "/(U1.F2)AIN6~3.3V"))
    (pad 1 thru_hole rect (at -21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 VDD_5V))
  )
  (module "PocketBeagle.pretty:TH-2X18-(35MIL-DIA)-W_O-SILK" (layer Top) (tedit 59924F19)
    (at 148.5011 92.3036)
    (attr virtual)
    (fp_text reference P2 (at -18.6055 -3.15468 180) (layer F.SilkS))
    (fp_text value ~ (at 0 0) (layer F.SilkS))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 43 "/(U1.N13)AIN7~1.8V"))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 42 "/(U1.F3)AIN5~3.3V"))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 41 "/(U1.B3)PRU-0.5"))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 "/(U1.R6)"))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 "/(U1.B2)PRU-0.2"))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 "/(U1.A4)SPI1.CS"))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 "/(U1.B1)PRU-0.3"))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "/(U1.C5)SPI1.CLK"))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "/(U1.C3)PRU-0.6"))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 "/(U1.C12)SPI1.MISO"))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 "/(U1.R11)RESET#"))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "/(U1.C13)SPI1.MOSI"))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 "/(U1.P6)"))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 VDD_3V3B))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 "/(U1.T6)PRU-0.14"))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 "/(U1.R7)"))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 "/(U1.T5)"))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 "/(U1.P7)PRU-0.15"))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "/(U1.T7)"))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /BAT.TEMP))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 VIN.BAT))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 SYS_5V))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 "/(U1.T11)PWR.BTN"))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "/(U1.A11)I2C1.SDA"))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 "/(U1.R13)"))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "/(U1.B11)I2C1.SCL"))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 "/(U1.N14)"))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 "/(U1.R16)UART4.TX"))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 "/(U1.T15)"))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "/(U1.P15)UART4.RX"))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "/(U1.R15)"))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "/(U1.P5)GPIO-0.23"))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "/(U1.T16)"))
    (pad 1 thru_hole rect (at -21.59 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "/(U1.P12)PWM1A"))
  )
  (module "PocketBeagle.pretty:SON-6(TI)-DRY" (layer Top) (tedit 200000)
    (at 131.0341 102.9456 90)
    (attr smd)
    (fp_text reference U3 (at -1.1182 1.4015) (layer F.SilkS))
    (fp_text value TPD4S012DRY (at -0.88 1.85 90) (layer F.SilkS) hide)
    (pad 6 smd rect (at -0.49784 -0.37338 90) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 5 USB_DC))
    (pad 5 smd rect (at 0 -0.37338 90) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 73 "Net-(U3-Pad5)"))
    (pad 4 smd rect (at 0.49784 -0.37338 90) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.49784 0.37338 90) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 74 "/(U1.K14)USBC.ID"))
    (pad 2 smd rect (at 0 0.37338 90) (size 0.29972 0.48768) (layers Top F.Paste F.Mask)
      (net 75 "/(U1.K16)USBC.D-"))
    (pad 1 smd rect (at -0.49784 0.37846 90) (size 0.29972 0.51816) (layers Top F.Paste F.Mask)
      (net 76 "/(U1.K15)USBC.D+"))
  )
  (module PocketBeagle.pretty:CRYSTAL_5X3.2MM (layer Top) (tedit 200000)
    (at 128.6211 98.6276 90)
    (attr smd)
    (fp_text reference Y1 (at -2.5787 -1.89288 90) (layer F.SilkS))
    (fp_text value "24 MHz" (at -3.048 2.794 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.94818 0 90) (size 1.89992 2.39776) (layers Top F.Paste F.Mask)
      (net 122 /OSC.IN))
    (pad 1 smd rect (at -1.94818 0 90) (size 1.89992 2.39776) (layers Top F.Paste F.Mask)
      (net 129 /OSC.OUT))
  )
  (module "PocketBeagle.pretty:10118192-0001LF(MICRO-USB-B-AMPHENOL-FCI)" (layer Top) (tedit 200000)
    (at 122.4511 105.0036 270)
    (attr smd)
    (fp_text reference X1 (at -4.9022 0.8105) (layer F.SilkS))
    (fp_text value 10118192-0001LF (at 6.2 1.45 180) (layer F.SilkS) hide)
    (fp_text user "Edge of PCB" (at 1.397 1.47066 270) (layer F.SilkS))
    (pad VBUS smd rect (at -1.29794 -2.67462 270) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 12 VBUS.RAW))
    (pad ID smd rect (at 0.6477 -2.67462 270) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 74 "/(U1.K14)USBC.ID"))
    (pad GND smd rect (at 1.29794 -2.67462 270) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad D- smd rect (at -0.6477 -2.67462 270) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 75 "/(U1.K16)USBC.D-"))
    (pad D+ smd rect (at 0 -2.67462 270) (size 0.39878 1.34874) (layers Top F.Paste F.Mask)
      (net 76 "/(U1.K15)USBC.D+"))
    (pad CGND smd rect (at -3.0988 -2.54762 270) (size 2.09804 1.59766) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad CGND smd rect (at 3.0988 -2.54762 270) (size 2.09804 1.59766) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad CGND smd rect (at 3.79984 0 270) (size 1.79832 1.89992) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad CGND smd rect (at 1.19888 0 270) (size 1.89992 1.89992) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad CGND smd rect (at -1.19888 0 270) (size 1.89992 1.89992) (layers Top F.Paste F.Mask)
      (net 10 CGND))
    (pad CGND smd rect (at -3.79984 0 270) (size 1.79832 1.89992) (layers Top F.Paste F.Mask)
      (net 10 CGND))
  )
  (module "PocketBeagle.pretty:SC70(TI-DCK)" (layer Top) (tedit 200000)
    (at 124.6841 98.6276 90)
    (attr smd)
    (fp_text reference U2 (at -1.25536 0.83254) (layer F.SilkS))
    (fp_text value SN74LVC1G07DCK (at -2.159 3.048 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 0.6477 1.09982 90) (size 0.39878 0.89916) (layers Top F.Paste F.Mask)
      (net 4 VDD_RTC))
    (pad 4 smd rect (at -0.6477 1.09982 90) (size 0.39878 0.89916) (layers Top F.Paste F.Mask)
      (net 33 "/(U1.R11)RESET#"))
    (pad 3 smd rect (at -0.6477 -1.09982 90) (size 0.39878 0.89916) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.09982 90) (size 0.39878 0.89916) (layers Top F.Paste F.Mask)
      (net 77 /PMIC_PGOOD))
    (pad 1 smd rect (at 0.6477 -1.09982 90) (size 0.39878 0.89916) (layers Top F.Paste F.Mask))
  )
  (module PocketBeagle.pretty:OSD335X-BGA-256 locked (layer Top) (tedit 200000)
    (at 143.0991 104.9776 90)
    (attr smd)
    (fp_text reference U1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value OSD3358-512M-BSM (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user 16 (at -9.9314 -9.8298 90) (layer F.SilkS))
    (fp_text user 1 (at -10.2362 9.2202 90) (layer F.SilkS))
    (fp_text user T (at 9.8298 10.36066 90) (layer F.SilkS))
    (fp_text user A (at -9.2202 10.36066 90) (layer F.SilkS))
    (pad T16 smd circle (at 9.52246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 14 "/(U1.T16)"))
    (pad T15 smd circle (at 9.52246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 18 "/(U1.T15)"))
    (pad T14 smd circle (at 9.52246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 109 "/(U1.T14)USR1"))
    (pad T13 smd circle (at 9.52246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 110 "Net-(U1-PadT13)"))
    (pad T12 smd circle (at 9.52246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 111 "Net-(U1-PadT12)"))
    (pad T11 smd circle (at 9.52246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 24 "/(U1.T11)PWR.BTN"))
    (pad T10 smd circle (at 9.52246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 6 VDD_5V))
    (pad T9 smd circle (at 9.52246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 5 USB_DC))
    (pad T8 smd circle (at 9.52246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 11 VIN.BAT))
    (pad T7 smd circle (at 9.52246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 26 "/(U1.T7)"))
    (pad T6 smd circle (at 9.52246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 30 "/(U1.T6)PRU-0.14"))
    (pad T5 smd circle (at 9.52246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 28 "/(U1.T5)"))
    (pad T4 smd circle (at 9.52246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 112 "Net-(U1-PadT4)"))
    (pad T3 smd circle (at 9.52246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 113 "Net-(U1-PadT3)"))
    (pad T2 smd circle (at 9.52246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 114 "Net-(U1-PadT2)"))
    (pad T1 smd circle (at 9.52246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 115 "Net-(U1-PadT1)"))
    (pad R16 smd circle (at 8.25246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 19 "/(U1.R16)UART4.TX"))
    (pad R15 smd circle (at 8.25246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 16 "/(U1.R15)"))
    (pad R14 smd circle (at 8.25246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 116 "/(U1.R14)USR2"))
    (pad R13 smd circle (at 8.25246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 22 "/(U1.R13)"))
    (pad R12 smd circle (at 8.25246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 117 "Net-(U1-PadR12)"))
    (pad R11 smd circle (at 8.25246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 33 "/(U1.R11)RESET#"))
    (pad R10 smd circle (at 8.25246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 6 VDD_5V))
    (pad R9 smd circle (at 8.25246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 5 USB_DC))
    (pad R8 smd circle (at 8.25246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 11 VIN.BAT))
    (pad R7 smd circle (at 8.25246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 29 "/(U1.R7)"))
    (pad R6 smd circle (at 8.25246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 40 "/(U1.R6)"))
    (pad R5 smd circle (at 8.25246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 46 "/(U1.R5)GPIO-0.26"))
    (pad R4 smd circle (at 8.25246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 118 "Net-(U1-PadR4)"))
    (pad R3 smd circle (at 8.25246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 119 "Net-(U1-PadR3)"))
    (pad R2 smd circle (at 8.25246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 120 "Net-(U1-PadR2)"))
    (pad R1 smd circle (at 8.25246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 121 "Net-(U1-PadR1)"))
    (pad P16 smd circle (at 6.98246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 122 /OSC.IN))
    (pad P15 smd circle (at 6.98246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 17 "/(U1.P15)UART4.RX"))
    (pad P14 smd circle (at 6.98246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 123 "/(U1.P14)USR3"))
    (pad P13 smd circle (at 6.98246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 124 "/(U1.P13)USR0"))
    (pad P12 smd circle (at 6.98246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 13 "/(U1.P12)PWM1A"))
    (pad P11 smd circle (at 6.98246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 77 /PMIC_PGOOD))
    (pad P10 smd circle (at 6.98246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 6 VDD_5V))
    (pad P9 smd circle (at 6.98246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 5 USB_DC))
    (pad P8 smd circle (at 6.98246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 11 VIN.BAT))
    (pad P7 smd circle (at 6.98246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 27 "/(U1.P7)PRU-0.15"))
    (pad P6 smd circle (at 6.98246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 31 "/(U1.P6)"))
    (pad P5 smd circle (at 6.98246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 15 "/(U1.P5)GPIO-0.23"))
    (pad P4 smd circle (at 6.98246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 125 "Net-(U1-PadP4)"))
    (pad P3 smd circle (at 6.98246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 126 "Net-(U1-PadP3)"))
    (pad P2 smd circle (at 6.98246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 127 "Net-(U1-PadP2)"))
    (pad P1 smd circle (at 6.98246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 128 "Net-(U1-PadP1)"))
    (pad N16 smd circle (at 5.71246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 129 /OSC.OUT))
    (pad N15 smd circle (at 5.71246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 130 /OSC.GND))
    (pad N14 smd circle (at 5.71246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 20 "/(U1.N14)"))
    (pad N13 smd circle (at 5.71246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 43 "/(U1.N13)AIN7~1.8V"))
    (pad N12 smd circle (at 5.71246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 77 /PMIC_PGOOD))
    (pad N11 smd circle (at 5.71246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 131 /N$27))
    (pad N10 smd circle (at 5.71246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 131 /N$27))
    (pad N9 smd circle (at 5.71246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad N8 smd circle (at 5.71246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad N7 smd circle (at 5.71246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 11 VIN.BAT))
    (pad N6 smd circle (at 5.71246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 25 /BAT.TEMP))
    (pad N5 smd circle (at 5.71246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 132 /N$24))
    (pad N4 smd circle (at 5.71246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 132 /N$24))
    (pad N3 smd circle (at 5.71246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 133 "/(U1.M2)EEPROM.WP"))
    (pad N2 smd circle (at 5.71246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 134 "Net-(U1-PadN2)"))
    (pad N1 smd circle (at 5.71246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 135 "Net-(U1-PadN1)"))
    (pad M16 smd circle (at 4.44246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 136 /N$22))
    (pad M15 smd circle (at 4.44246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 69 "/(U1.M15)USB1.VBUS"))
    (pad M14 smd circle (at 4.44246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 71 "/(U1.M14)USB1.DRVVBUS"))
    (pad M13 smd circle (at 4.44246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 137 "Net-(U1-PadM13)"))
    (pad M12 smd circle (at 4.44246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M11 smd circle (at 4.44246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M10 smd circle (at 4.44246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M9 smd circle (at 4.44246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M8 smd circle (at 4.44246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M7 smd circle (at 4.44246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M6 smd circle (at 4.44246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M5 smd circle (at 4.44246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad M4 smd circle (at 4.44246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 138 /N$25))
    (pad M3 smd circle (at 4.44246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 91 "/(U1.M3)LCD.D15.R7"))
    (pad M2 smd circle (at 4.44246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 133 "/(U1.M2)EEPROM.WP"))
    (pad M1 smd circle (at 4.44246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 139 "Net-(U1-PadM1)"))
    (pad L16 smd circle (at 3.17246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 66 "/(U1.L16)USB1.D-"))
    (pad L15 smd circle (at 3.17246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 64 "/(U1.L15)USB1.D+"))
    (pad L14 smd circle (at 3.17246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 62 "/(U1.L14)USB1.ID"))
    (pad L13 smd circle (at 3.17246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 140 "Net-(U1-PadL13)"))
    (pad L12 smd circle (at 3.17246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad L11 smd circle (at 3.17246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 4 VDD_RTC))
    (pad L10 smd circle (at 3.17246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad L9 smd circle (at 3.17246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad L8 smd circle (at 3.17246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad L7 smd circle (at 3.17246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 9 SYS_5V))
    (pad L6 smd circle (at 3.17246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 9 SYS_5V))
    (pad L5 smd circle (at 3.17246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad L4 smd circle (at 3.17246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 138 /N$25))
    (pad L3 smd circle (at 3.17246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 90 "/(U1.L3)LCD.D12.R4"))
    (pad L2 smd circle (at 3.17246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 88 "/(U1.L2)LCD.D13.R5"))
    (pad L1 smd circle (at 3.17246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 89 "/(U1.L1)LCD.D14.R6"))
    (pad K16 smd circle (at 1.90246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 75 "/(U1.K16)USBC.D-"))
    (pad K15 smd circle (at 1.90246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 76 "/(U1.K15)USBC.D+"))
    (pad K14 smd circle (at 1.90246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 74 "/(U1.K14)USBC.ID"))
    (pad K13 smd circle (at 1.90246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 141 "Net-(U1-PadK13)"))
    (pad K12 smd circle (at 1.90246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad K11 smd circle (at 1.90246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 4 VDD_RTC))
    (pad K10 smd circle (at 1.90246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad K9 smd circle (at 1.90246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad K8 smd circle (at 1.90246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad K7 smd circle (at 1.90246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 9 SYS_5V))
    (pad K6 smd circle (at 1.90246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 9 SYS_5V))
    (pad K5 smd circle (at 1.90246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad K4 smd circle (at 1.90246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 142 "Net-(U1-PadK4)"))
    (pad K3 smd circle (at 1.90246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 78 "/(U1.K3)LCD.D9.G6"))
    (pad K2 smd circle (at 1.90246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 79 "/(U1.K2)LCD.D10.G7"))
    (pad K1 smd circle (at 1.90246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 81 "/(U1.K1)LCD.D11.R3"))
    (pad J16 smd circle (at 0.63246 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 5 USB_DC))
    (pad J15 smd circle (at 0.63246 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 143 "Net-(U1-PadJ15)"))
    (pad J14 smd circle (at 0.63246 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 144 "Net-(U1-PadJ14)"))
    (pad J13 smd circle (at 0.63246 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad J12 smd circle (at 0.63246 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad J11 smd circle (at 0.63246 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad J10 smd circle (at 0.63246 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad J9 smd circle (at 0.63246 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad J8 smd circle (at 0.63246 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad J7 smd circle (at 0.63246 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad J6 smd circle (at 0.63246 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 145 "Net-(U1-PadJ6)"))
    (pad J5 smd circle (at 0.63246 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad J4 smd circle (at 0.63246 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad J3 smd circle (at 0.63246 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 93 "/(U1.J3)LCD.D6.G3"))
    (pad J2 smd circle (at 0.63246 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 95 "/(U1.J2)LCD.D7.G4"))
    (pad J1 smd circle (at 0.63246 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 80 "/(U1.J1)LCD.D8.G5"))
    (pad H16 smd circle (at -0.635 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 146 "Net-(U1-PadH16)"))
    (pad H15 smd circle (at -0.635 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 147 "Net-(U1-PadH15)"))
    (pad H14 smd circle (at -0.635 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 148 "Net-(U1-PadH14)"))
    (pad H13 smd circle (at -0.635 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad H12 smd circle (at -0.635 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad H11 smd circle (at -0.635 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad H10 smd circle (at -0.635 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad H9 smd circle (at -0.635 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad H8 smd circle (at -0.635 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad H7 smd circle (at -0.635 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad H6 smd circle (at -0.635 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 149 "Net-(U1-PadH6)"))
    (pad H5 smd circle (at -0.635 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad H4 smd circle (at -0.635 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad H3 smd circle (at -0.635 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 99 "/(U1.H3)LCD.D3.B6"))
    (pad H2 smd circle (at -0.635 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 94 "/(U1.H2)LCD.D4.B7"))
    (pad H1 smd circle (at -0.635 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 92 "/(U1.H1)LCD.D5.G2"))
    (pad G16 smd circle (at -1.905 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 150 "Net-(U1-PadG16)"))
    (pad G15 smd circle (at -1.905 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 151 "Net-(U1-PadG15)"))
    (pad G14 smd circle (at -1.905 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 152 "Net-(U1-PadG14)"))
    (pad G13 smd circle (at -1.905 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 153 /N$11))
    (pad G12 smd circle (at -1.905 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad G11 smd circle (at -1.905 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 8 VDD_3V3AUX))
    (pad G10 smd circle (at -1.905 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad G9 smd circle (at -1.905 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad G8 smd circle (at -1.905 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad G7 smd circle (at -1.905 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad G6 smd circle (at -1.905 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad G5 smd circle (at -1.905 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad G4 smd circle (at -1.905 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 154 /N$9))
    (pad G3 smd circle (at -1.905 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 98 "/(U1.G3)LCD.D0.B3"))
    (pad G2 smd circle (at -1.905 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 96 "/(U1.G2)LCD.D1.B4"))
    (pad G1 smd circle (at -1.905 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 97 "/(U1.G1)LCD.D2.B5"))
    (pad F16 smd circle (at -3.175 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 155 "Net-(U1-PadF16)"))
    (pad F15 smd circle (at -3.175 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 156 "Net-(U1-PadF15)"))
    (pad F14 smd circle (at -3.175 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 157 "Net-(U1-PadF14)"))
    (pad F13 smd circle (at -3.175 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 158 /N$10))
    (pad F12 smd circle (at -3.175 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad F11 smd circle (at -3.175 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 8 VDD_3V3AUX))
    (pad F10 smd circle (at -3.175 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 3 VDD_1V8))
    (pad F9 smd circle (at -3.175 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad F8 smd circle (at -3.175 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 2 VDD_3V3A))
    (pad F7 smd circle (at -3.175 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad F6 smd circle (at -3.175 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
    (pad F5 smd circle (at -3.175 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad F4 smd circle (at -3.175 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 159 /N$7))
    (pad F3 smd circle (at -3.175 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 42 "/(U1.F3)AIN5~3.3V"))
    (pad F2 smd circle (at -3.175 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 72 "/(U1.F2)AIN6~3.3V"))
    (pad F1 smd circle (at -3.175 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 45 "/(U1.F1)"))
    (pad E16 smd circle (at -4.445 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 160 "Net-(U1-PadE16)"))
    (pad E15 smd circle (at -4.445 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 161 "Net-(U1-PadE15)"))
    (pad E14 smd circle (at -4.445 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 162 "Net-(U1-PadE14)"))
    (pad E13 smd circle (at -4.445 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 163 "Net-(U1-PadE13)"))
    (pad E12 smd circle (at -4.445 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E11 smd circle (at -4.445 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E10 smd circle (at -4.445 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E9 smd circle (at -4.445 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E8 smd circle (at -4.445 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E7 smd circle (at -4.445 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E6 smd circle (at -4.445 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E5 smd circle (at -4.445 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad E4 smd circle (at -4.445 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 164 /N$26))
    (pad E3 smd circle (at -4.445 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 165 /JTAG_EMU1))
    (pad E2 smd circle (at -4.445 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 166 /JTAG_EMU0))
    (pad E1 smd circle (at -4.445 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 70 "/(U1.E1)"))
    (pad D16 smd circle (at -5.715 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 167 "Net-(U1-PadD16)"))
    (pad D15 smd circle (at -5.715 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 168 "Net-(U1-PadD15)"))
    (pad D14 smd circle (at -5.715 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 169 "Net-(U1-PadD14)"))
    (pad D13 smd circle (at -5.715 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 170 "Net-(U1-PadD13)"))
    (pad D12 smd circle (at -5.715 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 171 "Net-(U1-PadD12)"))
    (pad D11 smd circle (at -5.715 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 172 /N$31))
    (pad D10 smd circle (at -5.715 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 173 /N$32))
    (pad D9 smd circle (at -5.715 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad D8 smd circle (at -5.715 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad D7 smd circle (at -5.715 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 174 /N$12))
    (pad D6 smd circle (at -5.715 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 174 /N$12))
    (pad D5 smd circle (at -5.715 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 175 "Net-(U1-PadD5)"))
    (pad D4 smd circle (at -5.715 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 164 /N$26))
    (pad D3 smd circle (at -5.715 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 176 /JTAG_TRST#))
    (pad D2 smd circle (at -5.715 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 177 /JTAG_TMS))
    (pad D1 smd circle (at -5.715 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 178 /JTAG_TCK))
    (pad C16 smd circle (at -6.985 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 103 "/(U1.C16)MMC0.D2"))
    (pad C15 smd circle (at -6.985 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 101 "/(U1.C15)MMC0.D3"))
    (pad C14 smd circle (at -6.985 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 104 "/(U1.C14)MMC0.CD"))
    (pad C13 smd circle (at -6.985 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 32 "/(U1.C13)SPI1.MOSI"))
    (pad C12 smd circle (at -6.985 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 34 "/(U1.C12)SPI1.MISO"))
    (pad C11 smd circle (at -6.985 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 172 /N$31))
    (pad C10 smd circle (at -6.985 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 173 /N$32))
    (pad C9 smd circle (at -6.985 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 86 "/(U1.C9)AIN6~1.8V"))
    (pad C8 smd circle (at -6.985 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 87 "/(U1.C8)AIN5~1.8V"))
    (pad C7 smd circle (at -6.985 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 53 "/(U1.C7)AIN4~1.8V"))
    (pad C6 smd circle (at -6.985 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 55 "/(U1.C6)AIN3~1.8V"))
    (pad C5 smd circle (at -6.985 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 36 "/(U1.C5)SPI1.CLK"))
    (pad C4 smd circle (at -6.985 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 51 "/(U1.C4)PRU-0.7"))
    (pad C3 smd circle (at -6.985 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 35 "/(U1.C3)PRU-0.6"))
    (pad C2 smd circle (at -6.985 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 179 /JTAG_TDO))
    (pad C1 smd circle (at -6.985 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 180 /JTAG_TDI))
    (pad B16 smd circle (at -8.255 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 100 "/(U1.B16)MMC0.CMD"))
    (pad B15 smd circle (at -8.255 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 102 "/(U1.B15)MMC0.CLK"))
    (pad B14 smd circle (at -8.255 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 63 "/(U1.B14)SPI0.MOSI"))
    (pad B13 smd circle (at -8.255 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 65 "/(U1.B13)SPI0.MISO"))
    (pad B12 smd circle (at -8.255 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 50 "/(U1.B12)UART0.TX"))
    (pad B11 smd circle (at -8.255 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 21 "/(U1.B11)I2C1.SCL"))
    (pad B10 smd circle (at -8.255 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 54 "/(U1.B10)I2C2.SDA"))
    (pad B9 smd circle (at -8.255 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 61 "/(U1.B9)VREF-"))
    (pad B8 smd circle (at -8.255 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 57 "/(U1.B8)AIN1~1.8V"))
    (pad B7 smd circle (at -8.255 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 60 "/(U1.B7)VREF+"))
    (pad B6 smd circle (at -8.255 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 56 "/(U1.B6)AIN2~1.8V"))
    (pad B5 smd circle (at -8.255 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 181 "Net-(U1-PadB5)"))
    (pad B4 smd circle (at -8.255 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 58 "/(U1.B4)PRU-0.16"))
    (pad B3 smd circle (at -8.255 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 41 "/(U1.B3)PRU-0.5"))
    (pad B2 smd circle (at -8.255 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 39 "/(U1.B2)PRU-0.2"))
    (pad B1 smd circle (at -8.255 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 37 "/(U1.B1)PRU-0.3"))
    (pad A16 smd circle (at -9.525 -9.52246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 107 "/(U1.A16)MMC0.D0"))
    (pad A15 smd circle (at -9.525 -8.25246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 105 "/(U1.A15)MMC0.D1"))
    (pad A14 smd circle (at -9.525 -6.98246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 68 "/(U1.A14)SPI0.CS"))
    (pad A13 smd circle (at -9.525 -5.71246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 67 "/(U1.A13)SPI0.CLK"))
    (pad A12 smd circle (at -9.525 -4.44246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 48 "/(U1.A12)UART0.RX"))
    (pad A11 smd circle (at -9.525 -3.17246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 23 "/(U1.A11)I2C1.SDA"))
    (pad A10 smd circle (at -9.525 -1.90246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 52 "/(U1.A10)I2C2.SCL"))
    (pad A9 smd circle (at -9.525 -0.63246 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 61 "/(U1.B9)VREF-"))
    (pad A8 smd circle (at -9.525 0.635 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 59 "/(U1.A8)AIN0~1.8V"))
    (pad A7 smd circle (at -9.525 1.905 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 60 "/(U1.B7)VREF+"))
    (pad A6 smd circle (at -9.525 3.175 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 182 "Net-(U1-PadA6)"))
    (pad A5 smd circle (at -9.525 4.445 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 183 "Net-(U1-PadA5)"))
    (pad A4 smd circle (at -9.525 5.715 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 38 "/(U1.A4)SPI1.CS"))
    (pad A3 smd circle (at -9.525 6.985 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 49 "/(U1.A3)PRU-0.4"))
    (pad A2 smd circle (at -9.525 8.255 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 47 "/(U1.A2)PRU-0.1"))
    (pad A1 smd circle (at -9.525 9.525 90) (size 0.49784 0.49784) (layers Top F.Paste F.Mask)
      (net 44 "/(U1.A1)PWM0A"))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 131.4151 100.2786 180)
    (attr smd)
    (fp_text reference C3 (at -0.7919 -0.6102) (layer F.SilkS))
    (fp_text value "18pF, 50V" (at 0 -0.5 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 129 /OSC.OUT))
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 130 /OSC.GND))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 156.7389 105.13 90)
    (attr smd)
    (fp_text reference C5 (at 0.73 0.4111 90) (layer F.SilkS))
    (fp_text value "0.1uF, 6.3V" (at 0 -0.5 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
  )
  (module PocketBeagle.pretty:0603 (layer Top) (tedit 200000)
    (at 155.9007 110.2354 180)
    (attr smd)
    (fp_text reference C6 (at -0.7493 -0.7646) (layer F.SilkS))
    (fp_text value "10uF, 10V" (at 0 -0.7 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 7 VDD_3V3B))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 128.4941 105.8666)
    (attr smd)
    (fp_text reference R3 (at 0.8935 0.4578) (layer F.SilkS))
    (fp_text value 10k (at 0 -0.5) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 136 /N$22))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 131.4151 96.9766 180)
    (attr smd)
    (fp_text reference C2 (at -0.70808 2.29556) (layer F.SilkS))
    (fp_text value "18pF, 50V" (at 0 -0.5 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 122 /OSC.IN))
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 130 /OSC.GND))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 131.4151 98.6276 90)
    (attr smd)
    (fp_text reference R2 (at 2.96104 0.73856) (layer F.SilkS))
    (fp_text value "1M, 1%" (at 0 -0.5 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 122 /OSC.IN))
    (pad 1 smd rect (at -0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 129 /OSC.OUT))
  )
  (module PocketBeagle.pretty:0603 (layer Top) (tedit 200000)
    (at 127.7321 102.9456)
    (attr smd)
    (fp_text reference FB1 (at -1.2655 1.8548) (layer F.SilkS))
    (fp_text value ~ (at 0 -0.7) (layer F.SilkS))
    (pad 2 smd rect (at 0.84836 0) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 5 USB_DC))
    (pad 1 smd rect (at -0.84836 0) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 12 VBUS.RAW))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 129.7641 102.9456 90)
    (attr smd)
    (fp_text reference C4 (at -1.0928 0.7919 180) (layer F.SilkS))
    (fp_text value ".1uF, 6.3V" (at 0 -0.5 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.49784 0 90) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 5 USB_DC))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 124.6841 93.5476)
    (attr smd)
    (fp_text reference R1 (at -0.8083 -0.5328 180) (layer F.SilkS))
    (fp_text value 1k (at 0 -0.5) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 187 /N$4))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 124.6841 96.5956 180)
    (attr smd)
    (fp_text reference C1 (at -0.7538 -0.41208 180) (layer F.SilkS))
    (fp_text value "0.1uF, 6.3V" (at 0 -0.5 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 4 VDD_RTC))
  )
  (module PocketBeagle.pretty:0603 (layer Top) (tedit 200000)
    (at 171.7503 114.1978 180)
    (attr smd)
    (fp_text reference FB2 (at -2.68166 -1.16646 270) (layer F.SilkS))
    (fp_text value ~ (at 0 -0.7) (layer F.SilkS))
    (pad 2 smd rect (at 0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.84836 0 180) (size 0.99822 1.09982) (layers Top F.Paste F.Mask)
      (net 10 CGND))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 167.5593 114.1978)
    (attr smd)
    (fp_text reference C7 (at -1.0093 -0.2978) (layer F.SilkS))
    (fp_text value "0.1uF, 6.3V" (at 0 -0.5) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 61 "/(U1.B9)VREF-"))
    (pad 1 smd rect (at -0.49784 0) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 60 "/(U1.B7)VREF+"))
  )
  (module PocketBeagle.pretty:0402 (layer Top) (tedit 200000)
    (at 162.3777 113.893 180)
    (attr smd)
    (fp_text reference R12 (at -1.2999 -0.534) (layer F.SilkS))
    (fp_text value 10k (at 0 -0.5 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 176 /JTAG_TRST#))
    (pad 1 smd rect (at -0.49784 0 180) (size 0.49784 0.59944) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_text OSD3358 (at 154.20594 114.87404) (layer F.SilkS))
  (gr_line (start 166.0011 87.5036) (end 131.0011 87.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.0011 97.5036) (end 131.0011 87.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.0011 97.5036) (end 121.0011 112.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 131.0011 112.5036) (end 121.0011 112.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.0011 122.5036) (end 166.0011 122.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.0011 112.5036) (end 166.0011 122.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.0011 112.5036) (end 176.0011 97.5036) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.0011 97.5036) (end 176.0011 97.5036) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "75 Mils back-->\nTry to move back 75 Mils <---" (at 161.5011 106.7536) (layer Cmts.User))
  (gr_text "PocketBeagle Rev A2a" (at 148.5093 89.255) (layer F.SilkS))
  (gr_text beagleboard.org/pocket (at 148.5093 121.6654) (layer F.SilkS))
  (gr_text 1 (at 126.95 120.0906) (layer F.SilkS))
  (gr_text 2 (at 126.9701 89.1026) (layer F.SilkS))
  (gr_text 36 (at 171.0436 91.059) (layer F.SilkS))
  (gr_text 35 (at 171.2468 118.999) (layer F.SilkS))
  (gr_text 35 (at 171.1198 93.5736) (layer F.SilkS))
  (gr_text 36 (at 171.1452 116.4336) (layer F.SilkS))
  (gr_text 2 (at 127.35 114.55) (layer F.SilkS))
  (gr_text 1 (at 126.9701 94.6906) (layer F.SilkS))
  (gr_text "AIN (1.8V)" (at 153.4496 122.2496) (layer B.SilkS))
  (gr_text RST (at 157.3866 90.1821 -270) (layer B.SilkS))
  (gr_text A+ (at 147.193 115.189 -270) (layer B.SilkS))
  (gr_text 20 (at 149.7666 115.189 -270) (layer B.SilkS))
  (gr_text GND (at 152.3066 115.189 -270) (layer B.SilkS))
  (gr_text VOUT (at 154.8466 115.189 -270) (layer B.SilkS))
  (gr_text SDA (at 157.3866 115.189 -270) (layer B.SilkS))
  (gr_text SCL (at 159.9266 115.189 -270) (layer B.SilkS))
  (gr_text TX (at 162.4666 115.189 -270) (layer B.SilkS))
  (gr_text RX (at 165.0066 115.189 -270) (layer B.SilkS))
  (gr_text 26 (at 167.5466 115.189 -270) (layer B.SilkS))
  (gr_text GND (at 144.6866 115.189 -270) (layer B.SilkS))
  (gr_text +3.3V (at 142.1466 115.189 -270) (layer B.SilkS))
  (gr_text MOSI (at 139.6066 115.189 -270) (layer B.SilkS))
  (gr_text MISO (at 137.0666 115.189 -270) (layer B.SilkS))
  (gr_text CLK (at 134.5266 115.189 -270) (layer B.SilkS))
  (gr_text CS0 (at 131.9866 115.189 -270) (layer B.SilkS))
  (gr_text 89 (at 129.4466 115.189 -270) (layer B.SilkS))
  (gr_text A6/87 (at 126.9066 115.189 -270) (layer B.SilkS))
  (gr_text 44 (at 154.8466 90.1821 -270) (layer B.SilkS))
  (gr_text 46 (at 152.3066 90.1821 -270) (layer B.SilkS))
  (gr_text 64 (at 149.7666 90.1821 -270) (layer B.SilkS))
  (gr_text 47 (at 147.2266 90.1821 -270) (layer B.SilkS))
  (gr_text T (at 144.653 89.916 -270) (layer B.SilkS))
  (gr_text + (at 142.1466 90.1821 -270) (layer B.SilkS))
  (gr_text PB (at 139.6066 90.1821 -270) (layer B.SilkS))
  (gr_text 52 (at 137.0666 90.1821 -270) (layer B.SilkS))
  (gr_text 60 (at 134.5266 90.1821 -270) (layer B.SilkS))
  (gr_text 57 (at 131.9866 90.1821 -270) (layer B.SilkS))
  (gr_text 58 (at 129.4466 90.1821 -270) (layer B.SilkS))
  (gr_text 59 (at 124.3666 91.5156 -270) (layer B.SilkS))
  (gr_text 6 (at 159.9266 90.1821 -270) (layer B.SilkS))
  (gr_text 3 (at 162.4666 90.1821 -270) (layer B.SilkS))
  (gr_text 2 (at 165.0066 90.1821 -270) (layer B.SilkS))
  (gr_text 5 (at 167.5466 90.1821 -270) (layer B.SilkS))
  (gr_text "A7(1.8)" (at 172.6266 90.8806 -270) (layer B.SilkS))
  (gr_text PWM1A (at 126.9066 94.6906 -270) (layer B.SilkS))
  (gr_text 23 (at 129.413 94.869 -270) (layer B.SilkS))
  (gr_text RX (at 131.9866 94.869 -270) (layer B.SilkS))
  (gr_text TX (at 134.5266 94.869 -270) (layer B.SilkS))
  (gr_text SCL (at 137.0666 94.869 -270) (layer B.SilkS))
  (gr_text SDA (at 139.6066 94.869 -270) (layer B.SilkS))
  (gr_text VOUT (at 142.1466 94.869 -270) (layer B.SilkS))
  (gr_text GND (at 144.6866 94.869 -270) (layer B.SilkS))
  (gr_text 65 (at 147.2266 94.869 -270) (layer B.SilkS))
  (gr_text 27 (at 149.7666 94.869 -270) (layer B.SilkS))
  (gr_text GND (at 152.3066 94.869 -270) (layer B.SilkS))
  (gr_text +3.3V (at 154.8466 94.6906 -270) (layer B.SilkS))
  (gr_text MOSI (at 157.3866 94.869 -270) (layer B.SilkS))
  (gr_text MISO (at 159.9266 94.869 -270) (layer B.SilkS))
  (gr_text CLK (at 162.4666 94.6906 -270) (layer B.SilkS))
  (gr_text CS1 (at 165.0066 94.869 -270) (layer B.SilkS))
  (gr_text 45 (at 167.5466 94.869 -270) (layer B.SilkS))
  (gr_text A5/86 (at 170.0866 94.869 -270) (layer B.SilkS))
  (gr_text EN (at 129.345 119.8112 -270) (layer B.SilkS))
  (gr_text VB (at 131.885 119.8112 -270) (layer B.SilkS))
  (gr_text VI (at 134.425 119.8112 -270) (layer B.SilkS))
  (gr_text - (at 136.965 119.8112 -270) (layer B.SilkS))
  (gr_text + (at 139.505 119.8112 -270) (layer B.SilkS))
  (gr_text ID (at 142.045 119.8112 -270) (layer B.SilkS))
  (gr_text GND (at 144.5768 119.8626 -270) (layer B.SilkS))
  (gr_text - (at 147.14024 119.92042 -270) (layer B.SilkS))
  (gr_text 0 (at 149.68024 119.92042 -270) (layer B.SilkS))
  (gr_text 1 (at 152.22024 119.92042 -270) (layer B.SilkS))
  (gr_text 2 (at 154.76024 119.92042 -270) (layer B.SilkS))
  (gr_text 3 (at 157.30024 119.92042 -270) (layer B.SilkS))
  (gr_text 4 (at 159.84024 119.92042 -270) (layer B.SilkS))
  (gr_text 7 (at 162.4666 119.91026 -270) (layer B.SilkS))
  (gr_text 4 (at 165.0066 119.91026 -270) (layer B.SilkS))
  (gr_text 1 (at 167.5466 119.91026 -270) (layer B.SilkS))
  (gr_text P1.10 (at 172.6901 119.3286 -270) (layer B.SilkS))
  (gr_text PWM0A (at 170.0866 115.3 -270) (layer B.SilkS))
  (gr_text VIN (at 124.4301 118.5666 -270) (layer B.SilkS))
  (gr_text PRU0 (at 164.8796 122.2496) (layer B.SilkS))
  (gr_text PRU0 (at 163.8001 88.7851) (layer B.SilkS))
  (gr_text BAT (at 143.3531 88.7851) (layer B.SilkS))
  (gr_text SPI0 (at 133.2566 111.7721) (layer B.SilkS))
  (gr_text USB1 (at 138.5906 122.2496) (layer B.SilkS))
  (gr_text I2C2 (at 158.6566 111.7721) (layer B.SilkS))
  (gr_text SPI1 (at 163.8001 99.2626) (layer B.SilkS))
  (gr_text I2C1 (at 138.1461 99.2626) (layer B.SilkS))
  (gr_text U4 (at 133.1931 99.2626) (layer B.SilkS))
  (gr_text P1 (at 173.5791 111.0101) (layer B.SilkS))
  (gr_text P2 (at 171.5516 97.4598) (layer B.SilkS))
  (gr_text U0 (at 163.7366 111.7721) (layer B.SilkS))
  (gr_text TS:VDD_3V3AUX:1:8::L2 (at 140.4323 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:1:8::L2 (at 141.3213 106.6288 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:2:8::L2 (at 141.3213 106.6284 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:2:8::L2 (at 141.3213 100.2788 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:3:8::L2 (at 141.3213 100.2784 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:3:8::L2 (at 143.0993 98.5008 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:4:8::L2 (at 140.4323 102.4374 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:4:8::L2 (at 140.4323 100.0248 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:5:8::L2 (at 140.4323 100.0244 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:5:8::L2 (at 142.7183 97.7388 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:6:8::L2 (at 142.7183 97.7384 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:6:8::L2 (at 142.7183 96.9768 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:7:8::L2 (at 142.7183 96.9764 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:7:8::L2 (at 140.6863 94.9448 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:8:8::L2 (at 140.6863 94.9444 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:8:8::L2 (at 140.6863 93.0398 310) (layer Eco1.User))
  (gr_text V:CGND:1:48 (at 125.62775 108.672375 35) (layer Eco1.User))
  (gr_text V:CGND:2:48 (at 124.68795 108.672375 35) (layer Eco1.User))
  (gr_text V:CGND:3:48 (at 124.68795 107.249975 35) (layer Eco1.User))
  (gr_text V:CGND:4:48 (at 125.62775 107.249975 35) (layer Eco1.User))
  (gr_text V:CGND:5:48 (at 123.21475 108.088175 35) (layer Eco1.User))
  (gr_text V:CGND:6:48 (at 121.99555 108.088175 35) (layer Eco1.User))
  (gr_text V:CGND:7:48 (at 121.99555 109.231175 35) (layer Eco1.User))
  (gr_text V:CGND:8:48 (at 123.21475 106.691175 35) (layer Eco1.User))
  (gr_text V:CGND:9:48 (at 121.99555 106.691175 35) (layer Eco1.User))
  (gr_text V:CGND:10:48 (at 121.99555 105.446575 35) (layer Eco1.User))
  (gr_text V:CGND:11:48 (at 123.21475 105.446575 35) (layer Eco1.User))
  (gr_text V:CGND:12:48 (at 121.99555 104.278175 35) (layer Eco1.User))
  (gr_text V:CGND:13:48 (at 123.21475 104.278175 35) (layer Eco1.User))
  (gr_text V:CGND:14:48 (at 123.21475 103.033575 35) (layer Eco1.User))
  (gr_text V:CGND:15:48 (at 121.99555 103.033575 35) (layer Eco1.User))
  (gr_text V:CGND:16:48 (at 121.99555 101.636575 35) (layer Eco1.User))
  (gr_text V:CGND:17:48 (at 123.21475 101.636575 35) (layer Eco1.User))
  (gr_text V:CGND:18:48 (at 123.21475 100.493575 35) (layer Eco1.User))
  (gr_text V:CGND:19:48 (at 121.99555 100.493575 35) (layer Eco1.User))
  (gr_text V:CGND:20:48 (at 158.80015 97.674175 35) (layer Eco1.User))
  (gr_text V:CGND:21:48 (at 159.48595 97.674175 35) (layer Eco1.User))
  (gr_text V:CGND:22:48 (at 159.48595 98.512375 35) (layer Eco1.User))
  (gr_text V:CGND:23:48 (at 167.94415 96.912175 35) (layer Eco1.User))
  (gr_text V:CGND:24:48 (at 167.94415 97.445575 35) (layer Eco1.User))
  (gr_text V:CGND:25:48 (at 169.46815 96.912175 35) (layer Eco1.User))
  (gr_text V:CGND:26:48 (at 169.46815 97.445575 35) (layer Eco1.User))
  (gr_text V:CGND:27:48 (at 168.70615 97.445575 35) (layer Eco1.User))
  (gr_text V:CGND:28:48 (at 168.70615 96.912175 35) (layer Eco1.User))
  (gr_text V:CGND:29:48 (at 169.46815 112.990375 35) (layer Eco1.User))
  (gr_text V:CGND:30:48 (at 169.46815 112.456975 35) (layer Eco1.User))
  (gr_text V:CGND:31:48 (at 167.94415 112.456975 35) (layer Eco1.User))
  (gr_text V:CGND:32:48 (at 167.94415 112.990375 35) (layer Eco1.User))
  (gr_text V:CGND:33:48 (at 168.70615 112.456975 35) (layer Eco1.User))
  (gr_text V:CGND:34:48 (at 168.70615 112.990375 35) (layer Eco1.User))
  (gr_text V:GND:35:48 (at 143.25535 109.916975 35) (layer Eco1.User))
  (gr_text V:GND:36:48 (at 138.17535 104.836975 35) (layer Eco1.User))
  (gr_text V:GND:37:48 (at 143.25535 99.756975 35) (layer Eco1.User))
  (gr_text V:GND:38:48 (at 148.33535 104.836975 35) (layer Eco1.User))
  (gr_text V:GND:39:48 (at 139.44535 108.646975 35) (layer Eco1.User))
  (gr_text V:GND:40:48 (at 139.44535 101.026975 35) (layer Eco1.User))
  (gr_text V:GND:41:48 (at 147.06535 101.026975 35) (layer Eco1.User))
  (gr_text V:GND:42:48 (at 147.06535 108.646975 35) (layer Eco1.User))
  (gr_text V:GND:43:48 (at 156.89515 103.693975 35) (layer Eco1.User))
  (gr_text V:GND:44:48 (at 127.02475 106.056175 35) (layer Eco1.User))
  (gr_text V:VDD_3V3AUX:45:48 (at 140.58835 107.376975 35) (layer Eco1.User))
  (gr_text V:VDD_3V3B:46:48 (at 145.79535 107.376975 35) (layer Eco1.User))
  (gr_text V:VDD_3V3B:47:48 (at 157.19995 111.161575 35) (layer Eco1.User))
  (gr_text V:VDD_RTC:48:48 (at 140.58835 102.296975 35) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:1:484 (at 125.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:2:484 (at 124.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:7:484 (at 129.92035 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:8:484 (at 129.92035 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:9:484 (at 156.89515 105.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:10:484 (at 156.89515 104.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:11:484 (at 156.90695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:12:484 (at 155.20695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:17:484 (at 127.03835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:18:484 (at 128.73835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:19:484 (at 172.75655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:20:484 (at 171.05655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:96:484 (at 127.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:97:484 (at 131.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:100:484 (at 124.09035 95.032537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:102:484 (at 124.34035 93.508537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:106:484 (at 128.15035 105.827537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:112:484 (at 123.404269 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:113:484 (at 123.95535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:114:484 (at 124.45535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:115:484 (at 125.006431 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:120:484 (at 155.79495 98.119619 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:123:484 (at 155.79495 96.517456 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:128:484 (at 155.79495 101.701019 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:129:484 (at 155.79495 101.149937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:130:484 (at 155.79495 100.649937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:131:484 (at 155.79495 100.098856 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:136:484 (at 155.79495 104.139419 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:137:484 (at 155.79495 103.588337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:138:484 (at 155.79495 103.088337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:139:484 (at 155.79495 102.537256 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:144:484 (at 155.79495 106.577819 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:145:484 (at 155.79495 106.026737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:146:484 (at 155.79495 105.526737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:147:484 (at 155.79495 104.975656 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:148:484 (at 155.79495 109.016219 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:149:484 (at 155.79495 108.465137 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:150:484 (at 155.79495 107.965137 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:151:484 (at 155.79495 107.414056 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:160:484 (at 162.039631 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:161:484 (at 161.48855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:162:484 (at 160.98855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:163:484 (at 160.437469 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:165:484 (at 164.38415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:166:484 (at 163.88415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:167:484 (at 163.333069 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:172:484 (at 163.03395 113.853937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:238:484 (at 143.89035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:239:484 (at 142.62035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:251:484 (at 147.70035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:252:484 (at 146.43035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:253:484 (at 145.16035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:254:484 (at 143.89035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:255:484 (at 142.62035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:256:484 (at 141.35035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:257:484 (at 140.08035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:258:484 (at 138.81035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:267:484 (at 147.70035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:268:484 (at 146.43035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:269:484 (at 145.16035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:270:484 (at 143.89035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:271:484 (at 142.62035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:272:484 (at 141.35035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:273:484 (at 140.08035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:274:484 (at 138.81035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:283:484 (at 147.70035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:284:484 (at 146.43035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:285:484 (at 145.16035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:286:484 (at 143.89035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:287:484 (at 142.62035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:288:484 (at 141.35035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:289:484 (at 140.08035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:290:484 (at 138.81035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:298:484 (at 148.97035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:299:484 (at 147.70035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:301:484 (at 145.16035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:302:484 (at 143.89035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:303:484 (at 142.62035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:304:484 (at 141.35035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:305:484 (at 140.08035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:306:484 (at 138.81035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:307:484 (at 137.54035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:314:484 (at 148.97035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:315:484 (at 147.70035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:317:484 (at 145.16035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:318:484 (at 143.89035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:319:484 (at 142.62035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:320:484 (at 141.35035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:321:484 (at 140.08035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:322:484 (at 138.81035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:323:484 (at 137.54035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:326:484 (at 133.73035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:331:484 (at 147.70035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:332:484 (at 146.43035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:333:484 (at 145.16035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:334:484 (at 143.89035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:335:484 (at 142.62035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:336:484 (at 141.35035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:337:484 (at 140.08035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:338:484 (at 138.81035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:347:484 (at 147.70035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:348:484 (at 146.43035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:349:484 (at 145.16035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:350:484 (at 143.89035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:351:484 (at 142.62035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:352:484 (at 141.35035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:353:484 (at 140.08035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:354:484 (at 138.81035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:363:484 (at 147.70035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:364:484 (at 146.43035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:365:484 (at 145.16035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:366:484 (at 143.89035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:367:484 (at 142.62035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:368:484 (at 141.35035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:369:484 (at 140.08035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:370:484 (at 138.81035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:381:484 (at 145.16035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:382:484 (at 143.89035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:383:484 (at 142.62035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:398:484 (at 143.89035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:399:484 (at 142.62035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:400:484 (at 141.35035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:414:484 (at 143.89035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:415:484 (at 142.62035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:416:484 (at 141.35035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:430:484 (at 143.89035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:431:484 (at 142.62035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:432:484 (at 141.35035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:441:484 (at 123.74035 99.238537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:443:484 (at 125.94035 97.938537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:447:484 (at 130.81535 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:449:484 (at 130.81535 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:459:484 (at 122.60735 101.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:460:484 (at 122.60735 103.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:461:484 (at 122.60735 106.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:462:484 (at 122.60735 108.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:463:484 (at 125.15735 108.064537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:464:484 (at 125.15735 101.864537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:467:484 (at 125.28235 106.264537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:469:484 (at 125.28235 103.664537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:473:484 (at 158.62095 106.148538 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:475:484 (at 158.62095 108.348537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:479:484 (at 159.22095 112.808537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:480:484 (at 168.72095 112.798537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:481:484 (at 168.72095 97.298537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:482:484 (at 159.12095 98.198537 10) (layer Eco1.User))
  (gr_text TS:CGND:1:28::L19 (at 158.6441 98.6528 50) (layer Eco1.User))
  (gr_text TE:CGND:1:28::L19 (at 125.4717 101.1932 310) (layer Eco1.User))
  (gr_text TS:GND:2:28::L19 (at 124.6843 97.7384 50) (layer Eco1.User))
  (gr_text TE:GND:2:28::L19 (at 124.4453 99.2778 310) (layer Eco1.User))
  (gr_text TS:GND:3:28::L19 (at 152.3113 93.5734 50) (layer Eco1.User))
  (gr_text TE:GND:3:28::L19 (at 155.1389 95.6814 310) (layer Eco1.User))
  (gr_text TS:GND:4:28::L19 (at 169.7693 114.1976 50) (layer Eco1.User))
  (gr_text TE:GND:4:28::L19 (at 163.6733 113.8932 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:5:28::L19 (at 140.4323 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:5:28::L19 (at 140.4323 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:6:28::L19 (at 139.9243 108.1524 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:6:28::L19 (at 140.4323 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:7:28::L19 (at 140.4323 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:7:28::L19 (at 139.9243 108.1528 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3AUX:8:28::L19 (at 139.9243 106.8824 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3AUX:8:28::L19 (at 140.4323 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:9:28::L19 (at 145.6393 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:9:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:10:28::L19 (at 157.0439 111.302 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:10:28::L19 (at 157.0439 111.3024 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:11:28::L19 (at 157.0439 111.302 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:11:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:12:28::L19 (at 142.1513 116.4334 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:12:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:13:28::L19 (at 145.0043 108.1524 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:13:28::L19 (at 142.1513 116.4338 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:14:28::L19 (at 145.6393 107.5174 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:14:28::L19 (at 145.0043 108.1528 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:15:28::L19 (at 145.0043 106.8824 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:15:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:16:28::L19 (at 146.2743 106.8824 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:16:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:17:28::L19 (at 146.2743 108.1524 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:17:28::L19 (at 145.6393 107.5178 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:18:28::L19 (at 155.6389 106.616681 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:18:28::L19 (at 146.2743 106.8828 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:19:28::L19 (at 155.6389 107.452919 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:19:28::L19 (at 155.6389 106.617081 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:20:28::L19 (at 156.7391 105.6298 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:20:28::L19 (at 155.6389 106.617081 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:21:28::L19 (at 158.4649 106.1874 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:21:28::L19 (at 156.7391 105.6302 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:22:28::L19 (at 156.7509 110.2352 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:22:28::L19 (at 155.6389 107.453319 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:23:28::L19 (at 157.0439 111.302 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:23:28::L19 (at 156.7509 110.2356 310) (layer Eco1.User))
  (gr_text TS:VDD_3V3B:24:28::L19 (at 156.6081 100.6888 50) (layer Eco1.User))
  (gr_text TE:VDD_3V3B:24:28::L19 (at 156.7391 105.6302 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:25:28::L19 (at 140.4323 102.4374 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:25:28::L19 (at 140.4323 102.4378 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:26:28::L19 (at 139.9243 103.0724 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:26:28::L19 (at 140.4323 102.4378 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:27:28::L19 (at 140.4323 102.4374 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:27:28::L19 (at 139.9243 103.0728 310) (layer Eco1.User))
  (gr_text TS:VDD_RTC:28:28::L19 (at 139.9243 101.8024 50) (layer Eco1.User))
  (gr_text TE:VDD_RTC:28:28::L19 (at 140.4323 102.4378 310) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:1:532 (at 125.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:2:532 (at 124.34035 96.556537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:7:532 (at 129.92035 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:8:532 (at 129.92035 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:9:532 (at 156.89515 105.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:10:532 (at 156.89515 104.590937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:11:532 (at 156.90695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:12:532 (at 155.20695 110.196337 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:17:532 (at 127.03835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:18:532 (at 128.73835 102.906537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:19:532 (at 172.75655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:20:532 (at 171.05655 114.158737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:96:532 (at 127.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:97:532 (at 131.41235 107.490537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:100:532 (at 124.09035 95.032537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:102:532 (at 124.34035 93.508537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:106:532 (at 128.15035 105.827537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:112:532 (at 123.404269 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:113:532 (at 123.95535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:114:532 (at 124.45535 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:115:532 (at 125.006431 116.487537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:120:532 (at 155.79495 98.119619 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:123:532 (at 155.79495 96.517456 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:128:532 (at 155.79495 101.701019 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:129:532 (at 155.79495 101.149937 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:130:532 (at 155.79495 100.649937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:131:532 (at 155.79495 100.098856 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:136:532 (at 155.79495 104.139419 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:137:532 (at 155.79495 103.588337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:138:532 (at 155.79495 103.088337 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:139:532 (at 155.79495 102.537256 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:144:532 (at 155.79495 106.577819 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:145:532 (at 155.79495 106.026737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:146:532 (at 155.79495 105.526737 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:147:532 (at 155.79495 104.975656 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:148:532 (at 155.79495 109.016219 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:149:532 (at 155.79495 108.465137 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:150:532 (at 155.79495 107.965137 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:151:532 (at 155.79495 107.414056 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:160:532 (at 162.039631 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:161:532 (at 161.48855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:162:532 (at 160.98855 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:163:532 (at 160.437469 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:165:532 (at 164.38415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:166:532 (at 163.88415 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:167:532 (at 163.333069 95.294537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:172:532 (at 163.03395 113.853937 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:238:532 (at 143.89035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:239:532 (at 142.62035 110.653537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:251:532 (at 147.70035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:252:532 (at 146.43035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:253:532 (at 145.16035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:254:532 (at 143.89035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:255:532 (at 142.62035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:256:532 (at 141.35035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:257:532 (at 140.08035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:258:532 (at 138.81035 109.383537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:267:532 (at 147.70035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:268:532 (at 146.43035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:269:532 (at 145.16035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:270:532 (at 143.89035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:271:532 (at 142.62035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:272:532 (at 141.35035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:273:532 (at 140.08035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:274:532 (at 138.81035 108.113537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:283:532 (at 147.70035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:284:532 (at 146.43035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:285:532 (at 145.16035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:286:532 (at 143.89035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:287:532 (at 142.62035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:288:532 (at 141.35035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3AUX:289:532 (at 140.08035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:290:532 (at 138.81035 106.843537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:298:532 (at 148.97035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:299:532 (at 147.70035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:301:532 (at 145.16035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:302:532 (at 143.89035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:303:532 (at 142.62035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:304:532 (at 141.35035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:305:532 (at 140.08035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:306:532 (at 138.81035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:307:532 (at 137.54035 105.573537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:314:532 (at 148.97035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:315:532 (at 147.70035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:317:532 (at 145.16035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:318:532 (at 143.89035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:319:532 (at 142.62035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:320:532 (at 141.35035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:321:532 (at 140.08035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:322:532 (at 138.81035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:323:532 (at 137.54035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:326:532 (at 133.73035 104.303537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:331:532 (at 147.70035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:332:532 (at 146.43035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:333:532 (at 145.16035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:334:532 (at 143.89035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:335:532 (at 142.62035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:336:532 (at 141.35035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:337:532 (at 140.08035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:338:532 (at 138.81035 103.033537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:347:532 (at 147.70035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:348:532 (at 146.43035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:SYS_5V:349:532 (at 145.16035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:350:532 (at 143.89035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3A:351:532 (at 142.62035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_1V8:352:532 (at 141.35035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:353:532 (at 140.08035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:354:532 (at 138.81035 101.763537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:363:532 (at 147.70035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:364:532 (at 146.43035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:365:532 (at 145.16035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:366:532 (at 143.89035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:367:532 (at 142.62035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:368:532 (at 141.35035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:369:532 (at 140.08035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:370:532 (at 138.81035 100.493537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:381:532 (at 145.16035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:382:532 (at 143.89035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:383:532 (at 142.62035 99.223537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:398:532 (at 143.89035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:399:532 (at 142.62035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:400:532 (at 141.35035 97.953537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:414:532 (at 143.89035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:415:532 (at 142.62035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:416:532 (at 141.35035 96.683537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VIN.BAT:430:532 (at 143.89035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:431:532 (at 142.62035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_5V:432:532 (at 141.35035 95.413537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:441:532 (at 123.74035 99.238537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_RTC:443:532 (at 125.94035 97.938537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:447:532 (at 130.81535 102.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:USB_DC:449:532 (at 130.81535 103.406537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:507:532 (at 122.60735 101.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:508:532 (at 122.60735 103.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:509:532 (at 122.60735 106.164537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:510:532 (at 122.60735 108.764537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:511:532 (at 125.15735 108.064537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:512:532 (at 125.15735 101.864537 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:515:532 (at 125.28235 106.264537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VBUS.RAW:517:532 (at 125.28235 103.664537 10) (layer Eco1.User))
  (gr_text FillOverPAD:VDD_3V3B:521:532 (at 158.62095 106.148538 10) (layer Eco1.User))
  (gr_text FillOverPAD:GND:523:532 (at 158.62095 108.348537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:527:532 (at 159.22095 112.808537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:528:532 (at 168.72095 112.798537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:529:532 (at 168.72095 97.298537 10) (layer Eco1.User))
  (gr_text FillOverPAD:CGND:530:532 (at 159.12095 98.198537 10) (layer Eco1.User))
  (zone (net 1) (net_name GND) (layer DigitalGND) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 120.5011 87.0036) (xy 176.5011 87.0036) (xy 176.5011 123.0036) (xy 120.5011 123.0036)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 138.5271 103.5806) (xy 138.5271 100.4056) (xy 141.7021 100.4056) (xy 142.3371 99.7706) (xy 142.3371 99.1356)
        (xy 143.8611 99.1356) (xy 143.8611 99.7706) (xy 144.4961 100.4056) (xy 147.6711 100.4056) (xy 147.6711 103.5806)
        (xy 148.3061 104.2156) (xy 148.9411 104.2156) (xy 148.9411 105.7396) (xy 148.3061 105.7396) (xy 147.6711 106.3746)
        (xy 147.6711 109.5496) (xy 144.4961 109.5496) (xy 143.8611 110.1846) (xy 143.8611 110.8196) (xy 142.3371 110.8196)
        (xy 142.3371 110.1846) (xy 141.7021 109.5496) (xy 138.5271 109.5496) (xy 138.5271 106.3746) (xy 137.8921 105.7396)
        (xy 137.2571 105.7396) (xy 137.2571 104.2156) (xy 137.8921 104.2156)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 155.3673 105.5872) (xy 155.8245 105.5872) (xy 155.8245 104.8252) (xy 157.4247 104.8252) (xy 157.4247 102.3106)
        (xy 158.1867 101.5486) (xy 158.1867 99.796) (xy 157.5009 99.1102) (xy 156.7389 99.1102) (xy 156.2817 99.5674)
        (xy 155.2911 99.5674) (xy 155.2149 99.6436) (xy 155.2149 105.4348)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 124.0491 106.1206) (xy 124.0491 106.5778) (xy 124.2777 106.8064) (xy 125.9541 106.8064) (xy 126.1827 107.035)
        (xy 126.1827 107.8732) (xy 126.5637 108.2542) (xy 132.2787 108.2542) (xy 132.4311 108.1018) (xy 132.4311 107.035)
        (xy 132.0501 106.654) (xy 128.8497 106.654) (xy 128.5449 106.3492) (xy 128.5449 105.6634) (xy 128.3163 105.4348)
        (xy 126.6399 105.4348) (xy 125.9541 106.1206)
      )
    )
  )
  (zone (net 2) (net_name VDD_3V3A) (layer Top) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 142.3371 101.6756) (xy 143.8611 101.6756) (xy 143.8611 103.5806) (xy 144.4961 104.2156) (xy 145.1311 104.2156)
        (xy 145.1311 105.7396) (xy 144.4961 105.7396) (xy 143.8611 106.3746) (xy 143.8611 108.2796) (xy 142.3371 108.2796)
      )
    )
  )
  (zone (net 3) (net_name VDD_1V8) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 141.06144 101.66858) (xy 141.0671 103.5806) (xy 140.3051 104.3426) (xy 139.7889 104.3432) (xy 139.7889 105.6132)
        (xy 140.3051 105.6126) (xy 141.0671 106.3746) (xy 141.0716 108.2802) (xy 141.3256 108.2802) (xy 141.31544 101.66858)
      )
    )
  )
  (zone (net 4) (net_name VDD_RTC) (layer Top) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 139.7971 101.6756) (xy 140.4321 101.6756) (xy 140.6861 101.9296) (xy 140.6861 102.9456) (xy 140.4321 103.1996)
        (xy 139.7971 103.1996)
      )
    )
  )
  (zone (net 5) (net_name USB_DC) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 127.7321 102.8186) (xy 127.7321 103.9616) (xy 127.8591 104.0886) (xy 129.8911 104.0886) (xy 130.2721 104.4696)
        (xy 130.6531 104.4696) (xy 131.0341 104.0886) (xy 130.7801 103.8346) (xy 130.7801 103.4536) (xy 129.8911 103.4536)
        (xy 129.8911 103.0726) (xy 129.5101 103.0726) (xy 129.1291 102.8186)
      )
    )
  )
  (zone (net 5) (net_name USB_DC) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 142.5911 95.3256) (xy 141.9561 95.3256) (xy 141.7021 95.5796) (xy 141.7021 97.8656) (xy 141.9561 98.1196)
        (xy 142.5911 98.1196)
      )
    )
  )
  (zone (net 6) (net_name VDD_5V) (layer Top) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 141.3211 95.3256) (xy 140.6861 95.3256) (xy 140.4321 95.5796) (xy 140.4321 97.8656) (xy 140.6861 98.1196)
        (xy 141.3211 98.1196)
      )
    )
  )
  (zone (net 7) (net_name VDD_3V3B) (layer VDD) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 120.2511 86.7536) (xy 176.7511 86.7536) (xy 176.7511 123.2536) (xy 120.2511 123.2536)
      )
    )
  )
  (zone (net 7) (net_name VDD_3V3B) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 144.8308 108.331) (xy 144.8308 106.68) (xy 146.431 106.68) (xy 146.431 108.331)
      )
    )
  )
  (zone (net 7) (net_name VDD_3V3B) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 156.591 111.5308) (xy 157.2768 111.5308) (xy 157.5054 111.3022) (xy 157.5054 106.8826) (xy 157.6578 106.7302)
        (xy 158.6484 106.7302) (xy 158.6484 105.6634) (xy 156.3624 105.6634) (xy 155.9814 106.0444) (xy 155.448 106.0444)
        (xy 155.2956 106.1968) (xy 155.2956 107.5684) (xy 155.3718 107.6446) (xy 155.9814 107.6446) (xy 156.21 107.8732)
        (xy 156.21 111.1498)
      )
    )
  )
  (zone (net 8) (net_name VDD_3V3AUX) (layer Top) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 139.7971 106.7556) (xy 140.4321 106.7556) (xy 140.6861 107.0096) (xy 140.6861 108.0256) (xy 140.4321 108.2796)
        (xy 139.7971 108.2796)
      )
    )
  )
  (zone (net 9) (net_name SYS_5V) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 144.8054 101.6508) (xy 146.4564 101.6508) (xy 146.4564 103.2256) (xy 144.8054 103.2256)
      )
    )
  )
  (zone (net 10) (net_name CGND) (layer Top) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 177.0011 123.5036) (xy 120.0011 123.5036) (xy 120.0011 86.5036) (xy 177.0011 86.5036)
      )
    )
    (polygon
      (pts
        (xy 126.4875 90.1186) (xy 125.8779 90.7282) (xy 125.8779 102.2344) (xy 124.9635 102.2344) (xy 123.7511 103.4468)
        (xy 123.7511 106.8132) (xy 124.1253 107.1874) (xy 125.6493 107.1874) (xy 125.6493 113.7406) (xy 126.3351 114.4264)
        (xy 129.6117 114.4264) (xy 131.1357 115.9504) (xy 131.1357 116.8648) (xy 131.6691 117.3982) (xy 137.6889 117.3982)
        (xy 138.8319 118.5412) (xy 138.8319 119.3794) (xy 139.2891 119.8366) (xy 170.6835 119.8366) (xy 170.6835 116.7124)
        (xy 171.6741 115.7218) (xy 171.6741 113.512) (xy 166.4925 113.512) (xy 166.4925 106.0444) (xy 167.5333 105.0036)
        (xy 167.5593 105.0036) (xy 167.5593 96.5956) (xy 168.4737 95.6812) (xy 169.3881 95.6812) (xy 171.0645 94.0048)
        (xy 171.0645 90.652) (xy 170.5311 90.1186)
      )
    )
  )
  (zone (net 10) (net_name CGND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 176.2511 122.7536) (xy 120.7511 122.7536) (xy 120.7511 87.2536) (xy 176.2511 87.2536)
      )
    )
    (polygon
      (pts
        (xy 128.0115 90.1186) (xy 128.0115 119.9128) (xy 165.3495 119.9128) (xy 165.9591 119.3032) (xy 165.9591 116.1028)
        (xy 165.3495 115.4932) (xy 161.6919 115.4932) (xy 156.4341 110.2354) (xy 156.4341 97.129) (xy 159.0249 94.5382)
        (xy 167.8641 94.5382) (xy 168.4737 93.9286) (xy 168.4737 90.652) (xy 167.9403 90.1186)
      )
    )
  )
  (zone (net 11) (net_name VIN.BAT) (layer Top) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 143.8611 98.1196) (xy 143.8611 94.8176) (xy 143.4801 94.4366) (xy 143.4801 90.6266) (xy 142.5911 89.7376)
        (xy 141.7021 89.7376) (xy 140.9401 90.4996) (xy 140.9401 91.6426) (xy 141.5751 92.2776) (xy 142.5911 92.2776)
        (xy 143.2261 92.9126) (xy 143.2261 95.3256) (xy 142.9721 95.5796) (xy 142.9721 97.8656) (xy 143.2261 98.1196)
      )
    )
  )
  (zone (net 12) (net_name VBUS.RAW) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 124.50572 103.5812) (xy 125.9541 103.5806) (xy 126.0811 103.4536) (xy 126.0811 102.8186) (xy 126.2081 102.6916)
        (xy 127.0971 102.6916) (xy 127.0971 103.9616) (xy 126.9701 104.0886) (xy 126.0811 104.0886) (xy 125.8271 103.8346)
        (xy 124.50572 103.8352)
      )
    )
  )
)
