(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "/GND")
  (net 2 "/VOUT")
  (net 3 "/VIN1")
  (net 4 "/ON")
  (net 5 "/VIN2")
  (net 6 "/ST")
  (footprint "Hubtech_Custom:SOTFL50P160X60-8N" locked placed (layer "F.Cu")
    (at 134.6075 120.65)
    (descr "DRL0008A")
    (tags "Integrated Circuit")
    (property "Height" "0.6")
    (property "Manufacturer_Name" "Texas Instruments")
    (property "Manufacturer_Part_Number" "LM66200DRLR")
    (property "Mouser Part Number" "595-LM66200DRLR")
    (property "Mouser Price/Stock" "https://www.mouser.ca/ProductDetail/Texas-Instruments/LM66200DRLR?qs=Rp5uXu7WBW90hnpZAkIOdQ%3D%3D")
    (property "Sheetfile" "LM66200 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "1.6-V to 5.5-V, 40-m, 2.5-A, low-IQ, dual ideal diode")
    (attr smd)
    (fp_text reference "IC1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LM66200DRLR" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -0.838 -0.75 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "2" smd rect locked (at -0.838 -0.25 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/VOUT") (pinfunction "VOUT_1") (pintype "passive"))
    (pad "3" smd rect locked (at -0.838 0.25 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/VIN1") (pinfunction "VIN1") (pintype "passive"))
    (pad "4" smd rect locked (at -0.838 0.75 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/ON") (pinfunction "~{ON}") (pintype "passive"))
    (pad "5" smd rect locked (at 0.838 0.75 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "6" smd rect locked (at 0.838 0.25 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/VIN2") (pinfunction "VIN2") (pintype "passive"))
    (pad "7" smd rect locked (at 0.838 -0.25 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/VOUT") (pinfunction "VOUT_2") (pintype "passive"))
    (pad "8" smd rect locked (at 0.838 -0.75 90) (size 0.3 0.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/ST") (pinfunction "ST") (pintype "passive"))
    (model "${HUBTECH_CUSTOM_DIR}/3dshapes/LM66200DRLR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" locked (layer "F.Cu")
    (at 130.835 116.85)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "LM66200 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 0 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "/GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/VOUT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/VIN1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/ON") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 -1.7))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" locked placed (layer "F.Cu")
    (at 138.43 124.47 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "LM66200 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 0 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "/GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/VIN2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/VOUT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/ST") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 -1.7))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (gr_rect locked (start 129.37 115.4) (end 139.89 125.95)
    (fill none) (layer "Edge.Cuts"))
  (gr_text locked "2" (at 137.142 121.91) (layer "B.SilkS"))
  (gr_text locked "ON" (at 132.147 124.46) (layer "B.SilkS"))
  (gr_text locked "VOUT" (at 134.62 119.38) (layer "B.SilkS"))
  (gr_text locked "1" (at 132.147 121.95) (layer "B.SilkS"))
  (gr_text locked "GND" (at 132.147 116.84) (layer "B.SilkS"))
  (gr_text locked "ST" (at 137.082 116.84) (layer "B.SilkS"))
  (gr_text locked "GND" (at 137.082 124.46) (layer "B.SilkS"))
  (gr_text locked "VIN" (at 134.602 121.92) (layer "B.SilkS"))
  (gr_text locked "VIN" (at 134.62 122.555) (layer "F.SilkS"))
  (gr_text locked "VOUT" (at 134.62 118.7) (layer "F.SilkS"))
  (gr_text locked "GND" (at 132.165 116.85) (layer "F.SilkS"))
  (gr_text locked "ST" (at 137.1 116.85) (layer "F.SilkS"))
  (gr_text locked "GND" (at 137.1 124.47) (layer "F.SilkS"))
  (gr_text locked "ON" (at 132.165 124.47) (layer "F.SilkS"))
  (gr_text locked "2" (at 137.16 121.92) (layer "F.SilkS"))
  (gr_text locked "1" (at 132.165 121.96) (layer "F.SilkS"))
  (zone (net 3) (net_name "/VIN1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.562744 121.831388)
        (xy 132.350612 121.619256)
        (xy 131.160281 121.144702)
        (xy 130.834293 121.930707)
        (xy 131.160281 122.715298)
      )
    )
  )
  (zone (net 2) (net_name "/VOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.684798 119.43607)
        (xy 136.89693 119.648202)
        (xy 138.104719 120.175298)
        (xy 138.430707 119.389293)
        (xy 138.104719 118.604702)
      )
    )
  )
  (zone (net 5) (net_name "/VIN2") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.899743 121.654611)
        (xy 136.687611 121.866743)
        (xy 138.104719 122.715298)
        (xy 138.430707 121.930707)
        (xy 138.104719 121.144702)
      )
    )
  )
  (zone (net 1) (net_name "/GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.535 117)
        (xy 132.535 116.7)
        (xy 131.685 116)
        (xy 130.834 116.85)
        (xy 131.685 117.7)
      )
    )
  )
  (zone (net 2) (net_name "/VOUT") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.353425 119.683557)
        (xy 132.565557 119.471425)
        (xy 131.160281 118.604702)
        (xy 130.834293 119.389293)
        (xy 131.160281 120.175298)
      )
    )
  )
  (zone (net 6) (net_name "/ST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.73 116.7)
        (xy 136.73 117)
        (xy 138.104719 117.635298)
        (xy 138.431 116.85)
        (xy 138.104719 116.064702)
      )
    )
  )
  (zone (net 4) (net_name "/ON") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.535 124.62)
        (xy 132.535 124.32)
        (xy 131.160281 123.684702)
        (xy 130.834 124.47)
        (xy 131.160281 125.255298)
      )
    )
  )
  (zone (net 1) (net_name "/GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 136.73 124.32)
        (xy 136.73 124.62)
        (xy 137.58 125.32)
        (xy 138.431 124.47)
        (xy 137.58 123.62)
      )
    )
  )
  (zone locked (net 1) (net_name "/GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 129.24 115.3)
        (xy 140 115.3)
        (xy 139.9 126.1)
        (xy 129.24 126.1)
      )
    )
  )
)
