(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 0)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 14)
    (tracks 128)
    (zones 0)
    (modules 6)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Housings_SSOP:MSOP-16-1EP_3x4mm_Pitch0.5mm (layer F.Cu) (tedit 59A28CD3)
    (at 189.23 130.81)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference MSOP16 (at 0 -3.35) (layer F.SilkS))
    (fp_text value MSOP-16-1EP_3x4mm_Pitch0.5mm (at 0 3.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.2 -1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.2 -0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.2 -0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.2 0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.2 0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.2 -0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.2 -0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.2 -1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.2 -1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.2 0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.2 1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2.2 1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 2.2 0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.2 1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.2 1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 0 -0.1) (size 1.65 2.85) (layers F.Cu F.Paste F.Mask))
    (model Housings_SSOP.3dshapes/MSOP-16_3x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 59A28A48)
    (at 182.88 121.92)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x08 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 59A28A4B)
    (at 195.58 121.92)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x08 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 59A28B25)
    (at 187.96 139.7)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference REF** (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer B.Cu) (tedit 59A28CCA)
    (at 189.23 130.81 180)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference SOIC16 (at 0 6 180) (layer B.SilkS))
    (fp_text value SOIC-16_3.9x9.9mm_Pitch1.27mm (at 0 -6 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.7 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.7 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -2.7 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -2.7 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.7 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.7 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -2.7 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -2.7 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 2.7 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 2.7 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 2.7 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 2.7 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 2.7 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 2.7 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 2.7 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at 2.7 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 59A28EBE)
    (at 189.23 122.809)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 197.485 120.015) (end 180.975 120.015) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 197.485 141.605) (end 197.485 120.015) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.975 141.605) (end 197.485 141.605) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.975 120.015) (end 180.975 141.605) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text NC (at 190.627 139.573 90) (layer B.SilkS))
  (gr_text 9 (at 185.166 139.7) (layer B.SilkS))
  (gr_text 8 (at 193.167 139.7) (layer B.SilkS))
  (gr_text 16 (at 185.674 121.92) (layer B.SilkS))
  (gr_text 1 (at 193.167 121.92) (layer B.SilkS))
  (gr_text Pad (at 190.627 139.7 90) (layer F.SilkS))
  (gr_text 9 (at 193.167 139.7) (layer F.SilkS))
  (gr_text 8 (at 185.166 139.7) (layer F.SilkS))
  (gr_text 16 (at 192.659 121.92) (layer F.SilkS))
  (gr_text 1 (at 185.166 121.92) (layer F.SilkS))
)
