<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>ERR</text>
<text>STS</text>
<text>3V3</text>
<text>+5V</text>
<text>VID</text>
<text>GND</text>
<text>CAM</text>
<text>VID
OUT</text>
<text>+5V</text>
<text>GND</text>
<text>OSD ALPHA
TIM KOSTKA
2016-AUG-11</text>
<text>VTX</text>
</plain>
<libraries>
<library name="kcl_connectors_auto">
<packages>
<package name="SAM-TSW-103-XX-X-S-RA">
</package>
</packages>
</library>
<library name="kcl_ics">
<packages>
<package name="TSSOP16-4P4X5MM">
</package>
<package name="SOIC8N">
<description>SOIC8, 3.8mm (0.150") body.</description>
</package>
<package name="VFSOP8-2P3X2MM">
<description>TI DCU Package</description>
</package>
<package name="UFQFPN48EP-7X7MM">
<description>UFQFPN48, 7x7mm package.</description>
</package>
<package name="SOT23-5">
<description>TI's SOT23-5 PACKAGE
DVB (R-PDSO-G5)</description>
</package>
<package name="SG-210STF">
<description>Epson oscillator</description>
</package>
</packages>
</library>
<library name="kcl_pdb360">
<packages>
<package name="FRAME36MM">
<description>36mm x 36mm frame</description>
</package>
</packages>
</library>
<library name="kcl_passives">
<packages>
<package name="C0603R">
<description>Chip capacitor land pattern, reflow soldering, size 0603.</description>
</package>
<package name="C0402R">
<description>Chip capacitor land pattern, reflow soldering, size 0402.</description>
</package>
<package name="RES0402R">
<description>Vishay MCS 0402 resistor footprint for reflow soldering.</description>
</package>
<package name="VIS-VLMX1500">
<description>0402 CHIPLED
Vishay VLMX-1500

(OSRAM LT QH9G-Q2S2-25-1)</description>
</package>
<package name="SOD-523">
</package>
</packages>
</library>
<library name="kcl_connectors">
<packages>
<package name="SAM-FTSH-105-XX-X-DV-K">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="kcl_connectors_auto" package="SAM-TSW-103-XX-X-S-RA" value="CONN3TSW-S-RA">
<attribute name="PN" value="TSW-101-08-F-S-RA"/>
</element>
<element name="J2" library="kcl_connectors_auto" package="SAM-TSW-103-XX-X-S-RA" value="CONN3TSW-S-RA">
<attribute name="PN" value="TSW-101-08-F-S-RA"/>
</element>
<element name="F1" library="kcl_pdb360" package="FRAME36MM" value="FRAME36MM"/>
<element name="U5" library="kcl_ics" package="SOIC8N" value="NCS2553">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="NCS2553DR2G"/>
</element>
<element name="C2" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="C0402C104K4RACTU"/>
</element>
<element name="R1" library="kcl_passives" package="RES0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW040275R0FKED"/>
</element>
<element name="R7" library="kcl_passives" package="RES0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW040275R0FKED"/>
</element>
<element name="R8" library="kcl_passives" package="RES0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW040275R0FKED"/>
</element>
<element name="R9" library="kcl_passives" package="RES0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW040275R0FKED"/>
</element>
<element name="R10" library="kcl_passives" package="RES0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW040275R0FKED"/>
</element>
<element name="U3" library="kcl_ics" package="TSSOP16-4P4X5MM" value="74VHC4051TSSOP">
<attribute name="NAME"/>
<attribute name="PN" value="74VHC4051AFT"/>
</element>
<element name="U2" library="kcl_ics" package="VFSOP8-2P3X2MM" value="SN74LVC2G53DCU">
<attribute name="NAME"/>
<attribute name="PN" value="SN74LVC2G53DCUR"/>
</element>
<element name="R2" library="kcl_passives" package="RES0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW040275R0FKED"/>
</element>
<element name="R3" library="kcl_passives" package="RES0402R" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW040275R0FKED"/>
</element>
<element name="R4" library="kcl_passives" package="RES0402R" value="9.53K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04029K53FKED"/>
</element>
<element name="R5" library="kcl_passives" package="RES0402R" value="562">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW0402562RFKED"/>
</element>
<element name="R6" library="kcl_passives" package="RES0402R" value="8.87K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04028K87FKED"/>
</element>
<element name="R11" library="kcl_passives" package="RES0402R" value="1.13K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04021K13FKED"/>
</element>
<element name="R12" library="kcl_passives" package="RES0402R" value="8.87K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04028K87FKED"/>
</element>
<element name="R13" library="kcl_passives" package="RES0402R" value="1.24K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04021K24FKED"/>
</element>
<element name="R14" library="kcl_passives" package="RES0402R" value="7.50K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04027K50FKED"/>
</element>
<element name="R15" library="kcl_passives" package="RES0402R" value="2.26K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04022K26FKED"/>
</element>
<element name="R16" library="kcl_passives" package="RES0402R" value="8.87K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04028K87FKED"/>
</element>
<element name="R17" library="kcl_passives" package="RES0402R" value="1.07K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04021K07FKED"/>
</element>
<element name="R18" library="kcl_passives" package="RES0402R" value="2.80K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04022K80FKED"/>
</element>
<element name="U4" library="kcl_ics" package="UFQFPN48EP-7X7MM" value="STM32F411-48UFQFPN48EP">
<attribute name="PN" value="STM32F411CEU6"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="C0603C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="kcl_passives" package="RES0402R" value="10K">
<attribute name="PN" value="CRCW040210K0FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="kcl_passives" package="RES0402R" value="10K">
<attribute name="PN" value="CRCW040210K0FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="kcl_passives" package="VIS-VLMX1500" value="BLU">
<attribute name="PN" value="VLMB1500-GS08"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="kcl_passives" package="VIS-VLMX1500" value="RED">
<attribute name="PN" value="VLMS1500-GS08"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="kcl_passives" package="RES0402R" value="1K">
<attribute name="PN" value="CRCW04021K00FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="kcl_passives" package="RES0402R" value="1K">
<attribute name="PN" value="CRCW04021K00FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="kcl_passives" package="RES0402R" value="1K">
<attribute name="PN" value="CRCW04021K00FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="kcl_passives" package="VIS-VLMX1500" value="GRN">
<attribute name="PN" value="VLMG1500-GS08"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="kcl_ics" package="SOIC8N" value="LM1881SOIC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="LM1881M/NOPB"/>
</element>
<element name="C8" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="kcl_passives" package="RES0402R" value="680K">
<attribute name="PN" value="CRCW0402680KFKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="kcl_passives" package="RES0402R" value="8.45K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04028K45FKED"/>
</element>
<element name="R26" library="kcl_passives" package="RES0402R" value="1.62K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04021K62FKED"/>
</element>
<element name="R27" library="kcl_passives" package="RES0402R" value="4.32K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04024K32FKED"/>
</element>
<element name="R28" library="kcl_passives" package="RES0402R" value="9.09K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04029K09FKED"/>
</element>
<element name="R29" library="kcl_passives" package="RES0402R" value="976">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW0402976RFKED"/>
</element>
<element name="R30" library="kcl_passives" package="RES0402R" value="4.02K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04024K02FKED"/>
</element>
<element name="R31" library="kcl_passives" package="RES0402R" value="9.09K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04029K09FKED"/>
</element>
<element name="R32" library="kcl_passives" package="RES0402R" value="931">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW0402931RFKED"/>
</element>
<element name="R33" library="kcl_passives" package="RES0402R" value="8.87K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="CRCW04028K87FKED"/>
</element>
<element name="R34" library="kcl_passives" package="RES0402R" value="10K">
<attribute name="PN" value="CRCW040210K0FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="kcl_passives" package="RES0402R" value="10K">
<attribute name="PN" value="CRCW040210K0FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="kcl_passives" package="RES0402R" value="10K">
<attribute name="PN" value="CRCW040210K0FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="kcl_passives" package="RES0402R" value="10K">
<attribute name="PN" value="CRCW040210K0FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="C0402C104K4RACTU"/>
</element>
<element name="C11" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="C0603C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="C0402C104K4RACTU"/>
</element>
<element name="C13" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="C0603C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="C0402C104K4RACTU"/>
</element>
<element name="C15" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="C0603C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="C0402C104K4RACTU"/>
</element>
<element name="C17" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="C0603C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="kcl_connectors" package="SAM-FTSH-105-XX-X-DV-K" value="CONN2X05FTSH">
<attribute name="PN" value="SAM-FTSH-105-01-L-DV-K"/>
<attribute name="NAME"/>
</element>
<element name="D2" library="kcl_passives" package="SOD-523" value="SCHOTTKYSOD-523">
<attribute name="PN" value="NSR0520V2T1G"/>
<attribute name="NAME"/>
</element>
<element name="C18" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="C0603C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="kcl_passives" package="C0603R" value="2.2uF">
<attribute name="PN" value="C0603C225K8RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="kcl_ics" package="SOT23-5" value="MIC5219">
<attribute name="PN" value="MIC5225-3.3YM5-TR"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="kcl_passives" package="SOD-523" value="SCHOTTKYSOD-523">
<attribute name="PN" value="NSR0520V2T1G"/>
<attribute name="NAME"/>
</element>
<element name="Y1" library="kcl_ics" package="SG-210STF" value="SG-210STF">
<attribute name="NAME"/>
<attribute name="PN" value="SG-210STF 14.31818ML"/>
</element>
<element name="C19" library="kcl_passives" package="C0402R" value="0.1uF">
<attribute name="PN" value="C0402C104K4RACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+5V">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="U5" pad="4"/>
<contactref element="U3" pad="16"/>
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="U7" pad="8"/>
<contactref element="U2" pad="8"/>
<contactref element="R25" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="D1" pad="C"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="F1" pad="1@31"/>
<contactref element="F1" pad="1@32"/>
<contactref element="F1" pad="1@33"/>
<contactref element="F1" pad="1@34"/>
<contactref element="F1" pad="1@35"/>
<contactref element="F1" pad="1@36"/>
<contactref element="F1" pad="1@37"/>
<contactref element="F1" pad="1@38"/>
<contactref element="F1" pad="1@39"/>
<contactref element="F1" pad="1@40"/>
<contactref element="F1" pad="1@21"/>
<contactref element="F1" pad="1@22"/>
<contactref element="F1" pad="1@23"/>
<contactref element="F1" pad="1@24"/>
<contactref element="F1" pad="1@25"/>
<contactref element="F1" pad="1@26"/>
<contactref element="F1" pad="1@27"/>
<contactref element="F1" pad="1@28"/>
<contactref element="F1" pad="1@29"/>
<contactref element="F1" pad="1@30"/>
<contactref element="F1" pad="1@11"/>
<contactref element="F1" pad="1@12"/>
<contactref element="F1" pad="1@13"/>
<contactref element="F1" pad="1@14"/>
<contactref element="F1" pad="1@15"/>
<contactref element="F1" pad="1@16"/>
<contactref element="F1" pad="1@17"/>
<contactref element="F1" pad="1@18"/>
<contactref element="F1" pad="1@19"/>
<contactref element="F1" pad="1@20"/>
<contactref element="F1" pad="1@1"/>
<contactref element="F1" pad="1@2"/>
<contactref element="F1" pad="1@3"/>
<contactref element="F1" pad="1@4"/>
<contactref element="F1" pad="1@5"/>
<contactref element="F1" pad="1@6"/>
<contactref element="F1" pad="1@7"/>
<contactref element="F1" pad="1@8"/>
<contactref element="F1" pad="1@9"/>
<contactref element="F1" pad="1@10"/>
<contactref element="R1" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="6"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="23"/>
<contactref element="U4" pad="35"/>
<contactref element="U4" pad="47"/>
<contactref element="U4" pad="PAD"/>
<contactref element="R19" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="U7" pad="4"/>
<contactref element="R26" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="C22" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="J9" pad="9"/>
<contactref element="J9" pad="5"/>
<contactref element="J9" pad="3"/>
<contactref element="C19" pad="2"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="VID_OUT">
<contactref element="J2" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="VID_OSD">
<contactref element="U3" pad="3"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U5" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U5" pad="8"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="VID_IN">
<contactref element="C2" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U5" pad="7"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U5" pad="6"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="VID_MUXED">
<contactref element="U5" pad="3"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="SIG_RED">
<contactref element="U3" pad="13"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="SIG_GRN">
<contactref element="U3" pad="14"/>
<contactref element="R25" pad="1"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="SIG_BLU">
<contactref element="U3" pad="15"/>
<contactref element="R28" pad="1"/>
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="SIG_WHT">
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="SIG_BLK">
<contactref element="U3" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="SIG_BLANK">
<contactref element="U3" pad="5"/>
<contactref element="R6" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="SIG_SYNC">
<contactref element="U3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SIG_BURST">
<contactref element="R31" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="N$1">
<contactref element="R9" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="+3V3">
<contactref element="U4" pad="48"/>
<contactref element="U4" pad="36"/>
<contactref element="U4" pad="24"/>
<contactref element="U4" pad="9"/>
<contactref element="U4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="C22" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="C19" pad="1"/>
<contactref element="Y1" pad="4"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="BOOT0">
<contactref element="U4" pad="44"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="NRST">
<contactref element="U4" pad="7"/>
<contactref element="R20" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="J9" pad="10"/>
</signal>
<signal name="SWDIO">
<contactref element="U4" pad="34"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="U4" pad="37"/>
<contactref element="J9" pad="4"/>
</signal>
<signal name="USART1_TX">
<contactref element="U4" pad="30"/>
<contactref element="J9" pad="8"/>
</signal>
<signal name="SPI1_SCK1">
</signal>
<signal name="SPI1_MISO1">
</signal>
<signal name="SPI1_MOSI1">
</signal>
<signal name="SPI1_SCK2">
</signal>
<signal name="SPI1_MISO2">
</signal>
<signal name="SPI1_MOSI2">
</signal>
<signal name="SPI1_SCK3">
</signal>
<signal name="SPI1_MISO3">
</signal>
<signal name="SPI1_MOSI3">
</signal>
<signal name="N$23">
<contactref element="R22" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="R21" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="LED_ERR">
<contactref element="R21" pad="1"/>
<contactref element="U4" pad="46"/>
</signal>
<signal name="LED_STS">
<contactref element="R22" pad="1"/>
<contactref element="U4" pad="45"/>
</signal>
<signal name="N$35">
<contactref element="R23" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="CSYNC">
<contactref element="U7" pad="1"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U7" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="VSYNC">
<contactref element="U7" pad="3"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="OEOUT">
<contactref element="U7" pad="7"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="BPOUT">
<contactref element="U7" pad="5"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U7" pad="6"/>
<contactref element="C9" pad="1"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="TIM2_CH2">
<contactref element="U4" pad="11"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="TIM2_CH3">
<contactref element="U4" pad="12"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="TIM2_CH1">
<contactref element="U4" pad="10"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U4" pad="22"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U4" pad="39"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R36" pad="2"/>
<contactref element="U4" pad="43"/>
</signal>
<signal name="N$13">
<contactref element="R35" pad="2"/>
<contactref element="U4" pad="42"/>
</signal>
<signal name="TIM1_CH1">
<contactref element="U4" pad="29"/>
<contactref element="U4" pad="26"/>
<contactref element="U4" pad="25"/>
<contactref element="U4" pad="15"/>
<contactref element="U4" pad="21"/>
</signal>
<signal name="SPI2_MISO">
<contactref element="U4" pad="27"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="SPI1_MISO">
<contactref element="U4" pad="16"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="SPI3_MISO">
<contactref element="U4" pad="40"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="SPI4_MISO">
<contactref element="U3" pad="9"/>
<contactref element="U4" pad="32"/>
</signal>
<signal name="TIM2_CH4">
<contactref element="U4" pad="13"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U4" pad="41"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Y1" pad="3"/>
<contactref element="U4" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
