(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 10)
    (tracks 0)
    (zones 0)
    (modules 8)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module twinpeaks:drill1mm (layer F.Cu) (tedit 595EB003)
    (at 159.004 93.472)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value drill1 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module twinpeaks:drill1mm (layer F.Cu) (tedit 595EB003)
    (at 261.112 93.472)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value drill1 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module twinpeaks:drill1mm (layer F.Cu) (tedit 595EB003)
    (at 159.004 36.83)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value drill1 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module twinpeaks:old-coop (layer F.Cu) (tedit 0)
    (at 253.746 51.054)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module twinpeaks:coop3 (layer B.Cu) (tedit 0)
    (at 184.404 67.818)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module twinpeaks:zig (layer F.Cu) (tedit 0)
    (at 212.09 65.278)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module twinpeaks:drill1mm (layer F.Cu) (tedit 595EB003)
    (at 261.112 36.83)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value drill1 (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module twinpeaks:coop (layer F.Cu) (tedit 0)
    (at 164.592 49.022)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_line (start 157.734 35.56) (end 157.734 94.742) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 159.004 36.83) (end 159.512 37.084) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 159.004 93.472) (end 158.496 93.218) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 261.112 93.472) (end 260.604 93.218) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 261.112 36.83) (end 260.604 36.576) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 262.382 94.742) (end 157.734 94.742) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 262.382 35.56) (end 262.382 94.742) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.734 35.56) (end 262.382 35.56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Diane,\n11:30 a.m.\nFebruary Twenty-fourth. \nEntering the town of Twin Peaks." (at 204.48 74.41 180) (layer B.Mask))
  (gr_text "this is the water and this is the well\ndrink full and descend\nthe horse is the white of the eyes and dark within" (at 211.582 45.212) (layer F.Mask))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.638 33.02) (xy 271.018 33.02) (xy 270.256 100.076) (xy 148.844 101.6) (xy 150.368 33.02)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.066 30.48) (xy 277.876 30.734) (xy 275.59 101.854) (xy 141.478 103.886) (xy 144.526 32.004)
      )
    )
  )
)
