(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/K")
	(net 2 "/A")
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.85 94.15 180)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.77 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 5.31 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "SiPM VUV-HD2 carrier board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.975 6.275 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/K")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 103 102)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H5"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "SiPM VUV-HD2 carrier board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 107.825 93)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H3"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "SiPM VUV-HD2 carrier board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 124.175 93)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H2"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "SiPM VUV-HD2 carrier board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Downloaded parts:SiPM"
		(layer "F.Cu")
		(at 116 93)
		(property "Reference" "D1"
			(at 0.03 9 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0.03 14.09 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Downloaded parts:SiPM"
			(at 0.03 13.09 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0.03 13.09 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0.03 13.09 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "SiPM VUV-HD2 carrier board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.03 15.59 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 10 10)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/K")
			(pinfunction "K")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole circle
			(at -2.375 7)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.375 7)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A")
			(pinfunction "A")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 116 84.825)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H1"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "SiPM VUV-HD2 carrier board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 103 82.95)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H4"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "SiPM VUV-HD2 carrier board.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
	)
	(gr_rect
		(start 100 80)
		(end 140 105)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "SiPM carrier board v1\nB.L."
		(at 124.7 103.75 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "/A")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111 99) (xy 121 99) (xy 121 101) (xy 111 101)
			)
		)
	)
)
