(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 54)
    (zones 0)
    (modules 11)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad1)")
  (net 2 "Net-(A2-Pad1)")
  (net 3 "Net-(B1-Pad1)")
  (net 4 "Net-(B2-Pad1)")
  (net 5 "Net-(H1-Pad1)")
  (net 6 "Net-(H2-Pad1)")
  (net 7 "Net-(J0-Pad10)")
  (net 8 "Net-(J0-Pad7)")
  (net 9 "Net-(J0-Pad9)")
  (net 10 "Net-(J0-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A2-Pad1)")
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B2-Pad1)")
    (add_net "Net-(H1-Pad1)")
    (add_net "Net-(H2-Pad1)")
    (add_net "Net-(J0-Pad10)")
    (add_net "Net-(J0-Pad7)")
    (add_net "Net-(J0-Pad8)")
    (add_net "Net-(J0-Pad9)")
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at -6.477 0.9525 90)
    (fp_text reference T2I (at 0 1.651 90 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J0-Pad7)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at -9.398 -3.937 180)
    (fp_text reference T1V (at 0 1.651 180 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 180) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(J0-Pad9)"))
  )
  (module top:cle-105-01-g-dv (layer F.Cu) (tedit 5D125A81)
    (at 0 -10.16 270)
    (fp_text reference J0 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Counter_Clockwise (at 0 6.35 90) (layer F.Fab) hide)
    (pad 10 smd rect (at -1.6002 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J0-Pad10)"))
    (pad 9 smd rect (at -0.8001 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J0-Pad9)"))
    (pad 8 smd rect (at 0 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J0-Pad8)"))
    (pad 6 smd rect (at 1.6002 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(B1-Pad1)"))
    (pad 7 smd rect (at 0.8001 1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J0-Pad7)"))
    (pad 5 smd rect (at 1.6002 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(B2-Pad1)"))
    (pad 4 smd rect (at 0.8001 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 3 smd rect (at 0 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(A2-Pad1)"))
    (pad 2 smd rect (at -0.8001 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 smd rect (at -1.6002 -1.9812 270) (size 0.508 1.3716) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (model /home/zach/research/pcbs/3d/CLE-105-01-G-DV.stp
      (offset (xyz 0 0 0.13716))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at 0 6.858 270)
    (fp_text reference A2 (at 0 1.905 270 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(A2-Pad1)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at 0 -5.08 270)
    (fp_text reference B2 (at 0 1.905 270 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(B2-Pad1)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at -11.303 -3.937 180)
    (fp_text reference T1I (at 0 1.651 180 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 180) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J0-Pad10)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at 0 -6.858 270)
    (fp_text reference B1 (at 0 1.905 270 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(B1-Pad1)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at -6.477 -0.9525 90)
    (fp_text reference T2V (at 0 1.651 90 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 90) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(J0-Pad8)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at -11.303 3.81)
    (fp_text reference H2 (at 0 1.905 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(H2-Pad1)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at -9.398 3.81)
    (fp_text reference H1 (at 0 1.905 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(H1-Pad1)"))
  )
  (module top:wire-pad (layer F.Cu) (tedit 5D1254A3)
    (at 0 5.08 270)
    (fp_text reference A1 (at 0 1.905 270 unlocked) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 270) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(A1-Pad1)"))
  )
  (gr_circle (center 0 0) (end 3.175 0) (layer Edge.Cuts) (width 0.127))
  (gr_circle (center -10.3251 0) (end -7.9121 0) (layer Edge.Cuts) (width 0.127))
  (gr_circle (center 10.3251 0) (end 12.7381 0) (layer Edge.Cuts) (width 0.127))
  (gr_circle (center 0 0) (end 13.335 0) (layer Edge.Cuts) (width 0.127))
)
