(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 0.1)
    (drawings 15)
    (tracks 41)
    (zones 0)
    (modules 10)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.16)
    (user_trace_width 0.1524)
    (user_trace_width 0.16)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.16)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.7 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.08)
    (pad_size 0.8 0.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.04)
    (solder_mask_min_width 0.102)
    (pad_to_paste_clearance -0.01)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x0100c_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /G)
  (net 3 /B)
  (net 4 /R)
  (net 5 /JR)
  (net 6 /JG)
  (net 7 /JB)
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.16)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /B)
    (add_net /G)
    (add_net /JB)
    (add_net /JG)
    (add_net /JR)
    (add_net /R)
    (add_net GND)
  )
  (module 03_wirepad:Wirepad_D1.3mm (layer F.Cu) (tedit 6173D631)
    (at 29.9 2.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference G1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value pad (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 5.2 2.4)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -0.9) (layer F.SilkS))
    (fp_text value R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /B))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /JB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 18.3 2.4 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 0.9) (layer F.SilkS))
    (fp_text value R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /G))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /JG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 11.3 2.4 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 0.9) (layer F.SilkS))
    (fp_text value R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /R))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /JR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 03_wirepad:Wirepad_D1.3mm (layer F.Cu) (tedit 6173D631)
    (at 2.9 2.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J3 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value pad (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 7 /JB))
  )
  (module 03_wirepad:Wirepad_D1.3mm (layer F.Cu) (tedit 6173D631)
    (at 20.8 2.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J2 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value pad (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 6 /JG))
  )
  (module 03_wirepad:Wirepad_D1.3mm (layer F.Cu) (tedit 6173D631)
    (at 13.6 2.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value pad (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.3 1.3) (layers F.Cu F.Mask)
      (net 5 /JR))
  )
  (module 01_LED:LED_RGB_1.6mmx1.6mm_cathode (layer F.Cu) (tedit 60FAFB99)
    (at 41.5 2.4 90)
    (tags "LED RGB Chip SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value LED_RGBC (at 0 1.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd roundrect (at -0.45 0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.45 0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 2 /G))
    (pad 3 smd roundrect (at 0.45 -0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 3 /B))
    (pad 1 smd roundrect (at -0.45 -0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 4 /R))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_LiteOn_LTST-C19HE1WT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Z:/PCB/3D models/LED/LED-0606.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module 01_LED:LED_RGB_1.6mmx1.6mm_cathode (layer F.Cu) (tedit 60FAFB99)
    (at 24.9 2.4 90)
    (tags "LED RGB Chip SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value LED_RGBC (at 0 1.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd roundrect (at -0.45 0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.45 0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 2 /G))
    (pad 3 smd roundrect (at 0.45 -0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 3 /B))
    (pad 1 smd roundrect (at -0.45 -0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 4 /R))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_LiteOn_LTST-C19HE1WT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Z:/PCB/3D models/LED/LED-0606.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module 01_LED:LED_RGB_1.6mmx1.6mm_cathode (layer F.Cu) (tedit 60FAFB99)
    (at 8.3 2.4 90)
    (tags "LED RGB Chip SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.8 90) (layer F.SilkS) hide)
    (fp_text value LED_RGBC (at 0 1.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd roundrect (at -0.45 0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.45 0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 2 /G))
    (pad 3 smd roundrect (at 0.45 -0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 3 /B))
    (pad 1 smd roundrect (at -0.45 -0.725 90) (size 0.6 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.3)
      (net 4 /R))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_LiteOn_LTST-C19HE1WT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Z:/PCB/3D models/LED/LED-0606.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (gr_text thefreeman (at 35.2 1.2) (layer F.SilkS))
  (gr_text B (at 3.9 1.6) (layer F.SilkS))
  (gr_text R (at 14.7 1.6) (layer F.SilkS))
  (gr_text G (at 22 1.7) (layer F.SilkS))
  (gr_text C (at 28.6 1.6) (layer F.SilkS))
  (gr_text "FWAA AUX v1.1" (at 35.2 2.5) (layer F.SilkS))
  (gr_line (start 49.3 0) (end 0.5 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.3 6.8) (end 49.3 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.5 6.8) (end 49.3 6.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.5 0) (end 0.5 6.8) (layer Edge.Cuts) (width 0.05))
)
