(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "24 pin Receptacle/Wiring Board")
    (date "2020-01-11")
    (rev "02")
    (company "Smith College Physics")
    (comment 1 "N. Fortune")
    (comment 2 "for use in 0.5\" diameter vacuum capsule")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "Net-(J1-Pad17)")
  (net 18 "Net-(J1-Pad18)")
  (net 19 "Net-(J1-Pad19)")
  (net 20 "Net-(J1-Pad20)")
  (net 21 "Net-(J1-Pad21)")
  (net 22 "Net-(J1-Pad22)")
  (net 23 "Net-(J1-Pad23)")
  (net 24 "Net-(J1-Pad24)")
  (net 25 "GND")
  (net 26 "+BATT")
  (net 27 "-BATT")
  (footprint "505066-2422:MOLEX_505066-2422" (layer "F.Cu")
    (tedit 5E1B47FC)
    (at 136.146001 102.009001)
    (attr through_hole)
    (fp_text reference "J1" (at -2.542001 -0.028001 90) (layer "F.SilkS"))
    (fp_text value "505066-2422" (at 5.585999 -0.028001 90) (layer "F.SilkS"))
    (fp_text user "12" (at 4.188999 1.749999 90) (layer "F.SilkS"))
    (fp_text user "24" (at 4.188999 -1.806001 90) (layer "F.SilkS"))
    (fp_text user "13" (at -3.431001 -2.187001 270) (layer "F.SilkS"))
    (fp_text user "1" (at -3.431001 2.257999 90) (layer "F.SilkS"))
    (fp_text user "1" (at -3.558001 1.749999) (layer "F.Fab"))
    (fp_text user "24" (at 3.426999 -1.679001) (layer "F.Fab"))
    (fp_text user "2" (at -3.558001 -1.679001) (layer "F.Fab"))
    (fp_text user "23" (at 3.426999 1.749999) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.925 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 1 "VCC"))
    (pad "2" smd rect locked (at -1.925 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(J1-Pad2)"))
    (pad "3" smd rect locked (at -1.575 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(J1-Pad3)"))
    (pad "4" smd rect locked (at -1.575 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(J1-Pad4)"))
    (pad "5" smd rect locked (at -1.225 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(J1-Pad5)"))
    (pad "6" smd rect locked (at -1.225 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(J1-Pad6)"))
    (pad "7" smd rect locked (at -0.875 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(J1-Pad7)"))
    (pad "8" smd rect locked (at -0.875 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(J1-Pad8)"))
    (pad "9" smd rect locked (at -0.525 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(J1-Pad9)"))
    (pad "10" smd rect locked (at -0.525 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(J1-Pad10)"))
    (pad "11" smd rect locked (at -0.175 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(J1-Pad11)"))
    (pad "12" smd rect locked (at -0.175 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 12 "Net-(J1-Pad12)"))
    (pad "13" smd rect locked (at 0.175 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 13 "Net-(J1-Pad13)"))
    (pad "14" smd rect locked (at 0.175 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 14 "Net-(J1-Pad14)"))
    (pad "15" smd rect locked (at 0.525 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(J1-Pad15)"))
    (pad "16" smd rect locked (at 0.525 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 16 "Net-(J1-Pad16)"))
    (pad "17" smd rect locked (at 0.875 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 17 "Net-(J1-Pad17)"))
    (pad "18" smd rect locked (at 0.875 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 18 "Net-(J1-Pad18)"))
    (pad "19" smd rect locked (at 1.225 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 19 "Net-(J1-Pad19)"))
    (pad "20" smd rect locked (at 1.225 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 20 "Net-(J1-Pad20)"))
    (pad "21" smd rect locked (at 1.575 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 21 "Net-(J1-Pad21)"))
    (pad "22" smd rect locked (at 1.575 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 22 "Net-(J1-Pad22)"))
    (pad "23" smd rect locked (at 1.925 0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 23 "Net-(J1-Pad23)"))
    (pad "24" smd rect locked (at 1.925 -0.95) (size 0.18 0.4) (layers "F.Cu" "F.Mask")
      (net 24 "Net-(J1-Pad24)"))
    (pad "S1" smd rect locked (at -3.205 -0.4825) (size 0.4 0.385) (layers "F.Cu" "F.Mask")
      (net 25 "GND"))
    (pad "S2" smd rect locked (at -3.205 0.4825) (size 0.4 0.385) (layers "F.Cu" "F.Mask")
      (net 25 "GND"))
    (pad "S3" smd rect locked (at 3.205 -0.4825) (size 0.4 0.385) (layers "F.Cu" "F.Mask")
      (net 25 "GND"))
    (pad "S4" smd rect locked (at 3.205 0.4825) (size 0.4 0.385) (layers "F.Cu" "F.Mask")
      (net 25 "GND"))
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 132.842 104.14 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad3)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 132.715 99.822 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad2)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad4)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 134.239 104.14 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pad7)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad5)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 134.239 99.822 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad6)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J1-Pad8)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 136.144 104.14 90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0.275 0 90) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.275 0 90) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 90) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J1-Pad11)"))
    (pad "2" smd roundrect locked (at 0.25 0 90) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J1-Pad9)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 137.668 99.822 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad14)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J1-Pad16)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 138.811 104.14 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J1-Pad19)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J1-Pad17)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 140.335 104.14 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -0.508 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J1-Pad23)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J1-Pad21)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 140.335 99.822 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.0635 -0.508 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J1-Pad22)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J1-Pad24)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 138.811 99.822 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.016 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J1-Pad18)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J1-Pad20)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 133.604 101.981 90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "RH2" (at 0 1 270) (layer "B.SilkS") hide)
    (fp_text value "1k" (at 0 -1 270) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.143 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at -0.275 0 90) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.275 0 90) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 90) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "+BATT"))
    (pad "2" smd roundrect locked (at 0.25 0 90) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "-BATT"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 135.763 99.822 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R6" (at 1.016 2.921) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J1-Pad10)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J1-Pad12)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_01005_0402Metric" (layer "B.Cu")
    (tedit 5B301BBD)
    (at 137.287 104.14 -90)
    (descr "Resistor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 1 90) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.889 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at -0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.275 0 270) (size 0.27 0.27) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J1-Pad15)"))
    (pad "2" smd roundrect locked (at 0.25 0 270) (size 0.4 0.3) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J1-Pad13)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 132.08 98.171) (end 143.002 98.171) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 143.002 98.171) (end 143.002 105.791) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 132.08 105.791) (end 132.08 98.171) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 143.002 105.791) (end 132.08 105.791) (layer "Edge.Cuts") (width 0.05))
  (gr_text "13" (at 132.842 101.092 90) (layer "B.SilkS"))
  (gr_text "1" (at 132.842 103.251 90) (layer "B.SilkS"))
  (gr_text "Fortune .1" (at 141.986 101.854 90) (layer "B.SilkS"))
  (zone (net 25) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.621 102.362)
        (xy 141.859 102.362)
        (xy 141.859 101.6)
        (xy 142.621 101.6)
      )
    )
  )
  (zone (net 25) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.986 105.029)
        (xy 132.334 105.029)
        (xy 132.334 98.679)
        (xy 141.986 98.679)
      )
    )
  )
  (zone (net 25) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.621 102.362)
        (xy 140.589 102.362)
        (xy 140.589 101.6)
        (xy 142.621 101.6)
      )
    )
  )
  (zone (net 25) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.748 105.537)
        (xy 132.334 105.537)
        (xy 132.334 98.425)
        (xy 142.748 98.425)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.367 105.029)
        (xy 141.351 105.029)
        (xy 141.351 98.933)
        (xy 142.367 98.933)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.494 105.156)
        (xy 141.351 105.156)
        (xy 141.351 98.806)
        (xy 142.494 98.806)
      )
    )
  )
)
