<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="40.132" x2="-0.254" y2="4.572" width="0" layer="20"/>
<wire x1="-0.254" y1="4.572" x2="11.176" y2="4.572" width="0" layer="20"/>
<wire x1="11.176" y1="4.572" x2="11.176" y2="0.762" width="0" layer="20"/>
<wire x1="11.176" y1="0.762" x2="26.406" y2="0.762" width="0" layer="20"/>
<wire x1="26.406" y1="0.762" x2="26.406" y2="40.132" width="0" layer="20"/>
<wire x1="26.406" y1="40.132" x2="14.986" y2="40.132" width="0" layer="20"/>
<wire x1="14.986" y1="40.132" x2="14.986" y2="38.862" width="0" layer="20"/>
<wire x1="14.986" y1="38.862" x2="4.826" y2="38.862" width="0" layer="20"/>
<wire x1="4.826" y1="38.862" x2="4.826" y2="40.132" width="0" layer="20"/>
<wire x1="4.826" y1="40.132" x2="-0.254" y2="40.132" width="0" layer="20"/>
<text>LaserBugV1.1</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F/PMX04A">
<description>&lt;b&gt;SPEAKER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun" package="1206" value="22pf">
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="1206GA220JAT2A"/>
<attribute name="OC_FARNELL" value="1301843"/>
</element>
<element name="C2" library="SparkFun" package="1206" value="22pf">
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="1206GA220JAT2A"/>
<attribute name="OC_FARNELL" value="1301843"/>
</element>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="LED1" library="led" package="CHIPLED_1206" value="red">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="LED2" library="led" package="CHIPLED_1206" value="red">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="Q1" library="adafruit" package="CTS406" value="16mhz">
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="CX2520SB16000D0FLJZZ"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="1657886"/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="330">
<attribute name="MF" value="MULTICOMP"/>
<attribute name="MPN" value="MCHP06W2F1200T5E"/>
<attribute name="OC_FARNELL" value="1576617"/>
</element>
<element name="R4" library="SparkFun-Passives" package="1206" value="330">
<attribute name="MF" value="MULTICOMP"/>
<attribute name="MPN" value="MCHP06W2F1200T5E"/>
<attribute name="OC_FARNELL" value="1576617"/>
</element>
<element name="U$1" library="atmel" package="TQFP32-08" value="ATMEGA328P">
<attribute name="MF" value="ATMEL"/>
<attribute name="MPN" value="ATMEGA328PB-AU"/>
<attribute name="OC_FARNELL" value="2523203"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="IR/output"/>
<element name="JP2" library="pinhead" package="1X02" value="LASER"/>
<element name="JP6" library="pinhead" package="1X02" value="VIN"/>
<element name="JP7" library="pinhead" package="1X03" value="IR/input"/>
<element name="JP8" library="pinhead" package="1X02" value="trigger"/>
<element name="SP1" library="buzzer" package="F/PMX04A" value="F/PMX04">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JP3" library="pinhead" package="1X03" value="RF433"/>
<element name="R2" library="SparkFun-Passives" package="1206" value="330">
<attribute name="MF" value="MULTICOMP"/>
<attribute name="MPN" value="MCHP06W2F1200T5E"/>
<attribute name="OC_FARNELL" value="1576617"/>
</element>
<element name="LED3" library="led" package="CHIPLED_1206" value="red">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R3" library="SparkFun-Passives" package="1206" value="330">
<attribute name="MF" value="MULTICOMP"/>
<attribute name="MPN" value="MCHP06W2F1200T5E"/>
<attribute name="OC_FARNELL" value="1576617"/>
</element>
<element name="LED4" library="led" package="CHIPLED_1206" value="red">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="5"/>
<contactref element="LED1" pad="C"/>
<contactref element="ISP1" pad="6"/>
<contactref element="LED2" pad="C"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP8" pad="2"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="SP1" pad="-"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="6"/>
<contactref element="ISP1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="2">
<contactref element="U$1" pad="15"/>
<contactref element="ISP1" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="3">
<contactref element="U$1" pad="16"/>
<contactref element="ISP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="17"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="29"/>
<contactref element="ISP1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="30"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="31"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="LASER">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="IR/IN">
<contactref element="JP7" pad="3"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="SHOOT">
<contactref element="JP8" pad="1"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="LEDG">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="LEDR">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="PIEZO">
<contactref element="SP1" pad="+"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="RF/OUT">
<contactref element="U$1" pad="13"/>
<contactref element="JP3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
