(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 146)
    (zones 0)
    (modules 13)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VBUS2)
  (net 2 /SENSE2)
  (net 3 GND)
  (net 4 /DN1)
  (net 5 /DN1_R)
  (net 6 /DP1_R)
  (net 7 /DP1)
  (net 8 /DP2)
  (net 9 /DP2_R)
  (net 10 /DN2_R)
  (net 11 /DN2)
  (net 12 /VBUS)
  (net 13 /SENSE1)
  (net 14 /PULLUP1)
  (net 15 /PULLUP2)
  (net 16 "Net-(J1-Pad4)")
  (net 17 "Net-(J2-Pad4)")
  (net 18 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /DN1)
    (add_net /DN1_R)
    (add_net /DN2)
    (add_net /DN2_R)
    (add_net /DP1)
    (add_net /DP1_R)
    (add_net /DP2)
    (add_net /DP2_R)
    (add_net /PULLUP1)
    (add_net /PULLUP2)
    (add_net /SENSE1)
    (add_net /SENSE2)
    (add_net /VBUS)
    (add_net /VBUS2)
    (add_net GND)
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad4)")
  )
  (module digikey-footprints:USB_Micro_B_Female_10118193-0001LF (layer F.Cu) (tedit 5BD21A05)
    (at 81.44489 67.31 270)
    (descr http://portal.fciconnect.com/Comergent//fci/drawing/10118193.pdf)
    (fp_text reference J2 (at -5.08 0.16489 270) (layer F.SilkS))
    (fp_text value 10118193-0001LF (at 0 4.5 270) (layer F.Fab))
    (fp_text user %R (at 0.06 1.86 270) (layer F.Fab))
    (pad 3 smd rect (at 0 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 7 /DP1))
    (pad 4 smd rect (at 0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at 1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 4 /DN1))
    (pad 1 smd rect (at -1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 12 /VBUS))
    (pad SH thru_hole oval (at 3.3 0 270) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad SH thru_hole oval (at -3.3 0 270) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad SH smd rect (at -3.2 -2.45 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad SH smd rect (at 3.2 -2.45 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad SH smd rect (at -1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad SH smd rect (at 1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 96.52 50.8 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -1.27 2.54 270) (layer F.SilkS))
    (fp_text value 5k1 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 /VBUS2))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 /SENSE2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 99.06 50.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 1.27 2.54 90) (layer F.SilkS))
    (fp_text value 5k1 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 /SENSE2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 94.225 62.23 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.785 0 180) (layer F.SilkS))
    (fp_text value 22R (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 /DN1))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 /DN1_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 94.225 64.77 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.785 0 180) (layer F.SilkS))
    (fp_text value 22R (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 /DP1_R))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 /DP1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 91.44 55.88 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 22R (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /DP2))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 /DP2_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 91.44 52.07 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 22R (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 /DN2_R))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 /DN2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 96.52 58.42 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 5k1 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 /VBUS))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 /SENSE1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 99.06 58.42 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value 5k1 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 /SENSE1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 88.9 66.04 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 /PULLUP1))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 /DP1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 87.63 54.61 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /DP2))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 /PULLUP2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:USB_Micro_B_Female_10118193-0001LF (layer F.Cu) (tedit 5BD21A05)
    (at 81.44489 52.07 270)
    (descr http://portal.fciconnect.com/Comergent//fci/drawing/10118193.pdf)
    (fp_text reference J1 (at 5.08 0.16489 270) (layer F.SilkS))
    (fp_text value 10118193-0001LF (at 0 4.5 270) (layer F.Fab))
    (fp_text user %R (at 0.06 1.86 270) (layer F.Fab))
    (pad SH smd rect (at 1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad SH smd rect (at -1.2 0 270) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad SH smd rect (at 3.2 -2.45 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad SH smd rect (at -3.2 -2.45 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad SH thru_hole oval (at -3.3 0 270) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad SH thru_hole oval (at 3.3 0 270) (size 0.9 1.6) (drill oval 0.5 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /VBUS2))
    (pad 2 smd rect (at -0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 11 /DN2))
    (pad 5 smd rect (at 1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 8 /DP2))
  )
  (module digikey-footprints:PinHeader_6x2_P2.54mm_Horizontal (layer F.Cu) (tedit 5B18017E)
    (at 104.14 52.07)
    (descr http://portal.fciconnect.com/Comergent//fci/drawing/68020.pdf)
    (fp_text reference J3 (at 2.54 -3.81) (layer F.SilkS))
    (fp_text value 68021-412HLF (at 1.6 15.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 3 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole circle (at 0 5.08) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 /SENSE1))
    (pad 7 thru_hole circle (at 0 7.62) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 /PULLUP1))
    (pad 9 thru_hole circle (at 0 10.16) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 /DN1_R))
    (pad 11 thru_hole circle (at 0 12.7) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 /DP1_R))
    (pad 12 thru_hole circle (at 2.54 12.7) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 /DP2_R))
    (pad 10 thru_hole circle (at 2.54 10.16) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 /DN2_R))
    (pad 8 thru_hole circle (at 2.54 7.62) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 /PULLUP2))
    (pad 6 thru_hole circle (at 2.54 5.08) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 /SENSE2))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 +3V3))
  )
  (gr_text "Dual USB PMOD" (at 99.06 69.85) (layer F.SilkS))
  (gr_line (start 78.74 72.39) (end 78.74 46.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 72.39) (end 78.74 72.39) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 46.99) (end 109.22 72.39) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 78.74 46.99) (end 109.22 46.99) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.74 46.99) (xy 109.22 46.99) (xy 109.22 72.39) (xy 78.74 72.39)
      )
    )
  )
)
