(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 30)
    (no_connects 0)
    (area 139.524999 100.124999 160.475001 109.875001)
    (thickness 0.8)
    (drawings 25)
    (tracks 147)
    (zones 0)
    (modules 15)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 2.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +2V8)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(Q1-Pad1)")
  (net 6 /~RST)
  (net 7 /MISO)
  (net 8 /MOSI)
  (net 9 /SCK)
  (net 10 "Net-(U2-Pad3)")
  (net 11 "Net-(U2-Pad4)")
  (net 12 /PB3)
  (net 13 /PB4)
  (net 14 "Net-(C1-Pad1)")
  (net 15 "Net-(D2-Pad2)")
  (net 16 "Net-(D2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PB3)
    (add_net /PB4)
    (add_net /SCK)
    (add_net /~RST)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad3)")
  )
  (net_class Tight ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Housings_SSOP:TSSOP-8_4.4x3mm_Pitch0.65mm (layer F.Cu) (tedit 58C5F0F1)
    (at 147.6 102)
    (descr "8-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value ATTINY45-20XUR (at 0 2.55) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 /~RST))
    (pad 2 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /PB3))
    (pad 3 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 /PB4))
    (pad 4 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /MOSI))
    (pad 6 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 7 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 8 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +2V8))
    (model Housings_SSOP.3dshapes/TSSOP-8_4.4x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58C5EDE2)
    (at 156.6 108 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 0 180) (layer F.SilkS))
    (fp_text value 47 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +2V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58C5F026)
    (at 155.2 108 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 0 540) (layer F.SilkS))
    (fp_text value 22u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +2V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bcan:HO_Rail_2_Length2.4mm_Width3mm (layer F.Cu) (tedit 58CB2889)
    (at 150 105)
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Rails (at 0 2.54) (layer F.Fab))
    (pad 1 smd rect (at -8.9 0) (size 3 2.4) (layers F.Cu F.Mask)
      (net 16 "Net-(D2-Pad3)"))
    (pad 2 smd rect (at 8.9 0) (size 3 2.4) (layers F.Cu F.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58C5EDDA)
    (at 155.2 105 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58CB11E2)
    (at 156.6 105 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 0 360) (layer F.SilkS) hide)
    (fp_text value IR (at 0 1.35 270) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-143 (layer F.Cu) (tedit 58C5E6EC)
    (at 147.2 108 180)
    (descr SOT-143)
    (tags SOT-143)
    (attr smd)
    (fp_text reference D2 (at 0.25 0 180) (layer F.SilkS))
    (fp_text value Rectifier (at -0.28 2.48 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.77 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0.95 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 1.1 0.95 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad3)"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-143.wrl
      (at (xyz 0 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58C5EDAD)
    (at 156.2 102)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -0.2 0 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58C5E67A)
    (at 152.6 108)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0.25 0) (layer F.SilkS))
    (fp_text value TPS70928DBV (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +2V8))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58C5F03D)
    (at 150 108 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 0 540) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58C5EEAF)
    (at 142.8 102 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +2V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /~RST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58C5EE36)
    (at 152.4 102 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58C5EE3C)
    (at 153.8 102 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bcan:Edge_Connector_1x04_Pitch2.54mm_SMD (layer B.Cu) (tedit 58CB2CF4)
    (at 150 100.2 90)
    (fp_text reference J1 (at -1 5.5 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X04 (at -1 -5.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1 3.81 90) (size 2 1.5) (layers B.Cu B.Mask)
      (net 9 /SCK))
    (pad 2 smd rect (at -1 1.27 90) (size 2 1.5) (layers B.Cu B.Mask)
      (net 7 /MISO))
    (pad 3 smd rect (at -1 -1.27 90) (size 2 1.5) (layers B.Cu B.Mask)
      (net 8 /MOSI))
    (pad 4 smd rect (at -1 -3.81 90) (size 2 1.5) (layers B.Cu B.Mask)
      (net 6 /~RST))
  )
  (module bcan:Edge_Connector_1x04_Pitch2.54mm_SMD (layer B.Cu) (tedit 58CB2CF8)
    (at 150 109.8 270)
    (fp_text reference J2 (at -1 5.5 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X04 (at -1 -5.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 3.81 270) (size 2 1.5) (layers B.Cu B.Mask)
      (net 13 /PB4))
    (pad 2 smd rect (at -1 1.27 270) (size 2 1.5) (layers B.Cu B.Mask)
      (net 12 /PB3))
    (pad 3 smd rect (at -1 -1.27 270) (size 2 1.5) (layers B.Cu B.Mask)
      (net 2 +2V8))
    (pad 4 smd rect (at -1 -3.81 270) (size 2 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (gr_text R (at 158.9 105) (layer B.SilkS))
  (gr_text L (at 141.1 105) (layer B.SilkS))
  (gr_text "Rev 1.0" (at 157 100.8 90) (layer B.SilkS))
  (gr_text R (at 146.05 103.505) (layer B.SilkS))
  (gr_text O (at 148.463 103.505) (layer B.SilkS))
  (gr_text I (at 151.13 103.505) (layer B.SilkS))
  (gr_text S (at 153.67 103.505) (layer B.SilkS))
  (gr_text V (at 151.13 106.553) (layer B.SilkS))
  (gr_text 4 (at 146.05 106.553) (layer B.SilkS))
  (gr_text 3 (at 148.59 106.553) (layer B.SilkS))
  (gr_line (start 142 103.8) (end 142 100.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.6 103.8) (end 142 103.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.6 106.2) (end 139.6 103.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142 106.2) (end 139.6 106.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142 109.8) (end 142 106.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 106.2) (end 158 109.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.4 106.2) (end 158 106.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.4 103.8) (end 160.4 106.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 103.8) (end 160.4 103.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 100.2) (end 158 103.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 109.8) (end 142 109.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142 100.2) (end 158 100.2) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 158 109.8) (xy 142 109.8) (xy 142 106.2) (xy 139.6 106.2) (xy 139.6 103.8)
        (xy 142 103.8) (xy 142 100.2) (xy 158 100.2) (xy 158 103.8) (xy 160.4 103.8)
        (xy 160.4 106.2) (xy 158 106.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 158 109.8) (xy 142 109.8) (xy 142 106.2) (xy 139.6 106.2) (xy 139.6 103.8)
        (xy 142 103.8) (xy 142 100.2) (xy 158 100.2) (xy 158 103.8) (xy 160.4 103.8)
        (xy 160.4 106.2) (xy 158 106.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 154.25 103.75) (xy 154.25 106.25) (xy 145.75 106.25) (xy 145.75 103.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 144 104.2) (xy 145 105.6) (xy 144.4 105.6) (xy 144.4 109) (xy 143.6 109)
        (xy 143.6 105.6) (xy 143 105.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 152.6 109.8) (xy 152.6 105) (xy 155.6 105) (xy 155.6 109.8)
      )
    )
  )
)
