(kicad_pcb (version 20171130) (host pcbnew 5.1.5-1.fc30)
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 314)
    (zones 0)
    (modules 38)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1016)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (user_via 0.635 0.381)
    (user_via 0.889 0.635)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFBE7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /VUSB)
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 "Net-(C11-Pad2)")
  (net 8 "Net-(C12-Pad2)")
  (net 9 /SDA)
  (net 10 "Net-(J3-Pad1)")
  (net 11 /D5)
  (net 12 /D6)
  (net 13 /D9)
  (net 14 /D12)
  (net 15 /D11)
  (net 16 /D10)
  (net 17 /D13)
  (net 18 /EN)
  (net 19 /VBAT)
  (net 20 /A1)
  (net 21 /A0)
  (net 22 /A2)
  (net 23 /A3)
  (net 24 /A4)
  (net 25 /MOSI)
  (net 26 /SCK)
  (net 27 /A5)
  (net 28 /MISO)
  (net 29 /D0)
  (net 30 /D1)
  (net 31 /AREF)
  (net 32 /~RESET)
  (net 33 "Net-(R2-Pad2)")
  (net 34 "Net-(U1-Pad4)")
  (net 35 "Net-(U2-Pad20)")
  (net 36 "Net-(U2-Pad13)")
  (net 37 "Net-(R2-Pad1)")
  (net 38 "Net-(C14-Pad1)")
  (net 39 "Net-(C15-Pad2)")
  (net 40 "Net-(C16-Pad1)")
  (net 41 "Net-(C18-Pad2)")
  (net 42 "Net-(C18-Pad1)")
  (net 43 "Net-(J2-Pad2)")
  (net 44 "Net-(J2-Pad3)")
  (net 45 "Net-(R4-Pad1)")
  (net 46 "Net-(R5-Pad2)")
  (net 47 "Net-(R6-Pad2)")
  (net 48 "Net-(U3-Pad8)")
  (net 49 "Net-(U3-Pad7)")
  (net 50 "Net-(JP3-Pad2)")
  (net 51 /SCL)
  (net 52 /+3.3VA)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /+3.3VA)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /AREF)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D5)
    (add_net /D6)
    (add_net /D9)
    (add_net /EN)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VBAT)
    (add_net /VUSB)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
  )
  (net_class "50 ohm" ""
    (clearance 0.3048)
    (trace_width 0.3048)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module footprints:ea (layer B.Cu) (tedit 0)
    (at 190.881 64.643)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 201.549 59.563)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at -0.127 -2.286) (layer F.SilkS))
    (fp_text value MCP1802 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 52 /+3.3VA))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /VUSB))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /VUSB))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 205.105 59.162 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 2.687 0 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /+3.3VA))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 198.374 59.624 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /VUSB))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 200.426 71.12)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -1.163 -3.048) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 204.531 72.517 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.347 0) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 200.406 69.342 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 1.016 -3.175) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C15-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C14-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 204.536 67.945)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -2.606 -0.127) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 204.681 69.469)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.456 -0.635) (layer F.SilkS))
    (fp_text value 100 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /MOSI))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 204.681 70.993)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.456 0.635) (layer F.SilkS))
    (fp_text value 100 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /SCK))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CUI_SJ-3523-SMT-TR (layer F.Cu) (tedit 5F18730B)
    (at 188.087 56.896 270)
    (fp_text reference J2 (at 3.429 -3.429 90) (layer F.SilkS))
    (fp_text value SJ-3523-SMT-TR (at 8.24479 5.97568 90) (layer F.Fab))
    (pad None np_thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 3 smd rect (at 0.9 -3.7 270) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J2-Pad3)"))
    (pad 1 smd rect (at -1.1 3.7 270) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 8.3 3.7 270) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J2-Pad2)"))
    (pad None np_thru_hole circle (at 7 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  )
  (module Adafruit_FeatherWing:PCB_FeatherWing (layer F.Cu) (tedit 58EF14C7)
    (at 203.1492 64.77)
    (fp_text reference PCB** (at 0 1) (layer F.Fab))
    (fp_text value VAL** (at 0 0 180) (layer F.Fab))
    (fp_text user 12 (at -8.89 -10.922) (layer Cmts.User))
    (fp_text user 11 (at -6.35 -10.922) (layer Cmts.User))
    (fp_text user 10 (at -3.81 -10.922) (layer Cmts.User))
    (fp_text user 9 (at -1.27 -10.922) (layer Cmts.User))
    (fp_text user 8 (at 1.27 -10.922) (layer Cmts.User))
    (fp_text user 7 (at 3.81 -10.922) (layer Cmts.User))
    (fp_text user 6 (at 6.35 -10.922) (layer Cmts.User))
    (fp_text user 5 (at 8.89 -10.922) (layer Cmts.User))
    (fp_text user 4 (at 11.43 -10.922) (layer Cmts.User))
    (fp_text user 3 (at 13.97 -10.922) (layer Cmts.User))
    (fp_text user 2 (at 16.51 -10.922) (layer Cmts.User))
    (fp_text user 1 (at 19.05 -10.922) (layer Cmts.User))
    (fp_text user 16 (at -19.05 10.922) (layer Cmts.User))
    (fp_text user 15 (at -16.51 10.922) (layer Cmts.User))
    (fp_text user 14 (at -13.97 10.922) (layer Cmts.User))
    (fp_text user 13 (at -11.43 10.922) (layer Cmts.User))
    (fp_text user 12 (at -8.89 10.922) (layer Cmts.User))
    (fp_text user 11 (at -6.35 10.922) (layer Cmts.User))
    (fp_text user 10 (at -3.81 10.922) (layer Cmts.User))
    (fp_text user 9 (at -1.27 10.922) (layer Cmts.User))
    (fp_text user 8 (at 1.27 10.922) (layer Cmts.User))
    (fp_text user 7 (at 3.81 10.922) (layer Cmts.User))
    (fp_text user 6 (at 6.35 10.922) (layer Cmts.User))
    (fp_text user 5 (at 8.89 10.922) (layer Cmts.User))
    (fp_text user 4 (at 11.43 10.922) (layer Cmts.User))
    (fp_text user 3 (at 13.97 10.922) (layer Cmts.User))
    (fp_text user 2 (at 16.51 10.922) (layer Cmts.User))
    (fp_text user 1 (at 19.05 10.922) (layer Cmts.User))
    (fp_text user %R (at 17.78 8.89 180) (layer Eco1.User))
    (pad "" np_thru_hole circle (at 22.86 8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -22.86 8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 22.86 -8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -22.86 -8.89) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 209.296 66.355 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 217.424 58.735 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.347 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 219.456 59.202 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -0.02 -1.397 90) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 217.3986 62.4586 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 /+3.3VA))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 212.237 66.929 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -2.647 -0.254) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 212.217 65.278 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.413 -0.127) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 214.63 69.088 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.143) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 211.775 70.612)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -0.066 1.143) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 210.546 69.088)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -1.758 1.27) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 180.34 61.087)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0.127 -2.286) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /SCL))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VUSB))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SMA_END (layer F.Cu) (tedit 58894D7D)
    (at 225.7044 64.5668)
    (fp_text reference J3 (at -3.4544 -1.3208) (layer F.SilkS))
    (fp_text value SMA (at 0 -0.5) (layer F.Fab))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad1)"))
  )
  (module Adafruit_FeatherWing:Conn_PinHeader_1x12 (layer F.Cu) (tedit 56B1F058)
    (at 208.2546 54.61)
    (fp_text reference JP1 (at 0 0.6 180) (layer F.Fab))
    (fp_text value PinHeader_01x12_2.54mm (at 0 -0.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer Eco1.User))
    (pad 11 thru_hole circle (at 11.43 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 51 /SCL))
    (pad 12 thru_hole circle (at 13.97 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SDA))
    (pad 10 thru_hole circle (at 8.89 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 /D5))
    (pad 9 thru_hole circle (at 6.35 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D6))
    (pad 8 thru_hole circle (at 3.81 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D9))
    (pad 5 thru_hole circle (at -3.81 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 /D12))
    (pad 6 thru_hole circle (at -1.27 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 /D11))
    (pad 7 thru_hole circle (at 1.27 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D10))
    (pad 4 thru_hole circle (at -6.35 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D13))
    (pad 3 thru_hole circle (at -8.89 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VUSB))
    (pad 2 thru_hole circle (at -11.43 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 /EN))
    (pad 1 thru_hole rect (at -13.97 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VBAT))
  )
  (module Adafruit_FeatherWing:Conn_PinHeader_1x16 (layer F.Cu) (tedit 58EF1B8A)
    (at 203.1746 74.9046)
    (fp_text reference JP2 (at 0 0.508 180) (layer F.Fab))
    (fp_text value PinHeader_01x16_2.54mm (at 0 -0.508 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer Eco1.User))
    (pad 11 thru_hole circle (at 6.35 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SCK))
    (pad 12 thru_hole circle (at 8.89 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 25 /MOSI))
    (pad 10 thru_hole circle (at 3.81 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 27 /A5))
    (pad 9 thru_hole circle (at 1.27 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 24 /A4))
    (pad 8 thru_hole circle (at -1.27 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 23 /A3))
    (pad 5 thru_hole circle (at -8.89 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A0))
    (pad 6 thru_hole circle (at -6.35 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 /A1))
    (pad 7 thru_hole circle (at -3.81 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A2))
    (pad 4 thru_hole circle (at -11.43 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -13.97 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 31 /AREF))
    (pad 2 thru_hole circle (at -16.51 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at -19.05 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 32 /~RESET))
    (pad 13 thru_hole circle (at 11.43 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 28 /MISO))
    (pad 14 thru_hole circle (at 13.97 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D0))
    (pad 15 thru_hole circle (at 16.51 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D1))
    (pad 16 thru_hole circle (at 19.05 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 216.027 66.378 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.456 1.016 90) (layer F.SilkS))
    (fp_text value 50 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Pulse_SMD_Balun (layer F.Cu) (tedit 5882856D)
    (at 219.5195 66.421 270)
    (fp_text reference T1 (at 2.286 -0.0635 90) (layer F.SilkS))
    (fp_text value TRANSFO4 (at 0 -0.5 90) (layer F.Fab))
    (pad 5 smd rect (at -1.27 -1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad1)"))
    (pad 4 smd rect (at 1.27 -1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.27 1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad2)"))
    (pad 3 smd rect (at 1.27 1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0 1.5875 270) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
  )
  (module Housings_SSOP:TSSOP-28_4.4x9.7mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 211.2264 60.579 270)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 -5.9 90) (layer F.SilkS))
    (fp_text value AD9203 (at 0 5.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 28 smd rect (at 2.85 -4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 /+3.3VA))
    (pad 27 smd rect (at 2.85 -3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 2.85 -2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad2)"))
    (pad 25 smd rect (at 2.85 -2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R2-Pad1)"))
    (pad 24 smd rect (at 2.85 -1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C11-Pad2)"))
    (pad 23 smd rect (at 2.85 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (pad 22 smd rect (at 2.85 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 21 smd rect (at 2.85 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 /+3.3VA))
    (pad 20 smd rect (at 2.85 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad20)"))
    (pad 19 smd rect (at 2.85 1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 2.85 2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (pad 17 smd rect (at 2.85 2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 2.85 3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.85 4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 /A5))
    (pad 14 smd rect (at -2.85 4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 13 smd rect (at -2.85 3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad13)"))
    (pad 12 smd rect (at -2.85 2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 /D13))
    (pad 11 smd rect (at -2.85 2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 /D12))
    (pad 10 smd rect (at -2.85 1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /D11))
    (pad 9 smd rect (at -2.85 0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 /D10))
    (pad 8 smd rect (at -2.85 0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /D9))
    (pad 7 smd rect (at -2.85 -0.325 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /D6))
    (pad 6 smd rect (at -2.85 -0.975 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /D5))
    (pad 5 smd rect (at -2.85 -1.625 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 /MISO))
    (pad 4 smd rect (at -2.85 -2.275 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /D0))
    (pad 3 smd rect (at -2.85 -2.925 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 /D1))
    (pad 2 smd rect (at -2.85 -3.575 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -2.85 -4.225 270) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-28_4.4x9.7mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 193.167 63.312 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 3.114 0 90) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C16-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 194.564 63.312 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -3.114 0 90) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 190.627 70.043 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C18-Pad2)"))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C18-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 189.314 72.517 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.084 1.143) (layer F.SilkS))
    (fp_text value 82K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 195.961 62.949 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.624 0 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 186.733 69.215)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.143) (layer F.SilkS))
    (fp_text value 330 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 194.183 69.215 270)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0.127 -3.302 90) (layer F.SilkS))
    (fp_text value TPA6139A2 (at 0 3.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at 2.95 -1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 13 smd rect (at 2.95 -1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R6-Pad2)"))
    (pad 12 smd rect (at 2.95 -0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R4-Pad1)"))
    (pad 11 smd rect (at 2.95 0 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.95 0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 9 smd rect (at 2.95 1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C18-Pad1)"))
    (pad 8 smd rect (at 2.95 1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U3-Pad8)"))
    (pad 7 smd rect (at -2.95 1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad7)"))
    (pad 6 smd rect (at -2.95 1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C18-Pad2)"))
    (pad 5 smd rect (at -2.95 0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C16-Pad1)"))
    (pad 4 smd rect (at -2.95 0 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at -2.95 -0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.95 -1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -2.95 -1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 200.406 64.196 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at -2.474 0) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillators:Oscillator_SMD_SeikoEpson_SG210-4pin_2.5x2.0mm_HandSoldering (layer F.Cu) (tedit 58CD3345)
    (at 203.454 64.262)
    (descr "SMD Crystal Oscillator Seiko Epson SG-210 https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-210SED, hand-soldering, 2.5x2.0mm^2 package")
    (tags "SMD SMT crystal oscillator hand-soldering")
    (attr smd)
    (fp_text reference U4 (at 0 -2.159) (layer F.SilkS))
    (fp_text value XTAL_OSC_OE (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.125 -0.875) (size 1.65 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 1.125 -0.875) (size 1.65 1.35) (layers F.Cu F.Paste F.Mask)
      (net 27 /A5))
    (pad 2 smd rect (at 1.125 0.875) (size 1.65 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.125 0.875) (size 1.65 1.35) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(JP3-Pad2)"))
    (model ${KISYS3DMOD}/Oscillators.3dshapes/Oscillator_SMD_SeikoEpson_SG210-4pin_2.5x2.0mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm (layer F.Cu) (tedit 5C756B4C)
    (at 198.247 64.643 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at -2.667 0 180) (layer F.SilkS))
    (fp_text value Jumper_3_Bridged12 (at 0 2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 1.3 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 50 "Net-(JP3-Pad2)"))
  )
  (gr_text "OrangeCrab ADC v0.2\n(c) 2020 E. Brombaugh" (at 207.645 58.674) (layer B.SilkS))
  (gr_text "OrangeCrab\nADC V0.2" (at 219.075 71.374) (layer F.SilkS))
  (gr_text GND (at 182.245 68.707 90) (layer F.SilkS))
  (gr_text SDA (at 182.245 66.294 90) (layer F.SilkS))
  (gr_text SCL (at 182.245 63.627 90) (layer F.SilkS))
  (gr_text +5 (at 182.245 61.087 90) (layer F.SilkS))
  (gr_arc (start 225.9838 55.88) (end 225.9838 53.34) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 180.2638 55.88) (end 177.7238 55.88) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.7238 55.88) (end 177.7238 73.66) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.2638 76.2) (end 225.9838 76.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.5238 73.66) (end 228.5238 55.88) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 225.9838 73.66) (end 228.5238 73.66) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.9838 53.34) (end 180.2638 53.34) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 180.2638 73.66) (end 180.2638 76.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 227.584 54.61) (xy 228.219 55.88) (xy 228.219 73.66) (xy 227.584 75.057) (xy 226.06 75.819)
        (xy 180.34 75.819) (xy 178.816 75.184) (xy 178.181 73.66) (xy 178.181 55.88) (xy 178.816 54.483)
        (xy 180.213 53.721) (xy 226.06 53.721)
      )
    )
  )
  (zone (net 2) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 227.584 54.61) (xy 228.219 55.88) (xy 228.219 73.787) (xy 227.584 75.057) (xy 226.06 75.819)
        (xy 180.34 75.819) (xy 178.816 75.184) (xy 178.181 73.66) (xy 178.181 55.88) (xy 178.816 54.483)
        (xy 180.213 53.721) (xy 226.06 53.721)
      )
    )
  )
)
