<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.1">
<drawing>
<board>
<plain>
<text>DTR   RXO   TXI     3V    CTS    GND</text>
<wire x1="5.715" y1="26.035" x2="15.24" y2="26.035" width="0.3556" layer="20"/>
<wire x1="28.575" y1="26.035" x2="41.91" y2="26.035" width="0.3556" layer="20"/>
<wire x1="41.91" y1="26.035" x2="48.26" y2="19.685" width="0.3556" layer="20" curve="-90"/>
<wire x1="48.26" y1="19.685" x2="48.26" y2="6.35" width="0.3556" layer="20"/>
<wire x1="48.26" y1="6.35" x2="41.91" y2="0" width="0.3556" layer="20" curve="-90"/>
<wire x1="41.91" y1="0" x2="5.715" y2="0" width="0.3556" layer="20"/>
<wire x1="5.715" y1="0" x2="-0.635" y2="6.35" width="0.3556" layer="20" curve="-90"/>
<wire x1="-0.635" y1="6.35" x2="-0.635" y2="19.685" width="0.3556" layer="20"/>
<wire x1="-0.635" y1="19.685" x2="5.715" y2="26.035" width="0.3556" layer="20" curve="-90"/>
<text>SDA     GND    V_IMU   SCL</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<hole x="18" y="23.5" drill="1.27"/>
<hole x="25.2" y="23.5" drill="1.27"/>
<wire x1="18.8" y1="25" x2="18.8" y2="23.1" width="0.3556" layer="20"/>
<wire x1="18.8" y1="23.1" x2="19.7" y2="23.1" width="0.3556" layer="20"/>
<wire x1="19.7" y1="23.1" x2="19.7" y2="25" width="0.3556" layer="20"/>
<wire x1="19.7" y1="25" x2="23.5" y2="25" width="0.3556" layer="20"/>
<wire x1="23.5" y1="25" x2="23.5" y2="23.1" width="0.3556" layer="20"/>
<wire x1="23.5" y1="23.1" x2="24.4" y2="23.1" width="0.3556" layer="20"/>
<wire x1="24.4" y1="23.1" x2="24.4" y2="25" width="0.3556" layer="20"/>
<wire x1="24.4" y1="25" x2="27.1" y2="25" width="0.3556" layer="20"/>
<wire x1="27.1" y1="25" x2="28.575" y2="26.035" width="0.3556" layer="20"/>
<wire x1="15.24" y1="26.035" x2="16.275" y2="25" width="0.3556" layer="20"/>
<wire x1="16.275" y1="25" x2="18.8" y2="25" width="0.3556" layer="20"/>
<text>GRN</text>
<text>BLK</text>
<text>0.1uF
RST</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>DFN6</text>
<text>SOT23-6</text>
<text>SOT323</text>
<text>VCC</text>
<text>PWR_PIN</text>
<text>VCC</text>
<text>BAT</text>
<text>P0</text>
<text>50mA</text>
<text>ALWAYS</text>
<hole x="9.525" y="19.685" drill="1.016"/>
<hole x="9.525" y="1.905" drill="1.016"/>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>SDA</text>
<text>SDA</text>
<text>SDA</text>
<text>SCL</text>
<text>SCL</text>
<text>SCL</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>7</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
<text>Not legal tender</text>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="8S1">
<description>&lt;b&gt;8S1&lt;/b&gt; 8-lead (0.150" Wide Body)&lt;p&gt;
Plastic Gull Wing Small Outline (JEDEC SOIC)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="AVRISP">
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="DFN-6">
</package>
</packages>
</library>
<library name="con-3m">
<description>&lt;b&gt;3M Connectors&lt;/b&gt;&lt;p&gt;
PCMCIA-CompactFlash Connectors&lt;p&gt;
Zero Insertion Force Socked&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PAK100/2500-10">
<description>&lt;b&gt;3M (TM) Pak 100 4-Wall Header&lt;/b&gt; Straight&lt;p&gt;
Source: 3M</description>
</package>
</packages>
</library>
<library name="USB3135-XX-X_REVB">
<packages>
<package name="GCT_USB3135-XX-X_REVB">
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_NO_NO-SILK">
</package>
<package name="SMT-JUMPER_2_NO_NO-SILK">
</package>
</packages>
</library>
<library name="mc33996">
<packages>
<package name="SOIC65P1030X265-33N">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-6L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DCK">
<description>&lt;b&gt;DCK R-PDSO-G5&lt;/b&gt; 5-Pin SC-70 Package (SOT323)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps3803-01.pdf</description>
</package>
</packages>
</library>
<library name="SmartPrj">
<packages>
<package name="RESONATOR">
</package>
</packages>
</library>
<library name="resistor-dil">
<packages>
<package name="CAY16">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="328P/328PB" library="atmel" package="TQFP32-08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MAX1555" library="linear" package="SOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$5" library="adafruit" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="P1" library="con-3m" package="PAK100/2500-10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JST-PH" library="adafruit" package="JST-PH-2-THM-RA" value="">
<attribute name="NAME"/>
</element>
<element name="100UF" library="adafruit" package="E3,5-8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB3135" library="USB3135-XX-X_REVB" package="GCT_USB3135-XX-X_REVB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$15" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$16" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$17" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$18" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$19" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$20" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$21" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$22" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$23" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$24" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$25" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$26" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="FAST_CHG" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_NO-SILK" value=""/>
<element name="SW1" library="adafruit" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LDK120" library="linear" package="SOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="adafruit" package="AVRISP" value="">
<attribute name="NAME"/>
</element>
<element name="E$1" library="adafruit" package="C050-025X075" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="adafruit" package="C050-025X075" value="">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="adafruit" package="C050-025X075" value="">
<attribute name="VALUE"/>
</element>
<element name="MC33996" library="mc33996" package="SOIC65P1030X265-33N" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$13" library="adafruit" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V_IMU1" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$2" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LBAT-" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$30" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="CHG+" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="SW3" library="adafruit" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="SIG-" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$33" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="E$34" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="E$35" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="RST" library="adafruit" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="L_PWR" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L_CHG" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SO_PWR" library="SparkFun-Jumpers" package="SMT-JUMPER_3_NO_NO-SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E$8" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="E$11" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="E$6" library="adafruit" package="DFN-6" value=""/>
<element name="E$7" library="maxim" package="SOT23-6L" value="">
<attribute name="VALUE"/>
</element>
<element name="E$9" library="texas" package="DCK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$10" library="texas" package="DCK" value="">
<attribute name="VALUE"/>
</element>
<element name="E$29" library="atmel" package="8S1" value=""/>
<element name="Y2" library="SmartPrj" package="RESONATOR" value="CSTCE8M0* 8MHZ">
<attribute name="VALUE"/>
</element>
<element name="1206-8" library="resistor-dil" package="CAY16" value="1K">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="S$2">
<contactref element="E$15" pad="2"/>
<contactref element="E$21" pad="2"/>
<contactref element="E$13" pad="1"/>
</signal>
<signal name="S$3">
<contactref element="E$16" pad="2"/>
<contactref element="E$22" pad="2"/>
<contactref element="E$13" pad="2"/>
</signal>
<signal name="S$4">
<contactref element="E$17" pad="2"/>
<contactref element="E$23" pad="2"/>
<contactref element="E$13" pad="3"/>
</signal>
<signal name="S$5">
<contactref element="E$18" pad="2"/>
<contactref element="E$24" pad="2"/>
<contactref element="E$13" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="E$20" pad="1"/>
<contactref element="E$19" pad="1"/>
<contactref element="E$17" pad="1"/>
<contactref element="E$18" pad="1"/>
<contactref element="E$15" pad="1"/>
<contactref element="E$16" pad="1"/>
<contactref element="328P/328PB" pad="27"/>
</signal>
<signal name="S$6">
</signal>
<signal name="S$11">
<contactref element="E$19" pad="2"/>
<contactref element="E$25" pad="2"/>
<contactref element="E$13" pad="5"/>
</signal>
<signal name="SCL">
<contactref element="E$26" pad="1"/>
<contactref element="E$25" pad="1"/>
<contactref element="E$23" pad="1"/>
<contactref element="E$24" pad="1"/>
<contactref element="E$21" pad="1"/>
<contactref element="E$22" pad="1"/>
<contactref element="328P/328PB" pad="28"/>
</signal>
<signal name="S$21">
<contactref element="E$20" pad="2"/>
<contactref element="E$26" pad="2"/>
<contactref element="E$13" pad="6"/>
</signal>
<signal name="TXD">
<contactref element="328P/328PB" pad="31"/>
<contactref element="E$5" pad="5"/>
</signal>
<signal name="RXD">
<contactref element="E$5" pad="4"/>
<contactref element="328P/328PB" pad="30"/>
</signal>
<signal name="USB">
<contactref element="USB3135" pad="1"/>
<contactref element="MAX1555" pad="1"/>
<contactref element="FAST_CHG" pad="2"/>
<contactref element="E$4" pad="1"/>
<contactref element="E$30" pad="A"/>
</signal>
<signal name="GND">
<contactref element="100UF" pad="-"/>
<contactref element="USB3135" pad="5"/>
<contactref element="JST-PH" pad="2"/>
<contactref element="MAX1555" pad="2"/>
<contactref element="328P/328PB" pad="5"/>
<contactref element="E$3" pad="2"/>
<contactref element="E$1" pad="2"/>
<contactref element="E$4" pad="2"/>
<contactref element="LDK120" pad="2"/>
<contactref element="MC33996" pad="25"/>
<contactref element="MC33996" pad="26"/>
<contactref element="MC33996" pad="33"/>
<contactref element="MC33996" pad="7"/>
<contactref element="MC33996" pad="8"/>
<contactref element="MC33996" pad="9"/>
<contactref element="MC33996" pad="10"/>
<contactref element="E$19" pad="3"/>
<contactref element="E$18" pad="3"/>
<contactref element="E$20" pad="3"/>
<contactref element="E$17" pad="3"/>
<contactref element="E$16" pad="3"/>
<contactref element="E$15" pad="3"/>
<contactref element="E$5" pad="2"/>
<contactref element="ICSP" pad="6"/>
<contactref element="E$5" pad="1"/>
<contactref element="MC33996" pad="24"/>
<contactref element="MC33996" pad="23"/>
<contactref element="E$2" pad="A"/>
<contactref element="E$33" pad="A"/>
<contactref element="L_CHG" pad="1"/>
<contactref element="E$8" pad="A"/>
<contactref element="Y2" pad="2"/>
</signal>
<signal name="DC">
<contactref element="FAST_CHG" pad="1"/>
<contactref element="MAX1555" pad="4"/>
</signal>
<signal name="BAT_RAW">
<contactref element="SW1" pad="3"/>
<contactref element="JST-PH" pad="1"/>
<contactref element="SW3" pad="3"/>
<contactref element="SW2" pad="3"/>
<contactref element="P1" pad="1"/>
<contactref element="P1" pad="2"/>
<contactref element="LDK120" pad="1"/>
<contactref element="MAX1555" pad="5"/>
</signal>
<signal name="L_PWR">
<contactref element="LBAT-" pad="A"/>
<contactref element="L_PWR" pad="3"/>
</signal>
<signal name="BATT_SW">
<contactref element="E$3" pad="1"/>
<contactref element="MC33996" pad="6"/>
<contactref element="V_IMU1" pad="3"/>
<contactref element="100UF" pad="+"/>
<contactref element="L_PWR" pad="2"/>
<contactref element="E$11" pad="C"/>
<contactref element="LDK120" pad="3"/>
<contactref element="SW3" pad="2"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="V_IMU">
<contactref element="V_IMU1" pad="2"/>
<contactref element="E$26" pad="3"/>
<contactref element="E$25" pad="3"/>
<contactref element="E$24" pad="3"/>
<contactref element="E$23" pad="3"/>
<contactref element="E$22" pad="3"/>
<contactref element="E$21" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="328P/328PB" pad="6"/>
<contactref element="E$1" pad="1"/>
<contactref element="LDK120" pad="5"/>
<contactref element="V_IMU1" pad="1"/>
<contactref element="E$5" pad="3"/>
<contactref element="ICSP" pad="2"/>
<contactref element="SO_PWR" pad="3"/>
<contactref element="328P/328PB" pad="18"/>
</signal>
<signal name="CS">
<contactref element="MC33996" pad="14"/>
<contactref element="328P/328PB" pad="9"/>
</signal>
<signal name="MOSI">
<contactref element="328P/328PB" pad="15"/>
<contactref element="MC33996" pad="19"/>
<contactref element="ICSP" pad="4"/>
</signal>
<signal name="SER_CLK">
<contactref element="328P/328PB" pad="17"/>
<contactref element="ICSP" pad="3"/>
<contactref element="MC33996" pad="11"/>
</signal>
<signal name="OUT8">
<contactref element="P1" pad="4"/>
<contactref element="MC33996" pad="17"/>
</signal>
<signal name="OUT9">
<contactref element="P1" pad="3"/>
<contactref element="MC33996" pad="18"/>
</signal>
<signal name="OUT10">
<contactref element="P1" pad="6"/>
<contactref element="MC33996" pad="20"/>
</signal>
<signal name="OUT11">
<contactref element="P1" pad="5"/>
<contactref element="MC33996" pad="21"/>
</signal>
<signal name="RST">
<contactref element="MC33996" pad="27"/>
</signal>
<signal name="OUT12">
<contactref element="P1" pad="8"/>
<contactref element="MC33996" pad="28"/>
</signal>
<signal name="OUT13">
<contactref element="P1" pad="7"/>
<contactref element="MC33996" pad="29"/>
</signal>
<signal name="OUT14">
<contactref element="P1" pad="10"/>
<contactref element="MC33996" pad="31"/>
</signal>
<signal name="OUT15">
<contactref element="P1" pad="9"/>
<contactref element="MC33996" pad="32"/>
</signal>
<signal name="PWR_PIN">
<contactref element="328P/328PB" pad="23"/>
<contactref element="SO_PWR" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="328P/328PB" pad="16"/>
<contactref element="MC33996" pad="22"/>
<contactref element="ICSP" pad="1"/>
</signal>
<signal name="PWM">
<contactref element="MC33996" pad="30"/>
<contactref element="328P/328PB" pad="13"/>
</signal>
<signal name="RESET">
<contactref element="328P/328PB" pad="29"/>
<contactref element="ICSP" pad="5"/>
<contactref element="RST" pad="C"/>
</signal>
<signal name="S$7">
<contactref element="SW1" pad="1"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW2" pad="1"/>
</signal>
<signal name="S$9">
<contactref element="E$2" pad="C"/>
<contactref element="LBAT-" pad="C"/>
</signal>
<signal name="DTR">
<contactref element="RST" pad="A"/>
<contactref element="E$5" pad="6"/>
</signal>
<signal name="L_SIG">
<contactref element="SIG-" pad="A"/>
<contactref element="328P/328PB" pad="24"/>
</signal>
<signal name="S$1">
<contactref element="E$33" pad="C"/>
<contactref element="SIG-" pad="C"/>
</signal>
<signal name="S$10">
<contactref element="CHG+" pad="C"/>
<contactref element="E$30" pad="C"/>
</signal>
<signal name="CHG">
<contactref element="L_CHG" pad="3"/>
<contactref element="MAX1555" pad="3"/>
</signal>
<signal name="S$12">
<contactref element="L_CHG" pad="2"/>
<contactref element="CHG+" pad="A"/>
</signal>
<signal name="S$8">
<contactref element="E$34" pad="1"/>
<contactref element="L_PWR" pad="1"/>
</signal>
<signal name="SO_PWR">
<contactref element="MC33996" pad="3"/>
<contactref element="SO_PWR" pad="2"/>
</signal>
<signal name="S$13">
<contactref element="328P/328PB" pad="25"/>
</signal>
<signal name="V_LVL">
<contactref element="E$11" pad="A"/>
<contactref element="E$8" pad="C"/>
<contactref element="328P/328PB" pad="22"/>
</signal>
<signal name="S$14">
<contactref element="Y2" pad="3"/>
<contactref element="328P/328PB" pad="7"/>
</signal>
<signal name="S$15">
<contactref element="Y2" pad="1"/>
<contactref element="328P/328PB" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
