(kicad_pcb (version 20170123) (host pcbnew "(2017-03-27 revision c7c172d36)-makepkg")
  (general
    (links 12)
    (no_connects 12)
    (area 113.4985 53.257666 148.2565 88.963501)
    (thickness 1.6)
    (drawings 17)
    (tracks 70)
    (zones 0)
    (modules 2)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad11)")
  (net 3 "Net-(J1-Pad10)")
  (net 4 "Net-(J1-Pad9)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 "Net-(J1-Pad4)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J1-Pad2)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 58E2EBB1)
    (at 144.78 58.42 270)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 0 30.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mynixies:mynixies-6844A-D-SUB (layer F.Cu) (tedit 200000)
    (at 130.81 74.3712)
    (descr "THIS FOOTPRINT USES FEMALE D-SUB PINS AS 'SOCKETS'.")
    (tags "THIS FOOTPRINT USES FEMALE D-SUB PINS AS 'SOCKETS'.")
    (attr virtual)
    (fp_text reference NX1 (at 0 -10.795) (layer F.SilkS))
    (fp_text value 6844A (at 0.635 0) (layer F.SilkS))
    (fp_text user Bot (at 0 5.7912) (layer F.SilkS))
    (fp_text user Top (at 0 -5.6388) (layer F.SilkS))
    (pad 0 thru_hole circle (at 6.51256 5.1943) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 1 thru_hole circle (at -6.51256 5.19176) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at -8.12038 1.85166) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at -8.12038 -1.8542) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 4 thru_hole circle (at -6.51256 -5.1943) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 5 thru_hole circle (at -3.61442 -7.5057) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 3.61442 -7.5057) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (pad 7 thru_hole circle (at 6.51256 -5.19176) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 8 thru_hole circle (at 8.12038 -1.85166) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(J1-Pad9)"))
    (pad 9 thru_hole circle (at 8.12038 1.85166) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(J1-Pad10)"))
    (pad A thru_hole circle (at 3.61442 7.5057) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad N/C thru_hole circle (at 0 8.3312) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask))
    (pad N/C2 thru_hole circle (at 0 -8.3312) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask))
  )
  (gr_text A (at 144.78 60.96) (layer F.SilkS))
  (gr_text 1 (at 142.24 60.96) (layer F.SilkS))
  (gr_text 2 (at 139.7 60.96) (layer F.SilkS))
  (gr_text 3 (at 137.16 60.96) (layer F.SilkS))
  (gr_text 4 (at 134.62 60.96) (layer F.SilkS))
  (gr_text 5 (at 132.08 60.96) (layer F.SilkS))
  (gr_text 6 (at 129.54 60.96) (layer F.SilkS))
  (gr_text 7 (at 127 60.96) (layer F.SilkS))
  (gr_text 8 (at 124.46 60.96) (layer F.SilkS))
  (gr_text 9 (at 121.92 60.96) (layer F.SilkS))
  (gr_text 0 (at 119.38 60.96) (layer F.SilkS))
  (gr_text A (at 116.84 60.96) (layer F.SilkS))
  (gr_line (start 114.3 88.9) (end 114.3 88.9) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 147.32 88.9) (end 114.3 88.9) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 147.32 55.88) (end 147.32 88.9) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 114.3 55.88) (end 147.32 55.88) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 114.3 88.9) (end 114.3 55.88) (layer Edge.Cuts) (width 0.127))
)
