(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 134)
    (zones 0)
    (modules 16)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +12V)
  (net 4 +3V3)
  (net 5 +1V8)
  (net 6 "Net-(J2-Pad1)")
  (net 7 "Net-(J2-Pad2)")
  (net 8 "Net-(J2-Pad3)")
  (net 9 "Net-(J2-Pad4)")
  (net 10 "Net-(J2-Pad5)")
  (net 11 "Net-(J2-Pad6)")
  (net 12 "Net-(J2-Pad7)")
  (net 13 "Net-(J2-Pad8)")
  (net 14 "Net-(J2-Pad9)")
  (net 15 "Net-(J2-Pad10)")
  (net 16 "Net-(J2-Pad11)")
  (net 17 "Net-(J2-Pad12)")
  (net 18 "Net-(U1-Pad1)")
  (net 19 "Net-(U1-Pad2)")
  (net 20 "Net-(U1-Pad3)")
  (net 21 "Net-(U1-Pad4)")
  (net 22 "Net-(U1-Pad5)")
  (net 23 "Net-(U1-Pad7)")
  (net 24 "Net-(U1-Pad8)")
  (net 25 "Net-(U1-Pad9)")
  (net 26 "Net-(U1-Pad10)")
  (net 27 "Net-(U1-Pad11)")
  (net 28 "Net-(U1-Pad12)")
  (net 29 "Net-(U1-Pad13)")
  (net 30 "Net-(U1-Pad14)")
  (net 31 "Net-(U1-Pad15)")
  (net 32 "Net-(U1-Pad16)")
  (net 33 "Net-(U1-Pad17)")
  (net 34 "Net-(U1-Pad18)")
  (net 35 "Net-(U1-Pad19)")
  (net 36 "Net-(U1-Pad20)")
  (net 37 "Net-(U1-Pad21)")
  (net 38 "Net-(U1-Pad22)")
  (net 39 "Net-(U1-Pad23)")
  (net 40 "Net-(U1-Pad24)")
  (net 41 "Net-(U1-Pad25)")
  (net 42 "Net-(U1-Pad26)")
  (net 43 "Net-(U1-Pad27)")
  (net 44 "Net-(U1-Pad28)")
  (net 45 "Net-(U1-Pad29)")
  (net 46 "Net-(U1-Pad30)")
  (net 47 "Net-(U1-Pad33)")
  (net 48 "Net-(U1-Pad34)")
  (net 49 "Net-(U2-Pad13)")
  (net 50 "Net-(U2-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.381)
    (diff_pair_width 0.3048)
    (add_net +12V)
    (add_net +1V8)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad16)")
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 121.6937 58.2168)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.5631 -1.4224) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-20_AVX-F_Pad2.25x2.35mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 123.1165 61.9125)
    (descr "Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C2 (at 2.9691 -2.55) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.55 0) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 2.55 0) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-20_AVX-F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-20_AVX-F_Pad2.25x2.35mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 122.9895 72.0725)
    (descr "Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C3 (at 3.9597 2.5019) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.55 0) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.55 0) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-20_AVX-F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-20_AVX-F_Pad2.25x2.35mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 170.053 71.3005 90)
    (descr "Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C4 (at -2.3595 2.921 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.55 0 90) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 4 +3V3))
    (pad 2 smd roundrect (at 2.55 0 90) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-20_AVX-F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 174.244 67.96 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -2.2964 0.762 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-20_AVX-F_Pad2.25x2.35mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 145.034 69.898414 270)
    (descr "Tantalum Capacitor SMD AVX-F (6032-20 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C6 (at -1.318414 2.8448) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 2.55 0 270) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.55 0 270) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 5 +1V8))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-20_AVX-F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.5405 74.549)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 1.3439 -1.4478) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 120.7516 47.4472 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at -0.0508 4.9784 180) (layer F.SilkS))
    (fp_text value "Power In" (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5C37ABAB)
    (at 196.85 46.228)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at -2.2352 2.032) (layer F.SilkS))
    (fp_text value SIGOUT (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad12)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Amphenol_132134-16_Vertical (layer F.Cu) (tedit 5B2F4D94)
    (at 153.797 70.5485)
    (descr https://www.amphenolrf.com/downloads/dl/file/id/1141/product/2978/132134_16_customer_drawing.pdf)
    (tags "SMA THT Female Jack Vertical ExtendedLegs")
    (fp_text reference J3 (at 4.7498 -3.6449) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 +1V8))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-16_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 165.5445 73.8505 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at -0.7239 7.4041 180) (layer F.SilkS))
    (fp_text value DDSPower (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +1V8))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 120.396 67.5155 270)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at -1.0183 -1.8288) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module arduino:ArduinoMicro (layer F.Cu) (tedit 5B523A25)
    (at 152.2095 55.245 90)
    (fp_text reference U1 (at 8.7122 -23.8887 -180) (layer F.SilkS))
    (fp_text value ArduinoMicro (at -5.461 -23.876 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 -20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 -12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 -10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at -7.62 -7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at -7.62 -5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at -7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at -7.62 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at -7.62 5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at -7.62 7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -7.62 10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at -7.62 12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at -7.62 15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at -7.62 17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad16)"))
    (pad 17 thru_hole circle (at -7.62 20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 7.62 20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 7.62 17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 7.62 15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad20)"))
    (pad 21 thru_hole circle (at 7.62 12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 7.62 7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 7.62 5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 7.62 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at 7.62 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad27)"))
    (pad 28 thru_hole circle (at 7.62 -5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad28)"))
    (pad 29 thru_hole circle (at 7.62 -7.62 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at 7.62 -10.16 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad30)"))
    (pad 31 thru_hole circle (at 7.62 -12.7 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 32 thru_hole circle (at 7.62 -15.24 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 33 thru_hole circle (at 7.62 -17.78 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad33)"))
    (pad 34 thru_hole circle (at 7.62 -20.32 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad34)"))
  )
  (module Package_DIP:DIP-16_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 178.1175 46.4185)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U2 (at 9.9949 18.1483 90) (layer F.SilkS))
    (fp_text value CD4050BE (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad15)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad12)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad14)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad10)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad34)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(U2-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad5)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad9)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad17)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U2-Pad16)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer F.Cu) (tedit 5A70A390)
    (at 181.960287 71.375979)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U3 (at 0.106913 -3.848499) (layer F.SilkS))
    (fp_text value LF33_TO252 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-2 (layer F.Cu) (tedit 5A70A390)
    (at 135.4105 69.597 180)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U4 (at 3.9909 -4.2662 180) (layer F.SilkS))
    (fp_text value LF18_TO252 (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525 180) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0 180) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -4.2 2.28 180) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V8))
    (pad 1 smd rect (at -4.2 -2.28 180) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text LF18 (at 134.9756 73.84892) (layer F.SilkS))
  (gr_text LF33 (at 185.8264 67.5132) (layer F.SilkS))
  (gr_text CD4050B (at 188.1124 58.5216 90) (layer F.SilkS))
  (gr_text "+12V\nGND" (at 122.3772 49.276 90) (layer F.SilkS))
  (gr_text CLKVDD (at 148.59 70.7644 90) (layer F.SilkS))
  (gr_text "1.8V\nGND\n3.3V" (at 161.5948 71.5264) (layer F.SilkS))
  (gr_text "SDIO_0\n\n\n\nP0\nP1\nP2\nP3\nIO_UP\nCSB\nSCLK\nRESET" (at 195.5165 60.325) (layer F.SilkS))
  (gr_line (start 198.6915 44.577) (end 198.6915 76.0095) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.4275 44.577) (end 198.6915 44.577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.4275 76.0095) (end 118.4275 44.577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.6915 76.0095) (end 118.4275 76.0095) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.4148 44.5516) (xy 198.6788 44.5516) (xy 198.7296 76.0476) (xy 118.4148 75.9968)
      )
    )
  )
)
