(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 90 120)
    (grid_origin 90 120)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/")
    )
  )
  (net 0 "")
  (net 1 "/LA03_N")
  (net 2 "/LA16_P")
  (net 3 "/LA16_N")
  (net 4 "/LA20_P")
  (net 5 "/LA20_N")
  (net 6 "/LA22_P")
  (net 7 "/LA22_N")
  (net 8 "unconnected-(J1-PadC30)")
  (net 9 "unconnected-(J1-PadC31)")
  (net 10 "/LA25_P")
  (net 11 "/LA25_N")
  (net 12 "unconnected-(J1-PadC34)")
  (net 13 "/LA29_P")
  (net 14 "/LA29_N")
  (net 15 "/LA33_P")
  (net 16 "/LA33_N")
  (net 17 "/LA04_P")
  (net 18 "/LA04_N")
  (net 19 "/LA07_P")
  (net 20 "/LA07_N")
  (net 21 "/LA11_P")
  (net 22 "/LA11_N")
  (net 23 "/LA15_P")
  (net 24 "/LA15_N")
  (net 25 "/LA19_P")
  (net 26 "/LA19_N")
  (net 27 "/LA21_P")
  (net 28 "/LA21_N")
  (net 29 "/LA24_P")
  (net 30 "/LA24_N")
  (net 31 "/LA28_P")
  (net 32 "/LA28_N")
  (net 33 "unconnected-(J1-PadD29)")
  (net 34 "unconnected-(J1-PadD30)")
  (net 35 "unconnected-(J1-PadD31)")
  (net 36 "unconnected-(J1-PadD32)")
  (net 37 "unconnected-(J1-PadD33)")
  (net 38 "unconnected-(J1-PadD34)")
  (net 39 "unconnected-(J1-PadD35)")
  (net 40 "/LA01_N_CC")
  (net 41 "/LA01_P_CC")
  (net 42 "unconnected-(J1-PadC2)")
  (net 43 "unconnected-(J1-PadC3)")
  (net 44 "unconnected-(J1-PadC6)")
  (net 45 "unconnected-(J1-PadC7)")
  (net 46 "unconnected-(J1-PadD1)")
  (net 47 "unconnected-(J1-PadD4)")
  (net 48 "unconnected-(J1-PadD5)")
  (net 49 "unconnected-(J1-PadG2)")
  (net 50 "unconnected-(J1-PadG3)")
  (net 51 "/LA00_P_CC")
  (net 52 "/LA00_N_CC")
  (net 53 "/LA03_P")
  (net 54 "unconnected-(J1-PadH1)")
  (net 55 "unconnected-(J1-PadH4)")
  (net 56 "unconnected-(J1-PadH5)")
  (net 57 "unconnected-(J1-PadG39)")
  (net 58 "unconnected-(J1-PadH40)")
  (net 59 "unconnected-(A1-Pad1)")
  (net 60 "unconnected-(A1-Pad3)")
  (net 61 "GND")
  (net 62 "unconnected-(A1-Pad7)")
  (net 63 "unconnected-(A1-Pad10)")
  (net 64 "unconnected-(A1-Pad12)")
  (net 65 "unconnected-(A1-Pad67)")
  (net 66 "unconnected-(A1-Pad68)")
  (net 67 "unconnected-(A1-Pad69)")
  (net 68 "unconnected-(A1-Pad70)")
  (net 69 "Net-(R1-Pad1)")
  (net 70 "Net-(R2-Pad1)")
  (net 71 "Net-(R5-Pad1)")
  (net 72 "Net-(R6-Pad1)")
  (net 73 "/LA06_P")
  (net 74 "/LA06_N")
  (net 75 "/LA10_P")
  (net 76 "/LA10_N")
  (net 77 "/LA14_P")
  (net 78 "/LA14_N")
  (net 79 "/LA26_P")
  (net 80 "/LA26_N")
  (net 81 "/CFG4")
  (net 82 "/CFG3")
  (net 83 "/CFG2")
  (net 84 "/CFG1")
  (net 85 "/PB1")
  (net 86 "/PB3")
  (net 87 "/PB2")
  (net 88 "/PB4")
  (net 89 "+3V3")
  (net 90 "Net-(A1-Pad26)")
  (net 91 "Net-(A1-Pad28)")
  (net 92 "Net-(A1-Pad32)")
  (net 93 "Net-(A1-Pad34)")
  (net 94 "unconnected-(J1-PadC35)")
  (net 95 "unconnected-(J1-PadC37)")
  (net 96 "/LA18_P_CC")
  (net 97 "/LA18_N_CC")
  (net 98 "unconnected-(J3-Pad2)")
  (net 99 "unconnected-(J3-Pad3)")
  (net 100 "unconnected-(J3-Pad5)")
  (net 101 "unconnected-(J3-Pad11)")
  (net 102 "unconnected-(J3-Pad17)")
  (net 103 "unconnected-(J3-Pad19)")
  (net 104 "unconnected-(A1-Pad8)")
  (net 105 "unconnected-(A1-Pad2)")
  (net 106 "unconnected-(A1-Pad4)")
  (net 107 "/SWO")
  (net 108 "/SWDIO")
  (net 109 "/SWDCLK")
  (net 110 "/nRESET")
  (net 111 "/LA27_N")
  (net 112 "/LA27_P")
  (net 113 "unconnected-(J1-PadD24)")
  (net 114 "unconnected-(J1-PadD23)")
  (net 115 "unconnected-(J1-PadD17)")
  (net 116 "unconnected-(J1-PadD15)")
  (net 117 "unconnected-(J1-PadD14)")
  (net 118 "unconnected-(J1-PadD12)")
  (net 119 "unconnected-(J1-PadD11)")
  (net 120 "unconnected-(J1-PadH37)")
  (net 121 "unconnected-(J1-PadH35)")
  (net 122 "unconnected-(J1-PadH34)")
  (net 123 "unconnected-(J1-PadG34)")
  (net 124 "unconnected-(J1-PadG33)")
  (net 125 "unconnected-(J1-PadG13)")
  (net 126 "unconnected-(J1-PadG12)")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.8 80 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at -3.7 0 -270) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/CFG4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 160.5 107 180)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW4" (at 0.15 -2.6) (layer "F.SilkS"))
    (fp_text value "SW_SPST" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "1" smd rect (at 2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(R6-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(R6-Pad1)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.3 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 3.1 0.1 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/PB3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.4 102.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -3 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/PB4") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 130.5 107 180)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0.15 -2.6) (layer "F.SilkS"))
    (fp_text value "SW_SPST" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "1" smd rect (at -2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(R1-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(R1-Pad1)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Testpoint:TestPoint_Harwin_S2761-46R" (layer "F.Cu")
    (tedit 0)
    (at 126 74.5)
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP1" (at 2.75 0 unlocked) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.3 1.8 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.4 4 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(A1-Pad26)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.5 102.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -3.1 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/PB3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Testpoint:TestPoint_Harwin_S2761-46R" (layer "F.Cu")
    (tedit 0)
    (at 126 78.5)
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP2" (at 2.75 0.25 unlocked) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.3 1.8 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.4 4 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(A1-Pad28)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 153 59 -90)
    (descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -6.1 90) (layer "F.SilkS"))
    (fp_text value "Conn_ARM_JTAG_SWD_20" (at 1.27 28.96 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 11.43) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 89 "+3V3") (pinfunction "VTREF") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "unconnected-(J3-Pad2)") (pinfunction "VCC/NC") (pintype "power_in+no_connect"))
    (pad "3" thru_hole circle (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "unconnected-(J3-Pad3)") (pinfunction "~{TRST}") (pintype "output+no_connect"))
    (pad "4" thru_hole circle (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "unconnected-(J3-Pad5)") (pinfunction "TDI") (pintype "output+no_connect"))
    (pad "6" thru_hole circle (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "/SWDIO") (pinfunction "TMS/SWDIO") (pintype "output"))
    (pad "8" thru_hole circle (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "9" thru_hole circle (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "/SWDCLK") (pinfunction "TCK/SWDCLK") (pintype "output"))
    (pad "10" thru_hole circle (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "unconnected-(J3-Pad11)") (pinfunction "RTCK") (pintype "input+no_connect"))
    (pad "12" thru_hole circle (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "/SWO") (pinfunction "TDO/SWO") (pintype "input"))
    (pad "14" thru_hole circle (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "15" thru_hole circle (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "/nRESET") (pinfunction "~{SRST}") (pintype "bidirectional"))
    (pad "16" thru_hole circle (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "unconnected-(J3-Pad17)") (pinfunction "DBGRQ/NC") (pintype "output+no_connect"))
    (pad "18" thru_hole circle (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "19" thru_hole circle (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "unconnected-(J3-Pad19)") (pinfunction "DBGACK/NC") (pintype "input+no_connect"))
    (pad "20" thru_hole circle (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.9 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 3.1 0.1 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/PB1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 163 114.55)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 -0.05) (size 2.7 2.7) (drill 2.7) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.3 80 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -3.7 0 -270) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/CFG3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 108.4 117)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 163 57.95)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.5 102.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -3 -0.1 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/PB2") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 148.8 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 3 0 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/PB2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Testpoint:TestPoint_Harwin_S2761-46R" (layer "F.Cu")
    (tedit 0)
    (at 126 82.5)
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP3" (at 2.75 0 unlocked) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.3 1.8 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.4 4 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(A1-Pad32)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.7 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 3 0 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/PB4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 95 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "/LA14_P") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "/LA10_N") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "/LA10_P") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "/LA06_N") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "/LA06_P") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/LA01_N_CC") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/LA01_P_CC") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 150.5 107 180)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW3" (at 0.15 -2.6) (layer "F.SilkS"))
    (fp_text value "SW_SPST" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "1" smd rect (at 2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(R5-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(R5-Pad1)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.6 102.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -3.1 -0.1 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/PB1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO14580" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 108.4 54)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO14580")
    (tags "mounting hole 2.7mm no annular m2.5 iso14580")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 140.5 107 180)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at 0.15 -2.6) (layer "F.SilkS"))
    (fp_text value "SW_SPST" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "1" smd rect (at 2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(R2-Pad1)") (pinfunction "B") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(R2-Pad1)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Testpoint:TestPoint_Harwin_S2761-46R" (layer "F.Cu")
    (tedit 0)
    (at 126 86.5)
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP4" (at 2.75 0 unlocked) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0.3 1.8 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.4 4 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1.8 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Net-(A1-Pad34)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 155.7 80 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -3.7 0.1 -270) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/CFG2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.3 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 3.1 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/PB1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.2 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 3 0.1 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/PB2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 138.7 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 3.1 0 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/PB3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.2 80 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -3.3 0 -270) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "/CFG1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 162.1 102.6 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 3 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/PB4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Testpoint:Shorting_Link_5.08mm" (layer "F.Cu")
    (tedit 0)
    (at 136 115 90)
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -4.8 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0.5 6.2 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 4.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 -2.54 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 95 64)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "/LA26_N") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "/LA27_N") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "/LA26_P") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "/LA27_P") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "/LA18_N_CC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "/LA18_P_CC") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "/LA14_N") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ORBTrace:ORBTrace" (layer "F.Cu")
    (tedit 62BEA749)
    (at 123 52.5 180)
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A1" (at -2.21 -1.28) (layer "F.SilkS"))
    (fp_text value "ORBTrace" (at 16 4) (layer "F.Fab"))
    (fp_text user "Note: Stencil is based on 0.12 mm metal mask thickness" (at 8.3 -17.45) (layer "F.Fab"))
    (fp_text user "HIROSE_DF40C-70DS-0.4V_51_" (at 13 -19 180 unlocked) (layer "F.Fab"))
    (pad "" smd custom (at 30.7 -1.3) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" np_thru_hole circle (at 3 -63 180) (size 6 6) (drill 3.7) (layers "F.Cu" "F.Mask"))
    (pad "" smd custom (at 1.3 -61.28 270) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 27.28 -4.72 180) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.144868 0.149752) (end 1.416167 -0.48172) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.083718 0.093065) (end 1.409903 -0.564961) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.151882 -0.142722) (end 1.41014 -0.900894) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 4.7 -61.3) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 30.73 -64.7 90) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 1.3 -1.28 270) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 4.73 -4.7 90) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 30.7 -61.3) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" np_thru_hole circle (at 29 -3 180) (size 6 6) (drill 3.7) (layers "F.Cu" "F.Mask"))
    (pad "" smd custom (at 27.28 -64.72 180) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.144868 0.149752) (end 1.416167 -0.48172) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.083718 0.093065) (end 1.409903 -0.564961) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.151882 -0.142722) (end 1.41014 -0.900894) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 4.73 -64.7 90) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 30.73 -4.7 90) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 4.7 -1.3) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" np_thru_hole circle (at 3 -3 180) (size 6 6) (drill 3.7) (layers "F.Cu" "F.Mask"))
    (pad "" np_thru_hole circle (at 29 -63 180) (size 6 6) (drill 3.7) (layers "F.Cu" "F.Mask"))
    (pad "" smd custom (at 1.28 -64.72 180) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.144868 0.149752) (end 1.416167 -0.48172) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.083718 0.093065) (end 1.409903 -0.564961) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.151882 -0.142722) (end 1.41014 -0.900894) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 27.3 -61.28 270) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 27.3 -1.28 270) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.143503 0.151122) (end 1.412334 -0.481196) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.082304 0.094488) (end 1.405927 -0.564426) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.153501 -0.141093) (end 1.405578 -0.900359) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "" smd custom (at 1.28 -4.72 180) (size 0.7 0.7) (layers "F.Paste")
      (options (clearance outline) (anchor circle))
      (primitives
    (gr_arc (start -0.314399 1.423011) (mid 0.260852 0.26947) (end 1.410951 -0.31263) (width 0.16666))
    (gr_arc (start -0.398552 1.423011) (mid 0.202493 0.209976) (end 1.412531 -0.397079) (width 0.16666))
    (gr_arc (start -0.482641 1.423011) (mid 0.144868 0.149752) (end 1.416167 -0.48172) (width 0.16666))
    (gr_arc (start -0.566675 1.423011) (mid 0.083718 0.093065) (end 1.409903 -0.564961) (width 0.16666))
    (gr_arc (start -0.650659 1.423011) (mid 0.027385 0.031542) (end 1.417178 -0.649932) (width 0.16666))
    (gr_arc (start -0.734599 1.423011) (mid -0.035817 -0.023081) (end 1.405134 -0.732404) (width 0.16666))
    (gr_arc (start -0.818498 1.423011) (mid -0.09097 -0.085796) (end 1.415743 -0.817651) (width 0.16666))
    (gr_arc (start -0.902361 1.423011) (mid -0.151882 -0.142722) (end 1.41014 -0.900894) (width 0.16666))
    (gr_arc (start -0.986191 1.423011) (mid -0.21248 -0.199961) (end 1.405416 -0.984233) (width 0.16666))
    (gr_arc (start -1.069991 1.423011) (mid -0.269326 -0.260973) (end 1.411266 -1.068734) (width 0.16666))
        (gr_line (start 1.423011 -0.314399) (end 1.423011 -1.069991) (width 0.16666))
        (gr_line (start -0.314399 1.423011) (end -1.069991 1.423011) (width 0.16666))
      ))
    (pad "1" smd rect (at 4.54 -22.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 59 "unconnected-(A1-Pad1)") (pinfunction "3V3") (pintype "power_out+no_connect"))
    (pad "2" smd rect (at 1.46 -22.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 105 "unconnected-(A1-Pad2)") (pinfunction "5V") (pintype "power_out+no_connect"))
    (pad "3" smd rect (at 4.54 -22.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 60 "unconnected-(A1-Pad3)") (pinfunction "3V3") (pintype "power_out+no_connect"))
    (pad "4" smd rect (at 1.46 -22.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 106 "unconnected-(A1-Pad4)") (pinfunction "5V") (pintype "power_out+no_connect"))
    (pad "5" smd rect (at 4.54 -23 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "6" smd rect (at 1.46 -23 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "7" smd rect (at 4.54 -23.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 62 "unconnected-(A1-Pad7)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "8" smd rect (at 1.46 -23.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 104 "unconnected-(A1-Pad8)") (pinfunction "LED_EXT") (pintype "output+no_connect"))
    (pad "9" smd rect (at 4.54 -23.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 30 "/LA24_N") (pinfunction "JTMS") (pintype "input"))
    (pad "10" smd rect (at 1.46 -23.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 63 "unconnected-(A1-Pad10)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "11" smd rect (at 4.54 -24.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 29 "/LA24_P") (pinfunction "JTCK") (pintype "input"))
    (pad "12" smd rect (at 1.46 -24.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 64 "unconnected-(A1-Pad12)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "13" smd rect (at 4.54 -24.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 11 "/LA25_N") (pinfunction "JTDI") (pintype "input+no_connect"))
    (pad "14" smd rect (at 1.46 -24.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 32 "/LA28_N") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd rect (at 4.54 -25 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 10 "/LA25_P") (pinfunction "JTDO") (pintype "output+no_connect"))
    (pad "16" smd rect (at 1.46 -25 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 31 "/LA28_P") (pinfunction "SCL") (pintype "output"))
    (pad "17" smd rect (at 4.54 -25.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "18" smd rect (at 1.46 -25.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "19" smd rect (at 4.54 -25.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 28 "/LA21_N") (pinfunction "P19") (pintype "bidirectional"))
    (pad "20" smd rect (at 1.46 -25.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 14 "/LA29_N") (pinfunction "P20") (pintype "bidirectional+no_connect"))
    (pad "21" smd rect (at 4.54 -26.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 27 "/LA21_P") (pinfunction "P21") (pintype "bidirectional"))
    (pad "22" smd rect (at 1.46 -26.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 13 "/LA29_P") (pinfunction "P22") (pintype "bidirectional+no_connect"))
    (pad "23" smd rect (at 4.54 -26.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "24" smd rect (at 1.46 -26.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "25" smd rect (at 4.54 -27 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 7 "/LA22_N") (pinfunction "P25") (pintype "bidirectional"))
    (pad "26" smd rect (at 1.46 -27 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 90 "Net-(A1-Pad26)") (pinfunction "P26") (pintype "bidirectional"))
    (pad "27" smd rect (at 4.54 -27.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 6 "/LA22_P") (pinfunction "P27") (pintype "bidirectional"))
    (pad "28" smd rect (at 1.46 -27.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 91 "Net-(A1-Pad28)") (pinfunction "P28") (pintype "bidirectional"))
    (pad "29" smd rect (at 4.54 -27.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "30" smd rect (at 1.46 -27.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "31" smd rect (at 4.54 -28.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 26 "/LA19_N") (pinfunction "P31") (pintype "bidirectional"))
    (pad "32" smd rect (at 1.46 -28.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 92 "Net-(A1-Pad32)") (pinfunction "P32") (pintype "bidirectional"))
    (pad "33" smd rect (at 4.54 -28.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 25 "/LA19_P") (pinfunction "P33") (pintype "bidirectional"))
    (pad "34" smd rect (at 1.46 -28.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 93 "Net-(A1-Pad34)") (pinfunction "P34") (pintype "bidirectional"))
    (pad "35" smd rect (at 4.54 -29 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "36" smd rect (at 1.46 -29 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "37" smd rect (at 4.54 -29.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 5 "/LA20_N") (pinfunction "P37") (pintype "bidirectional"))
    (pad "38" smd rect (at 1.46 -29.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 20 "/LA07_N") (pinfunction "P38") (pintype "bidirectional"))
    (pad "39" smd rect (at 4.54 -29.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 4 "/LA20_P") (pinfunction "P39") (pintype "bidirectional"))
    (pad "40" smd rect (at 1.46 -29.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 19 "/LA07_P") (pinfunction "P40") (pintype "bidirectional"))
    (pad "41" smd rect (at 4.54 -30.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "42" smd rect (at 1.46 -30.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "43" smd rect (at 4.54 -30.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 24 "/LA15_N") (pinfunction "P43") (pintype "bidirectional"))
    (pad "44" smd rect (at 1.46 -30.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 18 "/LA04_N") (pinfunction "P44") (pintype "bidirectional"))
    (pad "45" smd rect (at 4.54 -31 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 23 "/LA15_P") (pinfunction "P45") (pintype "bidirectional"))
    (pad "46" smd rect (at 1.46 -31 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 17 "/LA04_P") (pinfunction "P46") (pintype "bidirectional"))
    (pad "47" smd rect (at 4.54 -31.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "48" smd rect (at 1.46 -31.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "49" smd rect (at 4.54 -31.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 3 "/LA16_N") (pinfunction "P49") (pintype "bidirectional"))
    (pad "50" smd rect (at 1.46 -31.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 1 "/LA03_N") (pinfunction "P50") (pintype "bidirectional"))
    (pad "51" smd rect (at 4.54 -32.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 2 "/LA16_P") (pinfunction "P51") (pintype "bidirectional"))
    (pad "52" smd rect (at 1.46 -32.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 53 "/LA03_P") (pinfunction "P52") (pintype "bidirectional"))
    (pad "53" smd rect (at 4.54 -32.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "54" smd rect (at 1.46 -32.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "55" smd rect (at 4.54 -33 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 22 "/LA11_N") (pinfunction "P55") (pintype "bidirectional"))
    (pad "56" smd rect (at 1.46 -33 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 52 "/LA00_N_CC") (pinfunction "P56") (pintype "bidirectional"))
    (pad "57" smd rect (at 4.54 -33.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 21 "/LA11_P") (pinfunction "P57") (pintype "bidirectional"))
    (pad "58" smd rect (at 1.46 -33.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 51 "/LA00_P_CC") (pinfunction "P58") (pintype "bidirectional"))
    (pad "59" smd rect (at 4.54 -33.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "60" smd rect (at 1.46 -33.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "61" smd rect (at 4.54 -34.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 84 "/CFG1") (pinfunction "P61") (pintype "bidirectional"))
    (pad "62" smd rect (at 1.46 -34.2 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 88 "/PB4") (pinfunction "P62") (pintype "bidirectional"))
    (pad "63" smd rect (at 4.54 -34.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 83 "/CFG2") (pinfunction "P63") (pintype "bidirectional"))
    (pad "64" smd rect (at 1.46 -34.6 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 87 "/PB2") (pinfunction "P64") (pintype "bidirectional"))
    (pad "65" smd rect (at 4.54 -35 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "66" smd rect (at 1.46 -35 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 61 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "67" smd rect (at 4.54 -35.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 65 "unconnected-(A1-Pad67)") (pinfunction "3V3") (pintype "power_out+no_connect"))
    (pad "68" smd rect (at 1.46 -35.4 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 66 "unconnected-(A1-Pad68)") (pinfunction "5V") (pintype "power_out+no_connect"))
    (pad "69" smd rect (at 4.54 -35.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 67 "unconnected-(A1-Pad69)") (pinfunction "3V3") (pintype "power_out+no_connect"))
    (pad "70" smd rect (at 1.46 -35.8 270) (size 0.2 0.7) (layers "F.Cu" "F.Mask")
      (net 68 "unconnected-(A1-Pad70)") (pinfunction "5V") (pintype "power_out+no_connect"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 82.2)
          (xy 121.19 82.4)
          (xy 120.75 82.4)
          (xy 120.75 82.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 79)
          (xy 119.25 79.2)
          (xy 118.81 79.2)
          (xy 118.81 79)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 84.2)
          (xy 119.25 84.4)
          (xy 118.81 84.4)
          (xy 118.81 84.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 79.4)
          (xy 119.25 79.6)
          (xy 118.81 79.6)
          (xy 118.81 79.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 79.8)
          (xy 119.25 80)
          (xy 118.81 80)
          (xy 118.81 79.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 81.4)
          (xy 121.19 81.6)
          (xy 120.75 81.6)
          (xy 120.75 81.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 79.8)
          (xy 121.19 80)
          (xy 120.75 80)
          (xy 120.75 79.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 86.2)
          (xy 121.19 86.4)
          (xy 120.75 86.4)
          (xy 120.75 86.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 75.4)
          (xy 119.25 75.6)
          (xy 118.81 75.6)
          (xy 118.81 75.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 77)
          (xy 121.19 77.2)
          (xy 120.75 77.2)
          (xy 120.75 77)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 83)
          (xy 121.19 83.2)
          (xy 120.75 83.2)
          (xy 120.75 83)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 81)
          (xy 119.25 81.2)
          (xy 118.81 81.2)
          (xy 118.81 81)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 86.6)
          (xy 119.25 86.8)
          (xy 118.81 86.8)
          (xy 118.81 86.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 75)
          (xy 119.25 75.2)
          (xy 118.81 75.2)
          (xy 118.81 75)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 79)
          (xy 119.25 79.2)
          (xy 118.81 79.2)
          (xy 118.81 79)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 87.8)
          (xy 119.25 88)
          (xy 118.81 88)
          (xy 118.81 87.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 83)
          (xy 121.19 83.2)
          (xy 120.75 83.2)
          (xy 120.75 83)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 88.2)
          (xy 121.19 88.4)
          (xy 120.75 88.4)
          (xy 120.75 88.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 88.2)
          (xy 119.25 88.4)
          (xy 118.81 88.4)
          (xy 118.81 88.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 78.2)
          (xy 119.25 78.4)
          (xy 118.81 78.4)
          (xy 118.81 78.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 85.8)
          (xy 119.25 86)
          (xy 118.81 86)
          (xy 118.81 85.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 81.4)
          (xy 119.25 81.6)
          (xy 118.81 81.6)
          (xy 118.81 81.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 83)
          (xy 119.25 83.2)
          (xy 118.81 83.2)
          (xy 118.81 83)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 81.8)
          (xy 119.25 82)
          (xy 118.81 82)
          (xy 118.81 81.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 79.4)
          (xy 121.19 79.6)
          (xy 120.75 79.6)
          (xy 120.75 79.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 81.8)
          (xy 119.25 82)
          (xy 118.81 82)
          (xy 118.81 81.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 80.2)
          (xy 121.19 80.4)
          (xy 120.75 80.4)
          (xy 120.75 80.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 87)
          (xy 119.25 87.2)
          (xy 118.81 87.2)
          (xy 118.81 87)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 78.2)
          (xy 121.19 78.4)
          (xy 120.75 78.4)
          (xy 120.75 78.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 87)
          (xy 121.19 87.2)
          (xy 120.75 87.2)
          (xy 120.75 87)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 76.6)
          (xy 119.25 76.8)
          (xy 118.81 76.8)
          (xy 118.81 76.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 81)
          (xy 121.19 81.2)
          (xy 120.75 81.2)
          (xy 120.75 81)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 84.2)
          (xy 121.19 84.4)
          (xy 120.75 84.4)
          (xy 120.75 84.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 80.2)
          (xy 121.19 80.4)
          (xy 120.75 80.4)
          (xy 120.75 80.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 77.8)
          (xy 119.25 78)
          (xy 118.81 78)
          (xy 118.81 77.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 86.6)
          (xy 121.19 86.8)
          (xy 120.75 86.8)
          (xy 120.75 86.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 81.8)
          (xy 121.19 82)
          (xy 120.75 82)
          (xy 120.75 81.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 86.2)
          (xy 121.19 86.4)
          (xy 120.75 86.4)
          (xy 120.75 86.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 77)
          (xy 119.25 77.2)
          (xy 118.81 77.2)
          (xy 118.81 77)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 87.8)
          (xy 119.25 88)
          (xy 118.81 88)
          (xy 118.81 87.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 76.2)
          (xy 119.25 76.4)
          (xy 118.81 76.4)
          (xy 118.81 76.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 77)
          (xy 121.19 77.2)
          (xy 120.75 77.2)
          (xy 120.75 77)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 88.2)
          (xy 119.25 88.4)
          (xy 118.81 88.4)
          (xy 118.81 88.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 84.2)
          (xy 121.19 84.4)
          (xy 120.75 84.4)
          (xy 120.75 84.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 80.6)
          (xy 121.19 80.8)
          (xy 120.75 80.8)
          (xy 120.75 80.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 75.8)
          (xy 119.25 76)
          (xy 118.81 76)
          (xy 118.81 75.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 88.2)
          (xy 121.19 88.4)
          (xy 120.75 88.4)
          (xy 120.75 88.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 83.8)
          (xy 119.25 84)
          (xy 118.81 84)
          (xy 118.81 83.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 85)
          (xy 121.19 85.2)
          (xy 120.75 85.2)
          (xy 120.75 85)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 86.2)
          (xy 119.25 86.4)
          (xy 118.81 86.4)
          (xy 118.81 86.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 80.6)
          (xy 121.19 80.8)
          (xy 120.75 80.8)
          (xy 120.75 80.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 87.4)
          (xy 119.25 87.6)
          (xy 118.81 87.6)
          (xy 118.81 87.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 79)
          (xy 121.19 79.2)
          (xy 120.75 79.2)
          (xy 120.75 79)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 87.4)
          (xy 121.19 87.6)
          (xy 120.75 87.6)
          (xy 120.75 87.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 82.6)
          (xy 121.19 82.8)
          (xy 120.75 82.8)
          (xy 120.75 82.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 74.6)
          (xy 119.25 74.8)
          (xy 118.81 74.8)
          (xy 118.81 74.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 83.4)
          (xy 119.25 83.6)
          (xy 118.81 83.6)
          (xy 118.81 83.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 86.2)
          (xy 119.25 86.4)
          (xy 118.81 86.4)
          (xy 118.81 86.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 83.4)
          (xy 121.19 83.6)
          (xy 120.75 83.6)
          (xy 120.75 83.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 74.6)
          (xy 119.25 74.8)
          (xy 118.81 74.8)
          (xy 118.81 74.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 84.2)
          (xy 119.25 84.4)
          (xy 118.81 84.4)
          (xy 118.81 84.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 75)
          (xy 119.25 75.2)
          (xy 118.81 75.2)
          (xy 118.81 75)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 84.6)
          (xy 121.19 84.8)
          (xy 120.75 84.8)
          (xy 120.75 84.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 80.2)
          (xy 119.25 80.4)
          (xy 118.81 80.4)
          (xy 118.81 80.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 77.8)
          (xy 121.19 78)
          (xy 120.75 78)
          (xy 120.75 77.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 78.2)
          (xy 121.19 78.4)
          (xy 120.75 78.4)
          (xy 120.75 78.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 85)
          (xy 119.25 85.2)
          (xy 118.81 85.2)
          (xy 118.81 85)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 84.6)
          (xy 119.25 84.8)
          (xy 118.81 84.8)
          (xy 118.81 84.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 78.6)
          (xy 119.25 78.8)
          (xy 118.81 78.8)
          (xy 118.81 78.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 79.8)
          (xy 119.25 80)
          (xy 118.81 80)
          (xy 118.81 79.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 76.2)
          (xy 119.25 76.4)
          (xy 118.81 76.4)
          (xy 118.81 76.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 77.8)
          (xy 121.19 78)
          (xy 120.75 78)
          (xy 120.75 77.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 84.6)
          (xy 121.19 84.8)
          (xy 120.75 84.8)
          (xy 120.75 84.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 79)
          (xy 121.19 79.2)
          (xy 120.75 79.2)
          (xy 120.75 79)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 77.4)
          (xy 121.19 77.6)
          (xy 120.75 77.6)
          (xy 120.75 77.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 74.6)
          (xy 121.19 74.8)
          (xy 120.75 74.8)
          (xy 120.75 74.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 85)
          (xy 119.25 85.2)
          (xy 118.81 85.2)
          (xy 118.81 85)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 84.6)
          (xy 119.25 84.8)
          (xy 118.81 84.8)
          (xy 118.81 84.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 82.2)
          (xy 119.25 82.4)
          (xy 118.81 82.4)
          (xy 118.81 82.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 81.4)
          (xy 121.19 81.6)
          (xy 120.75 81.6)
          (xy 120.75 81.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 77.4)
          (xy 119.25 77.6)
          (xy 118.81 77.6)
          (xy 118.81 77.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 85.4)
          (xy 121.19 85.6)
          (xy 120.75 85.6)
          (xy 120.75 85.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 81)
          (xy 121.19 81.2)
          (xy 120.75 81.2)
          (xy 120.75 81)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 79.4)
          (xy 119.25 79.6)
          (xy 118.81 79.6)
          (xy 118.81 79.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 83.8)
          (xy 121.19 84)
          (xy 120.75 84)
          (xy 120.75 83.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 75.8)
          (xy 119.25 76)
          (xy 118.81 76)
          (xy 118.81 75.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 75.4)
          (xy 121.19 75.6)
          (xy 120.75 75.6)
          (xy 120.75 75.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 77)
          (xy 119.25 77.2)
          (xy 118.81 77.2)
          (xy 118.81 77)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 77.8)
          (xy 119.25 78)
          (xy 118.81 78)
          (xy 118.81 77.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 87.4)
          (xy 121.19 87.6)
          (xy 120.75 87.6)
          (xy 120.75 87.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 75.4)
          (xy 119.25 75.6)
          (xy 118.81 75.6)
          (xy 118.81 75.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 80.6)
          (xy 119.25 80.8)
          (xy 118.81 80.8)
          (xy 118.81 80.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 76.6)
          (xy 121.19 76.8)
          (xy 120.75 76.8)
          (xy 120.75 76.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 80.2)
          (xy 119.25 80.4)
          (xy 118.81 80.4)
          (xy 118.81 80.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 85)
          (xy 121.19 85.2)
          (xy 120.75 85.2)
          (xy 120.75 85)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 76.6)
          (xy 121.19 76.8)
          (xy 120.75 76.8)
          (xy 120.75 76.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 87.8)
          (xy 121.19 88)
          (xy 120.75 88)
          (xy 120.75 87.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 83.8)
          (xy 121.19 84)
          (xy 120.75 84)
          (xy 120.75 83.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 87)
          (xy 121.19 87.2)
          (xy 120.75 87.2)
          (xy 120.75 87)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 85.4)
          (xy 119.25 85.6)
          (xy 118.81 85.6)
          (xy 118.81 85.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 79.4)
          (xy 121.19 79.6)
          (xy 120.75 79.6)
          (xy 120.75 79.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 85.4)
          (xy 119.25 85.6)
          (xy 118.81 85.6)
          (xy 118.81 85.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 78.6)
          (xy 119.25 78.8)
          (xy 118.81 78.8)
          (xy 118.81 78.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 82.6)
          (xy 119.25 82.8)
          (xy 118.81 82.8)
          (xy 118.81 82.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 78.6)
          (xy 121.19 78.8)
          (xy 120.75 78.8)
          (xy 120.75 78.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 83.4)
          (xy 121.19 83.6)
          (xy 120.75 83.6)
          (xy 120.75 83.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 83)
          (xy 119.25 83.2)
          (xy 118.81 83.2)
          (xy 118.81 83)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 82.6)
          (xy 119.25 82.8)
          (xy 118.81 82.8)
          (xy 118.81 82.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 85.8)
          (xy 121.19 86)
          (xy 120.75 86)
          (xy 120.75 85.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 82.6)
          (xy 121.19 82.8)
          (xy 120.75 82.8)
          (xy 120.75 82.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 83.4)
          (xy 119.25 83.6)
          (xy 118.81 83.6)
          (xy 118.81 83.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 85.4)
          (xy 121.19 85.6)
          (xy 120.75 85.6)
          (xy 120.75 85.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 81)
          (xy 119.25 81.2)
          (xy 118.81 81.2)
          (xy 118.81 81)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 75)
          (xy 121.19 75.2)
          (xy 120.75 75.2)
          (xy 120.75 75)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 85.8)
          (xy 119.25 86)
          (xy 118.81 86)
          (xy 118.81 85.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 86.6)
          (xy 121.19 86.8)
          (xy 120.75 86.8)
          (xy 120.75 86.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 75.4)
          (xy 121.19 75.6)
          (xy 120.75 75.6)
          (xy 120.75 75.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 76.2)
          (xy 121.19 76.4)
          (xy 120.75 76.4)
          (xy 120.75 76.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 87)
          (xy 119.25 87.2)
          (xy 118.81 87.2)
          (xy 118.81 87)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 86.6)
          (xy 119.25 86.8)
          (xy 118.81 86.8)
          (xy 118.81 86.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 87.4)
          (xy 119.25 87.6)
          (xy 118.81 87.6)
          (xy 118.81 87.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 78.6)
          (xy 121.19 78.8)
          (xy 120.75 78.8)
          (xy 120.75 78.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 82.2)
          (xy 121.19 82.4)
          (xy 120.75 82.4)
          (xy 120.75 82.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 80.6)
          (xy 119.25 80.8)
          (xy 118.81 80.8)
          (xy 118.81 80.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 75)
          (xy 121.19 75.2)
          (xy 120.75 75.2)
          (xy 120.75 75)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 79.8)
          (xy 121.19 80)
          (xy 120.75 80)
          (xy 120.75 79.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 85.8)
          (xy 121.19 86)
          (xy 120.75 86)
          (xy 120.75 85.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 77.4)
          (xy 121.19 77.6)
          (xy 120.75 77.6)
          (xy 120.75 77.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 74.6)
          (xy 121.19 74.8)
          (xy 120.75 74.8)
          (xy 120.75 74.6)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 81.8)
          (xy 121.19 82)
          (xy 120.75 82)
          (xy 120.75 81.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 81.4)
          (xy 119.25 81.6)
          (xy 118.81 81.6)
          (xy 118.81 81.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 77.4)
          (xy 119.25 77.6)
          (xy 118.81 77.6)
          (xy 118.81 77.4)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 78.2)
          (xy 119.25 78.4)
          (xy 118.81 78.4)
          (xy 118.81 78.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 87.8)
          (xy 121.19 88)
          (xy 120.75 88)
          (xy 120.75 87.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 75.8)
          (xy 121.19 76)
          (xy 120.75 76)
          (xy 120.75 75.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 83.8)
          (xy 119.25 84)
          (xy 118.81 84)
          (xy 118.81 83.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 76.2)
          (xy 121.19 76.4)
          (xy 120.75 76.4)
          (xy 120.75 76.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 82.2)
          (xy 119.25 82.4)
          (xy 118.81 82.4)
          (xy 118.81 82.2)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 121.19 75.8)
          (xy 121.19 76)
          (xy 120.75 76)
          (xy 120.75 75.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.25 76.6)
          (xy 119.25 76.8)
          (xy 118.81 76.8)
          (xy 118.81 76.6)
        )
      )
    )
  )
  (footprint "Button_Switch_SMD:SW_DIP_SPSTx04_Slide_Omron_A6S-410x_W8.9mm_P2.54mm" (layer "F.Cu")
    (tedit 5AC88315)
    (at 157 88.1 90)
    (descr "SMD 4x-dip-switch SPST Omron_A6S-410x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)")
    (tags "SMD DIP Switch SPST Slide 8.9mm 350mil")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW5" (at 0 -6.61 90) (layer "F.SilkS"))
    (fp_text value "SW_DIP_x04" (at 0 6.61 90) (layer "F.Fab"))
    (fp_text user "on" (at 0.075 -4.955 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.3 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.45 -3.81 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pintype "passive"))
    (pad "2" smd rect (at -4.45 -1.27 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pintype "passive"))
    (pad "3" smd rect (at -4.45 1.27 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pintype "passive"))
    (pad "4" smd rect (at -4.45 3.81 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "GND") (pintype "passive"))
    (pad "5" smd rect (at 4.45 3.81 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/CFG4") (pintype "passive"))
    (pad "6" smd rect (at 4.45 1.27 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/CFG3") (pintype "passive"))
    (pad "7" smd rect (at 4.45 -1.27 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/CFG2") (pintype "passive"))
    (pad "8" smd rect (at 4.45 -3.81 90) (size 1.5 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/CFG1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx04_Slide_Omron_A6S-410x_W8.9mm_P2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Samtec:Samtec_FMC_ASP-134604-01_4x40_Vertical_Renamed" (layer "B.Cu")
    (tedit 5A29C41A)
    (at 106.4 85.5)
    (descr "https://suddendocs.samtec.com/prints/asp-134604-01-mkt.pdf")
    (tags "FMC LPC VITA ")
    (property "Sheetfile" "orbtrace-fmc-breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -8.5 0 90) (layer "B.SilkS"))
    (fp_text value "Samtec_ASP-134604-01" (at 9 0 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at 3.05 -27.19 270) (size 1.27 1.27) (drill 1.27) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 27.19 270) (size 1.27 1.27) (drill 1.27) (layers *.Cu *.Mask))
    (pad "C1" smd circle (at -3.175 24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "C2" smd circle (at -3.175 23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "unconnected-(J1-PadC2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "C3" smd circle (at -3.175 22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "unconnected-(J1-PadC3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "C4" smd circle (at -3.175 20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "C5" smd circle (at -3.175 19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "C6" smd circle (at -3.175 18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "unconnected-(J1-PadC6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "C7" smd circle (at -3.175 17.145 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "unconnected-(J1-PadC7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "C8" smd circle (at -3.175 15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "C9" smd circle (at -3.175 14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "C10" smd circle (at -3.175 13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "/LA06_P") (pinfunction "Pin_10") (pintype "passive"))
    (pad "C11" smd circle (at -3.175 12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "/LA06_N") (pinfunction "Pin_11") (pintype "passive"))
    (pad "C12" smd circle (at -3.175 10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "C13" smd circle (at -3.175 9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "C14" smd circle (at -3.175 8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/LA10_P") (pinfunction "Pin_14") (pintype "passive"))
    (pad "C15" smd circle (at -3.175 6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "/LA10_N") (pinfunction "Pin_15") (pintype "passive"))
    (pad "C16" smd circle (at -3.175 5.715 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (pad "C17" smd circle (at -3.175 4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "C18" smd circle (at -3.175 3.175 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "/LA14_P") (pinfunction "Pin_18") (pintype "passive"))
    (pad "C19" smd circle (at -3.175 1.905 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "/LA14_N") (pinfunction "Pin_19") (pintype "passive"))
    (pad "C20" smd circle (at -3.175 0.635 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (pad "C21" smd circle (at -3.175 -0.64 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "C22" smd circle (at -3.175 -1.905 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "/LA18_P_CC") (pinfunction "Pin_22") (pintype "passive"))
    (pad "C23" smd circle (at -3.175 -3.175 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "/LA18_N_CC") (pinfunction "Pin_23") (pintype "passive"))
    (pad "C24" smd circle (at -3.175 -4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "C25" smd circle (at -3.175 -5.715 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "C26" smd circle (at -3.175 -6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "/LA27_P") (pinfunction "Pin_26") (pintype "passive"))
    (pad "C27" smd circle (at -3.175 -8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "/LA27_N") (pinfunction "Pin_27") (pintype "passive"))
    (pad "C28" smd circle (at -3.175 -9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_28") (pintype "passive"))
    (pad "C29" smd circle (at -3.175 -10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "C30" smd circle (at -3.175 -12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "unconnected-(J1-PadC30)") (pinfunction "Pin_30") (pintype "passive+no_connect"))
    (pad "C31" smd circle (at -3.175 -13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "unconnected-(J1-PadC31)") (pinfunction "Pin_31") (pintype "passive+no_connect"))
    (pad "C32" smd circle (at -3.175 -14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_32") (pintype "passive"))
    (pad "C33" smd circle (at -3.175 -15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "C34" smd circle (at -3.175 -17.145 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "unconnected-(J1-PadC34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "C35" smd circle (at -3.175 -18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "unconnected-(J1-PadC35)") (pinfunction "Pin_35") (pintype "passive+no_connect"))
    (pad "C36" smd circle (at -3.175 -19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_36") (pintype "passive"))
    (pad "C37" smd circle (at -3.175 -20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "unconnected-(J1-PadC37)") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "C38" smd circle (at -3.175 -22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_38") (pintype "passive"))
    (pad "C39" smd circle (at -3.175 -23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "+3V3") (pinfunction "Pin_39") (pintype "passive"))
    (pad "C40" smd circle (at -3.175 -24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_40") (pintype "passive"))
    (pad "D1" smd circle (at -1.905 24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "unconnected-(J1-PadD1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "D2" smd circle (at -1.905 23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "D3" smd circle (at -1.905 22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "D4" smd circle (at -1.905 20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "unconnected-(J1-PadD4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "D5" smd circle (at -1.905 19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "unconnected-(J1-PadD5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "D6" smd circle (at -1.905 18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "D7" smd circle (at -1.905 17.145 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "D8" smd circle (at -1.905 15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/LA01_P_CC") (pinfunction "Pin_8") (pintype "passive"))
    (pad "D9" smd circle (at -1.905 14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/LA01_N_CC") (pinfunction "Pin_9") (pintype "passive"))
    (pad "D10" smd circle (at -1.905 13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "D11" smd circle (at -1.905 12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 119 "unconnected-(J1-PadD11)") (pinfunction "Pin_11") (pintype "passive+no_connect"))
    (pad "D12" smd circle (at -1.905 10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "unconnected-(J1-PadD12)") (pinfunction "Pin_12") (pintype "passive+no_connect"))
    (pad "D13" smd circle (at -1.905 9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "D14" smd circle (at -1.905 8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "unconnected-(J1-PadD14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "D15" smd circle (at -1.905 6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 116 "unconnected-(J1-PadD15)") (pinfunction "Pin_15") (pintype "passive+no_connect"))
    (pad "D16" smd circle (at -1.905 5.715 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (pad "D17" smd circle (at -1.905 4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "unconnected-(J1-PadD17)") (pinfunction "Pin_17") (pintype "passive+no_connect"))
    (pad "D18" smd circle (at -1.905 3.175 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "/SWO") (pinfunction "Pin_18") (pintype "passive"))
    (pad "D19" smd circle (at -1.905 1.91 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "D20" smd circle (at -1.905 0.635 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "/SWDIO") (pinfunction "Pin_20") (pintype "passive"))
    (pad "D21" smd circle (at -1.905 -0.635 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "/SWDCLK") (pinfunction "Pin_21") (pintype "passive"))
    (pad "D22" smd circle (at -1.905 -1.905 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_22") (pintype "passive"))
    (pad "D23" smd circle (at -1.905 -3.175 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "unconnected-(J1-PadD23)") (pinfunction "Pin_23") (pintype "passive+no_connect"))
    (pad "D24" smd circle (at -1.905 -4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 113 "unconnected-(J1-PadD24)") (pinfunction "Pin_24") (pintype "passive+no_connect"))
    (pad "D25" smd circle (at -1.905 -5.715 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "D26" smd circle (at -1.905 -6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "/LA26_P") (pinfunction "Pin_26") (pintype "passive"))
    (pad "D27" smd circle (at -1.905 -8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "/LA26_N") (pinfunction "Pin_27") (pintype "passive"))
    (pad "D28" smd circle (at -1.905 -9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_28") (pintype "passive"))
    (pad "D29" smd circle (at -1.905 -10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "unconnected-(J1-PadD29)") (pinfunction "Pin_29") (pintype "passive+no_connect"))
    (pad "D30" smd circle (at -1.905 -12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "unconnected-(J1-PadD30)") (pinfunction "Pin_30") (pintype "passive+no_connect"))
    (pad "D31" smd circle (at -1.905 -13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "unconnected-(J1-PadD31)") (pinfunction "Pin_31") (pintype "passive+no_connect"))
    (pad "D32" smd circle (at -1.905 -14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "unconnected-(J1-PadD32)") (pinfunction "Pin_32") (pintype "passive+no_connect"))
    (pad "D33" smd circle (at -1.905 -15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "unconnected-(J1-PadD33)") (pinfunction "Pin_33") (pintype "passive+no_connect"))
    (pad "D34" smd circle (at -1.905 -17.145 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "unconnected-(J1-PadD34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "D35" smd circle (at -1.905 -18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "unconnected-(J1-PadD35)") (pinfunction "Pin_35") (pintype "passive+no_connect"))
    (pad "D36" smd circle (at -1.905 -19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "+3V3") (pinfunction "Pin_36") (pintype "passive"))
    (pad "D37" smd circle (at -1.905 -20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_37") (pintype "passive"))
    (pad "D38" smd circle (at -1.905 -22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "+3V3") (pinfunction "Pin_38") (pintype "passive"))
    (pad "D39" smd circle (at -1.905 -23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_39") (pintype "passive"))
    (pad "D40" smd circle (at -1.905 -24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "+3V3") (pinfunction "Pin_40") (pintype "passive"))
    (pad "G1" smd circle (at 1.905 24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "G2" smd circle (at 1.905 23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "unconnected-(J1-PadG2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "G3" smd circle (at 1.905 22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "unconnected-(J1-PadG3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "G4" smd circle (at 1.905 20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "G5" smd circle (at 1.905 19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "G6" smd circle (at 1.905 18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "/LA00_P_CC") (pinfunction "Pin_6") (pintype "passive"))
    (pad "G7" smd circle (at 1.905 17.14 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "/LA00_N_CC") (pinfunction "Pin_7") (pintype "passive"))
    (pad "G8" smd circle (at 1.905 15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "G9" smd circle (at 1.905 14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "/LA03_P") (pinfunction "Pin_9") (pintype "passive"))
    (pad "G10" smd circle (at 1.905 13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/LA03_N") (pinfunction "Pin_10") (pintype "passive"))
    (pad "G11" smd circle (at 1.905 12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "G12" smd circle (at 1.905 10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "unconnected-(J1-PadG12)") (pinfunction "Pin_12") (pintype "passive+no_connect"))
    (pad "G13" smd circle (at 1.905 9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "unconnected-(J1-PadG13)") (pinfunction "Pin_13") (pintype "passive+no_connect"))
    (pad "G14" smd circle (at 1.905 8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "G15" smd circle (at 1.905 6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "/CFG4") (pinfunction "Pin_15") (pintype "passive"))
    (pad "G16" smd circle (at 1.905 5.715 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "/CFG3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "G17" smd circle (at 1.905 4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "G18" smd circle (at 1.905 3.17 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/LA16_P") (pinfunction "Pin_18") (pintype "passive"))
    (pad "G19" smd circle (at 1.905 1.905 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/LA16_N") (pinfunction "Pin_19") (pintype "passive"))
    (pad "G20" smd circle (at 1.905 0.635 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (pad "G21" smd circle (at 1.905 -0.635 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/LA20_P") (pinfunction "Pin_21") (pintype "passive"))
    (pad "G22" smd circle (at 1.905 -1.905 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/LA20_N") (pinfunction "Pin_22") (pintype "passive"))
    (pad "G23" smd circle (at 1.905 -3.175 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "G24" smd circle (at 1.905 -4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/LA22_P") (pinfunction "Pin_24") (pintype "passive"))
    (pad "G25" smd circle (at 1.905 -5.71 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/LA22_N") (pinfunction "Pin_25") (pintype "passive"))
    (pad "G26" smd circle (at 1.905 -6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_26") (pintype "passive"))
    (pad "G27" smd circle (at 1.905 -8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "/LA25_P") (pinfunction "Pin_27") (pintype "passive+no_connect"))
    (pad "G28" smd circle (at 1.905 -9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "/LA25_N") (pinfunction "Pin_28") (pintype "passive+no_connect"))
    (pad "G29" smd circle (at 1.905 -10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "G30" smd circle (at 1.905 -12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/LA29_P") (pinfunction "Pin_30") (pintype "passive+no_connect"))
    (pad "G31" smd circle (at 1.905 -13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/LA29_N") (pinfunction "Pin_31") (pintype "passive+no_connect"))
    (pad "G32" smd circle (at 1.905 -14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_32") (pintype "passive"))
    (pad "G33" smd circle (at 1.905 -15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "unconnected-(J1-PadG33)") (pinfunction "Pin_33") (pintype "passive+no_connect"))
    (pad "G34" smd circle (at 1.905 -17.145 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "unconnected-(J1-PadG34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "G35" smd circle (at 1.905 -18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_35") (pintype "passive"))
    (pad "G36" smd circle (at 1.905 -19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/LA33_P") (pinfunction "Pin_36") (pintype "passive+no_connect"))
    (pad "G37" smd circle (at 1.905 -20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/LA33_N") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "G38" smd circle (at 1.905 -22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_38") (pintype "passive"))
    (pad "G39" smd circle (at 1.905 -23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "unconnected-(J1-PadG39)") (pinfunction "Pin_39") (pintype "passive+no_connect"))
    (pad "G40" smd circle (at 1.905 -24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_40") (pintype "passive"))
    (pad "H1" smd circle (at 3.175 24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "unconnected-(J1-PadH1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "H2" smd circle (at 3.175 23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "H3" smd circle (at 3.175 22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "H4" smd circle (at 3.175 20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "unconnected-(J1-PadH4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "H5" smd circle (at 3.175 19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "unconnected-(J1-PadH5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "H6" smd circle (at 3.175 18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "H7" smd circle (at 3.175 17.14 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "/PB1") (pinfunction "Pin_7") (pintype "passive"))
    (pad "H8" smd circle (at 3.175 15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/PB3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "H9" smd circle (at 3.175 14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "H10" smd circle (at 3.175 13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "/LA04_P") (pinfunction "Pin_10") (pintype "passive"))
    (pad "H11" smd circle (at 3.175 12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "/LA04_N") (pinfunction "Pin_11") (pintype "passive"))
    (pad "H12" smd circle (at 3.175 10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "H13" smd circle (at 3.175 9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "/LA07_P") (pinfunction "Pin_13") (pintype "passive"))
    (pad "H14" smd circle (at 3.175 8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/LA07_N") (pinfunction "Pin_14") (pintype "passive"))
    (pad "H15" smd circle (at 3.175 6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "H16" smd circle (at 3.175 5.715 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/LA11_P") (pinfunction "Pin_16") (pintype "passive"))
    (pad "H17" smd circle (at 3.175 4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/LA11_N") (pinfunction "Pin_17") (pintype "passive"))
    (pad "H18" smd circle (at 3.175 3.17 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "H19" smd circle (at 3.175 1.905 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "/LA15_P") (pinfunction "Pin_19") (pintype "passive"))
    (pad "H20" smd circle (at 3.175 0.635 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/LA15_N") (pinfunction "Pin_20") (pintype "passive"))
    (pad "H21" smd circle (at 3.175 -0.635 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "H22" smd circle (at 3.175 -1.905 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/LA19_P") (pinfunction "Pin_22") (pintype "passive"))
    (pad "H23" smd circle (at 3.175 -3.175 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/LA19_N") (pinfunction "Pin_23") (pintype "passive"))
    (pad "H24" smd circle (at 3.175 -4.445 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "H25" smd circle (at 3.175 -5.715 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/LA21_P") (pinfunction "Pin_25") (pintype "passive"))
    (pad "H26" smd circle (at 3.175 -6.985 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/LA21_N") (pinfunction "Pin_26") (pintype "passive"))
    (pad "H27" smd circle (at 3.175 -8.255 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_27") (pintype "passive"))
    (pad "H28" smd circle (at 3.175 -9.525 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "/LA24_P") (pinfunction "Pin_28") (pintype "passive"))
    (pad "H29" smd circle (at 3.175 -10.795 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/LA24_N") (pinfunction "Pin_29") (pintype "passive"))
    (pad "H30" smd circle (at 3.175 -12.065 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "H31" smd circle (at 3.175 -13.335 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "/LA28_P") (pinfunction "Pin_31") (pintype "passive"))
    (pad "H32" smd circle (at 3.175 -14.605 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "/LA28_N") (pinfunction "Pin_32") (pintype "passive"))
    (pad "H33" smd circle (at 3.175 -15.875 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "H34" smd circle (at 3.175 -17.145 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "unconnected-(J1-PadH34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "H35" smd circle (at 3.175 -18.415 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "unconnected-(J1-PadH35)") (pinfunction "Pin_35") (pintype "passive+no_connect"))
    (pad "H36" smd circle (at 3.175 -19.685 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_36") (pintype "passive"))
    (pad "H37" smd circle (at 3.175 -20.955 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "unconnected-(J1-PadH37)") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "H38" smd circle (at 3.175 -22.225 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "/nRESET") (pinfunction "Pin_38") (pintype "passive"))
    (pad "H39" smd circle (at 3.175 -23.495 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "GND") (pinfunction "Pin_39") (pintype "passive"))
    (pad "H40" smd circle (at 3.175 -24.765 270) (size 0.64 0.64) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "unconnected-(J1-PadH40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Samtec.3dshapes/Samtec_FMC_ASP-134604-01_4x40_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 168.8 55.7) (end 162.5 55.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 146.9 120) (end 146.9 116.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 90 51) (end 151.7 51) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 90 120) (end 90 51) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 168.8 116.7) (end 168.8 55.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 146.9 116.7) (end 168.8 116.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 146.9 120) (end 90 120) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 162.5 53.6) (end 151.7 53.6) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 151.7 53.6) (end 151.7 51) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 162.5 55.7) (end 162.5 53.6) (layer "Edge.Cuts") (width 0.1))
  (gr_text "IDEX Biometrics Ltd \nRevision 0.2\n2023/08/04\nMini-ITX FMC Orbtrace Breakout Board" (at 161.7 70.1) (layer "B.SilkS"))
  (gr_text "User IO" (at 92.3 99 90) (layer "F.SilkS"))
  (gr_text "JLink" (at 141.25 53.5) (layer "F.SilkS"))
  (gr_text "User IO" (at 92.3 72.8 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 146.9 116.7) (xy 146.9 120))
    (height -32.6)
    (gr_text "3.3000 mm" (at 178.35 118.35 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 90 120) (xy 146.9 120))
    (height 4.4)
    (gr_text "56.90 mm" (at 118.45 123.25) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 168.8 116.7) (xy 90 116.68))
    (height -12.100001)
    (gr_text "78.8000 mm" (at 129.397221 127.640001 -0.01454207571) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 168.8 116.7) (xy 168.8 55.7))
    (height 6)
    (gr_text "61.00 mm" (at 173.65 86.2 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 2))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 90 51) (xy 151.7 51))
    (height -6.8)
    (gr_text "61.70 mm" (at 120.85 43.05) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 2))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 90 51) (xy 90 120))
    (height 5.4)
    (gr_text "69.00 mm" (at 83.45 85.5 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 146.9 116.7) (xy 168.8 116.7))
    (height 7.7)
    (gr_text "21.90 mm" (at 157.85 123.25) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 151.7 53.6) (xy 162.5 53.6))
    (height -9.4)
    (gr_text "10.80 mm" (at 157 42.7) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 2))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 162.5 55.7) (xy 168.8 55.7))
    (height -11.5)
    (gr_text "6.30 mm" (at 167.8 42.7) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 2))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 61) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.7 53.6)
        (xy 162.5 53.6)
        (xy 162.5 55.7)
        (xy 168.8 55.7)
        (xy 168.8 116.7)
        (xy 146.9 116.7)
        (xy 146.9 120)
        (xy 90 120)
        (xy 90 51)
        (xy 151.7 51)
      )
    )
  )
)
