(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 115)
    (no_connects 0)
    (area 25.949999 29.949999 91.050001 86.050001)
    (thickness 1.6)
    (drawings 44)
    (tracks 331)
    (zones 0)
    (modules 46)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.4318)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 1.016 0.635)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.75 2.75)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.07)
    (aux_axis_origin 26 86)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00008_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory meta/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(J1-Pad11)")
  (net 4 "Net-(J1-Pad12)")
  (net 5 "Net-(J1-Pad13)")
  (net 6 "Net-(J1-Pad15)")
  (net 7 "Net-(J1-Pad19)")
  (net 8 "Net-(J1-Pad22)")
  (net 9 "Net-(J1-Pad26)")
  (net 10 "Net-(J1-Pad31)")
  (net 11 "Net-(J1-Pad32)")
  (net 12 "Net-(J1-Pad33)")
  (net 13 "Net-(J1-Pad35)")
  (net 14 "Net-(J1-Pad36)")
  (net 15 "Net-(J1-Pad37)")
  (net 16 "Net-(J1-Pad38)")
  (net 17 "Net-(J1-Pad40)")
  (net 18 "Net-(U5-Pad7)")
  (net 19 "Net-(U5-Pad9)")
  (net 20 "Net-(U5-Pad10)")
  (net 21 "Net-(U5-Pad11)")
  (net 22 "Net-(U5-Pad12)")
  (net 23 "Net-(R1-Pad2)")
  (net 24 "Net-(BT1-Pad1)")
  (net 25 "Net-(U7-Pad1)")
  (net 26 "Net-(U7-Pad3)")
  (net 27 "Net-(U7-Pad4)")
  (net 28 /TC1+)
  (net 29 /TC1-)
  (net 30 /TC2+)
  (net 31 /TC2-)
  (net 32 /TC3+)
  (net 33 /TC3-)
  (net 34 /T_SDA)
  (net 35 /T_SCL)
  (net 36 /T_OW)
  (net 37 /TC_A1)
  (net 38 /TC_A0)
  (net 39 /TC_MISO)
  (net 40 /TC_CLK)
  (net 41 /ID_SD)
  (net 42 /ID_SC)
  (net 43 /~TC_CS1~)
  (net 44 /~TC_CS2~)
  (net 45 /~TC_CS3~)
  (net 46 +5V)
  (net 47 "Net-(BZ1-Pad2)")
  (net 48 /ALERT)
  (net 49 /TX)
  (net 50 /RX)
  (net 51 /TC_CE)
  (net 52 +3.3VA)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3.3VA)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ALERT)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /RX)
    (add_net /TC1+)
    (add_net /TC1-)
    (add_net /TC2+)
    (add_net /TC2-)
    (add_net /TC3+)
    (add_net /TC3-)
    (add_net /TC_A0)
    (add_net /TC_A1)
    (add_net /TC_CE)
    (add_net /TC_CLK)
    (add_net /TC_MISO)
    (add_net /TX)
    (add_net /T_OW)
    (add_net /T_SCL)
    (add_net /T_SDA)
    (add_net /~TC_CS1~)
    (add_net /~TC_CS2~)
    (add_net /~TC_CS3~)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BZ1-Pad2)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad31)")
    (add_net "Net-(J1-Pad32)")
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad9)")
    (add_net "Net-(U7-Pad1)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad4)")
  )
  (net_class +3V3 ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 1.016)
    (via_drill 0.635)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58B9C9FB)
    (at 44 61.5 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 3.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /TC2-))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /TC2+))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /TC_CLK))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /~TC_CS2~))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /TC_MISO))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 87.5 33.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 87.5 82.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CB9)
    (at 29.5 82.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 29.5 33.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Connectors_Phoenix:PhoenixContact_PTSM0,5_2-2,5-V_SMD (layer F.Cu) (tedit 58B9CAB6)
    (at 55 48 270)
    (descr "PhoenixContact PTSM0,5 2 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814702/pdf")
    (tags "PhoenixContact PTSM0.5 2 2.5mm vertical SMD spring clamp terminal block connector ")
    (attr smd)
    (fp_text reference J2 (at 4 3.5 360) (layer F.SilkS))
    (fp_text value "Push Terminal" (at -0.2 -5.43 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.25 1.58 90) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /TC1-))
    (pad 1 smd rect (at -1.25 1.58 90) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 28 /TC1+))
    (pad "" smd rect (at 5.05 -1.58 90) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -5.05 -1.58 90) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_Phoenix:PhoenixContact_PTSM0,5_2-2,5-V_SMD (layer F.Cu) (tedit 58B9CAB2)
    (at 55 61.5 270)
    (descr "PhoenixContact PTSM0,5 2 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814702/pdf")
    (tags "PhoenixContact PTSM0.5 2 2.5mm vertical SMD spring clamp terminal block connector ")
    (attr smd)
    (fp_text reference J3 (at 4 3.5 360) (layer F.SilkS))
    (fp_text value "Push Terminal" (at -0.2 -5.43 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.25 1.58 90) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 31 /TC2-))
    (pad 1 smd rect (at -1.25 1.58 90) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 30 /TC2+))
    (pad "" smd rect (at 5.05 -1.58 90) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -5.05 -1.58 90) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_Phoenix:PhoenixContact_PTSM0,5_2-2,5-V_SMD (layer F.Cu) (tedit 58B9CAAD)
    (at 55 75 270)
    (descr "PhoenixContact PTSM0,5 2 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814702/pdf")
    (tags "PhoenixContact PTSM0.5 2 2.5mm vertical SMD spring clamp terminal block connector ")
    (attr smd)
    (fp_text reference J4 (at 4 3.5 360) (layer F.SilkS))
    (fp_text value "Push Terminal" (at -0.2 -5.43 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.25 1.58 90) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /TC3-))
    (pad 1 smd rect (at -1.25 1.58 90) (size 1.4 3.4) (layers F.Cu F.Paste F.Mask)
      (net 32 /TC3+))
    (pad "" smd rect (at 5.05 -1.58 90) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -5.05 -1.58 90) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58B9CABC)
    (at 85.5 42 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.5 180) (layer F.SilkS))
    (fp_text value AT24CS32 (at 0 3.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /ID_SD))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /ID_SC))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58B9C9E2)
    (at 44 48 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 3.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /TC1-))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /TC1+))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /TC_CLK))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /~TC_CS1~))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /TC_MISO))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58B9CA10)
    (at 44 75 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -3.5 180) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 3.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /TC3-))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /TC3+))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /TC_CLK))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /~TC_CS3~))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /TC_MISO))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 58B9C9AE)
    (at 33 43 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at 0 3.5 180) (layer F.SilkS))
    (fp_text value 74LVC139 (at 0 3.55 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 /TC_CE))
    (pad 2 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 /TC_A0))
    (pad 3 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 /TC_A1))
    (pad 4 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 /~TC_CS1~))
    (pad 5 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 /~TC_CS2~))
    (pad 6 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 /~TC_CS3~))
    (pad 7 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U5-Pad7)"))
    (pad 8 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U5-Pad9)"))
    (pad 10 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U5-Pad10)"))
    (pad 11 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U5-Pad11)"))
    (pad 12 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U5-Pad12)"))
    (pad 13 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 14 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 15 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 16 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D675)
    (at 33 46.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.25 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D6BE)
    (at 85.5 45.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.5 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58C49A4A)
    (at 44 44.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.25 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D66F)
    (at 44 58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.25 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D64B)
    (at 44 71.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.25 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D672)
    (at 50 48 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2 0 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 /TC1+))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 29 /TC1-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D5FD)
    (at 50 61.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2 0 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 30 /TC2+))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 /TC2-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D5F9)
    (at 50 75 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2 0 360) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.5 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 /TC3+))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 /TC3-))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module raspberry-ml:Pin_Header_Straight_2x20 locked (layer F.Cu) (tedit 58B9C9C3)
    (at 58.5 33.5 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -3.584 -26.496 360) (layer F.SilkS))
    (fp_text value RPi_GPIO (at -1.27 -27.23 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 1.27 -24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 +5V))
    (pad 3 thru_hole oval (at -1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /T_SDA))
    (pad 4 thru_hole oval (at 1.27 -21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 +5V))
    (pad 5 thru_hole oval (at -1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /T_SCL))
    (pad 6 thru_hole oval (at 1.27 -19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at -1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /T_OW))
    (pad 8 thru_hole oval (at 1.27 -16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /TX))
    (pad 9 thru_hole oval (at -1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole oval (at 1.27 -13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /RX))
    (pad 11 thru_hole oval (at -1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 1.27 -11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at -1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 1.27 -8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole oval (at -1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 1.27 -6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /TC_A1))
    (pad 17 thru_hole oval (at -1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at 1.27 -3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /TC_A0))
    (pad 19 thru_hole oval (at -1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at 1.27 -1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole oval (at -1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /TC_MISO))
    (pad 22 thru_hole oval (at 1.27 1.27 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad22)"))
    (pad 23 thru_hole oval (at -1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /TC_CLK))
    (pad 24 thru_hole oval (at 1.27 3.81 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /TC_CE))
    (pad 25 thru_hole oval (at -1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 26 thru_hole oval (at 1.27 6.35 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad26)"))
    (pad 27 thru_hole oval (at -1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /ID_SD))
    (pad 28 thru_hole oval (at 1.27 8.89 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /ID_SC))
    (pad 29 thru_hole oval (at -1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /ALERT))
    (pad 30 thru_hole oval (at 1.27 11.43 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 31 thru_hole oval (at -1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad31)"))
    (pad 32 thru_hole oval (at 1.27 13.97 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad32)"))
    (pad 33 thru_hole oval (at -1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad33)"))
    (pad 34 thru_hole oval (at 1.27 16.51 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 35 thru_hole oval (at -1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad35)"))
    (pad 36 thru_hole oval (at 1.27 19.05 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad36)"))
    (pad 37 thru_hole oval (at -1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad37)"))
    (pad 38 thru_hole oval (at 1.27 21.59 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad38)"))
    (pad 39 thru_hole oval (at -1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 40 thru_hole oval (at 1.27 24.13 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad40)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58B9D6C5)
    (at 79.5 44)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.5 0) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58B9D689)
    (at 79.5 40)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.5 0) (layer F.SilkS))
    (fp_text value 3.9k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 /ID_SD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58B9D6C8)
    (at 79.5 42)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.5 0) (layer F.SilkS))
    (fp_text value 3.9k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 /ID_SC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-1000P-B (layer F.Cu) (tedit 58B9D6C2)
    (at 86.36 48.5)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, with Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value Write (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58C48966)
    (at 37 70 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2 0 360) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at -2.4 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /T_OW))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58B9D646)
    (at 34.6 61.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.4 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58C49BCE)
    (at 34.5 56.5 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at 0 3.75 360) (layer F.SilkS))
    (fp_text value DS3231M (at 0 3.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U7-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U7-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U7-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(BT1-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /T_SDA))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /T_SCL))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery_Holders:Keystone_3000_1x12mm-CoinCell (layer F.Cu) (tedit 58C49B7A)
    (at 81.5 71.5 90)
    (descr http://www.keyelco.com/product-pdf.cfm?p=777)
    (tags "Keystone type 3000 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 8 3.59 360) (layer F.SilkS))
    (fp_text value CR1225 (at 0 7.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -7.9 0 90) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at 7.9 0 90) (size 3.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 4 4) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Battery_Holders.3dshapes/Keystone_3000_1x12mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58B9D666)
    (at 36 49.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2 0 180) (layer F.SilkS))
    (fp_text value DNI (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /T_SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58B9D66A)
    (at 36 51.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2 0 180) (layer F.SilkS))
    (fp_text value DNI (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /T_SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58C48952)
    (at 37 75.25 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U6 (at -2.25 0 180) (layer F.SilkS))
    (fp_text value DS18S20 (at 1.27 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 36 /T_OW))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 52 +3.3VA))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module cui-ml:CMI-9655S-SMT (layer F.Cu) (tedit 58C49B71)
    (at 71 42.5 270)
    (descr "Buzzer, Magnetic Indicator")
    (tags CUI)
    (fp_text reference BZ1 (at 4.49 -6.47 360) (layer F.SilkS))
    (fp_text value Buzzer (at 0 6 270) (layer F.Fab) hide)
    (fp_text user + (at -4 -2 270) (layer F.Fab))
    (fp_text user %R (at 6.5 -4.5 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -4 0 270) (size 3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 46 +5V))
    (pad 2 smd rect (at 4 0 270) (size 3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(BZ1-Pad2)"))
    (model Buzzers_Beepers.3dshapes/MagneticBuzzer_Kingstate_KCG0601.wrl
      (at (xyz 0.124803 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58C45436)
    (at 71 50.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 3 360) (layer F.SilkS))
    (fp_text value NUD3124 (at 0 2.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 /ALERT))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(BZ1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58C49B54)
    (at 33.5 74 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -2.835 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.00mm (layer F.Cu) (tedit 58C49B1C)
    (at 31.5 76 180)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (fp_text reference P1 (at 0 -2 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 6.12 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /T_OW))
    (pad 3 thru_hole oval (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 +3.3VA))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58C4990C)
    (at 45.847 38.1 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P2 (at 0 7.493 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /TX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Symbols:OSHW-Logo_11.4x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 82 57.25 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_11.4x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 76.5 82.5)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D08E2F)
    (at 71 53.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.25 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /ALERT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58E2FA14)
    (at 58.25 39 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 1.5 450) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at -1.905 -0.127 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58E2F9EE)
    (at 65.25 39 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.25 0 450) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.032 0 360) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 46 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E2F88A)
    (at 44 43.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at -2.75 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E2F883)
    (at 44 56.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -2.75 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E2F87C)
    (at 44 70.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -2.75 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 58E8F0D0)
    (at 61.75 39.62 270)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3 Housing ")
    (attr smd)
    (fp_text reference U8 (at 3.88 0 360) (layer F.SilkS))
    (fp_text value MCP1754ST (at 0.45 3.25 270) (layer F.Fab) hide)
    (fp_text user %R (at 0.38 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.48 -1.5 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 46 +5V))
    (pad 2 smd rect (at -1.48 0 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.48 1.5 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 52 +3.3VA))
    (pad 2 smd rect (at 1.48 0 180) (size 2 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd trapezoid (at -0.37 0) (size 1.5 0.75) (rect_delta 0 0.5 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0.02 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Rev 1.2 Apr 2017\n" (at 73.35 62.445) (layer B.SilkS))
  (gr_text "by Mike Lawrence" (at 73.35 59.905) (layer B.SilkS))
  (gr_text "Thermocouple Hat" (at 73.25 55.75) (layer B.SilkS))
  (gr_text 1-Wire (at 26.67 69.215) (layer F.SilkS))
  (gr_text Console (at 35.25 38.1) (layer F.SilkS))
  (gr_text GND (at 50.927 40.386 90) (layer F.SilkS))
  (gr_text RX (at 48.387 40.386 90) (layer F.SilkS))
  (gr_text TX (at 45.847 40.386 90) (layer F.SilkS))
  (gr_text GND (at 29.5 76) (layer F.SilkS))
  (gr_text DQ (at 29.5 74) (layer F.SilkS))
  (gr_text VDD (at 29.5 72) (layer F.SilkS))
  (dimension 65 (width 0.15) (layer F.Fab)
    (gr_text "65 mm" (at 58.5 24.95) (layer F.Fab))
    (feature1 (pts (xy 26 29) (xy 26 23.9)))
    (feature2 (pts (xy 91 29) (xy 91 23.9)))
    (crossbar (pts (xy 91 26) (xy 26 26)))
    (arrow1a (pts (xy 26 26) (xy 27.126504 25.413579)))
    (arrow1b (pts (xy 26 26) (xy 27.126504 26.586421)))
    (arrow2a (pts (xy 91 26) (xy 89.873496 25.413579)))
    (arrow2b (pts (xy 91 26) (xy 89.873496 26.586421)))
  )
  (dimension 56.000019 (width 0.15) (layer F.Fab)
    (gr_text "56 mm" (at 96.072953 57.99668 270.0469723) (layer F.Fab))
    (feature1 (pts (xy 92.04591 86) (xy 97.145908 85.995819)))
    (feature2 (pts (xy 92 30) (xy 97.099998 29.995819)))
    (crossbar (pts (xy 94.999999 29.997541) (xy 95.045909 85.997541)))
    (arrow1a (pts (xy 95.045909 85.997541) (xy 94.458565 84.871518)))
    (arrow1b (pts (xy 95.045909 85.997541) (xy 95.631406 84.870557)))
    (arrow2a (pts (xy 94.999999 29.997541) (xy 94.414502 31.124525)))
    (arrow2b (pts (xy 94.999999 29.997541) (xy 95.587343 31.123564)))
  )
  (gr_text CR1225 (at 89.5 71.5 90) (layer F.SilkS))
  (gr_text TC3- (at 60 76.5) (layer F.SilkS))
  (gr_text TC3+ (at 60 73.5) (layer F.SilkS))
  (gr_text TC2- (at 60 63) (layer F.SilkS))
  (gr_text TC2+ (at 60 60) (layer F.SilkS))
  (gr_text TC1- (at 60 49.5) (layer F.SilkS))
  (gr_text TC1+ (at 60 46.5) (layer F.SilkS))
  (gr_text Write (at 86.36 51.5) (layer F.SilkS))
  (gr_text "Rev 1.2 Apr 2017\n" (at 68.75 59) (layer F.SilkS))
  (gr_text "by Mike Lawrence" (at 68.75 56.5) (layer F.SilkS))
  (gr_text "Thermocouple Hat" (at 38.1 83.82) (layer F.SilkS))
  (gr_arc (start 88 33) (end 88 30) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 29 30) (end 88 30) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 29 33) (end 26 33) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 71 81.5) (end 69.5 81.5) (angle -180) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 71 67.5) (end 69.5 67.5) (angle 180) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.5 67.5) (end 72.5 81.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.5 67.5) (end 69.5 81.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 27 67.5) (end 26 67.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 30 65.5) (end 31 65.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 30 50.5) (end 30 49.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 27 48.5) (end 27 49.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 88 83) (end 91 83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 29 83) (end 29 86) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 26 67.5) (end 26 83) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 26 33) (end 26 48.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 27 66.5) (end 30 66.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 27 49.5) (end 30 49.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31 50.5) (end 31 65.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 29 86) (end 88 86) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91 33) (end 91 83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2286)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 91 86) (xy 26 86) (xy 26 30) (xy 91 30)
      )
    )
  )
  (zone (net 1) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2286)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 91 86) (xy 26 86) (xy 26 30) (xy 91 30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 86) (xy 26 86) (xy 26 65.5) (xy 40.5 65.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26 65.5) (xy 40.5 65.5) (xy 40.5 86) (xy 26 86)
      )
    )
  )
)
