<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="42.525" y2="0" width="0" layer="20"/>
<wire x1="42.525" y1="0" x2="42.525" y2="22.53" width="0" layer="20"/>
<wire x1="42.525" y1="22.53" x2="0" y2="22.53" width="0" layer="20"/>
<wire x1="0" y1="22.53" x2="0" y2="0" width="0" layer="20"/>
<text>AC IN
(8-34v)</text>
<text>V+</text>
<text>V-</text>
</plain>
<libraries>
<library name="rectifier">
<description>&lt;b&gt;Rectifiers&lt;/b&gt;&lt;p&gt;
General Instrument, Semikron, Diotec, Fagor&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W0G">
<description>&lt;b&gt;RECTIFIER&lt;/b&gt;&lt;p&gt;
1 A</description>
</package>
</packages>
</library>
<library name="rc-master">
<description>&lt;b&gt;R/C MASTER! - v1.19 (10/25/2011)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD and through hole resistors and capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
As a general guideline, SMD resistors are typically rated as follows:&lt;p&gt;
0402 = 1/16 watt&lt;br&gt;
0603 = 1/10 watt&lt;br&gt;
0805 = 1/8  watt&lt;br&gt;
1206 = 1/4  watt&lt;br&gt;
2010 = 1/2  watt&lt;br&gt;
2512 = 1    watt&lt;br&gt;&lt;p&gt;
&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007-2008, Bob Starr&lt;br&gt; 
&lt;a href="http://www.bobstarr.net"&gt;http://www.bobstarr.net&lt;/a&gt;
&lt;/author&gt;</description>
<packages>
<package name="CE-050X100">
<description>&lt;b&gt;POLCAP RADIAL&lt;/b&gt;&lt;p&gt;
5.0 mm lead spacing, 10 mm diameter, grid 0.0125 inch</description>
</package>
<package name="CE-020X050">
<description>&lt;b&gt;POLCAP RADIAL&lt;/b&gt;&lt;p&gt;
2.0 mm lead spacing, 5 mm diameter, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;MALE Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78LXX">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="79LXX">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B1" library="rectifier" package="W0G" value="821-W10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rc-master" package="CE-050X100" value="1000uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rc-master" package="CE-050X100" value="1000uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rc-master" package="CE-020X050" value="10uf">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="rc-master" package="CE-020X050" value="10uf">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="con-lstb" package="MA03-1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="con-lstb" package="MA04-1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="v-reg" package="78LXX" value="78LXXLP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="v-reg" package="79LXX" value="79LXX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="+"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="+"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="N$1">
<contactref element="B1" pad="AC1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="B1" pad="AC2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="B1" pad="-"/>
<contactref element="U2" pad="2"/>
<contactref element="C2" pad="-"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="B1" pad="+"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$6">
<contactref element="U2" pad="3"/>
<contactref element="J2" pad="4"/>
<contactref element="C4" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
