<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="22.86" y2="0" width="0" layer="20"/>
<wire x1="22.86" y1="0" x2="25.4" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="25.4" y1="2.54" x2="25.4" y2="8.89" width="0" layer="20"/>
<wire x1="25.4" y1="8.89" x2="29.21" y2="8.89" width="0" layer="20"/>
<wire x1="29.21" y1="8.89" x2="30.48" y2="10.16" width="0" layer="20" curve="90"/>
<wire x1="30.48" y1="10.16" x2="30.48" y2="15.24" width="0" layer="20"/>
<wire x1="30.48" y1="15.24" x2="29.21" y2="16.51" width="0" layer="20" curve="90"/>
<wire x1="29.21" y1="16.51" x2="25.4" y2="16.51" width="0" layer="20"/>
<wire x1="25.4" y1="16.51" x2="25.4" y2="22.86" width="0" layer="20"/>
<wire x1="25.4" y1="22.86" x2="22.86" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="22.86" y1="25.4" x2="2.54" y2="25.4" width="0" layer="20"/>
<wire x1="2.54" y1="25.4" x2="0" y2="22.86" width="0" layer="20" curve="90"/>
<wire x1="0" y1="22.86" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="-3.81" y2="17.78" width="0" layer="20"/>
<wire x1="-3.81" y1="17.78" x2="-5.08" y2="16.51" width="0" layer="20" curve="90"/>
<wire x1="-5.08" y1="16.51" x2="-5.08" y2="8.89" width="0" layer="20"/>
<wire x1="-5.08" y1="8.89" x2="-3.81" y2="7.62" width="0" layer="20" curve="90"/>
<wire x1="-3.81" y1="7.62" x2="0" y2="7.62" width="0" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="2.54" width="0" layer="20"/>
</plain>
<libraries>
<library name="IRT2008Passive">
<packages>
<package name="603">
</package>
</packages>
</library>
<library name="IRT2008Active">
<packages>
<package name="SOT23-3">
</package>
<package name="SOT23-5">
</package>
<package name="SOT223A">
</package>
</packages>
</library>
<library name="IRT2008CON">
<packages>
<package name="WIREPAD60-40">
</package>
</packages>
</library>
<library name="Dan_Con">
<description>Dan Contract Library.</description>
<packages>
<package name="SO-8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C14" library="IRT2008Passive" package="603" value="10uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="IRT2008Passive" package="603" value="10uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="IRT2008Passive" package="603" value="2200pF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C17" library="IRT2008Passive" package="603" value="10uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="IRT2008Passive" package="603" value="1uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q1" library="IRT2008Active" package="SOT23-3" value="MMBT2222A">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R33" library="IRT2008Passive" package="603" value="9.76K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R35" library="IRT2008Passive" package="603" value="16.5K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U17" library="IRT2008Active" package="SOT23-5" value="TPS60400">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="IRT2008Active" package="SOT23-5" value="AD8638">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="IRT2008Active" package="SOT23-5" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="IRT2008Passive" package="603" value="10uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="IRT2008Passive" package="603" value="10K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="IRT2008Active" package="SOT23-5" value="AD8638">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U4" library="IRT2008Active" package="SOT23-5" value="AD8638">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="IRT2008Passive" package="603" value="2.94K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="IRT2008Passive" package="603" value="1.47K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U6" library="IRT2008Active" package="SOT223A" value="78M05">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C18" library="IRT2008Passive" package="603" value=".1uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C19" library="IRT2008Passive" package="603" value=".1uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="IRT2008Passive" package="603" value="1uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="IRT2008Passive" package="603" value="10K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="IRT2008Passive" package="603" value="10K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="IRT2008Passive" package="603" value="???">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="IRT2008Passive" package="603" value="???">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="IRT2008Passive" package="603" value="10uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="EFC" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40">
<attribute name="NAME"/>
</element>
<element name="/EFC" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40">
<attribute name="NAME"/>
</element>
<element name="PWM" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40">
<attribute name="NAME"/>
</element>
<element name="U5" library="Dan_Con" package="SO-8" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="EFCG" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40">
<attribute name="NAME"/>
</element>
<element name="C4" library="IRT2008Passive" package="603" value="1uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="3.3V" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40">
<attribute name="NAME"/>
</element>
<element name="GND" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40">
<attribute name="NAME"/>
</element>
<element name="+12" library="IRT2008CON" package="WIREPAD60-40" value="WIREPAD60-40">
<attribute name="NAME"/>
</element>
<element name="R8" library="IRT2008Passive" package="603" value="10">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C6" library="IRT2008Passive" package="603" value=".1uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="IRT2008Passive" package="603" value="10uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R33" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="U17" pad="4"/>
<contactref element="C14" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="U6" pad="TAB"/>
<contactref element="U6" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U5" pad="4"/>
<contactref element="EFCG" pad="P$1"/>
<contactref element="GND" pad="P$1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="+3.3V">
<contactref element="R35" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="3.3V" pad="P$1"/>
</signal>
<signal name="N$32">
<contactref element="R35" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$33">
<contactref element="U1" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U17" pad="3"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U17" pad="5"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="Q1" pad="3"/>
<contactref element="C19" pad="2"/>
<contactref element="U6" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="U5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="+12" pad="P$1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="+REF1">
<contactref element="U1" pad="3"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U4" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="/EFC" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U4" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="EFC" pad="P$1"/>
</signal>
<signal name="+5V">
<contactref element="U6" pad="3"/>
<contactref element="C18" pad="2"/>
<contactref element="U17" pad="2"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="-5V">
<contactref element="C5" pad="2"/>
<contactref element="U17" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="2"/>
<contactref element="PWM" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
