(kicad_pcb (version 20171130) (host pcbnew 5.0.0)
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 196)
    (zones 0)
    (modules 30)
    (nets 136)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 1.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 /GPIO0)
  (net 2 /GPIO1)
  (net 3 /GPIO2)
  (net 4 /GPIO3)
  (net 5 /RADIO_TR)
  (net 6 /RADIO_RR)
  (net 7 /GPIO4)
  (net 8 /GPIO5)
  (net 9 /GPIO6)
  (net 10 /GPIO7)
  (net 11 /GPIO8)
  (net 12 /GPIO9)
  (net 13 /GPIO10)
  (net 14 /GPIO11)
  (net 15 /GPIO12)
  (net 16 /GPIO13)
  (net 17 /RADIO_RX)
  (net 18 /RADIO_TX)
  (net 19 /12C2_SDA)
  (net 20 /I2C2_SCL)
  (net 21 /SYS_SPI_SCK)
  (net 22 /SYS_SPI_MISO)
  (net 23 /SYS_SPI_MOSI)
  (net 24 /SYS_SPI_NSS)
  (net 25 "Net-(P1-Pad27)")
  (net 26 "Net-(P1-Pad28)")
  (net 27 /SYS_RESET)
  (net 28 "Net-(P1-Pad31)")
  (net 29 /SGPIO7)
  (net 30 /SGPIO8)
  (net 31 /SGPIO9)
  (net 32 /SGPIO10)
  (net 33 /SGPIO11)
  (net 34 /SGPIO12)
  (net 35 /SGPIO13)
  (net 36 /SGPIO14)
  (net 37 /SYS_SDA)
  (net 38 "Net-(P1-Pad42)")
  (net 39 /SYS_SCL)
  (net 40 "Net-(P1-Pad44)")
  (net 41 "Net-(P1-Pad45)")
  (net 42 "Net-(P1-Pad46)")
  (net 43 /NBUFEN_PRI)
  (net 44 /NBUFEN_SEC)
  (net 45 /SGPIO5)
  (net 46 /SGPIO6)
  (net 47 /SGPIO0)
  (net 48 /SGPIO1)
  (net 49 /SGPIO2)
  (net 50 /SGPIO3)
  (net 51 /I2C3_SDA)
  (net 52 /I2C3_SCL)
  (net 53 /SGPIO4)
  (net 54 GND)
  (net 55 +5V)
  (net 56 "Net-(P2-Pad31)")
  (net 57 "Net-(P2-Pad42)")
  (net 58 "Net-(P2-Pad44)")
  (net 59 "Net-(P2-Pad45)")
  (net 60 "Net-(P2-Pad46)")
  (net 61 /SPI2_NSS)
  (net 62 /SPI2_SCK)
  (net 63 /SPI2_MISO)
  (net 64 /SPI2_MOSI)
  (net 65 "Net-(P3-Pad21)")
  (net 66 "Net-(P3-Pad22)")
  (net 67 "Net-(J1-Pad1)")
  (net 68 "Net-(J2-Pad1)")
  (net 69 "Net-(U1-Pad2)")
  (net 70 "Net-(U1-Pad7)")
  (net 71 "Net-(U10-Pad2)")
  (net 72 "Net-(U3-Pad4)")
  (net 73 "Net-(U4-Pad4)")
  (net 74 "Net-(U5-Pad2)")
  (net 75 "Net-(U6-Pad2)")
  (net 76 "Net-(U7-Pad2)")
  (net 77 "Net-(U14-Pad2)")
  (net 78 "Net-(U11-Pad4)")
  (net 79 "Net-(U10-Pad7)")
  (net 80 "Net-(U11-Pad2)")
  (net 81 "Net-(U12-Pad2)")
  (net 82 "Net-(U13-Pad2)")
  (net 83 "Net-(U15-Pad4)")
  (net 84 "Net-(U16-Pad11)")
  (net 85 "Net-(U17-Pad4)")
  (net 86 "Net-(P1-Pad8)")
  (net 87 "Net-(P1-Pad10)")
  (net 88 "Net-(P1-Pad11)")
  (net 89 "Net-(P1-Pad12)")
  (net 90 "Net-(P1-Pad13)")
  (net 91 "Net-(P1-Pad15)")
  (net 92 "Net-(P1-Pad16)")
  (net 93 "Net-(P1-Pad18)")
  (net 94 "Net-(P1-Pad19)")
  (net 95 "Net-(P1-Pad20)")
  (net 96 "Net-(P1-Pad23)")
  (net 97 "Net-(P1-Pad24)")
  (net 98 "Net-(P1-Pad33)")
  (net 99 "Net-(P1-Pad34)")
  (net 100 "Net-(P1-Pad35)")
  (net 101 "Net-(P1-Pad36)")
  (net 102 "Net-(P1-Pad37)")
  (net 103 "Net-(P1-Pad38)")
  (net 104 "Net-(P1-Pad39)")
  (net 105 "Net-(P1-Pad40)")
  (net 106 "Net-(P1-Pad41)")
  (net 107 "Net-(P1-Pad43)")
  (net 108 "Net-(P2-Pad25)")
  (net 109 "Net-(P2-Pad26)")
  (net 110 "Net-(P2-Pad27)")
  (net 111 "Net-(P2-Pad28)")
  (net 112 "Net-(P2-Pad30)")
  (net 113 "Net-(P2-Pad32)")
  (net 114 "Net-(P3-Pad5)")
  (net 115 "Net-(P3-Pad6)")
  (net 116 "Net-(P3-Pad9)")
  (net 117 "Net-(P3-Pad10)")
  (net 118 "Net-(P3-Pad13)")
  (net 119 "Net-(P3-Pad14)")
  (net 120 "Net-(P3-Pad17)")
  (net 121 "Net-(P3-Pad18)")
  (net 122 "Net-(P3-Pad26)")
  (net 123 "Net-(P3-Pad30)")
  (net 124 "Net-(P3-Pad41)")
  (net 125 "Net-(P3-Pad42)")
  (net 126 "Net-(P3-Pad45)")
  (net 127 "Net-(P3-Pad46)")
  (net 128 "Net-(P3-Pad49)")
  (net 129 "Net-(P3-Pad50)")
  (net 130 "Net-(P3-Pad53)")
  (net 131 "Net-(P3-Pad54)")
  (net 132 "Net-(P3-Pad57)")
  (net 133 "Net-(P3-Pad58)")
  (net 134 "Net-(P2-Pad49)")
  (net 135 "Net-(P2-Pad51)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /12C2_SDA)
    (add_net /GPIO0)
    (add_net /GPIO1)
    (add_net /GPIO10)
    (add_net /GPIO11)
    (add_net /GPIO12)
    (add_net /GPIO13)
    (add_net /GPIO2)
    (add_net /GPIO3)
    (add_net /GPIO4)
    (add_net /GPIO5)
    (add_net /GPIO6)
    (add_net /GPIO7)
    (add_net /GPIO8)
    (add_net /GPIO9)
    (add_net /I2C2_SCL)
    (add_net /I2C3_SCL)
    (add_net /I2C3_SDA)
    (add_net /NBUFEN_PRI)
    (add_net /NBUFEN_SEC)
    (add_net /RADIO_RR)
    (add_net /RADIO_RX)
    (add_net /RADIO_TR)
    (add_net /RADIO_TX)
    (add_net /SGPIO0)
    (add_net /SGPIO1)
    (add_net /SGPIO10)
    (add_net /SGPIO11)
    (add_net /SGPIO12)
    (add_net /SGPIO13)
    (add_net /SGPIO14)
    (add_net /SGPIO2)
    (add_net /SGPIO3)
    (add_net /SGPIO4)
    (add_net /SGPIO5)
    (add_net /SGPIO6)
    (add_net /SGPIO7)
    (add_net /SGPIO8)
    (add_net /SGPIO9)
    (add_net /SPI2_MISO)
    (add_net /SPI2_MOSI)
    (add_net /SPI2_NSS)
    (add_net /SPI2_SCK)
    (add_net /SYS_RESET)
    (add_net /SYS_SCL)
    (add_net /SYS_SDA)
    (add_net /SYS_SPI_MISO)
    (add_net /SYS_SPI_MOSI)
    (add_net /SYS_SPI_NSS)
    (add_net /SYS_SPI_SCK)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad27)")
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad31)")
    (add_net "Net-(P1-Pad33)")
    (add_net "Net-(P1-Pad34)")
    (add_net "Net-(P1-Pad35)")
    (add_net "Net-(P1-Pad36)")
    (add_net "Net-(P1-Pad37)")
    (add_net "Net-(P1-Pad38)")
    (add_net "Net-(P1-Pad39)")
    (add_net "Net-(P1-Pad40)")
    (add_net "Net-(P1-Pad41)")
    (add_net "Net-(P1-Pad42)")
    (add_net "Net-(P1-Pad43)")
    (add_net "Net-(P1-Pad44)")
    (add_net "Net-(P1-Pad45)")
    (add_net "Net-(P1-Pad46)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P2-Pad25)")
    (add_net "Net-(P2-Pad26)")
    (add_net "Net-(P2-Pad27)")
    (add_net "Net-(P2-Pad28)")
    (add_net "Net-(P2-Pad30)")
    (add_net "Net-(P2-Pad31)")
    (add_net "Net-(P2-Pad32)")
    (add_net "Net-(P2-Pad42)")
    (add_net "Net-(P2-Pad44)")
    (add_net "Net-(P2-Pad45)")
    (add_net "Net-(P2-Pad46)")
    (add_net "Net-(P2-Pad49)")
    (add_net "Net-(P2-Pad51)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad13)")
    (add_net "Net-(P3-Pad14)")
    (add_net "Net-(P3-Pad17)")
    (add_net "Net-(P3-Pad18)")
    (add_net "Net-(P3-Pad21)")
    (add_net "Net-(P3-Pad22)")
    (add_net "Net-(P3-Pad26)")
    (add_net "Net-(P3-Pad30)")
    (add_net "Net-(P3-Pad41)")
    (add_net "Net-(P3-Pad42)")
    (add_net "Net-(P3-Pad45)")
    (add_net "Net-(P3-Pad46)")
    (add_net "Net-(P3-Pad49)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad50)")
    (add_net "Net-(P3-Pad53)")
    (add_net "Net-(P3-Pad54)")
    (add_net "Net-(P3-Pad57)")
    (add_net "Net-(P3-Pad58)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad7)")
    (add_net "Net-(U11-Pad2)")
    (add_net "Net-(U11-Pad4)")
    (add_net "Net-(U12-Pad2)")
    (add_net "Net-(U13-Pad2)")
    (add_net "Net-(U14-Pad2)")
    (add_net "Net-(U15-Pad4)")
    (add_net "Net-(U16-Pad11)")
    (add_net "Net-(U17-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U6-Pad2)")
    (add_net "Net-(U7-Pad2)")
  )
  (net_class RF_Track ""
    (clearance 0.2)
    (trace_width 1.84)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Radiometer-RF-Board:eye (layer B.Cu) (tedit 0)
    (at 181.61 111.125 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Connectors_Samtec:MECF-30-01-NP-L-DV-WT_Socket (layer B.Cu) (tedit 5B16ECF0)
    (at 87.7824 106.8832 270)
    (descr "Highspeed card edge connector for 1.6mm PCB's with 30 contacts (not polarized)")
    (tags "conn samtec card-edge high-speed")
    (attr smd)
    (fp_text reference P3 (at 0 -3.81 270) (layer B.SilkS))
    (fp_text value CONN_02X30 (at 0 3.81 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad "" thru_hole circle (at 22.1 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -22.1 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 20.195 -1 270) (size 0 0) (drill 1.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -20.195 0 270) (size 0 0) (drill 1.45) (layers *.Cu *.Mask))
    (pad 60 smd rect (at 18.415 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 59 smd rect (at 18.415 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 58 smd rect (at 17.145 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 133 "Net-(P3-Pad58)"))
    (pad 57 smd rect (at 17.145 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 132 "Net-(P3-Pad57)"))
    (pad 56 smd rect (at 15.875 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 55 smd rect (at 15.875 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 54 smd rect (at 14.605 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(P3-Pad54)"))
    (pad 53 smd rect (at 14.605 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 130 "Net-(P3-Pad53)"))
    (pad 52 smd rect (at 13.335 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 51 smd rect (at 13.335 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 50 smd rect (at 12.065 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 129 "Net-(P3-Pad50)"))
    (pad 49 smd rect (at 12.065 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 128 "Net-(P3-Pad49)"))
    (pad 48 smd rect (at 10.795 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 47 smd rect (at 10.795 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 46 smd rect (at 9.525 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(P3-Pad46)"))
    (pad 45 smd rect (at 9.525 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(P3-Pad45)"))
    (pad 44 smd rect (at 8.255 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 43 smd rect (at 8.255 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 42 smd rect (at 6.985 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(P3-Pad42)"))
    (pad 41 smd rect (at 6.985 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 124 "Net-(P3-Pad41)"))
    (pad 40 smd rect (at 5.715 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 39 smd rect (at 5.715 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 38 smd rect (at 4.445 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 55 +5V))
    (pad 37 smd rect (at 4.445 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 55 +5V))
    (pad 36 smd rect (at 3.175 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 35 smd rect (at 3.175 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 34 smd rect (at 1.905 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 55 +5V))
    (pad 33 smd rect (at 1.905 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 55 +5V))
    (pad 32 smd rect (at 0.635 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 31 smd rect (at 0.635 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 30 smd rect (at -0.635 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 123 "Net-(P3-Pad30)"))
    (pad 29 smd rect (at -0.635 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 37 /SYS_SDA))
    (pad 28 smd rect (at -1.905 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 27 smd rect (at -1.905 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 26 smd rect (at -3.175 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(P3-Pad26)"))
    (pad 25 smd rect (at -3.175 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 39 /SYS_SCL))
    (pad 24 smd rect (at -4.445 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 23 smd rect (at -4.445 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 22 smd rect (at -5.715 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(P3-Pad22)"))
    (pad 21 smd rect (at -5.715 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(P3-Pad21)"))
    (pad 20 smd rect (at -6.985 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 19 smd rect (at -6.985 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 18 smd rect (at -8.255 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(P3-Pad18)"))
    (pad 17 smd rect (at -8.255 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(P3-Pad17)"))
    (pad 16 smd rect (at -9.525 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 15 smd rect (at -9.525 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 14 smd rect (at -10.795 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 119 "Net-(P3-Pad14)"))
    (pad 13 smd rect (at -10.795 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 118 "Net-(P3-Pad13)"))
    (pad 12 smd rect (at -12.065 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 11 smd rect (at -12.065 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 10 smd rect (at -13.335 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 117 "Net-(P3-Pad10)"))
    (pad 9 smd rect (at -13.335 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 116 "Net-(P3-Pad9)"))
    (pad 8 smd rect (at -14.605 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 7 smd rect (at -14.605 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 6 smd rect (at -15.875 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(P3-Pad6)"))
    (pad 5 smd rect (at -15.875 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(P3-Pad5)"))
    (pad 4 smd rect (at -17.145 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 3 smd rect (at -17.145 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -18.415 1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
    (pad 1 smd rect (at -18.415 -1.905 270) (size 0.66 1.35) (layers B.Cu B.Paste B.Mask)
      (net 54 GND))
  )
  (module Project:TAMP-1512GLN+ (layer F.Cu) (tedit 5B4E0C7A)
    (at 138.938 80.264)
    (fp_text reference U10 (at 8.763 -3.302) (layer F.SilkS))
    (fp_text value TAMP_1512GLN+ (at 8.89 10.922) (layer F.Fab))
    (pad 2 smd rect (at 1 3.8) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U10-Pad2)"))
    (pad 1 smd rect (at 1.1 8.6) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 11 smd rect (at 4.2 8.8) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 10 smd rect (at 6.75 8.8) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 9 smd rect (at 9.65 8.8) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 8 smd rect (at 12.2 8.8) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 7 smd rect (at 15.8 3.8) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U10-Pad7)"))
    (pad 6 smd rect (at 15.578 -1) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 5 smd rect (at 12.6 -1.2) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 55 +5V))
    (pad 4 smd rect (at 4.1 -1.2) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 3 smd rect (at 1.1 -1) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:CBP-1400E+ (layer F.Cu) (tedit 5B4E0BD5)
    (at 160.147 91.313 270)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*11.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 16.5mm width 11.2mm Capacitor")
    (fp_text reference U8 (at 9.906 -5.842 270) (layer F.SilkS))
    (fp_text value CBP-1400E+ (at 10.033 8.509 270) (layer F.Fab))
    (pad 1 smd rect (at 1.756 -1.784 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U14-Pad2)"))
    (pad 2 smd rect (at 1.756 1.01 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 3 smd rect (at 1.78 4.29 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 4.55 6.45 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 5 smd rect (at 7.09 6.45 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 6 smd rect (at 9.63 6.45 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 7 smd rect (at 12.17 6.45 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 8 smd rect (at 14.71 6.45 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 9 smd rect (at 17.48 4.29 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 10 smd rect (at 17.48 1.01 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 11 smd rect (at 17.48 -1.78 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U4-Pad4)"))
    (pad 12 smd rect (at 14.71 -4.07 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 13 smd rect (at 12.17 -4.07 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 14 smd rect (at 9.63 -4.07 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 15 smd rect (at 7.09 -4.07 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 16 smd rect (at 4.55 -4.07 270) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L16.5mm_W11.2mm_P15.00mm_MKT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Project:CSK_Header (layer F.Cu) (tedit 5AF48666)
    (at 94.8944 63.35776 90)
    (descr "Through hole straight socket strip, 2x26, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x26 2.54mm double row")
    (fp_text reference P1 (at -1.27 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_02X26 (at -1.27 157.48 90) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.683175 0.362681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /SGPIO0))
    (pad 2 thru_hole oval (at -0.143175 0.362681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /SGPIO1))
    (pad 3 thru_hole oval (at -2.683175 2.902681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /SGPIO2))
    (pad 4 thru_hole oval (at -0.143175 2.902681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /SGPIO3))
    (pad 5 thru_hole oval (at -2.683175 5.442681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /I2C3_SDA))
    (pad 6 thru_hole oval (at -0.143175 5.442681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /I2C3_SCL))
    (pad 7 thru_hole oval (at -2.683175 7.982681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /SGPIO4))
    (pad 8 thru_hole oval (at -0.143175 7.982681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at -2.683175 10.522681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 10 thru_hole oval (at -0.143175 10.522681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at -2.683175 13.062681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at -0.143175 13.062681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at -2.683175 15.602681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at -0.143175 15.602681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 15 thru_hole oval (at -2.683175 18.142681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at -0.143175 18.142681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at -2.683175 20.682681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 18 thru_hole oval (at -0.143175 20.682681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P1-Pad18)"))
    (pad 19 thru_hole oval (at -2.683175 23.222681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(P1-Pad19)"))
    (pad 20 thru_hole oval (at -0.143175 23.222681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(P1-Pad20)"))
    (pad 21 thru_hole oval (at -2.683175 25.762681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 22 thru_hole oval (at -0.143175 25.762681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 23 thru_hole oval (at -2.683175 28.302681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(P1-Pad23)"))
    (pad 24 thru_hole oval (at -0.143175 28.302681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(P1-Pad24)"))
    (pad 25 thru_hole oval (at -2.683175 30.842681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 +5V))
    (pad 26 thru_hole oval (at -0.143175 30.842681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 +5V))
    (pad 27 thru_hole oval (at -2.683175 33.382681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P1-Pad27)"))
    (pad 28 thru_hole oval (at -0.143175 33.382681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P1-Pad28)"))
    (pad 29 thru_hole oval (at -2.683175 35.922681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 30 thru_hole oval (at -0.143175 35.922681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 31 thru_hole oval (at -2.683175 38.462681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P1-Pad31)"))
    (pad 32 thru_hole oval (at -0.143175 38.462681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 33 thru_hole oval (at -2.683175 41.002681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(P1-Pad33)"))
    (pad 34 thru_hole oval (at -0.143175 41.002681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(P1-Pad34)"))
    (pad 35 thru_hole oval (at -2.683175 43.542681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(P1-Pad35)"))
    (pad 36 thru_hole oval (at -0.143175 43.542681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(P1-Pad36)"))
    (pad 37 thru_hole oval (at -2.683175 46.082681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(P1-Pad37)"))
    (pad 38 thru_hole oval (at -0.143175 46.082681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(P1-Pad38)"))
    (pad 39 thru_hole oval (at -2.683175 48.622681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(P1-Pad39)"))
    (pad 40 thru_hole oval (at -0.143175 48.622681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(P1-Pad40)"))
    (pad 41 thru_hole oval (at -2.683175 51.162681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(P1-Pad41)"))
    (pad 42 thru_hole oval (at -0.143175 51.162681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P1-Pad42)"))
    (pad 43 thru_hole oval (at -2.683175 53.702681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(P1-Pad43)"))
    (pad 44 thru_hole oval (at -0.143175 53.702681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P1-Pad44)"))
    (pad 45 thru_hole oval (at -2.683175 56.242681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P1-Pad45)"))
    (pad 46 thru_hole oval (at -0.143175 56.242681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P1-Pad46)"))
    (pad 47 thru_hole oval (at -2.683175 58.782681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 48 thru_hole oval (at -0.143175 58.782681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 GND))
    (pad 49 thru_hole oval (at -2.683175 61.322681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /SPI2_NSS))
    (pad 50 thru_hole oval (at -0.143175 61.322681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /SPI2_SCK))
    (pad 51 thru_hole oval (at -2.683175 63.862681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /SPI2_MISO))
    (pad 52 thru_hole oval (at -0.143175 63.862681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /SPI2_MOSI))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x26_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -31.74999952316284 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Project:CSK_Header (layer F.Cu) (tedit 5AF4865F)
    (at 94.8944 68.43776 90)
    (descr "Through hole straight socket strip, 2x26, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x26 2.54mm double row")
    (fp_text reference P2 (at -1.27 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_02X26 (at 0 153.67 90) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.683175 0.362681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GPIO0))
    (pad 2 thru_hole oval (at -0.143175 0.362681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GPIO1))
    (pad 3 thru_hole oval (at -2.683175 2.902681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GPIO2))
    (pad 4 thru_hole oval (at -0.143175 2.902681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /GPIO3))
    (pad 5 thru_hole oval (at -2.683175 5.442681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RADIO_TR))
    (pad 6 thru_hole oval (at -0.143175 5.442681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RADIO_RR))
    (pad 7 thru_hole oval (at -2.683175 7.982681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO4))
    (pad 8 thru_hole oval (at -0.143175 7.982681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO5))
    (pad 9 thru_hole oval (at -2.683175 10.522681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO6))
    (pad 10 thru_hole oval (at -0.143175 10.522681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /GPIO7))
    (pad 11 thru_hole oval (at -2.683175 13.062681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIO8))
    (pad 12 thru_hole oval (at -0.143175 13.062681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO9))
    (pad 13 thru_hole oval (at -2.683175 15.602681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO10))
    (pad 14 thru_hole oval (at -0.143175 15.602681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GPIO11))
    (pad 15 thru_hole oval (at -2.683175 18.142681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIO12))
    (pad 16 thru_hole oval (at -0.143175 18.142681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO13))
    (pad 17 thru_hole oval (at -2.683175 20.682681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /RADIO_RX))
    (pad 18 thru_hole oval (at -0.143175 20.682681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /RADIO_TX))
    (pad 19 thru_hole oval (at -2.683175 23.222681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /12C2_SDA))
    (pad 20 thru_hole oval (at -0.143175 23.222681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /I2C2_SCL))
    (pad 21 thru_hole oval (at -2.683175 25.762681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SYS_SPI_SCK))
    (pad 22 thru_hole oval (at -0.143175 25.762681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /SYS_SPI_MISO))
    (pad 23 thru_hole oval (at -2.683175 28.302681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /SYS_SPI_MOSI))
    (pad 24 thru_hole oval (at -0.143175 28.302681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SYS_SPI_NSS))
    (pad 25 thru_hole oval (at -2.683175 30.842681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(P2-Pad25)"))
    (pad 26 thru_hole oval (at -0.143175 30.842681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(P2-Pad26)"))
    (pad 27 thru_hole oval (at -2.683175 33.382681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(P2-Pad27)"))
    (pad 28 thru_hole oval (at -0.143175 33.382681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(P2-Pad28)"))
    (pad 29 thru_hole oval (at -2.683175 35.922681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SYS_RESET))
    (pad 30 thru_hole oval (at -0.143175 35.922681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(P2-Pad30)"))
    (pad 31 thru_hole oval (at -2.683175 38.462681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P2-Pad31)"))
    (pad 32 thru_hole oval (at -0.143175 38.462681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(P2-Pad32)"))
    (pad 33 thru_hole oval (at -2.683175 41.002681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SGPIO7))
    (pad 34 thru_hole oval (at -0.143175 41.002681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /SGPIO8))
    (pad 35 thru_hole oval (at -2.683175 43.542681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /SGPIO9))
    (pad 36 thru_hole oval (at -0.143175 43.542681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /SGPIO10))
    (pad 37 thru_hole oval (at -2.683175 46.082681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /SGPIO11))
    (pad 38 thru_hole oval (at -0.143175 46.082681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /SGPIO12))
    (pad 39 thru_hole oval (at -2.683175 48.622681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /SGPIO13))
    (pad 40 thru_hole oval (at -0.143175 48.622681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /SGPIO14))
    (pad 41 thru_hole oval (at -2.683175 51.162681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /SYS_SDA))
    (pad 42 thru_hole oval (at -0.143175 51.162681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P2-Pad42)"))
    (pad 43 thru_hole oval (at -2.683175 53.702681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SYS_SCL))
    (pad 44 thru_hole oval (at -0.143175 53.702681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P2-Pad44)"))
    (pad 45 thru_hole oval (at -2.683175 56.242681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P2-Pad45)"))
    (pad 46 thru_hole oval (at -0.143175 56.242681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P2-Pad46)"))
    (pad 47 thru_hole oval (at -2.683175 58.782681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /NBUFEN_PRI))
    (pad 48 thru_hole oval (at -0.143175 58.782681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /NBUFEN_SEC))
    (pad 49 thru_hole oval (at -2.683175 61.322681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(P2-Pad49)"))
    (pad 50 thru_hole oval (at -0.143175 61.322681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /SGPIO5))
    (pad 51 thru_hole oval (at -2.683175 63.862681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(P2-Pad51)"))
    (pad 52 thru_hole oval (at -0.143175 63.862681 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /SGPIO6))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x26_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -31.74999952316284 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module motherboard:Hole_0.125-0.250 (layer F.Cu) (tedit 583F8348)
    (at 90.17 63.5)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Hole_0.125-0.250 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask))
  )
  (module motherboard:Hole_0.125-0.250 (layer F.Cu) (tedit 583F8348)
    (at 163.83 63.5)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Hole_0.125-0.250 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask))
  )
  (module motherboard:Hole_0.125-0.250 (layer F.Cu) (tedit 583F8348)
    (at 86.36 149.225)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Hole_0.125-0.250 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask))
  )
  (module motherboard:Hole_0.125-0.250 (layer F.Cu) (tedit 583F8348)
    (at 166.37 149.225)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value Hole_0.125-0.250 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask))
  )
  (module Connectors_Samtec:MECF-30-01-NP-L-DV-WT_Socket (layer F.Cu) (tedit 5B16ECF0)
    (at 87.757 106.8578 90)
    (descr "Highspeed card edge connector for 1.6mm PCB's with 30 contacts (not polarized)")
    (tags "conn samtec card-edge high-speed")
    (attr smd)
    (fp_text reference P3 (at 0 3.81 90) (layer F.SilkS))
    (fp_text value CONN_02X30 (at 0 -3.81 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -18.415 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -18.415 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 3 smd rect (at -17.145 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at -17.145 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 5 smd rect (at -15.875 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(P3-Pad5)"))
    (pad 6 smd rect (at -15.875 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(P3-Pad6)"))
    (pad 7 smd rect (at -14.605 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 8 smd rect (at -14.605 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 9 smd rect (at -13.335 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(P3-Pad9)"))
    (pad 10 smd rect (at -13.335 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(P3-Pad10)"))
    (pad 11 smd rect (at -12.065 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 12 smd rect (at -12.065 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 13 smd rect (at -10.795 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(P3-Pad13)"))
    (pad 14 smd rect (at -10.795 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(P3-Pad14)"))
    (pad 15 smd rect (at -9.525 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 16 smd rect (at -9.525 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 17 smd rect (at -8.255 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(P3-Pad17)"))
    (pad 18 smd rect (at -8.255 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(P3-Pad18)"))
    (pad 19 smd rect (at -6.985 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 20 smd rect (at -6.985 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 21 smd rect (at -5.715 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(P3-Pad21)"))
    (pad 22 smd rect (at -5.715 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(P3-Pad22)"))
    (pad 23 smd rect (at -4.445 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 24 smd rect (at -4.445 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 25 smd rect (at -3.175 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 39 /SYS_SCL))
    (pad 26 smd rect (at -3.175 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(P3-Pad26)"))
    (pad 27 smd rect (at -1.905 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 28 smd rect (at -1.905 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 29 smd rect (at -0.635 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 37 /SYS_SDA))
    (pad 30 smd rect (at -0.635 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(P3-Pad30)"))
    (pad 31 smd rect (at 0.635 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 32 smd rect (at 0.635 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 33 smd rect (at 1.905 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 55 +5V))
    (pad 34 smd rect (at 1.905 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 55 +5V))
    (pad 35 smd rect (at 3.175 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 36 smd rect (at 3.175 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 37 smd rect (at 4.445 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 55 +5V))
    (pad 38 smd rect (at 4.445 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 55 +5V))
    (pad 39 smd rect (at 5.715 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 40 smd rect (at 5.715 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 41 smd rect (at 6.985 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(P3-Pad41)"))
    (pad 42 smd rect (at 6.985 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(P3-Pad42)"))
    (pad 43 smd rect (at 8.255 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 44 smd rect (at 8.255 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 45 smd rect (at 9.525 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(P3-Pad45)"))
    (pad 46 smd rect (at 9.525 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(P3-Pad46)"))
    (pad 47 smd rect (at 10.795 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 48 smd rect (at 10.795 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 49 smd rect (at 12.065 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(P3-Pad49)"))
    (pad 50 smd rect (at 12.065 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(P3-Pad50)"))
    (pad 51 smd rect (at 13.335 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 52 smd rect (at 13.335 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 53 smd rect (at 14.605 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(P3-Pad53)"))
    (pad 54 smd rect (at 14.605 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(P3-Pad54)"))
    (pad 55 smd rect (at 15.875 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 56 smd rect (at 15.875 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 57 smd rect (at 17.145 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(P3-Pad57)"))
    (pad 58 smd rect (at 17.145 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(P3-Pad58)"))
    (pad 59 smd rect (at 18.415 1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 60 smd rect (at 18.415 -1.905 90) (size 0.66 1.35) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad "" np_thru_hole circle (at -20.195 0 90) (size 0 0) (drill 1.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 20.195 1 90) (size 0 0) (drill 1.45) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -22.1 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 22.1 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
  )
  (module Connectors:SMA_SMD_Jack_Straight (layer F.Cu) (tedit 58C35474)
    (at 110.871 84.074)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference J1 (at 0 -5) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 smd rect (at 0.85 2.38 20) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -0.85 2.38 340) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 0.85 -2.38 340) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -0.85 -2.38 20) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 1.515 1.749 50) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -1.515 1.749 310) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 1.515 -1.749 310) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -1.515 -1.749 50) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 2.6 2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 0 2.8 90) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -2.6 2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 2.6 -2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 1 smd circle (at 0 0 90) (size 1.73 1.73) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 -2.8 90) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -2.6 -2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Connectors:SMA_SMD_Jack_Straight (layer F.Cu) (tedit 58C35474)
    (at 111.125 138.049)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference J2 (at 0 -5) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 smd rect (at 0.85 2.38 20) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -0.85 2.38 340) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 0.85 -2.38 340) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -0.85 -2.38 20) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 1.515 1.749 50) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -1.515 1.749 310) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 1.515 -1.749 310) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -1.515 -1.749 50) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 2.6 2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 0 2.8 90) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -2.6 2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at 2.6 -2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 1 smd circle (at 0 0 90) (size 1.73 1.73) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0 -2.8 90) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 2 smd rect (at -2.6 -2.38 90) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:TAMP-1512GLN+ (layer F.Cu) (tedit 5B4E0C7A)
    (at 147.828 105.283 180)
    (fp_text reference U1 (at 8.763 -3.302 180) (layer F.SilkS))
    (fp_text value TAMP_1512GLN+ (at 8.89 10.922 180) (layer F.Fab))
    (pad 2 smd rect (at 1 3.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at 1.1 8.6 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 11 smd rect (at 4.2 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 10 smd rect (at 6.75 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 9 smd rect (at 9.65 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 8 smd rect (at 12.2 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 7 smd rect (at 15.8 3.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at 15.578 -1 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 5 smd rect (at 12.6 -1.2 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 55 +5V))
    (pad 4 smd rect (at 4.1 -1.2 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 3 smd rect (at 1.1 -1 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:CBP-1400E+ (layer F.Cu) (tedit 5B4E0BD5)
    (at 117.856 85.852)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*11.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 16.5mm width 11.2mm Capacitor")
    (fp_text reference U2 (at 9.906 -5.842) (layer F.SilkS))
    (fp_text value CBP-1400E+ (at 10.033 8.509) (layer F.Fab))
    (pad 1 smd rect (at 1.756 -1.784) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 1.756 1.01) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 3 smd rect (at 1.78 4.29) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 4.55 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 5 smd rect (at 7.09 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 6 smd rect (at 9.63 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 7 smd rect (at 12.17 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 8 smd rect (at 14.71 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 9 smd rect (at 17.48 4.29) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 10 smd rect (at 17.48 1.01) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 11 smd rect (at 17.48 -1.78) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U10-Pad2)"))
    (pad 12 smd rect (at 14.71 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 13 smd rect (at 12.17 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 14 smd rect (at 9.63 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 15 smd rect (at 7.09 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 16 smd rect (at 4.55 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L16.5mm_W11.2mm_P15.00mm_MKT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 155.575 111.252 270)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U3 (at 1.778 -2.667 270) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556 270) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667 270) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at 0.5969 1.5621 270) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 161.163 111.125 270)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U4 (at 1.778 -2.667 270) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556 270) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667 270) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U3-Pad4)"))
    (pad 1 smd rect (at 2.3495 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U4-Pad4)"))
    (pad 3 smd rect (at 0.5969 1.5621 270) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 127.635 100.838 270)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U5 (at 1.778 -2.667 270) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556 270) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667 270) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U5-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-Pad7)"))
    (pad 3 smd rect (at 0.5969 1.5621 270) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 123.825 102.489 180)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U6 (at 1.778 -2.667 180) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556 180) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667 180) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621 180) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U6-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477 180) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477 180) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U5-Pad2)"))
    (pad 3 smd rect (at 0.5969 1.5621 180) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 118.491 100.838 270)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U7 (at 1.778 -2.667 270) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556 270) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667 270) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U7-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U6-Pad2)"))
    (pad 3 smd rect (at 0.5969 1.5621 270) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 113.538 102.87 270)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U9 (at 1.778 -2.667 270) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556 270) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667 270) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U11-Pad4)"))
    (pad 1 smd rect (at 2.3495 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U7-Pad2)"))
    (pad 3 smd rect (at 0.5969 1.5621 270) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 108.331 104.775 270)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U11 (at 1.778 -2.667 270) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556 270) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667 270) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U11-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477 270) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U11-Pad4)"))
    (pad 3 smd rect (at 0.5969 1.5621 270) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:TAMP-1512GLN+ (layer F.Cu) (tedit 5B4E0C7A)
    (at 136.017 136.779 180)
    (fp_text reference U12 (at 8.763 -3.302 180) (layer F.SilkS))
    (fp_text value TAMP_1512GLN+ (at 8.89 10.922 180) (layer F.Fab))
    (pad 2 smd rect (at 1 3.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U12-Pad2)"))
    (pad 1 smd rect (at 1.1 8.6 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 11 smd rect (at 4.2 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 10 smd rect (at 6.75 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 9 smd rect (at 9.65 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 8 smd rect (at 12.2 8.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 7 smd rect (at 15.8 3.8 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J2-Pad1)"))
    (pad 6 smd rect (at 15.578 -1 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 5 smd rect (at 12.6 -1.2 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 55 +5V))
    (pad 4 smd rect (at 4.1 -1.2 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 3 smd rect (at 1.1 -1 180) (size 2.2 2) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 106.299 110.109)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U13 (at 1.778 -2.667) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U13-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U11-Pad2)"))
    (pad 3 smd rect (at 0.5969 1.5621) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 157.988 84.709)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U14 (at 1.778 -2.667) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U14-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U10-Pad7)"))
    (pad 3 smd rect (at 0.5969 1.5621) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 134.239 122.555)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U15 (at 1.778 -2.667) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U12-Pad2)"))
    (pad 1 smd rect (at 2.3495 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U15-Pad4)"))
    (pad 3 smd rect (at 0.5969 1.5621) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:CBP-1400E+ (layer F.Cu) (tedit 5B4E0BD5)
    (at 110.363 113.538)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=16.5*11.2mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 16.5mm width 11.2mm Capacitor")
    (fp_text reference U16 (at 9.906 -5.842) (layer F.SilkS))
    (fp_text value CBP-1400E+ (at 10.033 8.509) (layer F.Fab))
    (pad 1 smd rect (at 1.756 -1.784) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U13-Pad2)"))
    (pad 2 smd rect (at 1.756 1.01) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 3 smd rect (at 1.78 4.29) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 4.55 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 5 smd rect (at 7.09 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 6 smd rect (at 9.63 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 7 smd rect (at 12.17 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 8 smd rect (at 14.71 6.45) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 9 smd rect (at 17.48 4.29) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 10 smd rect (at 17.48 1.01) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 11 smd rect (at 17.48 -1.78) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U16-Pad11)"))
    (pad 12 smd rect (at 14.71 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 13 smd rect (at 12.17 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 14 smd rect (at 9.63 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 15 smd rect (at 7.09 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 16 smd rect (at 4.55 -4.07) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L16.5mm_W11.2mm_P15.00mm_MKT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 132.334 117.856)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U17 (at 1.778 -2.667) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U15-Pad4)"))
    (pad 1 smd rect (at 2.3495 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U17-Pad4)"))
    (pad 3 smd rect (at 0.5969 1.5621) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module Project:LAT_1+ (layer F.Cu) (tedit 5B4E0C93)
    (at 130.302 112.395)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference U18 (at 1.778 -2.667) (layer F.SilkS))
    (fp_text value LAT (at 1.778 3.556) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.667) (layer F.Fab))
    (pad 2 smd rect (at 2.3495 1.5621) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U17-Pad4)"))
    (pad 1 smd rect (at 2.3495 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
    (pad 4 smd rect (at 0.4445 -0.6477) (size 0.889 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U16-Pad11)"))
    (pad 3 smd rect (at 0.5969 1.5621) (size 1.1938 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 54 GND))
  )
  (module breakoutBoard:Cysized (layer F.Cu) (tedit 0)
    (at 153.543 134.366)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "CySat 1 - RF Board" (at 119.507 146.177) (layer F.SilkS))
  (gr_line (start 137.668 154.305) (end 171.45 154.305) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.28 154.305) (end 117.348 154.305) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.28 116.5098) (end 81.28 154.305) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.28 58.42) (end 81.28 96.2152) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.668 58.42) (end 166.878 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.28 58.42) (end 117.348 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 81.407) (end 171.45 154.305) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.185 116.5098) (end 81.28 116.5098) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.185 96.2152) (end 83.185 116.5098) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.28 96.2152) (end 83.185 96.2152) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.668 151.384) (end 137.668 154.305) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.348 151.384) (end 137.668 151.384) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.348 154.305) (end 117.348 151.384) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.878 81.407) (end 171.45 81.407) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.878 58.42) (end 166.878 81.407) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.668 61.341) (end 137.668 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.348 61.341) (end 137.668 61.341) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.348 58.42) (end 117.348 61.341) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 55) (net_name +5V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.069 153.924) (xy 171.069 81.661) (xy 166.624 81.661) (xy 166.497 58.674) (xy 137.922 58.674)
        (xy 137.922 61.595) (xy 117.094 61.595) (xy 117.094 58.674) (xy 81.534 58.674) (xy 81.534 96.012)
        (xy 83.312 96.012) (xy 83.312 116.713) (xy 81.534 116.713) (xy 81.534 154.051) (xy 117.094 153.924)
        (xy 117.094 151.13) (xy 137.922 151.13) (xy 137.922 154.051)
      )
    )
  )
  (zone (net 54) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.069 153.924) (xy 171.069 81.661) (xy 166.624 81.661) (xy 166.497 58.674) (xy 137.922 58.674)
        (xy 137.922 61.595) (xy 117.094 61.595) (xy 117.094 58.674) (xy 81.534 58.674) (xy 81.534 96.012)
        (xy 83.312 96.012) (xy 83.312 116.713) (xy 81.534 116.713) (xy 81.534 154.051) (xy 117.094 153.924)
        (xy 117.094 151.13) (xy 137.922 151.13) (xy 137.922 154.051)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.3054 78.5622) (xy 95.1738 78.5368) (xy 95.1738 134.8486) (xy 81.4578 134.8486) (xy 81.4578 137.8712)
        (xy 97.4598 137.8204) (xy 97.4852 74.9046) (xy 81.2292 74.9046) (xy 81.2292 78.5622) (xy 81.4578 78.5368)
      )
    )
  )
  (zone (net 54) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.069 153.924) (xy 171.069 81.661) (xy 166.624 81.661) (xy 166.497 58.674) (xy 137.922 58.674)
        (xy 137.922 61.595) (xy 117.094 61.595) (xy 117.094 58.674) (xy 81.534 58.674) (xy 81.534 96.012)
        (xy 83.312 96.012) (xy 83.312 116.713) (xy 81.534 116.713) (xy 81.534 154.051) (xy 117.094 153.924)
        (xy 117.094 151.13) (xy 137.922 151.13) (xy 137.922 154.051)
      )
    )
  )
)
