(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 303)
    (zones 0)
    (modules 23)
    (nets 49)
  )
  (page A)
  (title_block
    (title "Beetje 32U4 Blok")
    (date 2018-08-10)
    (rev 0.0)
    (company www.MakersBox.us)
    (comment 1 648.ken@gmail.com)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.1524)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 3.500001)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 /10)
  (net 2 /04)
  (net 3 /05)
  (net 4 /06)
  (net 5 /07)
  (net 6 /08)
  (net 7 /09)
  (net 8 /11)
  (net 9 /12)
  (net 10 /18)
  (net 11 /19)
  (net 12 /20)
  (net 13 /03)
  (net 14 GND)
  (net 15 +5V)
  (net 16 "Net-(R1-Pad1)")
  (net 17 /A)
  (net 18 /LED1)
  (net 19 "Net-(D1-Pad1)")
  (net 20 "Net-(D2-Pad1)")
  (net 21 /LED2)
  (net 22 /D_IN)
  (net 23 /PT1_P)
  (net 24 /PT2_P)
  (net 25 "Net-(U1-Pad7)")
  (net 26 "Net-(D3-Pad2)")
  (net 27 "Net-(D3-Pad1)")
  (net 28 /VSS)
  (net 29 "Net-(J3-Pad2)")
  (net 30 /UDPI)
  (net 31 "Net-(U3-Pad6)")
  (net 32 "Net-(U3-Pad7)")
  (net 33 /INT)
  (net 34 "Net-(U3-Pad12)")
  (net 35 /01)
  (net 36 /02)
  (net 37 /13)
  (net 38 /14)
  (net 39 /15)
  (net 40 /16)
  (net 41 /17)
  (net 42 "Net-(U3-Pad20)")
  (net 43 "Net-(U3-Pad5)")
  (net 44 /SCL)
  (net 45 /SDA)
  (net 46 "Net-(U3-Pad9)")
  (net 47 "Net-(U3-Pad10)")
  (net 48 "Net-(U3-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /01)
    (add_net /02)
    (add_net /03)
    (add_net /04)
    (add_net /05)
    (add_net /06)
    (add_net /07)
    (add_net /08)
    (add_net /09)
    (add_net /10)
    (add_net /11)
    (add_net /12)
    (add_net /13)
    (add_net /14)
    (add_net /15)
    (add_net /16)
    (add_net /17)
    (add_net /18)
    (add_net /19)
    (add_net /20)
    (add_net /A)
    (add_net /D_IN)
    (add_net /INT)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /PT1_P)
    (add_net /PT2_P)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /UDPI)
    (add_net /VSS)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
  )
  (module footprints:Ultrafit2P (layer F.Cu) (tedit 6464F1C5)
    (at 13.75 -9.5 180)
    (fp_text reference J4 (at 4.5 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 5V! (at -4.25 10.5 180) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User))
    (fp_text user 1723101102 (at 1.749984 -15.36 180) (layer F.Fab))
    (fp_text user ULTRAFIT_RA_HEADER,_SINGLE_ROW_-2_CKT (at 1.749984 -12.82 180) (layer F.Fab))
    (fp_text user 1723101102 (at 1.749984 -15.36 180) (layer F.SilkS) hide)
    (fp_text user ULTRAFIT_RA_HEADER,_SINGLE_ROW_-2_CKT (at 1.749984 -12.82 180) (layer F.SilkS) hide)
    (fp_text user NOTE: (at 0 22.55 180) (layer Cmts.User))
    (fp_text user MAXIMUM_PACKAGE_HEIGHT:_8.96_MM (at 0 26.36 180) (layer Cmts.User))
    (fp_text user RECOMMENDED_PCB_THICKNESS:_1.60_-_2.40_MM (at 0 28.9 180) (layer Cmts.User))
    (fp_text user 172310-X1-0X_=_TIN_PLATING (at 0 32.71 180) (layer Cmts.User))
    (fp_text user 172310-X2-0X_=_15_MICROINCH_GOLD_PLATING (at 0 35.25 180) (layer Cmts.User))
    (fp_text user 172310-X3-0X_=_30_MICROINCH_GOLD_PLATING (at 0 37.79 180) (layer Cmts.User))
    (fp_text user "172310-1X-0X:_COLOUR_-_BLACK,_KEY_OPTION_-_KEY A" (at 0 41.6 180) (layer Cmts.User))
    (fp_text user "172310-2X-0X:_COLOUR_-_NATURAL,_KEY_OPTION_-_KEY B" (at 0 44.14 180) (layer Cmts.User))
    (fp_text user 0X_=_NO._OF_CIRCUIT (at 0 47.95 180) (layer Cmts.User))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 +5V))
    (pad 2 thru_hole circle (at 3.500001 0 180) (size 1.52 1.52) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad "" np_thru_hole circle (at 1.75 7.91 180) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 37 -2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 3 0.25) (layer F.Fab))
    (fp_text value 10K (at -1.5 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636E7B24)
    (at 30.2 -19)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value PT1 (at -2.7 0 unlocked) (layer F.SilkS))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 /LED1))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636E7B24)
    (at 33.8 -19 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value PT2 (at -2.95 0 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 /LED2))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module footprints:Harwin_Gecko-G125-FVX1605L0X_2x08_P1.25mm_Vertical (layer F.Cu) (tedit 63781711)
    (at 43 -10 180)
    (descr "Harwin Gecko Connector, 16 pins, dual row female, vertical entry, PN:G125-FVX1605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J1 (at 4.375 -3 180) (layer F.SilkS) hide)
    (fp_text value 40672 (at 4.75 4.25 180) (layer F.SilkS))
    (fp_text user %R (at 4.375 0 180) (layer F.Fab))
    (fp_text user G125-FV11605L0P (at 4 3) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 28 /VSS))
    (pad 2 thru_hole circle (at 1.25 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 28 /VSS))
    (pad 3 thru_hole circle (at 2.5 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 28 /VSS))
    (pad 4 thru_hole circle (at 3.75 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 28 /VSS))
    (pad 5 thru_hole circle (at 5 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 28 /VSS))
    (pad 6 thru_hole circle (at 6.25 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 22 /D_IN))
    (pad 7 thru_hole circle (at 7.5 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 8 thru_hole circle (at 8.75 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 9 thru_hole circle (at 0 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 10 thru_hole circle (at 1.25 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 11 thru_hole circle (at 2.5 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 12 thru_hole circle (at 3.75 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 13 thru_hole circle (at 5 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 23 /PT1_P))
    (pad 14 thru_hole circle (at 6.25 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 15 thru_hole circle (at 7.5 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 24 /PT2_P))
    (pad 16 thru_hole circle (at 8.75 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (model ${KIPRJMOD}/3D/G125-FV11605L0P.stp
      (offset (xyz 4.5 -0.5 2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical (layer F.Cu) (tedit 6378182F)
    (at 24 -11.25)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J2 (at 1.25 4.3) (layer F.SilkS) hide)
    (fp_text value 40577 (at 1.5 -3) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (fp_text user G125-FV10605L0P (at 1 3) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 22 /D_IN))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 4 thru_hole circle (at 0 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 28 /VSS))
    (pad 5 thru_hole circle (at 1.25 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 23 /PT1_P))
    (pad 6 thru_hole circle (at 2.5 1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 GND))
    (model ${KIPRJMOD}/3D/G125-FV10605L0P.stp
      (offset (xyz 1 -0.5 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 24.25 -19)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 40 -19 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 1K (at -1.905 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:DFN-8-1EP_3x2mm (layer F.Cu) (tedit 638826C0)
    (at 40.5 -2)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -2.55 180) (layer F.SilkS) hide)
    (fp_text value 24LC32 (at 0 2 180) (layer F.SilkS))
    (fp_text user %R (at -1.5 0 270) (layer F.Fab))
    (pad "" smd rect (at 0.325 0.375) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at 0.325 -0.375) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 0.375) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 -0.375) (size 0.5 0.6) (layers F.Paste))
    (pad 9 smd rect (at 0 0) (size 1.3 1.5) (layers F.Cu F.Mask))
    (pad 8 smd rect (at 1.45 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 7 smd rect (at 1.45 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at 1.45 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /SCL))
    (pad 5 smd rect (at 1.45 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /SDA))
    (pad 4 smd rect (at -1.45 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 3 smd rect (at -1.45 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 2 smd rect (at -1.45 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 1 smd rect (at -1.45 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MEC8-113-CARD_2 locked (layer F.Cu) (tedit 637EA67F)
    (at 0 -0.1 90)
    (fp_text reference X0 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer F.Fab))
    (fp_line (start -1 47.5) (end -1 7.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 21 50.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 10 51.5) (end 11.5 51.5) (angle -180) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 50.5) (end 20 51.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 50.5) (end -1 50.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 7.5) (end 0 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 7.5) (end 21 7.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 18.5 5.5) (end 17.5 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 1.5 5.5) (end 1.5 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.4 5.5) (end 8.4 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.8 5.5) (end 9.8 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 7.9 0.5) (end 8.4 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 11.3 0.5) (end 11.3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 17 0.5) (end 17.5 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 3 0.5) (end 3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (pad 14 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /11))
    (pad 1 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 35 /01))
    (pad 15 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /12))
    (pad 2 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 36 /02))
    (pad 16 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 37 /13))
    (pad 3 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 13 /03))
    (pad 17 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 38 /14))
    (pad 4 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 2 /04))
    (pad 18 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 39 /15))
    (pad 5 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /05))
    (pad 19 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 40 /16))
    (pad 6 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /06))
    (pad 20 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 41 /17))
    (pad 7 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 5 /07))
    (pad 21 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /18))
    (pad 8 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /08))
    (pad 22 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /19))
    (pad 9 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /09))
    (pad 23 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /20))
    (pad 10 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 /10))
    (pad 24 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 44 /SCL))
    (pad 11 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 33 /INT))
    (pad 25 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 45 /SDA))
    (pad 12 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 17 /A))
    (pad 26 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (pad 13 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +5V))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 29.25 -2.275 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.225 0 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 3 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 +5V))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 17.75 -2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 1uF (at 2.475 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603 (layer F.Cu) (tedit 636E7B24)
    (at 38.25 -4.5)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 2.032 0) (layer F.SilkS) hide)
    (fp_text value LED (at 0 -1.25 unlocked) (layer F.SilkS))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x03_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 45.25 -2 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (fp_text reference J3 (at -2 -1 180) (layer F.SilkS) hide)
    (fp_text value +UDPI- (at -2 2 180) (layer F.SilkS))
    (fp_text user %R (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 +5V))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x03_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 49.25 -4.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 100 (at 0 1.25 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /UDPI))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 46 -4.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 10K (at 0 1.25 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 42.25 -4.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 1K (at 0 -1.25) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 23.25 -3.25 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 1.25 3.25) (layer F.SilkS) hide)
    (fp_text value INA219AxD (at -0.25 -3.25) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 GND))
    (pad 2 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 GND))
    (pad 3 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /SDA))
    (pad 4 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /SCL))
    (pad 5 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 +5V))
    (pad 6 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 GND))
    (pad 7 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /VSS))
    (pad 8 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm (layer F.Cu) (tedit 5DC5F6A8)
    (at 33 -2.75)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (attr smd)
    (fp_text reference U3 (at 0 -2.8) (layer F.SilkS) hide)
    (fp_text value ATtiny816 (at 0 2.8) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd custom (at -1.45 -0.8) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 24 /PT2_P)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.299289 -0.05) (xy 0.35 0.000711) (xy 0.35 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 2 smd roundrect (at -1.45 -0.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /PT1_P))
    (pad 3 smd roundrect (at -1.45 0) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 GND))
    (pad 4 smd roundrect (at -1.45 0.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 +5V))
    (pad 5 smd custom (at -1.45 0.8) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U3-Pad5)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.35 -0.05) (xy 0.35 -0.000711) (xy 0.299289 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 6 smd custom (at -0.8 1.45) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U3-Pad6)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.299289) (xy 0.000711 -0.35) (xy 0.05 -0.35) (xy 0.05 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 7 smd roundrect (at -0.4 1.45) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(U3-Pad7)"))
    (pad 8 smd roundrect (at 0 1.45) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(U3-Pad8)"))
    (pad 9 smd roundrect (at 0.4 1.45) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(U3-Pad9)"))
    (pad 10 smd custom (at 0.8 1.45) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U3-Pad10)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy -0.000711 -0.35) (xy 0.05 -0.299289) (xy 0.05 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 11 smd custom (at 1.45 0.8) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 33 /INT)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 -0.05) (xy 0.35 -0.05) (xy 0.35 0.05) (xy -0.299289 0.05) (xy -0.35 -0.000711)
) (width 0.1))
      ))
    (pad 12 smd roundrect (at 1.45 0.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(U3-Pad12)"))
    (pad 13 smd roundrect (at 1.45 0) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /SDA))
    (pad 14 smd roundrect (at 1.45 -0.4) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /SCL))
    (pad 15 smd custom (at 1.45 -0.8) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad1)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.35 0.000711) (xy -0.299289 -0.05) (xy 0.35 -0.05) (xy 0.35 0.05) (xy -0.35 0.05)
) (width 0.1))
      ))
    (pad 16 smd custom (at 0.8 -1.45) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 22 /D_IN)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy 0.05 -0.35) (xy 0.05 0.299289) (xy -0.000711 0.35) (xy -0.05 0.35)
) (width 0.1))
      ))
    (pad 17 smd roundrect (at 0.4 -1.45) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /LED2))
    (pad 18 smd roundrect (at 0 -1.45) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /LED1))
    (pad 19 smd roundrect (at -0.4 -1.45) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /UDPI))
    (pad 20 smd custom (at -0.8 -1.45) (size 0.143431 0.143431) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U3-Pad20)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.35) (xy 0.05 -0.35) (xy 0.05 0.35) (xy 0.000711 0.35) (xy -0.05 0.299289)
) (width 0.1))
      ))
    (pad 21 smd rect (at 0 0) (size 1.7 1.7) (layers F.Cu F.Mask)
      (net 14 GND))
    (pad "" smd roundrect (at -0.425 -0.425) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 0.425) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 -0.425) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425) (size 0.69 0.69) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 12.5 -2.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 0 (at 0.0125 1.2 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 30.5 -9.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 10K (at 0.25 1.25 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /PT2_P))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 30.5 -12 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 10K (at 0 -1.25 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /PT1_P))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 12.2 -2.5 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -2.62) (layer F.SilkS) hide)
    (fp_text value 0.1 (at -0.2625 -2.45) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.178571)
      (net 28 /VSS))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.178571)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Rev 0.1\nMay 2023" (at 13.5 -1.25) (layer B.SilkS))
  (gr_text "Molex UltraFit\n1723101102" (at 12.3 -12.5) (layer B.SilkS))
  (gr_text ken.olsen@agilityrobotics.com (at 27 -1.5) (layer B.SilkS))
  (gr_text "LED PCBA TESTER" (at 32 -16.5) (layer F.SilkS))
  (gr_text "Rapid Prototyping Card" (at 27 -3) (layer B.SilkS))
)
